(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-2")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 63)
    (zones 0)
    (modules 13)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.3 3.1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J13-Pad3)")
  (net 3 "Net-(J13-Pad5)")
  (net 4 "Net-(J13-Pad7)")
  (net 5 "Net-(J13-Pad9)")
  (net 6 "Net-(J13-Pad2)")
  (net 7 "Net-(J13-Pad4)")
  (net 8 "Net-(J13-Pad6)")
  (net 9 "Net-(J10-Pad1)")
  (net 10 "Net-(J11-Pad1)")
  (net 11 "Net-(J12-Pad1)")
  (net 12 "Net-(J13-Pad8)")
  (net 13 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad2)")
    (add_net "Net-(J13-Pad3)")
    (add_net "Net-(J13-Pad4)")
    (add_net "Net-(J13-Pad5)")
    (add_net "Net-(J13-Pad6)")
    (add_net "Net-(J13-Pad7)")
    (add_net "Net-(J13-Pad8)")
    (add_net "Net-(J13-Pad9)")
  )
  (module Connector_FFC-FPC:TE_1-1734839-2_1x12-1MP_P0.5mm_Horizontal (layer F.Cu) (tedit 5EC60BBC)
    (at 0 0)
    (descr "TE FPC connector, 12 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0")
    (tags "te fpc 1734839")
    (attr smd)
    (fp_text reference J13 (at 0 -3.1) (layer F.SilkS) hide)
    (fp_text value Conn_01x13_Male (at 0 3.25) (layer Dwgs.User))
    (fp_text user %R (at 0 1.55) (layer F.Fab))
    (pad 13 smd rect (at 4.42 0.35) (size 2.3 3.1) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 13 smd rect (at -4.42 0.35) (size 2.3 3.1) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 12 smd rect (at 2.75 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J12-Pad1)"))
    (pad 11 smd rect (at 2.25 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J11-Pad1)"))
    (pad 10 smd rect (at 1.75 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J10-Pad1)"))
    (pad 9 smd rect (at 1.25 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J13-Pad9)"))
    (pad 8 smd rect (at 0.75 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J13-Pad8)"))
    (pad 7 smd rect (at 0.25 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J13-Pad7)"))
    (pad 6 smd rect (at -0.25 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J13-Pad6)"))
    (pad 5 smd rect (at -0.75 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J13-Pad5)"))
    (pad 4 smd rect (at -1.25 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J13-Pad4)"))
    (pad 3 smd rect (at -1.75 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J13-Pad3)"))
    (pad 2 smd rect (at -2.25 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J13-Pad2)"))
    (pad 1 smd rect (at -2.75 -1.35) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_1-1734839-2_1x12-1MP_P0.5mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 5 -4)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J12 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 11 "Net-(J12-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 5 -10)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J10 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 9 "Net-(J10-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 1.75 -7)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J8 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 12 "Net-(J13-Pad8)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at -1.75 -10)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J6 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 8 "Net-(J13-Pad6)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at -1.75 -4)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J4 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 7 "Net-(J13-Pad4)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at -5 -7)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J2 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 6 "Net-(J13-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 5 -7)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J11 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 10 "Net-(J11-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 1.75 -4)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J9 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 5 "Net-(J13-Pad9)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 1.75 -10)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J7 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 4 "Net-(J13-Pad7)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at -1.75 -7)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J5 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 3 "Net-(J13-Pad5)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at -5 -10)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J3 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 "Net-(J13-Pad3)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at -5 -4)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J1 (at 0 -1.648) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (gr_text "makho\n12P-FPC" (at -4 -3.4 90) (layer B.Mask))
  (gr_arc (start 5 0.7) (end 5 2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -5 0.7) (end -6.3 0.7) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -5 -11) (end -5 -12.3) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 5 -11) (end 6.3 -11) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -5 -12.3) (end 5 -12.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -6.3 0.7) (end -6.3 -11) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5 2) (end -5 2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 6.3 -11) (end 6.3 0.7) (layer Edge.Cuts) (width 0.05))
  (zone (net 13) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6.3 2) (xy -6.3 2) (xy -6.3 -12.3) (xy 6.3 -12.3)
      )
    )
  )
  (zone (net 13) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6.3 2) (xy -6.3 2) (xy -6.3 -12.3) (xy 6.3 -12.3)
      )
    )
  )
)
