(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 27)
    (zones 0)
    (modules 4)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 "Net-(JA1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(JCS1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(JA1-Pad2)")
    (add_net "Net-(JCS1-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
  )
  (module dfr0299:MODULE_DFR0299 (layer F.Cu) (tedit 5E591AAC)
    (at 130.556 105.156 270)
    (fp_text reference U1 (at -2.032 -1.524 180) (layer F.SilkS) hide)
    (fp_text value DFR0299 (at -1.51 11.065 90) (layer F.Fab))
    (pad 9 thru_hole circle (at 9.017 8.89 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(JCS1-Pad2)"))
    (pad 8 thru_hole circle (at -9.017 8.89 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(JA1-Pad2)"))
    (pad 16 thru_hole circle (at 9.017 -8.89 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -9.017 -8.89 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 10 thru_hole circle (at 9.017 6.35 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole circle (at -9.017 6.35 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 15 thru_hole circle (at 9.017 -6.35 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -9.017 -6.35 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 9.017 3.81 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 9.017 -3.81 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -9.017 -3.81 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -9.017 3.81 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 9.017 1.27 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 9.017 -1.27 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -9.017 1.27 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -9.017 -1.27 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module Connector_JST:JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical (layer B.Cu) (tedit 5B7745C2)
    (at 138.176 110.744 90)
    (descr "JST PH series connector, B3B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (fp_text reference Sensor (at 2 -4.572 270) (layer B.SilkS))
    (fp_text value Conn_01x03_Male (at 2 -4 90) (layer B.Fab))
    (fp_text user %R (at 2 -1.5 90) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(JCS1-Pad2)"))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical (layer B.Cu) (tedit 5B7745C2)
    (at 138.176 101.6 90)
    (descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (fp_text reference Battery (at 1 -4.572 270) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 1 -4 270) (layer B.Fab))
    (fp_text user %R (at 1 -1.5 270) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical (layer B.Cu) (tedit 5B7745C2)
    (at 122.936 103.632 270)
    (descr "JST PH series connector, B3B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (fp_text reference Amplifier (at 2.032 -4.572 270) (layer B.SilkS))
    (fp_text value Conn_01x03_Male (at 2 -4 270) (layer B.Fab))
    (fp_text user %R (at 2 -1.5 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(JA1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "DfPlayer Mini\nBreakout Board" (at 130.556 104.648) (layer F.SilkS))
  (gr_line (start 142.24 116.84) (end 142.24 93.472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.872 116.84) (end 142.24 116.84) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.872 93.472) (end 118.872 116.84) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.24 93.472) (end 118.872 93.472) (layer Edge.Cuts) (width 0.1))
)
