(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 154)
    (no_connects 0)
    (area 116.957857 94.655 164.982143 123.341667)
    (thickness 1.6)
    (drawings 10)
    (tracks 150)
    (zones 0)
    (modules 122)
    (nets 31)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (35 F.Paste user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7)
    (via_drill 0.35)
    (via_min_size 0.7)
    (via_min_drill 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.7 0.7)
    (pad_drill 0.35)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (grid_origin 118.11 121.92)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GNDD)
  (net 3 VAA)
  (net 4 GNDA)
  (net 5 M1)
  (net 6 M2)
  (net 7 "Net-(Q1-Pad4)")
  (net 8 "Net-(Q2-Pad4)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(R2-Pad2)")
  (net 11 OUTB)
  (net 12 "Net-(R4-Pad2)")
  (net 13 "Net-(R5-Pad2)")
  (net 14 OUTA)
  (net 15 "Net-(R7-Pad1)")
  (net 16 "Net-(R8-Pad2)")
  (net 17 "Net-(R9-Pad1)")
  (net 18 "Net-(R10-Pad1)")
  (net 19 "Net-(R11-Pad2)")
  (net 20 "Net-(R12-Pad1)")
  (net 21 "Net-(R13-Pad1)")
  (net 22 T1)
  (net 23 "Net-(R14-Pad1)")
  (net 24 T2)
  (net 25 "Net-(R15-Pad2)")
  (net 26 "Net-(R18-Pad2)")
  (net 27 "Net-(R19-Pad2)")
  (net 28 "Net-(R20-Pad2)")
  (net 29 ONB)
  (net 30 ONA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.7)
    (via_drill 0.35)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net M1)
    (add_net M2)
  )
  (net_class Driver ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.7)
    (via_drill 0.35)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Q2-Pad4)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R8-Pad2)")
  )
  (net_class Medium ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.7)
    (via_drill 0.35)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDA)
    (add_net GNDD)
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net ONA)
    (add_net ONB)
    (add_net OUTA)
    (add_net OUTB)
    (add_net T1)
    (add_net T2)
    (add_net VAA)
    (add_net VDD)
  )
  (net_class Thick ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1.4)
    (via_drill 0.7)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 149.606 108.966)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 149.606 109.728)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 150.368 108.966)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 150.368 109.728)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 151.13 108.966)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 151.13 109.728)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 143.256 98.425)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 142.494 98.425)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 141.605 113.03)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 141.605 113.792)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 144.145 114.681)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 144.145 113.919)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 144.018 112.395)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 143.256 112.395)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 144.018 111.633)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 143.256 111.633)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 140.081 106.045)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 140.843 106.045)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EBAA)
    (at 140.843 106.045)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 141.605 100.711)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 141.605 101.473)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7EAE3)
    (at 141.605 102.235)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 3 VAA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module gate_drivers:PG-TSSOP-8 (layer Top) (tedit 57F8018B)
    (at 143.51 106.045 180)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference U3 (at -2.794 2.159 360) (layer F.SilkS))
    (fp_text value 2EDN8524R (at 0 0 180) (layer F.Fab))
    (pad 8 smd rect (at -0.975 -2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 26 "Net-(R18-Pad2)"))
    (pad 1 smd rect (at -0.975 2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 25 "Net-(R15-Pad2)"))
    (pad 7 smd rect (at -0.325 -2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 27 "Net-(R19-Pad2)"))
    (pad 2 smd rect (at -0.325 2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 16 "Net-(R8-Pad2)"))
    (pad 6 smd rect (at 0.325 -2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (pad 3 smd rect (at 0.325 2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 5 smd rect (at 0.975 -2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 28 "Net-(R20-Pad2)"))
    (pad 4 smd rect (at 0.975 2.2 180) (size 0.4 1.3) (layers Top F.Paste F.Mask)
      (net 19 "Net-(R11-Pad2)"))
    (pad 9 smd rect (at 0 0 180) (size 2.05 1.75) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57EFEB4F)
    (at 141.732 116.586)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57EFEB4F)
    (at 141.732 115.824)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57EFEB4F)
    (at 144.018 115.824)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 145.415 116.967)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 144.145 117.856)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 139.446 110.871)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 139.446 110.109)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 140.208 110.109)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 140.208 110.871)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 145.288 103.505)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E855)
    (at 146.05 103.505)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E850)
    (at 146.05 104.267)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 145.288 104.267)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 151.13 113.665)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 150.368 113.665)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 149.606 113.665)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 151.13 114.427)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 150.368 114.427)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 149.606 114.427)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 147.955 106.807)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.082 118.237)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.082 117.475)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.082 116.713)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.082 115.951)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.082 115.189)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.082 113.665)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.082 114.427)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.844 114.427)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.844 113.665)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 147.955 102.997)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 147.955 102.235)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.844 102.997)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 149.606 102.997)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 150.368 102.997)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 151.13 102.997)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 151.13 102.235)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 150.368 102.235)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 149.606 102.235)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 148.844 102.235)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 147.955 106.045)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 147.955 103.759)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 147.955 104.521)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 147.955 105.283)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 145.288 107.315)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 145.288 106.553)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 145.288 105.791)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 145.288 105.029)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 141.732 107.315)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 141.732 106.553)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 141.732 105.791)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 141.732 105.029)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7E386)
    (at 141.605 114.808)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (solder_mask_margin -1) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57EFEB4F)
    (at 141.605 117.475)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57EFEB4F)
    (at 144.018 116.586)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F7FF39)
    (at 123.825 119.38 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -2.286 0.762 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 14 OUTA))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 57F7FF2F)
    (at 123.825 109.22 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value "100n 50V" (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 57F7FFB3)
    (at 142.875 100.33 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value "100n 50V" (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 57F80066)
    (at 142.24 110.49 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.762 1.397 180) (layer F.SilkS))
    (fp_text value "100n 50V" (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 57F80040)
    (at 142.875 115.062 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.032 0.127 360) (layer F.SilkS))
    (fp_text value "1µ 50V" (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mosfet:Power56 (layer Top) (tedit 57F800AC)
    (at 151.892 106.045 270)
    (fp_text reference Q1 (at 2.667 -0.254 360) (layer F.SilkS))
    (fp_text value FDMS7660ASCT (at 0 -5.2 270) (layer F.Fab))
    (pad PAD smd rect (at 0 -0.66 270) (size 3.91 3.75) (layers Top F.Paste F.Mask)
      (net 5 M1))
    (pad 8 smd rect (at -1.905 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 5 M1))
    (pad 7 smd rect (at -0.635 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 5 M1))
    (pad 6 smd rect (at 0.635 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 5 M1))
    (pad 5 smd rect (at 1.905 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 5 M1))
    (pad 4 smd rect (at 1.905 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad4)"))
    (pad 3 smd rect (at 0.635 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at -0.635 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 1 smd rect (at -1.905 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
  )
  (module mosfet:Power56 (layer Top) (tedit 57F8001F)
    (at 151.892 117.475 270)
    (fp_text reference Q2 (at 3.429 0 360) (layer F.SilkS))
    (fp_text value FDMS7660ASCT (at 0 -5.2 270) (layer F.Fab))
    (pad PAD smd rect (at 0 -0.66 270) (size 3.91 3.75) (layers Top F.Paste F.Mask)
      (net 6 M2))
    (pad 8 smd rect (at -1.905 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 6 M2))
    (pad 7 smd rect (at -0.635 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 6 M2))
    (pad 6 smd rect (at 0.635 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 6 M2))
    (pad 5 smd rect (at 1.905 -2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 6 M2))
    (pad 4 smd rect (at 1.905 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad4)"))
    (pad 3 smd rect (at 0.635 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at -0.635 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 1 smd rect (at -1.905 2.67 270) (size 0.61 1.27) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F7FED3)
    (at 124.46 102.235)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 470R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F7FF35)
    (at 123.825 114.3)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.286 -0.635) (layer F.SilkS))
    (fp_text value 0R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 10 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F7FF33)
    (at 123.825 111.76 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.286 0.889 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 11 OUTB))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F7FEDA)
    (at 124.46 104.775)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.524) (layer F.SilkS))
    (fp_text value 470R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F7FF37)
    (at 123.825 116.84)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.286 -0.635) (layer F.SilkS))
    (fp_text value 0R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F801C0)
    (at 139.7 102.235)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -1.778 -1.27) (layer F.SilkS))
    (fp_text value 0R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 15 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F801C2)
    (at 139.7 99.695 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 1.778 1.27 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 16 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F801B1)
    (at 139.7 115.062)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -2.54 -2.032) (layer F.SilkS))
    (fp_text value 1k8 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 17 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F801C4)
    (at 139.7 104.775)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -1.524 -1.27) (layer F.SilkS))
    (fp_text value 0R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 18 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F801C7)
    (at 139.7 107.315 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 1.524 1.27 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 19 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F8019F)
    (at 139.7 117.221)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -2.286 -1.651) (layer F.SilkS))
    (fp_text value 1k8 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 20 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F801A4)
    (at 139.7 119.38)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at -2.286 -1.27) (layer F.SilkS))
    (fp_text value 0R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 21 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 22 T1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F801B4)
    (at 139.7 112.776)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at -2.286 -2.286) (layer F.SilkS))
    (fp_text value 0R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 23 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 24 T2))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F800C4)
    (at 145.034 100.33 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 25 "Net-(R15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F8000D)
    (at 145.415 118.872 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 24 T2))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F80000)
    (at 142.875 118.872 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 22 T1))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F800CC)
    (at 147.193 100.33 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 26 "Net-(R18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F802A1)
    (at 146.05 110.109 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at -2.159 1.143 180) (layer F.SilkS))
    (fp_text value "0R | 10R" (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad4)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 27 "Net-(R19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F8017E)
    (at 146.05 112.141 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at -0.889 -1.397 180) (layer F.SilkS))
    (fp_text value "0 | 10R" (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad4)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 28 "Net-(R20-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F80090)
    (at 146.685 106.045 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 2.032 0 360) (layer F.SilkS))
    (fp_text value DNI (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer Top) (tedit 57F80175)
    (at 145.415 115.062 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at -2.032 1.397 180) (layer F.SilkS))
    (fp_text value DNI (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers Top F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "optocouplers:SMT-8 MCT6" (layer Top) (tedit 57F7FFA5)
    (at 132.08 103.505 90)
    (fp_text reference U1 (at 5.461 -3.302 180) (layer F.SilkS))
    (fp_text value MCT62SDCT (at 7.62 0 180) (layer F.Fab))
    (pad 8 smd rect (at 3.81 4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 16 "Net-(R8-Pad2)"))
    (pad 7 smd rect (at 1.27 4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 15 "Net-(R7-Pad1)"))
    (pad 6 smd rect (at -1.27 4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 18 "Net-(R10-Pad1)"))
    (pad 5 smd rect (at -3.81 4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 19 "Net-(R11-Pad2)"))
    (pad 4 smd rect (at -3.81 -4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 29 ONB))
    (pad 3 smd rect (at -1.27 -4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at 1.27 -4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at 3.81 -4.6 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 30 ONA))
  )
  (module "optocouplers:SMT-8 MCT6" (layer Top) (tedit 57F7FF0D)
    (at 132.08 115.57 270)
    (fp_text reference U2 (at 5.588 -3.302 360) (layer F.SilkS))
    (fp_text value MCT62SDCT (at 0 -7.2 270) (layer F.Fab))
    (pad 8 smd rect (at 3.81 4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 14 OUTA))
    (pad 7 smd rect (at 1.27 4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at -1.27 4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 10 "Net-(R2-Pad2)"))
    (pad 5 smd rect (at -3.81 4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 11 OUTB))
    (pad 4 smd rect (at -3.81 -4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 23 "Net-(R14-Pad1)"))
    (pad 3 smd rect (at -1.27 -4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 17 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 1.27 -4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 20 "Net-(R12-Pad1)"))
    (pad 1 smd rect (at 3.81 -4.6 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 21 "Net-(R13-Pad1)"))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F7FEA3)
    (at 120.015 107.95)
    (fp_text reference X1 (at 1.778 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F7FE85)
    (at 120.015 115.57)
    (fp_text reference X2 (at 1.778 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDD))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F7FE8D)
    (at 120.015 110.49)
    (fp_text reference X3 (at 1.778 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 OUTA))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F7FE88)
    (at 120.015 113.03)
    (fp_text reference X4 (at 1.778 0 180) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 OUTB))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F7FEAD)
    (at 120.015 102.87)
    (fp_text reference X5 (at 1.778 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 ONA))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F7FE92)
    (at 120.015 105.41)
    (fp_text reference X6 (at 1.778 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 ONB))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F80150)
    (at 161.925 120.015)
    (fp_text reference X7 (at -1.651 -0.762) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 T1))
  )
  (module solderpads:THTPAD-1x2 (layer Top) (tedit 57F8014C)
    (at 158.115 120.015)
    (fp_text reference X8 (at -1.778 -0.762) (layer F.SilkS))
    (fp_text value wirepad (at 0 -2.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 T2))
  )
  (module solderpads:THTPAD-2x4 (layer Top) (tedit 57F80139)
    (at 160.02 106.045)
    (fp_text reference X9 (at -3.429 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 5 M1))
  )
  (module solderpads:THTPAD-2x4 (layer Top) (tedit 57F80128)
    (at 160.02 116.205)
    (fp_text reference X10 (at -3.302 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 6 M2))
  )
  (module solderpads:THTPAD-2x4 (layer Top) (tedit 57F80140)
    (at 160.02 100.965)
    (fp_text reference X11 (at -3.302 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 VAA))
  )
  (module solderpads:THTPAD-2x4 (layer Top) (tedit 57F80130)
    (at 160.02 111.125)
    (fp_text reference X12 (at -3.175 0) (layer F.SilkS))
    (fp_text value wirepad (at 0 -3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 GNDA))
  )
  (module vias:VIA-0.7x0.35 (layer Top) (tedit 57F7F286)
    (at 147.32 120.65)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.7x0.35 (at 0 -0.5) (layer F.Fab) hide)
  )
  (module diodes:SMB (layer Top) (tedit 57F80204)
    (at 151.892 111.76 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D2 (at -0.381 -2.667 180) (layer F.SilkS))
    (fp_text value B360B-FDICT (at 0.05 4.7 180) (layer F.Fab))
    (fp_text user K (at -3.1 1.7 180) (layer F.SilkS))
    (fp_text user A (at 3 1.7 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers Top F.Paste F.Mask)
      (net 6 M2))
    (pad 2 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Diodes_SMD.3dshapes/SMB_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module diodes:SMB (layer Top) (tedit 57F80204)
    (at 151.892 100.33 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D1 (at -0.381 -2.667 180) (layer F.SilkS))
    (fp_text value B360B-FDICT (at 0.05 4.7 180) (layer F.Fab))
    (fp_text user K (at -3.1 1.7 180) (layer F.SilkS))
    (fp_text user A (at 3 1.7 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers Top F.Paste F.Mask)
      (net 5 M1))
    (pad 2 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers Top F.Paste F.Mask)
      (net 4 GNDA))
    (model Diodes_SMD.3dshapes/SMB_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_line (start 163.068 97.155) (end 118.872 97.155) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.83 97.917) (end 163.068 97.155) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.83 121.158) (end 163.83 97.917) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.068 121.92) (end 163.83 121.158) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.872 121.92) (end 163.068 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 121.158) (end 118.872 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 120.904) (end 118.11 121.158) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 120.65) (end 118.11 120.904) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 97.917) (end 118.11 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 97.917) (end 118.872 97.155) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name VDD) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.6))
    (polygon
      (pts
        (xy 118.491 121.539) (xy 129.54 121.539) (xy 129.54 97.536) (xy 118.491 97.536)
      )
    )
  )
  (zone (net 2) (net_name GNDD) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.6))
    (polygon
      (pts
        (xy 118.491 121.539) (xy 129.54 121.539) (xy 129.54 97.536) (xy 118.491 97.536)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 143.383 105.156) (xy 144.907 105.156) (xy 144.907 103.124) (xy 145.669 103.124) (xy 145.669 107.696)
        (xy 144.907 107.696) (xy 144.907 106.934) (xy 142.113 106.934) (xy 142.113 107.696) (xy 141.351 107.696)
        (xy 141.351 104.648) (xy 142.113 104.648) (xy 142.113 105.156) (xy 143.002 105.156) (xy 143.002 103.251)
        (xy 143.383 103.251)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 144.399 116.967) (xy 141.351 116.967) (xy 141.351 115.443) (xy 144.399 115.443)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 141.732 111.252) (xy 139.065 111.252) (xy 139.065 109.728) (xy 141.732 109.728)
      )
    )
  )
  (zone (net 3) (net_name VAA) (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.6))
    (polygon
      (pts
        (xy 163.449 121.539) (xy 134.747 121.539) (xy 134.747 97.536) (xy 163.449 97.536)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 151.003 101.854) (xy 151.511 101.854) (xy 151.511 103.505) (xy 149.86 103.505) (xy 149.86 106.934)
        (xy 148.336 106.934) (xy 148.336 107.188) (xy 147.574 107.188) (xy 147.574 101.854) (xy 148.463 101.854)
        (xy 148.463 99.187) (xy 151.003 99.187)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 151.003 113.284) (xy 151.511 113.284) (xy 151.511 114.935) (xy 149.86 114.935) (xy 149.86 118.364)
        (xy 148.463 118.364) (xy 148.463 118.618) (xy 147.701 118.618) (xy 147.701 113.284) (xy 148.463 113.284)
        (xy 148.463 110.617) (xy 151.003 110.617)
      )
    )
  )
  (zone (net 6) (net_name M2) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 155.321 114.046) (xy 161.036 114.046) (xy 162.052 115.062) (xy 162.052 117.348) (xy 161.036 118.364)
        (xy 157.099 118.364) (xy 155.829 119.634) (xy 153.924 119.634) (xy 153.924 119.38) (xy 150.749 119.38)
        (xy 150.749 115.57) (xy 152.781 115.57) (xy 152.781 113.284) (xy 152.781 110.617) (xy 155.321 110.617)
      )
    )
  )
  (zone (net 5) (net_name M1) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 155.321 103.886) (xy 160.909 103.886) (xy 162.179 105.156) (xy 162.179 106.934) (xy 160.909 108.204)
        (xy 153.924 108.204) (xy 153.924 107.95) (xy 150.749 107.95) (xy 150.749 104.14) (xy 152.781 104.14)
        (xy 152.781 99.187) (xy 155.321 99.187)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer Bottom) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.6))
    (polygon
      (pts
        (xy 163.449 121.539) (xy 134.747 121.539) (xy 134.747 97.536) (xy 163.449 97.536)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 143.51 99.822) (xy 142.24 99.822) (xy 142.24 98.171) (xy 143.51 98.171)
      )
    )
  )
  (zone (net 3) (net_name VAA) (layer Bottom) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 141.986 104.521) (xy 141.224 104.521) (xy 141.224 106.426) (xy 139.7 106.426) (xy 139.7 105.664)
        (xy 139.7 100.33) (xy 141.986 100.33)
      )
    )
  )
  (zone (net 3) (net_name VAA) (layer Bottom) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 151.511 110.109) (xy 148.59 113.03) (xy 147.574 113.03) (xy 145.542 115.062) (xy 143.002 115.062)
        (xy 142.113 114.173) (xy 141.224 114.173) (xy 141.224 112.649) (xy 142.875 112.649) (xy 142.875 111.252)
        (xy 146.558 111.252) (xy 149.225 108.585) (xy 151.511 108.585)
      )
    )
  )
)
