<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.635" y1="-0.635" x2="31.115" y2="-0.635" width="0" layer="20"/>
<wire x1="31.115" y1="-0.635" x2="31.115" y2="31.115" width="0" layer="20"/>
<wire x1="31.115" y1="31.115" x2="-0.635" y2="31.115" width="0" layer="20"/>
<wire x1="-0.635" y1="31.115" x2="-0.635" y2="-0.635" width="0" layer="20"/>
<text>TSL1401CL Adapter</text>
<text>Karl Bellve</text>
<text>Biomedical Imaging Group</text>
<text>Program in Molecular Medicine</text>
<text>University of Massachusetts</text>
<text>Medical School</text>
<text>September 30, 2013</text>
<text>GND</text>
<text>AO</text>
<text>SI</text>
<text>CLK</text>
<text>5V</text>
<text>Four Board Holes are 3.175mm (1/8") in diameter</text>
</plain>
<libraries>
<library name="BIG">
<packages>
<package name="TSL1401CL">
<description>TSL1401CL    SMD Version of the TSL1401</description>
</package>
<package name="M05JST-PTH">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="BIG" package="TSL1401CL" value="TSL1401CL"/>
<element name="U$2" library="SparkFun" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="1uF (16V)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="BIG" package="M05JST-PTH" value="M05"/>
</elements>
<signals>
<signal name="+5V">
<contactref element="U$1" pad="VDD"/>
<contactref element="C1" pad="1"/>
<contactref element="U$3" pad="P$5"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="SI">
<contactref element="U$1" pad="SI"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="AO">
<contactref element="U$1" pad="AO"/>
<contactref element="U$3" pad="P$4"/>
</signal>
<signal name="CLK">
<contactref element="U$1" pad="CLK"/>
<contactref element="U$3" pad="P$3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
