(kicad_pcb (version 4) (host pcbnew 4.1.0-alpha+201607281302+6996~46~ubuntu14.04.1-product)
  (general
    (links 49)
    (no_connects 0)
    (area 86.899999 86.899999 113.100001 113.100001)
    (thickness 1.6)
    (drawings 12)
    (tracks 168)
    (zones 0)
    (modules 18)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.16)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.9)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 /SBWTCK)
  (net 9 /SBWTDIO)
  (net 10 /RX)
  (net 11 /TX)
  (net 12 /SCL)
  (net 13 /SDA)
  (net 14 /MOSI)
  (net 15 /MISO)
  (net 16 /CLK)
  (net 17 /CS)
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.2)
    (via_dia 0.9)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /CS)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RX)
    (add_net /SBWTCK)
    (add_net /SBWTDIO)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (net_class Power ""
    (clearance 0.18)
    (trace_width 0.25)
    (via_dia 0.9)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class Vbat ""
    (clearance 0.18)
    (trace_width 0.4)
    (via_dia 0.9)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
  )
  (module MSP430FR2532IRGER:MSP430FR2532IRGER (layer F.Cu) (tedit 57D7A397)
    (at 100 100 225)
    (clearance 0.153)
    (fp_text reference U1 (at 0 3.1 225) (layer F.SilkS) hide)
    (fp_text value MSP430FR2532IRGET (at 1.979899 3.252691 225) (layer F.SilkS))
    (fp_text user 7 (at -1.272792 2.687006 225) (layer F.SilkS))
    (fp_text user 1 (at -2.687006 -1.272792 135) (layer F.SilkS))
    (pad 1 smd oval (at -1.899999 -1.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 9 /SBWTDIO))
    (pad 2 smd oval (at -1.899999 -0.750001 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 8 /SBWTCK))
    (pad 3 smd oval (at -1.899999 -0.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 4 smd oval (at -1.899999 0.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 5 smd oval (at -1.899999 0.750001 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 16 /CLK))
    (pad 6 smd oval (at -1.899999 1.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 17 /CS))
    (pad 7 smd oval (at -1.25 1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd oval (at -0.750001 1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd oval (at -0.25 1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 13 /SDA))
    (pad 10 smd oval (at 0.25 1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCL))
    (pad 11 smd oval (at 0.750001 1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd oval (at 1.25 1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd oval (at 1.899999 1.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd oval (at 1.899999 0.750001 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 10 /RX))
    (pad 15 smd oval (at 1.899999 0.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 11 /TX))
    (pad 16 smd oval (at 1.899999 -0.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 17 smd oval (at 1.899999 -0.750001 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd oval (at 1.899999 -1.25 315) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd oval (at 1.25 -1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 20 smd oval (at 0.750001 -1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd oval (at 0.25 -1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 22 smd oval (at -0.25 -1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 23 smd oval (at -0.750001 -1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd oval (at -1.25 -1.899999 225) (size 0.3416 0.701599) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 25 smd rect (at 0 0 225) (size 2.201601 2.201601) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 0 0 225) (size 0.0254 0.0254) (layers F.Cu F.Paste F.Mask))
    (pad V thru_hole circle (at 0 0.800001 225) (size 0.601599 0.601599) (drill 0.2032) (layers *.Cu))
    (pad V thru_hole circle (at 0.800001 0 225) (size 0.601599 0.601599) (drill 0.2032) (layers *.Cu))
    (pad V thru_hole circle (at 0 0 225) (size 0.601599 0.601599) (drill 0.2032) (layers *.Cu))
    (pad V thru_hole circle (at -0.800001 0 225) (size 0.601599 0.601599) (drill 0.2032) (layers *.Cu))
    (pad V thru_hole circle (at 0 -0.800001 225) (size 0.601599 0.601599) (drill 0.2032) (layers *.Cu))
    (pad EP smd rect (at 0 0 225) (size 5 5) (layers B.Cu))
  )
  (module TDFN-8:TDFN-8 (layer F.Cu) (tedit 57D7A39D)
    (at 103.4 94.75)
    (descr "TDFN - 8PIN, 2MMX3MM")
    (tags "TDFN - 8PIN, 2MMX3MM")
    (attr smd)
    (fp_text reference U2 (at -0.98298 -1.20142) (layer F.SilkS) hide)
    (fp_text value CY15B104Q (at 1.4 -1.55) (layer F.SilkS))
    (fp_text user 1 (at -2.1 -1.25) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 -0.7493) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 17 /CS))
    (pad 2 smd rect (at -1.39954 -0.24892) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 3 smd rect (at -1.39954 0.24892) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at -1.39954 0.7493) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.39954 0.7493) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 6 smd rect (at 1.39954 0.24892) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 16 /CLK))
    (pad 7 smd rect (at 1.39954 -0.24892) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 8 smd rect (at 1.39954 -0.7493) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad EP smd rect (at 0 0) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (clearance 0.153))
  )
  (module BME280:BME280 (layer F.Cu) (tedit 57D7A389)
    (at 94 94 270)
    (fp_text reference U3 (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value BME280 (at -1.5 -3.05) (layer F.SilkS))
    (fp_text user 1 (at 1.5 -1.6 270) (layer F.SilkS))
    (pad 1 smd rect (at 1.125 -0.975 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.125 -0.325 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at 1.125 0.325 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 13 /SDA))
    (pad 4 smd rect (at 1.125 0.975 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCL))
    (pad 5 smd rect (at -1.125 0.975 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.125 0.325 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 7 smd rect (at -1.125 -0.325 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -1.125 -0.975 270) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module S8421-45R:S8421-45R (layer B.Cu) (tedit 57D77878)
    (at 100 100)
    (fp_text reference B1 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value CR2032_holder (at 0 0.5) (layer B.Fab))
    (pad 1 smd rect (at 0 -10.7) (size 3.6 3) (layers B.Cu B.Paste B.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0 10.7) (size 2.6 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57D77AA5)
    (at 109.5 99.6 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -2.286 270) (layer F.SilkS) hide)
    (fp_text value Spy-Bi-Wire (at 0 2.5 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.7272 3) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at -1.27 0 270) (size 1.7272 2.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SBWTCK))
    (pad 3 thru_hole oval (at 1.27 0 270) (size 1.7272 2.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SBWTDIO))
    (pad 4 thru_hole oval (at 3.81 0 270) (size 1.7272 2.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57D77AAA)
    (at 93.75 106.25 315)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.286 315) (layer F.SilkS) hide)
    (fp_text value Serial (at -0.005001 -1.8935 315) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 315) (size 1.7272 3) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at -1.27 0 315) (size 1.7272 2.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /RX))
    (pad 3 thru_hole oval (at 1.27 0 315) (size 1.7272 2.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /TX))
    (pad 4 thru_hole oval (at 3.81 0 315) (size 1.7272 2.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D789A1)
    (at 98.1 103.1 225)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -1.7 225) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.06066 225) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0 225) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 225) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D7A3C4)
    (at 104.7 103.2 315)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -1.7 315) (layer F.SilkS) hide)
    (fp_text value 1uF (at 1.909188 -0.070711 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0 315) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 315) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D7A3C7)
    (at 103.3 104.6 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 -1.7 135) (layer F.SilkS) hide)
    (fp_text value 1uF (at -1.909188 0.070711 135) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D788D4)
    (at 100 104.2 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference D1 (at 0 -1.7 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 -1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D7A41D)
    (at 104.6 99.9 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference DC11 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -2.05 0.45 225) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D7A410)
    (at 103.6 99.9 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference DC12 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 1.9 -2.4 315) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D79106)
    (at 95.9 94.1 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference DC31 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 -1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57D78B67)
    (at 94.2 91.6)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference DC32 (at 0 -1.7) (layer F.SilkS) hide)
    (fp_text value 100n (at 2.3 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57D788D0)
    (at 100 106.2 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value 560E (at 0.25 1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57D782BE)
    (at 91.4 95.1)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value 4k7 (at 0 1) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCL))
    (model Resistors_SMD/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57D782C2)
    (at 94.1 96.6)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value 4k7 (at 0 1) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /SDA))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (model Resistors_SMD/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57D7A3E3)
    (at 102.3 102.3 45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference Y1 (at 0 -1.9 45) (layer F.SilkS) hide)
    (fp_text value "32768 Hz" (at 0.035355 3.429468 135) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model Capacitors_SMD/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 107.4 95.8) (layer F.SilkS))
  (gr_text + (at 89.8 102.2 45) (layer F.SilkS))
  (gr_circle (center 100 100) (end 113 100) (layer Edge.Cuts) (width 0.2))
  (gr_text RX (at 94 104.3 45) (layer F.SilkS))
  (gr_text TX (at 95.8 106 45) (layer F.SilkS))
  (gr_text SBW (at 109.5 105.5) (layer F.SilkS))
  (gr_text CK (at 107.9 98.4) (layer F.SilkS))
  (gr_text IO (at 107.9 100.9) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 85 85) (xy 115 85) (xy 115 115) (xy 85 115)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 85 85) (xy 115 85) (xy 115 115) (xy 85 115)
      )
    )
  )
)
