<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>STORMBOTS</text>
<text>Plastic Gadgeteer 
Port Cover</text>
<wire x1="39.878" y1="6.35" x2="9.398" y2="6.35" width="0.1524" layer="20"/>
<wire x1="9.398" y1="6.35" x2="8.89" y2="6.858" width="0.1524" layer="20" curve="-90"/>
<wire x1="8.89" y1="6.858" x2="8.89" y2="17.272" width="0.1524" layer="20"/>
<wire x1="8.89" y1="17.272" x2="8.382" y2="17.78" width="0.1524" layer="20" curve="90"/>
<wire x1="8.382" y1="17.78" x2="8.128" y2="17.78" width="0.1524" layer="20"/>
<wire x1="8.128" y1="17.78" x2="7.62" y2="18.288" width="0.1524" layer="20" curve="-90"/>
<wire x1="7.62" y1="18.288" x2="7.62" y2="32.004" width="0.1524" layer="20"/>
<wire x1="7.62" y1="32.004" x2="8.128" y2="32.512" width="0.1524" layer="20" curve="-90"/>
<wire x1="8.128" y1="32.512" x2="41.445578125" y2="32.512" width="0.1524" layer="20"/>
<wire x1="41.445578125" y1="32.512" x2="41.804790625" y2="32.363209375" width="0.1524" layer="20" curve="-45.000249"/>
<wire x1="41.804790625" y1="32.363209375" x2="43.031209375" y2="31.136790625" width="0.1524" layer="20"/>
<wire x1="43.031209375" y1="31.136790625" x2="43.390421875" y2="30.988" width="0.1524" layer="20" curve="45.000352"/>
<wire x1="43.390421875" y1="30.988" x2="46.271578125" y2="30.988" width="0.1524" layer="20"/>
<wire x1="46.271578125" y1="30.988" x2="46.630790625" y2="31.136790625" width="0.1524" layer="20" curve="45.000249"/>
<wire x1="46.630790625" y1="31.136790625" x2="47.857209375" y2="32.363209375" width="0.1524" layer="20"/>
<wire x1="47.857209375" y1="32.363209375" x2="48.216421875" y2="32.512" width="0.1524" layer="20" curve="-45.000352"/>
<wire x1="48.216421875" y1="32.512" x2="48.514" y2="32.512" width="0.1524" layer="20"/>
<wire x1="48.514" y1="32.512" x2="49.022" y2="32.004" width="0.1524" layer="20" curve="-90"/>
<wire x1="49.022" y1="32.004" x2="49.022" y2="18.288" width="0.1524" layer="20"/>
<wire x1="49.022" y1="18.288" x2="48.514" y2="17.78" width="0.1524" layer="20" curve="-90"/>
<wire x1="48.514" y1="17.78" x2="47.962421875" y2="17.78" width="0.1524" layer="20"/>
<wire x1="47.962421875" y1="17.78" x2="47.603209375" y2="17.928790625" width="0.1524" layer="20" curve="-45.000249"/>
<wire x1="47.603209375" y1="17.928790625" x2="46.630790625" y2="18.901209375" width="0.1524" layer="20"/>
<wire x1="46.630790625" y1="18.901209375" x2="46.271578125" y2="19.05" width="0.1524" layer="20" curve="45.000352"/>
<wire x1="46.271578125" y1="19.05" x2="43.390421875" y2="19.05" width="0.1524" layer="20"/>
<wire x1="43.390421875" y1="19.05" x2="43.031209375" y2="18.901209375" width="0.1524" layer="20" curve="45.000249"/>
<wire x1="43.031209375" y1="18.901209375" x2="42.058790625" y2="17.928790625" width="0.1524" layer="20"/>
<wire x1="42.058790625" y1="17.928790625" x2="41.699578125" y2="17.78" width="0.1524" layer="20" curve="-45.000352"/>
<wire x1="41.699578125" y1="17.78" x2="40.894" y2="17.78" width="0.1524" layer="20"/>
<wire x1="40.894" y1="17.78" x2="40.386" y2="17.272" width="0.1524" layer="20" curve="90"/>
<wire x1="40.386" y1="17.272" x2="40.386" y2="6.858" width="0.1524" layer="20"/>
<wire x1="40.386" y1="6.858" x2="39.878" y2="6.35" width="0.1524" layer="20" curve="-90"/>
<text>Rio-&gt;CTRE Mag
Breakout</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
</plain>
<libraries>
<library name="tekdemo">
<packages>
<package name="M2X05_M_SHROUDED">
</package>
<package name="1X03_LOCK_LONGPADS_MOLEX">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads w/ Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Stormbots">
<packages>
<package name="TALONSRX">
<description>Mechanical description of the Talon SRX and Gadgeteer Breakout. Includes 
&lt;ul&gt;
&lt;li&gt;Gadgeteer port + screw holes
&lt;li&gt;Signal LEDs
&lt;li&gt;Brake/Coast button
&lt;li&gt;Mounting Straps and holes
&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RIOA1" library="tekdemo" package="1X03_LOCK_LONGPADS_MOLEX" value="">
<attribute name="VALUE"/>
</element>
<element name="RIOA2" library="tekdemo" package="1X03_LOCK_LONGPADS_MOLEX" value="">
<attribute name="VALUE"/>
</element>
<element name="RIOA3" library="tekdemo" package="1X03_LOCK_LONGPADS_MOLEX" value="">
<attribute name="VALUE"/>
</element>
<element name="RIOA0" library="tekdemo" package="1X03_LOCK_LONGPADS_MOLEX" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Stormbots" package="TALONSRX" value=""/>
<element name="ANALOG_0" library="tekdemo" package="M2X05_M_SHROUDED" value="M05X02M_SHROUDED"/>
<element name="ANALOG_1" library="tekdemo" package="M2X05_M_SHROUDED" value="M05X02M_SHROUDED"/>
<element name="ANALOG_2" library="tekdemo" package="M2X05_M_SHROUDED" value="M05X02M_SHROUDED"/>
<element name="ANALOG_3" library="tekdemo" package="M2X05_M_SHROUDED" value="M05X02M_SHROUDED"/>
</elements>
<signals>
<signal name="A1">
<contactref element="RIOA1" pad="3"/>
<contactref element="ANALOG_1" pad="P$3"/>
</signal>
<signal name="A2">
<contactref element="RIOA2" pad="3"/>
<contactref element="ANALOG_2" pad="P$3"/>
</signal>
<signal name="A3">
<contactref element="RIOA3" pad="3"/>
<contactref element="ANALOG_3" pad="P$3"/>
</signal>
<signal name="A0">
<contactref element="RIOA0" pad="3"/>
<contactref element="ANALOG_0" pad="P$3"/>
</signal>
<signal name="5V.0">
<contactref element="ANALOG_0" pad="P$2"/>
<contactref element="RIOA0" pad="2"/>
</signal>
<signal name="GND.2">
<contactref element="ANALOG_2" pad="P$10"/>
<contactref element="RIOA2" pad="1"/>
</signal>
<signal name="GND.3">
<contactref element="ANALOG_3" pad="P$10"/>
<contactref element="RIOA3" pad="1"/>
</signal>
<signal name="5V.3">
<contactref element="ANALOG_3" pad="P$2"/>
<contactref element="RIOA3" pad="2"/>
</signal>
<signal name="5V.2">
<contactref element="ANALOG_2" pad="P$2"/>
<contactref element="RIOA2" pad="2"/>
</signal>
<signal name="5V.1">
<contactref element="ANALOG_1" pad="P$2"/>
<contactref element="RIOA1" pad="2"/>
</signal>
<signal name="GND.1">
<contactref element="RIOA1" pad="1"/>
<contactref element="ANALOG_1" pad="P$10"/>
</signal>
<signal name="GND.0">
<contactref element="RIOA0" pad="1"/>
<contactref element="ANALOG_0" pad="P$10"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
