(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 141)
    (zones 0)
    (modules 3)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad19)")
  (net 2 "Net-(J1-Pad18)")
  (net 3 "Net-(J1-Pad17)")
  (net 4 "Net-(J1-Pad16)")
  (net 5 "Net-(J1-Pad15)")
  (net 6 "Net-(J1-Pad14)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad12)")
  (net 9 "Net-(J1-Pad11)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad9)")
  (net 12 "Net-(J1-Pad8)")
  (net 13 "Net-(J1-Pad7)")
  (net 14 "Net-(J1-Pad6)")
  (net 15 "Net-(J1-Pad5)")
  (net 16 "Net-(J1-Pad4)")
  (net 17 "Net-(J1-Pad3)")
  (net 18 "Net-(J1-Pad2)")
  (net 19 "Net-(J1-Pad1)")
  (net 20 "Net-(J2-Pad19)")
  (net 21 "Net-(J2-Pad18)")
  (net 22 "Net-(J2-Pad17)")
  (net 23 "Net-(J2-Pad16)")
  (net 24 "Net-(J2-Pad15)")
  (net 25 "Net-(J2-Pad14)")
  (net 26 "Net-(J2-Pad13)")
  (net 27 "Net-(J2-Pad12)")
  (net 28 "Net-(J2-Pad11)")
  (net 29 "Net-(J2-Pad10)")
  (net 30 "Net-(J2-Pad9)")
  (net 31 "Net-(J2-Pad8)")
  (net 32 "Net-(J2-Pad7)")
  (net 33 "Net-(J2-Pad6)")
  (net 34 "Net-(J2-Pad5)")
  (net 35 "Net-(J2-Pad4)")
  (net 36 "Net-(J2-Pad3)")
  (net 37 "Net-(J2-Pad2)")
  (net 38 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module Package_SO:TSSOP-38_4.4x9.7mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 147.32 101.902)
    (descr "TSSOP38: plastic thin shrink small outline package; 38 leads; body width 4.4 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot510-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -5.9) (layer F.SilkS))
    (fp_text value TSSOP-38 (at 0 5.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 38 smd rect (at 2.85 -4.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad19)"))
    (pad 37 smd rect (at 2.85 -4) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad18)"))
    (pad 36 smd rect (at 2.85 -3.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad17)"))
    (pad 35 smd rect (at 2.85 -3) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad16)"))
    (pad 34 smd rect (at 2.85 -2.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-Pad15)"))
    (pad 33 smd rect (at 2.85 -2) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J2-Pad14)"))
    (pad 32 smd rect (at 2.85 -1.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad13)"))
    (pad 31 smd rect (at 2.85 -1) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J2-Pad12)"))
    (pad 30 smd rect (at 2.85 -0.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J2-Pad11)"))
    (pad 29 smd rect (at 2.85 0) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad10)"))
    (pad 28 smd rect (at 2.85 0.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-Pad9)"))
    (pad 27 smd rect (at 2.85 1) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-Pad8)"))
    (pad 26 smd rect (at 2.85 1.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J2-Pad7)"))
    (pad 25 smd rect (at 2.85 2) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J2-Pad6)"))
    (pad 24 smd rect (at 2.85 2.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-Pad5)"))
    (pad 23 smd rect (at 2.85 3) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad4)"))
    (pad 22 smd rect (at 2.85 3.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (pad 21 smd rect (at 2.85 4) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad2)"))
    (pad 20 smd rect (at 2.85 4.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad1)"))
    (pad 19 smd rect (at -2.85 4.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad19)"))
    (pad 18 smd rect (at -2.85 4) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad18)"))
    (pad 17 smd rect (at -2.85 3.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad17)"))
    (pad 16 smd rect (at -2.85 3) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 15 smd rect (at -2.85 2.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (pad 14 smd rect (at -2.85 2) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 13 smd rect (at -2.85 1.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 12 smd rect (at -2.85 1) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad12)"))
    (pad 11 smd rect (at -2.85 0.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 10 smd rect (at -2.85 0) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at -2.85 -0.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at -2.85 -1) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad8)"))
    (pad 7 smd rect (at -2.85 -1.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at -2.85 -2) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at -2.85 -2.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad5)"))
    (pad 4 smd rect (at -2.85 -3) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at -2.85 -3.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -2.85 -4) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2.85 -4.5) (size 1.1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-38_4.4x9.7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x19_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 156.718 123.698)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J2 (at -3.048 0.254) (layer B.SilkS))
    (fp_text value Conn_01x19_Male (at -8.382 -45.72) (layer B.Fab))
    (fp_text user %R (at 0 -22.86 -90) (layer B.Fab))
    (pad 19 thru_hole oval (at 0 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad19)"))
    (pad 18 thru_hole oval (at 0 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x19_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x19_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 137.922 77.978)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J1 (at 2.794 0) (layer F.SilkS))
    (fp_text value Conn_01x19_Male (at 8.636 45.72) (layer F.Fab))
    (fp_text user %R (at 0 22.86 90) (layer F.Fab))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad19)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x19_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 136.144 125.476) (end 136.144 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.496 125.476) (end 136.144 125.476) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.496 76.2) (end 158.496 125.476) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136.144 76.2) (end 158.496 76.2) (layer Edge.Cuts) (width 0.05))
)
