(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 143)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3756)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.85 0.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 137.795 94.615 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (offset (xyz 0 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connectors_Molex:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 587D2992)
    (at 147.955 104.14 180)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J2 (at -1.72 7.11 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.89 0.46) (layers B.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.89 0.46) (layers B.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.89 0.46) (layers F.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.89 0.46) (layers F.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5CE986D1)
    (at 135.255 104.14)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.375) (layer F.SilkS))
    (fp_text value HMC431 (at 0 3.375) (layer F.Fab))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)") (solder_paste_margin_ratio -0.2))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "RF Out" (at 142.875 106.68) (layer F.SilkS))
  (gr_text "Vtune\n" (at 132.715 98.425 270) (layer F.SilkS))
  (gr_text "GND\n" (at 135.255 97.79 270) (layer F.SilkS))
  (gr_text VCC (at 137.795 97.79 270) (layer F.SilkS))
  (gr_text "Analog Devices \nHMC Series VCO" (at 139.065 103.505) (layer B.SilkS))
  (gr_line (start 130.429 110.236) (end 130.175 109.982) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.273 110.236) (end 130.429 110.236) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.654 109.855) (end 152.273 110.236) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.524 108.331) (end 130.175 109.982) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.524 93.599) (end 128.524 108.331) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.921 92.202) (end 128.524 93.599) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.844 92.202) (end 129.921 92.202) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.654 96.012) (end 148.844 92.202) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.654 109.855) (end 152.654 96.012) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.6))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.429 110.236) (xy 152.273 110.236) (xy 152.654 109.855) (xy 152.654 96.012) (xy 148.844 92.202)
        (xy 129.921 92.202) (xy 128.524 93.599) (xy 128.524 108.331)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.652 103.632) (xy 137.795 103.632) (xy 137.795 103.124) (xy 146.431 103.124) (xy 146.558 102.997)
        (xy 146.558 102.87) (xy 146.685 102.616) (xy 146.939 102.489) (xy 147.193 102.489) (xy 152.654 102.489)
        (xy 152.654 105.791) (xy 146.939 105.791) (xy 146.685 105.664) (xy 146.558 105.41) (xy 146.558 104.648)
        (xy 137.795 104.648) (xy 137.795 104.14) (xy 136.652 104.14)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.429 110.236) (xy 152.273 110.236) (xy 152.654 109.855) (xy 152.654 96.012) (xy 148.844 92.202)
        (xy 129.921 92.202) (xy 128.524 93.599) (xy 128.524 108.331)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.921 92.202) (xy 148.844 92.202) (xy 152.654 96.012) (xy 152.654 109.855) (xy 152.273 110.236)
        (xy 130.429 110.236) (xy 128.524 108.331) (xy 128.524 93.599)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.921 92.202) (xy 148.844 92.202) (xy 152.654 96.012) (xy 152.654 109.855) (xy 152.273 110.236)
        (xy 130.429 110.236) (xy 128.524 108.331) (xy 128.524 93.599)
      )
    )
  )
)
