(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~88~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 153)
    (zones 0)
    (modules 10)
    (nets 41)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 38.608 35.814)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 /RESET)
  (net 5 /GPIO23)
  (net 6 /GPIO22)
  (net 7 /TX)
  (net 8 /RX)
  (net 9 /GPIO21)
  (net 10 "Net-(IC1-Pad32)")
  (net 11 /GPIO19)
  (net 12 /GPIO18)
  (net 13 /GPIO5)
  (net 14 "Net-(IC1-Pad28)")
  (net 15 "Net-(IC1-Pad27)")
  (net 16 /GPIO4)
  (net 17 /GPIO0)
  (net 18 /GPIO15)
  (net 19 "Net-(IC1-Pad22)")
  (net 20 "Net-(IC1-Pad21)")
  (net 21 "Net-(IC1-Pad20)")
  (net 22 "Net-(IC1-Pad19)")
  (net 23 "Net-(IC1-Pad18)")
  (net 24 "Net-(IC1-Pad17)")
  (net 25 "Net-(IC1-Pad16)")
  (net 26 "Net-(IC1-Pad14)")
  (net 27 /GPIO14)
  (net 28 /GPIO27)
  (net 29 /GPIO26)
  (net 30 /GPIO25)
  (net 31 /GPIO33)
  (net 32 /GPIO32)
  (net 33 "Net-(IC1-Pad6)")
  (net 34 "Net-(IC1-Pad5)")
  (net 35 "Net-(IC1-Pad4)")
  (net 36 /DTR)
  (net 37 /RTS)
  (net 38 "Net-(U1-Pad4)")
  (net 39 /GPIO2)
  (net 40 "Net-(IC1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /DTR)
    (add_net /GPIO0)
    (add_net /GPIO14)
    (add_net /GPIO15)
    (add_net /GPIO18)
    (add_net /GPIO19)
    (add_net /GPIO2)
    (add_net /GPIO21)
    (add_net /GPIO22)
    (add_net /GPIO23)
    (add_net /GPIO25)
    (add_net /GPIO26)
    (add_net /GPIO27)
    (add_net /GPIO32)
    (add_net /GPIO33)
    (add_net /GPIO4)
    (add_net /GPIO5)
    (add_net /RESET)
    (add_net /RTS)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(U1-Pad4)")
  )
  (module "B6B-ZR(LF)(SN):JST_B6B-ZR(LF)(SN)" (layer F.Cu) (tedit 5FEB46F9)
    (at 56.896 62.992 180)
    (descr "<b>Dual In Line Package</b>")
    (fp_text reference J1 (at -1.51593 -3.9307 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Male (at 6.74809 2.40393 180) (layer F.Fab))
    (pad 5 thru_hole circle (at -2.25 0 180) (size 1.208 1.208) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 /RTS))
    (pad 6 thru_hole circle (at -3.75 0 180) (size 1.208 1.208) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -0.75 0 180) (size 1.208 1.208) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 /DTR))
    (pad 3 thru_hole circle (at 0.75 0 180) (size 1.208 1.208) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 /RX))
    (pad 2 thru_hole circle (at 2.25 0 180) (size 1.208 1.208) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 1 thru_hole rect (at 3.75 0 180) (size 1.208 1.208) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
  )
  (module ESP32-WROVER-E:ESP32WROVEREM213EH6464PH3Q0 (layer F.Cu) (tedit 0)
    (at 50.038 43.434)
    (descr "ESP32-WROVER-E(M213EH6464PH3Q0)-1")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at -0.25 0) (layer F.SilkS) hide)
    (fp_text value ESP32-WROVER-E_M213EH6464PH3Q0_ (at -0.25 0) (layer F.SilkS) hide)
    (fp_text user %R (at -0.25 0) (layer F.Fab))
    (pad 47 smd rect (at -1 -2.595 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at 0.835 -2.595 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 45 smd rect (at 0.835 -0.76 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at 0.835 1.075 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 43 smd rect (at -1 1.075 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 42 smd rect (at -2.835 1.075 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 41 smd rect (at -2.835 -0.76 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -2.835 -2.595 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at -1 -0.76 90) (size 1.33 1.33) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 38 smd rect (at 8.5 -8.26 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 8.5 -6.99 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 5 /GPIO23))
    (pad 36 smd rect (at 8.5 -5.72 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 6 /GPIO22))
    (pad 35 smd rect (at 8.5 -4.45 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /TX))
    (pad 34 smd rect (at 8.5 -3.18 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 8 /RX))
    (pad 33 smd rect (at 8.5 -1.91 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /GPIO21))
    (pad 32 smd rect (at 8.5 -0.64 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad32)"))
    (pad 31 smd rect (at 8.5 0.63 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /GPIO19))
    (pad 30 smd rect (at 8.5 1.9 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /GPIO18))
    (pad 29 smd rect (at 8.5 3.17 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 13 /GPIO5))
    (pad 28 smd rect (at 8.5 4.44 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad28)"))
    (pad 27 smd rect (at 8.5 5.71 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad27)"))
    (pad 26 smd rect (at 8.5 6.98 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 16 /GPIO4))
    (pad 25 smd rect (at 8.5 8.25 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 17 /GPIO0))
    (pad 24 smd rect (at 8.5 9.52 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 39 /GPIO2))
    (pad 23 smd rect (at 8.5 10.79 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO15))
    (pad 22 smd rect (at 8.5 12.06 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad22)"))
    (pad 21 smd rect (at 8.5 13.33 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad21)"))
    (pad 20 smd rect (at 8.5 14.6 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad20)"))
    (pad 19 smd rect (at -8.5 14.6 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad19)"))
    (pad 18 smd rect (at -8.5 13.33 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad18)"))
    (pad 17 smd rect (at -8.5 12.06 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad17)"))
    (pad 16 smd rect (at -8.5 10.79 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad16)"))
    (pad 15 smd rect (at -8.5 9.52 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -8.5 8.25 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad14)"))
    (pad 13 smd rect (at -8.5 6.98 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 27 /GPIO14))
    (pad 12 smd rect (at -8.5 5.71 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 28 /GPIO27))
    (pad 11 smd rect (at -8.5 4.44 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 29 /GPIO26))
    (pad 10 smd rect (at -8.5 3.17 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 30 /GPIO25))
    (pad 9 smd rect (at -8.5 1.9 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /GPIO33))
    (pad 8 smd rect (at -8.5 0.63 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 32 /GPIO32))
    (pad 7 smd rect (at -8.5 -0.64 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at -8.5 -1.91 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad6)"))
    (pad 5 smd rect (at -8.5 -3.18 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad5)"))
    (pad 4 smd rect (at -8.5 -4.45 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad4)"))
    (pad 3 smd rect (at -8.5 -5.72 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (pad 2 smd rect (at -8.5 -6.99 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -8.5 -8.26 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ESP32-WROVER-E_M213EH6464PH3Q0_.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 49.8875 60.452)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /RESET))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 5FEA2212)
    (at 38.608 35.814 180)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x10_Male (at 0 -25.19 180) (layer B.Fab))
    (fp_text user %R (at 0 -11.43 90) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /GPIO14))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /GPIO27))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /GPIO26))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /GPIO25))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /GPIO33))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /GPIO32))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 5FEA21F8)
    (at 61.468 35.814 180)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J3 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x10_Male (at 0 -25.19 180) (layer B.Fab))
    (fp_text user %R (at 0 -11.43 90) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIO15))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /GPIO2))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO4))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO5))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO18))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIO19))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO21))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO22))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIO23))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 42.418 62.484 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value XC6220B331MR (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 45.593 62.484 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.68 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 54.9645 60.452)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /RESET))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 39.243 62.484 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.68 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MUN5214DW1T1G:On_Semiconductor-MUN5214DW1T1G-Manufacturer_Recommended (layer F.Cu) (tedit 5EFF8995)
    (at 49.53 63.5 90)
    (fp_text reference Q1 (at -2.35 -1.975003 90) (layer F.SilkS) hide)
    (fp_text value MUN5214DW1T1G (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.920001 -0.650001 180) (size 0.299999 0.660001) (layers F.Cu F.Paste F.Mask)
      (net 37 /RTS))
    (pad 2 smd rect (at -0.920001 -0.000001 180) (size 0.299999 0.660001) (layers F.Cu F.Paste F.Mask)
      (net 36 /DTR))
    (pad 3 smd rect (at -0.920001 0.649999 180) (size 0.299999 0.660001) (layers F.Cu F.Paste F.Mask)
      (net 17 /GPIO0))
    (pad 4 smd rect (at 0.919998 0.649999 180) (size 0.299999 0.660001) (layers F.Cu F.Paste F.Mask)
      (net 36 /DTR))
    (pad 5 smd rect (at 0.919998 -0.000001 180) (size 0.299999 0.660001) (layers F.Cu F.Paste F.Mask)
      (net 37 /RTS))
    (pad 6 smd rect (at 0.919998 -0.650001 180) (size 0.299999 0.660001) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (model ${KIPRJMOD}/kicad-library/MUN5214DW1T1G/MUN5214DW1T1G.models/On_Semiconductor_-_MUN5214DW1T1G.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "François Gervais\n29 dec 2020\nrev 1.0" (at 59.69 55.626) (layer B.SilkS))
  (gr_arc (start 61.468 64.516) (end 61.468 65.786) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38.608 64.516) (end 37.338 64.516) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 61.468 35.052) (end 62.738 35.052) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38.608 35.052) (end 38.608 33.782) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text 15 (at 60.198 57.658) (layer F.SilkS))
  (gr_text 2 (at 60.452 55.118) (layer F.SilkS))
  (gr_text 4 (at 60.452 52.578) (layer F.SilkS))
  (gr_text 5 (at 60.452 50.038) (layer F.SilkS))
  (gr_text 18 (at 60.198 47.498) (layer F.SilkS))
  (gr_text 19 (at 60.198 44.958) (layer F.SilkS))
  (gr_text 21 (at 60.198 42.418) (layer F.SilkS))
  (gr_text 22 (at 60.198 39.878) (layer F.SilkS))
  (gr_text GND (at 60.452 34.544) (layer F.SilkS))
  (gr_text 23 (at 60.198 37.338) (layer F.SilkS))
  (gr_text 14 (at 39.878 50.038) (layer F.SilkS))
  (gr_text GND (at 39.624 52.324) (layer F.SilkS))
  (gr_text 5V (at 39.878 57.404) (layer F.SilkS))
  (gr_text 3V3 (at 39.624 54.864) (layer F.SilkS))
  (gr_text 27 (at 39.878 47.498) (layer F.SilkS))
  (gr_text 26 (at 39.878 44.958) (layer F.SilkS))
  (gr_text 25 (at 39.878 42.418) (layer F.SilkS))
  (gr_text 33 (at 39.878 39.878) (layer F.SilkS))
  (gr_text RST (at 39.624 34.544) (layer F.SilkS))
  (gr_text 32 (at 39.878 37.338) (layer F.SilkS))
  (gr_line (start 61.468 33.782) (end 38.608 33.782) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 62.738 64.516) (end 62.738 35.052) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 38.608 65.786) (end 61.468 65.786) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 37.338 35.052) (end 37.338 64.516) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet))
    (polygon
      (pts
        (xy 41.148 59.944) (xy 44.323 59.944) (xy 44.323 62.484) (xy 37.338 62.484) (xy 37.338 58.166)
        (xy 41.148 58.166)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet))
    (polygon
      (pts
        (xy 45.212 57.912) (xy 48.006 60.706) (xy 48.006 67.056) (xy 36.576 67.056) (xy 36.576 62.738)
        (xy 44.704 62.738) (xy 45.466 60.706) (xy 43.434 58.674) (xy 41.402 58.674) (xy 41.402 37.084)
        (xy 41.402 35.306) (xy 45.4025 35.306)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet))
    (polygon
      (pts
        (xy 63.741446 67.564) (xy 36.068 67.564) (xy 35.814 35.306) (xy 63.754 35.306)
      )
    )
  )
)
