(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (34 "B.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J_GND-CK-DATA1-Pad3)")
  (net 2 "Net-(J_GND-CK-DATA1-Pad2)")
  (net 3 "Net-(J_GND-CK-DATA1-Pad1)")
  (net 4 "unconnected-(J_OP-CE-SELECT-LED1-Pad1)")
  (net 5 "Net-(J_OP-CE-SELECT-LED1-Pad3)")
  (net 6 "Net-(J_OP-CE-SELECT-LED1-Pad4)")
  (net 7 "Net-(J_GND-CK-DATA1-Pad4)")
  (net 8 "Net-(J_GND-CK-DATA1-Pad5)")
  (net 9 "Net-(J_GND-CK-DATA1-Pad6)")
  (net 10 "Net-(J_GND-CK-DATA1-Pad7)")
  (net 11 "Net-(J_OP-CE-SELECT-LED1-Pad2)")
  (net 12 "Net-(TP1-Pad1)")
  (net 13 "Net-(TP13-Pad1)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 84.0762 68.0406)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J_GND-CK-DATA1" (at 3.1238 7.8594 -90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x07_Male" (at 0 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J_GND-CK-DATA1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J_GND-CK-DATA1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J_GND-CK-DATA1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J_GND-CK-DATA1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J_GND-CK-DATA1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J_GND-CK-DATA1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J_GND-CK-DATA1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 68.834 80.772)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J_OP-CE-SELECT-LED1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Male" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J_OP-CE-SELECT-LED1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J_OP-CE-SELECT-LED1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J_OP-CE-SELECT-LED1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J_OP-CE-SELECT-LED1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 64.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "GND" (at -1.9938 -0.2 90) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 12 "Net-(TP1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 66.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "CE" (at 0.0062 -2.2 90) (layer "F.SilkS"))
    (fp_text value "CE" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(J_OP-CE-SELECT-LED1-Pad3)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 68.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "Vdd1" (at 0 -3.2 90) (layer "F.SilkS"))
    (fp_text value "Vdd1" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(J_GND-CK-DATA1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 70.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "Vdd2" (at 0 -3.2 90) (layer "F.SilkS"))
    (fp_text value "Vdd2 (NC)" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 13 "Net-(TP13-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 72.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "CK1" (at 0 -2.7 90) (layer "F.SilkS"))
    (fp_text value "CK1" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(J_GND-CK-DATA1-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 74.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "CK2" (at 0.0062 -2.7 90) (layer "F.SilkS"))
    (fp_text value "CK2" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(J_GND-CK-DATA1-Pad3)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 76.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "OP" (at 0 -2.2 90) (layer "F.SilkS"))
    (fp_text value "OP" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(J_OP-CE-SELECT-LED1-Pad4)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 78.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "D1" (at 0.0062 -2.2 90) (layer "F.SilkS"))
    (fp_text value "D1" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(J_GND-CK-DATA1-Pad4)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 80.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "D2" (at 0 -2.2 90) (layer "F.SilkS"))
    (fp_text value "D2" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(J_GND-CK-DATA1-Pad5)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 82.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "D3" (at 0 -2.2 90) (layer "F.SilkS"))
    (fp_text value "D3" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(J_GND-CK-DATA1-Pad6)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 84.9938 103.7)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "D4" (at 0 -2.2 90) (layer "F.SilkS"))
    (fp_text value "D4" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(J_GND-CK-DATA1-Pad7)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 76.4 87.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Reset" (at 0 2.5) (layer "B.SilkS"))
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers F&B.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 86 99)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 64 99)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 76.5 67.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers F&B.Cu *.Mask))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "B.Cu")
    (tedit 5A0F774F)
    (at 67.5 62.5 180)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "Select" (at 0 -1.5 270 unlocked) (layer "B.SilkS"))
    (fp_text value "ROM Select" (at 0 -1.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.45) (layer "B.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 11 "Net-(J_OP-CE-SELECT-LED1-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "B.Cu")
    (tedit 5A0F774F)
    (at 74 62.25 180)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "GND" (at 0 -1.5 270 unlocked) (layer "B.SilkS"))
    (fp_text value "GND" (at 0 -1.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.45) (layer "B.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 12 "Net-(TP1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "B.Cu")
    (tedit 5A0F774F)
    (at 79 62.25 180)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "Vdd1" (at 0 -1.1 270 unlocked) (layer "B.SilkS"))
    (fp_text value "Vdd1" (at 0 -1.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.45) (layer "B.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(J_GND-CK-DATA1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "B.Cu")
    (tedit 5A0F774F)
    (at 76.5 62.25 180)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "CasioROMemu.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "Vdd2" (at 0 -1.1 270 unlocked) (layer "B.SilkS"))
    (fp_text value "Vdd2" (at 0 -1.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.45) (layer "B.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 13 "Net-(TP13-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (gr_line (start 60 60.5) (end 63 60.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 65 60.5) (end 90 60.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 60 60.5) (end 60 107) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 65 60.5) (mid 64 61.5) (end 63 60.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 60 107) (end 90 107) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 90 107) (end 90 60.5) (layer "Edge.Cuts") (width 0.05))
  (gr_text "OP" (at 66.2065 88.392) (layer "B.SilkS"))
  (gr_text "ra226.net" (at 61.722 62 270) (layer "B.SilkS"))
  (gr_text "GND" (at 87.352 68.1125) (layer "B.SilkS"))
  (gr_text "__________" (at 73.2 61.55 -90) (layer "B.SilkS"))
  (gr_text "D1" (at 86.9075 75.6055) (layer "B.SilkS"))
  (gr_text "CK1" (at 87.4155 70.6525) (layer "B.SilkS"))
  (gr_text "D3" (at 86.9075 80.749) (layer "B.SilkS"))
  (gr_text "ROM" (at 81.1 64.25 -90) (layer "B.SilkS"))
  (gr_text "CK2" (at 87.4155 73.1925) (layer "B.SilkS"))
  (gr_text "__________" (at 80.6 64.45 -90) (layer "B.SilkS"))
  (gr_text "RO-226" (at 76.5 77 -90) (layer "B.SilkS"))
  (gr_text "D4" (at 86.9075 83.289) (layer "B.SilkS"))
  (gr_text "D2" (at 86.9075 78.2725) (layer "B.SilkS"))
  (gr_text "CE" (at 66.27 85.852) (layer "B.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 89.9962 60.5006) (xy 59.9962 60.5006))
    (height 4.0006)
    (gr_text "30.00 mm" (at 74.9962 55.35) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 60 60.5) (xy 60 107))
    (height 4)
    (gr_text "46.50 mm" (at 54.85 83.75 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 90 99) (xy 90 107))
    (height -4)
    (gr_text "8.00 mm" (at 95.5 103 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 86 107) (xy 90 107))
    (height 4)
    (gr_text "4.00 mm" (at 88 112.5) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 67 106) (xy 65 106))
    (height -5)
    (gr_text "2.00 mm" (at 66 112.5) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
)
