<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-29.5" y1="28.25" x2="-32.5" y2="25.25" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="52.5" y1="25.25" x2="49.5" y2="28.25" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="49.5" y1="-28.25" x2="52.5" y2="-25.25" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="-32.5" y1="-25.25" x2="-29.5" y2="-28.25" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="-31.5" y1="-8.75" x2="-32.5" y2="-9.75" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="-28.798709375" y1="-8.75" x2="-27.798709375" y2="-7.75" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="-27.798709375" y1="7.25" x2="-28.798709375" y2="8.25" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="-32.5" y1="9.25" x2="-31.5" y2="8.25" width="0.01" layer="20" curve="90" locked="yes"/>
<wire x1="-29.5" y1="28.25" x2="49.5" y2="28.25" width="0.01" layer="20" locked="yes"/>
<wire x1="-32.5" y1="25.25" x2="-32.5" y2="9.25" width="0.01" layer="20" locked="yes"/>
<wire x1="-29.5" y1="-28.25" x2="49.5" y2="-28.25" width="0.01" layer="20" locked="yes"/>
<wire x1="52.5" y1="25.25" x2="52.5" y2="-25.25" width="0.01" layer="20" locked="yes"/>
<wire x1="-31.5" y1="8.25" x2="-28.798709375" y2="8.25" width="0.01" layer="20" locked="yes"/>
<wire x1="-27.798709375" y1="7.25" x2="-27.798709375" y2="-7.75" width="0.01" layer="20" locked="yes"/>
<wire x1="-28.798709375" y1="-8.75" x2="-31.5" y2="-8.75" width="0.01" layer="20" locked="yes"/>
<wire x1="-32.5" y1="-9.75" x2="-32.5" y2="-25.25" width="0.01" layer="20" locked="yes"/>
<text>15V+</text>
<text>15V-</text>
<text>5V</text>
<text>3.3V</text>
<text>L_V</text>
<text>D_V</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>Colter Barney
Zane Goldhahn
Cameron Zupancic</text>
<text>Reference Simulator
Interface Board</text>
<hole x="-29" y="24.25" drill="2.75"/>
<hole x="29" y="24.25" drill="2.75"/>
<hole x="29" y="-24.75" drill="2.75"/>
<hole x="-29" y="-24.75" drill="2.75"/>
</plain>
<libraries>
<library name="RFSIM">
<packages>
<package name="0805">
<description>0805 (2012 Metric)</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="MSOP10">
<description>10-Lead Mini Small Outline Package [MSOP]</description>
</package>
<package name="SO-8_S_LIT-M">
</package>
<package name="LA_55-P_LEM">
</package>
<package name="21-0051H_MXM-M">
</package>
<package name="SO-8_ILD-M">
</package>
<package name="CONN6_282857-6_TEC">
</package>
<package name="CONN9_282834-9_TEC">
</package>
<package name="RASPI_GPIO_B+_PIN">
<description>40-pin connector for Raspberry Pi GPIO model B+&lt;br/&gt;
 &amp;nbsp; just the two rows of pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="RFSIM" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="R1" library="RFSIM" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R13" library="RFSIM" package="R0805" value="82.5">
<attribute name="NAME"/>
</element>
<element name="R14" library="RFSIM" package="R0805" value="82.5">
<attribute name="NAME"/>
</element>
<element name="R2" library="RFSIM" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R3" library="RFSIM" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R4" library="RFSIM" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R5" library="RFSIM" package="R0805" value="52.5k">
<attribute name="NAME"/>
</element>
<element name="R6" library="RFSIM" package="R0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R7" library="RFSIM" package="R0805" value="217">
<attribute name="NAME"/>
</element>
<element name="R8" library="RFSIM" package="R0805" value="217">
<attribute name="NAME"/>
</element>
<element name="U1" library="RFSIM" package="MSOP10" value="ADS1115IDGST">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="X"/>
</element>
<element name="U2" library="RFSIM" package="SO-8_S_LIT-M" value="LT6201CS8PBFSO-8_S_LIT-M">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LT6201CS8#PBF"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="LinearTech_2016_03_08"/>
<attribute name="VENDOR" value="Linear Technology"/>
</element>
<element name="U3" library="RFSIM" package="SO-8_S_LIT-M" value="LT6201CS8PBFSO-8_S_LIT-M">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LT6201CS8#PBF"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="LinearTech_2016_03_08"/>
<attribute name="VENDOR" value="Linear Technology"/>
</element>
<element name="U5" library="RFSIM" package="LA_55-P_LEM" value="LA_55-P">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.lem.com/sites/default/files/products_datasheets/la_55-p_e.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LA 55-P"/>
<attribute name="SOURCELIBRARY" value="LEM_2020-01-10"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="LEM"/>
</element>
<element name="U6" library="RFSIM" package="LA_55-P_LEM" value="LA_55-P">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.lem.com/sites/default/files/products_datasheets/la_55-p_e.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LA 55-P"/>
<attribute name="SOURCELIBRARY" value="LEM_2020-01-10"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="LEM"/>
</element>
<element name="U7" library="RFSIM" package="21-0051H_MXM-M" value="MAX5491LA01000+T21-0051H_MXM-M">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MAX5491LA01000+T"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Maxim_2015-01-06"/>
<attribute name="VENDOR" value="Maxim Integrated Products"/>
</element>
<element name="U8" library="RFSIM" package="SO-8_ILD-M" value="ILD207TSO-8_ILD-M">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ILD207T"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vishay"/>
</element>
<element name="VSENSE_REF1" library="RFSIM" package="CONN6_282857-6_TEC" value="282857-6">
<attribute name="BUILT_BY" value="SunStream"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&amp;DocId=Customer+Drawing%7F282857%7FF1%7Fpdf%7FEnglish%7FENG_CD_282857_F1.pdf%7F282857-6"/>
<attribute name="DESCRIPTION" value="TERMINAL BLOCK PCB MOUNT SIDE WIRE  ENTRY, STACKING W/INTERLOCK  5.08MM PITCH."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="282857-6"/>
<attribute name="SOURCELIBRARY" value="TE_Connectivity_600_Part_Delivery_14_2020-03-09"/>
<attribute name="VENDOR" value="TE Connectivity"/>
</element>
<element name="X1" library="RFSIM" package="RASPI_GPIO_B+_PIN" value="RASPI_GPIO_B+#_PIN"/>
<element name="J1" library="RFSIM" package="CONN9_282834-9_TEC" value="282834-9">
<attribute name="BUILT_BY" value="SunStream"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&amp;DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf%7F282834-9"/>
<attribute name="DESCRIPTION" value="TERMINAL BLOCK, PCB MOUNT, SIDE WIRE ENTRY STACKING 2.54MM PITCH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="282834-9"/>
<attribute name="SOURCELIBRARY" value="TE_Connectivity_600_Part_Delivery_14_2020-03-09"/>
<attribute name="VENDOR" value="TE Connectivity"/>
</element>
<element name="R9" library="RFSIM" package="R0805" value="52.5k">
<attribute name="NAME"/>
</element>
<element name="R10" library="RFSIM" package="R0805" value="52.5k">
<attribute name="NAME"/>
</element>
<element name="R11" library="RFSIM" package="R0805" value="52.5k">
<attribute name="NAME"/>
</element>
<element name="R12" library="RFSIM" package="R0805" value="52.5k">
<attribute name="NAME"/>
</element>
<element name="C4" library="RFSIM" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C5" library="RFSIM" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="RFSIM" package="0805" value="1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="RFSIM" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C6" library="RFSIM" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="U2" pad="4"/>
<contactref element="U7" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="U8" pad="4"/>
<contactref element="X1" pad="39"/>
<contactref element="X1" pad="6"/>
<contactref element="X1" pad="9"/>
<contactref element="X1" pad="14"/>
<contactref element="X1" pad="20"/>
<contactref element="X1" pad="25"/>
<contactref element="X1" pad="30"/>
<contactref element="X1" pad="34"/>
<contactref element="J1" pad="9"/>
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="VSENSE_REF1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="10"/>
<contactref element="R1" pad="2"/>
<contactref element="X1" pad="5"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="SDA">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="X1" pad="3"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="ADDR">
<contactref element="U1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="U3" pad="8"/>
<contactref element="U7" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="4"/>
<contactref element="X1" pad="17"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="ALERT">
<contactref element="U1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="X1" pad="12"/>
</signal>
<signal name="LOAD_VOLTAGE_DIV">
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="DEVICE_VOLTAGE">
<contactref element="U2" pad="5"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="LOAD_CURRENT">
<contactref element="R13" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="DEVICE_CURRENT">
<contactref element="U6" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="LOAD_VOLTAGE">
<contactref element="R5" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="1.65V_1">
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="1.65V_2">
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="7"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="1.65V">
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="5"/>
<contactref element="U7" pad="3"/>
</signal>
<signal name="+15V">
<contactref element="U5" pad="3"/>
<contactref element="U6" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="-15V">
<contactref element="U5" pad="2"/>
<contactref element="U6" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="SHUTDOWN2">
<contactref element="X1" pad="11"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="SHUTDOWN1">
<contactref element="R8" pad="1"/>
<contactref element="X1" pad="13"/>
</signal>
<signal name="N$22">
<contactref element="U8" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U8" pad="3"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="CH1_COL">
<contactref element="U8" pad="8"/>
<contactref element="VSENSE_REF1" pad="3"/>
</signal>
<signal name="CH1_EMM">
<contactref element="U8" pad="7"/>
<contactref element="VSENSE_REF1" pad="4"/>
</signal>
<signal name="CH2_COL">
<contactref element="U8" pad="6"/>
<contactref element="VSENSE_REF1" pad="5"/>
</signal>
<signal name="CH2_EMM">
<contactref element="U8" pad="5"/>
<contactref element="VSENSE_REF1" pad="6"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="3"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="2"/>
<contactref element="VSENSE_REF1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="6"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="DEVICE_VOLTAGE_DIV">
<contactref element="U2" pad="7"/>
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
