(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 136)
    (zones 0)
    (modules 12)
    (nets 14)
  )
  (page User 148.006 105.004)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./SKEWISP_R2_181024"))
  )
  (net 0 "")
  (net 1 /RST)
  (net 2 GND)
  (net 3 /HEARTBEAT)
  (net 4 "Net-(D1-Pad1)")
  (net 5 /ERROR)
  (net 6 "Net-(D2-Pad1)")
  (net 7 VCC)
  (net 8 "Net-(J1-Pad3)")
  (net 9 /SCK)
  (net 10 /MISO)
  (net 11 /MOSI)
  (net 12 /RESET)
  (net 13 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ERROR)
    (add_net /HEARTBEAT)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net VCC)
  )
  (net_class cut ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module procsynth:ICSP_th (layer F.Cu) (tedit 5BD046DE)
    (at 68.935 31.152 270)
    (fp_text reference J4 (at 5.588 0) (layer F.Fab))
    (fp_text value ICSP_header (at 2.286 3.302 90) (layer F.SilkS) hide)
    (pad 5 thru_hole circle (at 2.54 1.29 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 /RESET))
    (pad 4 thru_hole circle (at 0 -1.25 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 /MOSI))
    (pad 6 thru_hole rect (at 2.54 -1.25 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -1.25 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 3 thru_hole circle (at 0 1.29 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SCK))
    (pad 1 thru_hole circle (at -2.54 1.29 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 /MISO))
  )
  (module Capacitors_THT:CP_Radial_D4.0mm_P2.00mm placed (layer F.Cu) (tedit 5A393CD7)
    (at 61.93 32.835 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1 -3.31 270) (layer F.Fab))
    (fp_text value 10uF (at 1.016 -3.048 270) (layer F.SilkS))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 /RST))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm placed (layer B.Cu) (tedit 5A393CF1)
    (at 54.564 42.836)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 2.54 1.27) (layer B.Fab))
    (fp_text value "UNO POWER" (at 2.54 -3.81 90) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /RST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm placed (layer B.Cu) (tedit 5A393CFD)
    (at 102.824 28.612 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 2.54 -15.24 180) (layer B.Fab))
    (fp_text value "UNO PIN 8-13, GND" (at 2.54 -5.08 270) (layer B.Fab))
    (fp_text user %R (at 0 -7.62 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SCK))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /MOSI))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /RESET))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /HEARTBEAT))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ERROR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket placed (layer F.Cu) (tedit 597E3A29)
    (at 88.6 28.612)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference S8 (at 3.81 1.27) (layer F.Fab))
    (fp_text value "ATTINY x5" (at -2.54 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /RESET))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /MOSI))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /SCK))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_Socket placed (layer F.Cu) (tedit 597E3A22)
    (at 75.265 28.612)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference S14 (at 3.81 1.27) (layer F.Fab))
    (fp_text value "ATTINY x4" (at -2.54 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /SCK))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /RESET))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /MOSI))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A393D5D)
    (at 96.982 41.312)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 1.27) (layer F.SilkS))
    (fp_text value HEARTBEAT (at -5.08 0) (layer F.SilkS))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /HEARTBEAT))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A393D58)
    (at 96.982 43.852)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 1.397) (layer F.SilkS))
    (fp_text value ERROR (at -3.81 0) (layer F.SilkS))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /ERROR))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A393C8F)
    (at 94 39.026 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.86 0 180) (layer F.SilkS))
    (fp_text value R (at 2.032 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A393C80)
    (at 88.407 39.026 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.86 0 180) (layer F.SilkS))
    (fp_text value R (at 2.032 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 5BD04677)
    (at 64.47 43.979)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference J5 (at 3.125 2.5) (layer F.SilkS) hide)
    (fp_text value "microblade 6" (at 3.125 -3.25) (layer F.Fab))
    (fp_text user %R (at 3.125 -1.25) (layer F.Fab))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 /RESET))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 /MOSI))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 /SCK))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610_06x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C76A5FC)
    (at 61 39 90)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value Jumper_3_Bridged12 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -1.3 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 13 "Net-(J1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
        (gr_poly (pts
           (xy 0.4 -0.3) (xy 0.9 -0.3) (xy 0.9 0.3) (xy 0.4 0.3)) (width 0))
      ))
    (pad 3 smd custom (at 1.3 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 8 "Net-(J1-Pad3)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 7 VCC))
  )
  (gr_text "RST  GND" (at 68.9785 37.121) (layer F.SilkS))
  (gr_text "SCK  MOSI" (at 69.042 36.359) (layer F.SilkS))
  (gr_text "MISO  VCC" (at 68.7245 35.597) (layer F.SilkS))
  (gr_text "MISO\nVCC\nSCK\nMOSI\nRST\nGND" (at 67.5 40.5 90) (layer F.SilkS))
  (gr_text "PicoBlade 6" (at 67.5 41.2) (layer F.SilkS))
  (gr_text "UNO\n" (at 62.946 30.136) (layer F.Mask))
  (gr_text "antoine.pintout.com\n02/19 — rev 4\n" (at 100.965 44.45) (layer B.Mask))
  (gr_text ISP (at 59.898 30.136) (layer F.SilkS))
  (gr_text SKEW (at 61.676 28.358) (layer F.Mask))
  (gr_text SKEW (at 61.676 28.358) (layer F.Cu))
  (gr_text GND (at 56.088 42.836) (layer F.SilkS))
  (gr_text 5v (at 56.088 40.296) (layer F.SilkS))
  (gr_text 3v3 (at 56.088 37.756) (layer F.SilkS))
  (gr_text "RST\n" (at 56.088 35.216) (layer F.SilkS))
  (gr_text 8 (at 101.046 43.852) (layer F.SilkS))
  (gr_text 9 (at 101.046 41.312) (layer F.SilkS))
  (gr_text 10 (at 101.046 38.772) (layer F.SilkS))
  (gr_text 11 (at 101.046 36.232) (layer F.SilkS))
  (gr_text 12 (at 101.046 33.692) (layer F.SilkS))
  (gr_text 13 (at 101.046 31.152) (layer F.SilkS))
  (gr_text GND (at 101.046 28.612) (layer F.SilkS))
  (gr_line (start 59 26.5) (end 105 26.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.75 27.75) (end 59 26.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.75 32) (end 57.75 27.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56.5 33.25) (end 57.75 32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.5 46) (end 56.5 45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.75 46) (end 57.5 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58 46) (end 57.75 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105 46) (end 58 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105 26.5) (end 105 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.5 45) (end 56.5 45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.5 33.25) (end 52.5 45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56.5 33.25) (end 52.5 33.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52 25.25) (xy 106 25.25) (xy 106 47.25) (xy 52 47.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.12 29.374) (xy 58.12 31.152) (xy 65.232 31.152) (xy 65.232 29.374)
      )
    )
  )
)
