(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 143)
    (zones 0)
    (modules 4)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFDEF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 87.73 110.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 53.64 110.53)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59DE0251)
    (at 59.69 81.28 90)
    (descr "Through hole straight IDC box header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x10 2.54mm double row")
    (fp_text reference PCC (at 1.27 -6.604 90) (layer F.SilkS))
    (fp_text value IDC-Header_2x10_P2.54mm_Vertical (at -5.08 12.7) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43 90) (layer F.Fab))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_FFC-FPC:Hirose_FH12-24S-0.5SH_1x24-1MP_P0.50mm_Horizontal (layer F.Cu) (tedit 5D24667B)
    (at 69.85 104.14)
    (descr "Hirose FH12, FFC/FPC connector, FH12-24S-0.5SH, 24 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (attr smd)
    (fp_text reference FPC (at 0 -3.7) (layer F.SilkS))
    (fp_text value "1x24 P0.50mm" (at 0 5.6) (layer F.Fab))
    (fp_text user %R (at 0 3.7) (layer F.Fab))
    (pad 24 smd rect (at 5.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 5.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 4.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 4.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 3.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 3.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 2.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 1.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 0.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -0.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -1.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -1.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -3.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -3.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -5.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -5.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at -7.65 1.4) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at 7.65 1.4) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-24S-0.5SH_1x24-1MP_P0.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Mouser TF Lite\nPPC to FPC Adapter" (at 58.19 95.39) (layer F.SilkS))
  (gr_line (start 91.44 72.39) (end 91.44 110.49) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 87.63 110.49) (end 87.63 114.3) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.53 114.3) (end 49.53 72.39) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.63 114.3) (end 49.53 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 49.53 72.39) (end 91.44 72.39) (layer Edge.Cuts) (width 0.15))
)
