(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 58)
    (tracks 32)
    (zones 0)
    (modules 20)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 7)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(FL1-Pad1)")
  (net 6 "Net-(FL1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 7)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(FL1-Pad1)")
    (add_net "Net-(FL1-Pad2)")
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 73.4314 82.2706)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 73.4314 24.260384)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 114.173 82.2452)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 32.6644 82.2706)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 114.173 24.260384)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 32.675146 24.260384)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module SamacSys_Parts:CAPPRD500W65D1250H2700 (layer F.Cu) (tedit 5CEB06DD)
    (at 73.25 47)
    (descr EEUFP1E202)
    (tags Capacitor)
    (fp_text reference C1 (at -2.9936 -6.2076) (layer F.SilkS))
    (fp_text value "2000 uF" (at 2.5 3) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model "C:\\Users\\Administrator\\Google Drive\\KiCAD User Library\\SamacSys_Parts.3dshapes\\EEU-FP1E202.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:CAPPRD500W65D1250H2700 (layer F.Cu) (tedit 5CEB06DD)
    (at 79 60 180)
    (descr EEUFP1E202)
    (tags Capacitor)
    (fp_text reference C2 (at 7.9054 -5.7352) (layer F.SilkS))
    (fp_text value "2000 uF" (at 2.16 -2.98) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model "C:\\Users\\Administrator\\Google Drive\\KiCAD User Library\\SamacSys_Parts.3dshapes\\EEU-FP1E202.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:CAPPRD500W65D1250H2700 (layer F.Cu) (tedit 5CEB06DD)
    (at 94.75 58 180)
    (descr EEUFP1E202)
    (tags Capacitor)
    (fp_text reference C3 (at -3.302 5.08) (layer F.SilkS))
    (fp_text value "2000 uF" (at 2.54 3.302) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model "C:\\Users\\Administrator\\Google Drive\\KiCAD User Library\\SamacSys_Parts.3dshapes\\EEU-FP1E202.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module acw:Coilcraft_CMT4 (layer F.Cu) (tedit 5CEAC563)
    (at 41.75 34.25)
    (fp_text reference FL1 (at -6.55 -1.5) (layer F.SilkS))
    (fp_text value EMI_Filter_LL_1423 (at 13.7 11.5) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 0 0) (size 4.8 4.8) (drill 2.06) (layers *.Cu *.Mask)
      (net 5 "Net-(FL1-Pad1)"))
    (pad 2 thru_hole circle (at 22.9 0) (size 4.8 4.8) (drill 2.06) (layers *.Cu *.Mask)
      (net 6 "Net-(FL1-Pad2)"))
    (pad 3 thru_hole circle (at 22.9 38.1) (size 4.8 4.8) (drill 2.06) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 38.1) (size 4.8 4.8) (drill 2.06) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module SamacSys_Parts:VER2923682KL (layer F.Cu) (tedit 0)
    (at 85.25 29)
    (descr VER2923-682KL-3)
    (tags Inductor)
    (fp_text reference L1 (at 0.88 13.778) (layer F.SilkS))
    (fp_text value "22 uH" (at 16.35 -1.695) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 16.51 5.23) (size 7.604 7.604) (drill 5.0696) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 7.604 7.604) (drill 5.0696) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model "C:\\Users\\Administrator\\Google Drive\\KiCAD User Library\\SamacSys_Parts.3dshapes\\VER2923-103KL.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:VER2923682KL (layer F.Cu) (tedit 0)
    (at 85.75 73)
    (descr VER2923-682KL-3)
    (tags Inductor)
    (fp_text reference L2 (at -0.66 13.36) (layer F.SilkS))
    (fp_text value "22 uH" (at 11.38 -3.06) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7.604 7.604) (drill 5.0696) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 16.51 5.23) (size 7.604 7.604) (drill 5.0696) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model "C:\\Users\\Administrator\\Google Drive\\KiCAD User Library\\SamacSys_Parts.3dshapes\\VER2923-103KL.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 35 52.25)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference TP1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.33) (layer Dwgs.User) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(FL1-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 74 34.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference TP2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.33) (layer Dwgs.User))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 113.75 35.25)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference TP3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.33) (layer Dwgs.User))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 114.25 69.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference TP4 (at -0.31576 -2.98248) (layer F.SilkS))
    (fp_text value TestPoint (at 5.13 -0.285) (layer Dwgs.User) hide)
    (fp_text user %R (at -0.31322 -2.9901) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 74.75 72.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference TP5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.33) (layer Dwgs.User))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 25 39.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference TP6 (at 0 -2.33) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -0.13) (layer Dwgs.User) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(FL1-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5556-04A_2x02x4.20mm_Straight (layer F.Cu) (tedit 58A28952)
    (at 31.5 62 270)
    (descr "Molex Mini-Fit JR, PN:5556-04A, dual row, top entry type, through hole")
    (tags "connector molex mini-fit 5556")
    (fp_text reference J1 (at -4.76262 3.1454 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 2.1 -4 90) (layer Dwgs.User) hide)
    (pad 4 thru_hole circle (at 4.2 5.5 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(FL1-Pad1)"))
    (pad 3 thru_hole circle (at 0 5.5 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(FL1-Pad1)"))
    (pad 2 thru_hole circle (at 4.2 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(FL1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(FL1-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MiniFit-JR-5556-04A_2x02x4.20mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5556-04B_2x02x4.20mm_Straight (layer F.Cu) (tedit 58A28952)
    (at 105.25 54.75 90)
    (descr "Molex Mini-Fit JR, PN:5556-04B, dual row, top entry type, through hole, with plastic PCB locators")
    (tags "connector molex mini-fit 5556")
    (fp_text reference J2 (at 11.7857 2.4856 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Female (at 2.1 -4 90) (layer Dwgs.User) hide)
    (fp_text user %R (at 2.1 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -4.7 5.04 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 8.9 5.04 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MiniFit-JR-5556-04B_2x02x4.20mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 71.12 72.644) (layer F.SilkS))
  (gr_text BLK (at 36.068 66.04) (layer F.SilkS))
  (gr_text RED (at 36.068 61.976) (layer F.SilkS))
  (gr_text GRN (at 22.352 67.056) (layer F.SilkS))
  (gr_text WHT (at 22.352 60.96) (layer F.SilkS))
  (gr_text RED (at 105.156 58.928) (layer F.SilkS))
  (gr_text BLK (at 105.156 46.736) (layer F.SilkS))
  (gr_text GRN (at 114.808 49.784) (layer F.SilkS))
  (gr_text WHT (at 114.808 55.372) (layer F.SilkS))
  (gr_line (start 118.349172 18.760384) (end 118.349172 87.760384) (layer Edge.Cuts) (width 0.4))
  (gr_text "Power Side\nGND" (at 25.4 42.545) (layer F.SilkS))
  (gr_text "Power Side\nSignal" (at 33.655 47.625) (layer F.SilkS))
  (gr_text "Fan Side\nSignal" (at 114.46256 73.17486) (layer F.SilkS))
  (gr_text "Power Out" (at 109.22 41.656) (layer F.SilkS))
  (gr_text "Power\nIn" (at 30.48 71.755) (layer F.SilkS))
  (gr_text BLK (at 34.925 66.04) (layer B.SilkS))
  (gr_text RED (at 34.925 62.0014) (layer B.SilkS))
  (gr_text GRN (at 22.225 66.04) (layer B.SilkS))
  (gr_text WHT (at 22.225 62.23) (layer B.SilkS))
  (gr_text GRN (at 114.808 50.292) (layer B.SilkS))
  (gr_text WHT (at 114.808 55.372) (layer B.SilkS))
  (gr_text BLK (at 105.156 47.752) (layer B.SilkS))
  (gr_text RED (at 105.156 57.404) (layer B.SilkS))
  (gr_text L2 (at 93.726 74.2696) (layer B.SilkS))
  (gr_text L1 (at 93.1926 32.004) (layer B.SilkS))
  (gr_line (start 28.501119 78.960384) (end 28.501119 87.760384) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 18.925146 36.336357) (end 18.925146 70.184411) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 18.925146 70.184411) (end 19.725146 70.184411) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 19.725146 78.960384) (end 28.501119 78.960384) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 19.725146 36.336357) (end 18.925146 36.336357) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 28.501119 87.760384) (end 118.349172 87.760384) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 28.501119 18.760384) (end 28.501119 27.560384) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 118.349172 18.760384) (end 28.501119 18.760384) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 19.725146 27.560384) (end 19.725146 36.336357) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_text FL1 (at 51.75 34.75) (layer B.SilkS))
  (gr_text "EMI Filter Arctic Air V1" (at 53.34 85.344) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.85))
    (polygon
      (pts
        (xy 17.887724 16.75) (xy 141.387724 16.75) (xy 141 92.5) (xy 17.5 92.5)
      )
    )
  )
)
