<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="39.27866875" x2="0" y2="2.81610625" width="0" layer="20"/>
<wire x1="0" y1="2.81610625" x2="2.81610625" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.81610625" y1="0" x2="54.703325" y2="0" width="0" layer="20"/>
<wire x1="54.703325" y1="0" x2="57.385271875" y2="2.681365625" width="0" layer="20" curve="89.987582"/>
<wire x1="57.385271875" y1="2.681365625" x2="57.402725" y2="39.47604375" width="0" layer="20"/>
<wire x1="57.402725" y1="39.47604375" x2="54.715003125" y2="42.164" width="0" layer="20" curve="90.02718"/>
<wire x1="54.715003125" y1="42.164" x2="2.88533125" y2="42.164" width="0" layer="20"/>
<wire x1="2.88533125" y1="42.164" x2="0" y2="39.27866875" width="0" layer="20" curve="90"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>1&gt;6 = Inputs
7 = NC
8 = GND</text>
<text>2016-03-16
JL</text>
<text>APEX
PHOENIX
BOB
V2</text>
<text>Input 6 connected internally
to indicate BOB Disconnect.</text>
</plain>
<libraries>
<library name="001 Jeff Mystere">
<packages>
<package name="1X08_LONGPADS">
</package>
<package name="1X02_LONGPADS_3.5">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="BIPCOT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="001 Jeff Mystere" package="1X08_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="X1" library="001 Jeff Mystere" package="1X02_LONGPADS_3.5" value=""/>
<element name="X2" library="001 Jeff Mystere" package="1X02_LONGPADS_3.5" value=""/>
<element name="X3" library="001 Jeff Mystere" package="1X02_LONGPADS_3.5" value=""/>
<element name="X4" library="001 Jeff Mystere" package="1X02_LONGPADS_3.5" value=""/>
<element name="X5" library="001 Jeff Mystere" package="1X02_LONGPADS_3.5" value=""/>
<element name="JP2" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP3" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP4" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP5" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP6" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP7" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP8" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP9" library="001 Jeff Mystere" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$1" library="001 Jeff Mystere" package="BIPCOT" value="BIPCOT"/>
</elements>
<signals>
<signal name="1">
<contactref element="JP1" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="2">
<contactref element="JP1" pad="2"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="3">
<contactref element="JP1" pad="3"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="4">
<contactref element="JP1" pad="4"/>
<contactref element="X4" pad="2"/>
</signal>
<signal name="5">
<contactref element="JP1" pad="5"/>
<contactref element="X5" pad="2"/>
</signal>
<signal name="COMMON">
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="8"/>
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="X4" pad="1"/>
<contactref element="X5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
