(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 308)
    (no_connects 0)
    (area 99.924999 39.924999 200.075001 140.075001)
    (thickness 1.6)
    (drawings 142)
    (tracks 1864)
    (zones 0)
    (modules 145)
    (nets 144)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.8001)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 /GPIO1)
  (net 5 /GPIO2)
  (net 6 /GPIO3)
  (net 7 /GPIO4)
  (net 8 "Net-(P3-Pad7)")
  (net 9 "Net-(P3-Pad8)")
  (net 10 /TxD)
  (net 11 /RxD)
  (net 12 "Net-(P5-Pad1)")
  (net 13 +15V)
  (net 14 GNDA)
  (net 15 +5VD)
  (net 16 /DATA)
  (net 17 /CLOCK)
  (net 18 /LOAD)
  (net 19 /RESET)
  (net 20 "Net-(R3-Pad1)")
  (net 21 "Net-(R4-Pad1)")
  (net 22 GNDD)
  (net 23 /I2C_SDA2)
  (net 24 /I2C_SCL2)
  (net 25 /UART3_TX)
  (net 26 /UART3_RX)
  (net 27 /PH2)
  (net 28 /I2C_SDA)
  (net 29 /I2C_SCL)
  (net 30 "Net-(C13-Pad1)")
  (net 31 /RXD2)
  (net 32 /TXD2)
  (net 33 /CTS2)
  (net 34 /MOSI)
  (net 35 /MISO)
  (net 36 /RTS2)
  (net 37 /SCLK)
  (net 38 /CE0)
  (net 39 /PI3)
  (net 40 /PI14)
  (net 41 "Net-(P11-Pad1)")
  (net 42 "Net-(D1-Pad1)")
  (net 43 "Net-(D1-Pad2)")
  (net 44 /CANTX)
  (net 45 /CANRX)
  (net 46 "Net-(D2-Pad1)")
  (net 47 "Net-(D3-Pad1)")
  (net 48 /CB3)
  (net 49 /CB1)
  (net 50 /CB2)
  (net 51 /CB4)
  (net 52 /CB5)
  (net 53 /CB6)
  (net 54 /CB7)
  (net 55 /CB8)
  (net 56 /CVCC)
  (net 57 "Net-(P17-Pad3)")
  (net 58 "Net-(P17-Pad10)")
  (net 59 "Net-(P17-Pad7)")
  (net 60 "Net-(P17-Pad6)")
  (net 61 "Net-(P17-Pad9)")
  (net 62 "Net-(P17-Pad5)")
  (net 63 /CANL)
  (net 64 /CANH)
  (net 65 /S88_3)
  (net 66 /S88_1)
  (net 67 /S88_2)
  (net 68 /S88_4)
  (net 69 /S88_5)
  (net 70 /S88_6)
  (net 71 /S88_7)
  (net 72 /S88_8)
  (net 73 "Net-(P20-Pad10)")
  (net 74 "Net-(C12-Pad1)")
  (net 75 "Net-(C12-Pad2)")
  (net 76 "Net-(C13-Pad2)")
  (net 77 "Net-(C14-Pad1)")
  (net 78 "Net-(C14-Pad2)")
  (net 79 "Net-(C15-Pad2)")
  (net 80 "Net-(C20-Pad1)")
  (net 81 "Net-(P2-Pad2)")
  (net 82 "Net-(P2-Pad1)")
  (net 83 "Net-(P2-Pad3)")
  (net 84 "Net-(P2-Pad4)")
  (net 85 "Net-(P2-Pad5)")
  (net 86 "Net-(P2-Pad6)")
  (net 87 "Net-(P5-Pad2)")
  (net 88 "Net-(P8-Pad2)")
  (net 89 "Net-(P8-Pad1)")
  (net 90 "Net-(P9-Pad1)")
  (net 91 "Net-(P9-Pad2)")
  (net 92 "Net-(P9-Pad3)")
  (net 93 "Net-(P9-Pad4)")
  (net 94 "Net-(P16-Pad3)")
  (net 95 "Net-(P16-Pad10)")
  (net 96 "Net-(P16-Pad7)")
  (net 97 "Net-(P16-Pad6)")
  (net 98 "Net-(P16-Pad9)")
  (net 99 "Net-(P16-Pad5)")
  (net 100 "Net-(P18-Pad3)")
  (net 101 "Net-(P18-Pad10)")
  (net 102 "Net-(P18-Pad7)")
  (net 103 "Net-(P18-Pad6)")
  (net 104 "Net-(P18-Pad9)")
  (net 105 "Net-(P18-Pad5)")
  (net 106 "Net-(P19-Pad2)")
  (net 107 "Net-(P20-Pad16)")
  (net 108 "Net-(R1-Pad1)")
  (net 109 "Net-(R2-Pad1)")
  (net 110 "Net-(R6-Pad2)")
  (net 111 "Net-(R16-Pad1)")
  (net 112 "Net-(R17-Pad1)")
  (net 113 "Net-(U13-Pad6)")
  (net 114 "Net-(U13-Pad16)")
  (net 115 "Net-(U13-Pad2)")
  (net 116 +5VA)
  (net 117 VCOM)
  (net 118 "Net-(C10-Pad1)")
  (net 119 "Net-(C10-Pad2)")
  (net 120 "Net-(P10-Pad2)")
  (net 121 "Net-(P23-Pad1)")
  (net 122 "Net-(P15-Pad2)")
  (net 123 "Net-(D4-Pad2)")
  (net 124 "Net-(D5-Pad2)")
  (net 125 "Net-(U13-Pad15)")
  (net 126 "Net-(C22-Pad1)")
  (net 127 "Net-(C23-Pad1)")
  (net 128 "Net-(C24-Pad1)")
  (net 129 /RxLED)
  (net 130 /TxLED)
  (net 131 "Net-(P1-Pad2)")
  (net 132 "Net-(P1-Pad4)")
  (net 133 /CB6')
  (net 134 "Net-(P31-Pad2)")
  (net 135 "Net-(J5-Pad5)")
  (net 136 "Net-(J5-Pad3)")
  (net 137 "Net-(D6-Pad2)")
  (net 138 /GND_)
  (net 139 /rt_)
  (net 140 /br_)
  (net 141 /VCC_)
  (net 142 /CANL_)
  (net 143 /CANH_)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3048)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CANH)
    (add_net /CANL)
    (add_net /CANRX)
    (add_net /CANTX)
    (add_net /CB1)
    (add_net /CB2)
    (add_net /CB3)
    (add_net /CB4)
    (add_net /CB5)
    (add_net /CB7)
    (add_net /CB8)
    (add_net /CE0)
    (add_net /CLOCK)
    (add_net /CTS2)
    (add_net /DATA)
    (add_net /GPIO1)
    (add_net /GPIO2)
    (add_net /GPIO3)
    (add_net /GPIO4)
    (add_net /I2C_SCL)
    (add_net /I2C_SCL2)
    (add_net /I2C_SDA)
    (add_net /I2C_SDA2)
    (add_net /LOAD)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PH2)
    (add_net /PI14)
    (add_net /PI3)
    (add_net /RESET)
    (add_net /RTS2)
    (add_net /RXD2)
    (add_net /RxD)
    (add_net /RxLED)
    (add_net /S88_1)
    (add_net /S88_2)
    (add_net /S88_3)
    (add_net /S88_4)
    (add_net /S88_5)
    (add_net /S88_6)
    (add_net /S88_7)
    (add_net /S88_8)
    (add_net /SCLK)
    (add_net /TXD2)
    (add_net /TxD)
    (add_net /TxLED)
    (add_net /UART3_RX)
    (add_net /UART3_TX)
    (add_net GND)
    (add_net GNDA)
    (add_net GNDD)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P16-Pad10)")
    (add_net "Net-(P16-Pad3)")
    (add_net "Net-(P16-Pad5)")
    (add_net "Net-(P16-Pad6)")
    (add_net "Net-(P16-Pad7)")
    (add_net "Net-(P16-Pad9)")
    (add_net "Net-(P17-Pad10)")
    (add_net "Net-(P17-Pad3)")
    (add_net "Net-(P17-Pad5)")
    (add_net "Net-(P17-Pad6)")
    (add_net "Net-(P17-Pad7)")
    (add_net "Net-(P17-Pad9)")
    (add_net "Net-(P18-Pad10)")
    (add_net "Net-(P18-Pad3)")
    (add_net "Net-(P18-Pad5)")
    (add_net "Net-(P18-Pad6)")
    (add_net "Net-(P18-Pad7)")
    (add_net "Net-(P18-Pad9)")
    (add_net "Net-(P19-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P20-Pad10)")
    (add_net "Net-(P20-Pad16)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P31-Pad2)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad3)")
    (add_net "Net-(P9-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U13-Pad15)")
    (add_net "Net-(U13-Pad16)")
    (add_net "Net-(U13-Pad2)")
    (add_net "Net-(U13-Pad6)")
    (add_net VCOM)
  )
  (net_class Power ""
    (clearance 0.4)
    (trace_width 0.6096)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net +5V)
    (add_net +5VA)
    (add_net +5VD)
    (add_net /CVCC)
  )
  (net_class "Power Large" ""
    (clearance 0.2)
    (trace_width 1.2)
    (via_dia 1.6)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CB6)
    (add_net /CB6')
    (add_net "Net-(P15-Pad2)")
    (add_net "Net-(P23-Pad1)")
  )
  (net_class "Power Small" ""
    (clearance 0.2)
    (trace_width 0.4064)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
  )
  (net_class RJ45_ADDON ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CANH_)
    (add_net /CANL_)
    (add_net /GND_)
    (add_net /VCC_)
    (add_net /br_)
    (add_net /rt_)
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad5)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 589723D3)
    (at 180.594 78.5114 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P32 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 138 /GND_))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(J5-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 141 /VCC_))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 142 /CANL_))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 143 /CANH_))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 56953C59)
    (at 152.9588 61.976 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -2.667 270) (layer F.SilkS))
    (fp_text value TERM (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(P5-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_logo:Logo_copper_CC-BY-NC-SA_5x2mm (layer B.Cu) (tedit 0)
    (at 194.5 72 270)
    (descr "CC BY-NC-SA logo, 5x2mm")
    (fp_text reference G*** (at 0.2 0.7 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.2 -0.2 270) (layer B.SilkS) hide)
  )
  (module w_conn_pc:megb8-8 (layer F.Cu) (tedit 5897099A)
    (at 197.1294 72.009 90)
    (descr "RJ45 + led indicators, Wiznet P/N RB1-125BAG1A")
    (fp_text reference J5 (at 0.5796 -0.275 90) (layer F.SilkS))
    (fp_text value RJ45 (at 0.351 1.884 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at -1.905 -6.34 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 136 "Net-(J5-Pad3)"))
    (pad 1 thru_hole circle (at -4.445 -6.34 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 139 /rt_))
    (pad 2 thru_hole circle (at -3.175 -8.88 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 140 /br_))
    (pad 4 thru_hole circle (at -0.635 -8.88 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 138 /GND_))
    (pad 5 thru_hole circle (at 0.635 -6.34 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 135 "Net-(J5-Pad5)"))
    (pad 6 thru_hole circle (at 1.905 -8.88 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 141 /VCC_))
    (pad 7 thru_hole circle (at 3.175 -6.34 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 142 /CANL_))
    (pad 8 thru_hole circle (at 4.445 -8.88 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 143 /CANH_))
    (pad 13 thru_hole circle (at -7.75 -3.05 90) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 7.75 -3.05 90) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5.715 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916655)
    (at 197 84)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R02 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916655)
    (at 182 84)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R02 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916655)
    (at 182 60)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R02 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916655)
    (at 197 60)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R02 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691684E)
    (at 177.25 62.5 90)
    (fp_text reference E05 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691684E)
    (at 175.25 62.5 90)
    (fp_text reference E05 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691684E)
    (at 174.25 81.5 270)
    (fp_text reference E05 (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691684E)
    (at 179.75 81.5 270)
    (fp_text reference E05 (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691684E)
    (at 176.4 101.6 180)
    (fp_text reference E05 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 57B5D5D9)
    (at 109.22 82.9945 180)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U3 (at 0.0635 0.0635 180) (layer F.SilkS))
    (fp_text value 6N137 (at 6.1214 -0.0635 450) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -1.27 3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(R2-Pad1)"))
    (pad 3 thru_hole oval (at 1.27 3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO1))
    (pad 4 thru_hole oval (at 3.81 3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 3.81 -3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (pad 6 thru_hole oval (at 1.27 -3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 /RESET))
    (pad 7 thru_hole oval (at -1.27 -3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 8 thru_hole oval (at -3.81 -3.81 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5898755B)
    (at 107.5055 89.408 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at -0.3048 1.9431 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 57B6C1B4)
    (at 119.38 82.9945)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U6 (at 0.0635 0.0635) (layer F.SilkS))
    (fp_text value 6N137 (at 6.5024 -0.0381 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -1.27 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(R6-Pad2)"))
    (pad 3 thru_hole oval (at 1.27 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 /DATA))
    (pad 4 thru_hole oval (at 3.81 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 3.81 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 1.27 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GPIO4))
    (pad 7 thru_hole oval (at -1.27 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 8 thru_hole oval (at -3.81 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pc:conn_usb_B (layer F.Cu) (tedit 58986AF0)
    (at 103.8352 55.6006 270)
    (descr "USB B-type receptacle, Lumberg P/N 2411-02")
    (tags USB)
    (fp_text reference P13 (at 0.6604 -9.2583 270) (layer F.SilkS))
    (fp_text value USB (at 0.508 -11.3284 270) (layer F.SilkS))
    (pad 3 thru_hole circle (at -1.2446 -5.0038 270) (size 1.50114 1.50114) (drill 0.94996) (layers *.Cu *.Mask)
      (net 128 "Net-(C24-Pad1)"))
    (pad 4 thru_hole circle (at 1.2446 -5.0038 270) (size 1.50114 1.50114) (drill 0.94996) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.2446 -7.0104 270) (size 1.50114 1.50114) (drill 0.94996) (layers *.Cu *.Mask)
      (net 126 "Net-(C22-Pad1)"))
    (pad 2 thru_hole circle (at -1.2446 -7.0104 270) (size 1.50114 1.50114) (drill 0.94996) (layers *.Cu *.Mask)
      (net 127 "Net-(C23-Pad1)"))
    (pad "" thru_hole circle (at -6.0198 -2.286 270) (size 3.50012 3.50012) (drill 2.30124) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 6.0198 -2.286 270) (size 3.50012 3.50012) (drill 2.30124) (layers *.Cu *.Mask))
    (model walter/conn_pc/usb_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_copper_CC-BY-NC-SA_5x2mm (layer F.Cu) (tedit 0)
    (at 190.119 137.033)
    (descr "CC BY-NC-SA logo, 5x2mm")
    (fp_text reference G*** (at 0.2 -0.7) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.2 0.2) (layer F.SilkS) hide)
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 58984BD3)
    (at 159.131 56.388)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R23 (at 0 0) (layer F.SilkS))
    (fp_text value 0 (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 GNDA))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x04 (layer B.Cu) (tedit 56A6485A)
    (at 116.1034 51.3842)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at -2.8194 -1.7272) (layer B.SilkS))
    (fp_text value CONN_02X04 (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /GPIO1))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 /GPIO2))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 /GPIO3))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 /GPIO4))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(P3-Pad8)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz 0.15 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x13 (layer B.Cu) (tedit 56927642)
    (at 108.4834 45.212)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -2.8575 1.5875) (layer B.SilkS))
    (fp_text value BPi (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 131 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 /I2C_SDA2))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 132 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 /I2C_SCL2))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 39 /PI3))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 /UART3_TX))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 /UART3_RX))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 /RXD2))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 /PH2))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 /TXD2))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 /CTS2))
    (pad 16 thru_hole oval (at 17.78 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 44 /CANTX))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at 20.32 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 45 /CANRX))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 /MOSI))
    (pad 20 thru_hole oval (at 22.86 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 35 /MISO))
    (pad 22 thru_hole oval (at 25.4 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 36 /RTS2))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 37 /SCLK))
    (pad 24 thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 38 /CE0))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 26 thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 40 /PI14))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x13.wrl
      (at (xyz 0.6 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module w_conn_pc:megb8-8 (layer F.Cu) (tedit 569245BB)
    (at 119.9 136.8)
    (descr "RJ45 + led indicators, Wiznet P/N RB1-125BAG1A")
    (fp_text reference J1 (at 0.0388 -0.021) (layer F.SilkS))
    (fp_text value RJ45 (at -0.139 2.011) (layer F.SilkS))
    (pad 3 thru_hole circle (at -1.905 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 /CB3))
    (pad 1 thru_hole circle (at -4.445 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 /CB1))
    (pad 2 thru_hole circle (at -3.175 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 /CB2))
    (pad 4 thru_hole circle (at -0.635 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 /CB4))
    (pad 5 thru_hole circle (at 0.635 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 /CB5))
    (pad 6 thru_hole circle (at 1.905 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 /CB6))
    (pad 7 thru_hole circle (at 3.175 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 /CB7))
    (pad 8 thru_hole circle (at 4.445 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 /CB8))
    (pad 13 thru_hole circle (at -7.75 -3.05) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 7.75 -3.05) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5.715 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691682A)
    (at 145 101.5 180)
    (fp_text reference E03 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691682A)
    (at 145 104 180)
    (fp_text reference E03 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 133.0325 58.4835 180)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C15 (at 1.25 -3.8 180) (layer F.SilkS))
    (fp_text value 10uf (at 1.25 3.8 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(C14-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(C15-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 132.334 64.897 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C13 (at 1.25 -3.8 90) (layer F.SilkS))
    (fp_text value 10uf (at 1.25 3.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(C13-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691683C)
    (at 111.5 101.5 180)
    (fp_text reference E04 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691682A)
    (at 111.5 104 180)
    (fp_text reference E03 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 5691685D)
    (at 176.4 104 180)
    (fp_text reference E06 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 56916818)
    (at 161.2 121.4 90)
    (fp_text reference E02 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 133.223 69.85 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C14 (at 1.25 -3.8 90) (layer F.SilkS))
    (fp_text value 10uf (at 1.25 3.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(C14-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916720)
    (at 196.5 136.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R012 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916702)
    (at 196.5 106.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R010 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 569166E5)
    (at 166.5 106.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference RR08 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916714)
    (at 166.5 136.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R011 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 569166D8)
    (at 156.5 136.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R08 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 569166B5)
    (at 156.5 106.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R06 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 569166A0)
    (at 103.5 106.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R05 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 569166CA)
    (at 103.5 136.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R07 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916670)
    (at 103 92)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R03 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 145.963 56.388)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.246 2.159) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 56942E6E)
    (at 143.129 69.85 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.524 -2.286 180) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer B.Cu) (tedit 56A6494F)
    (at 126.2634 48.8442)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 1.3716 2.0828) (layer B.SilkS))
    (fp_text value "BPi Con" (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.72 1.72) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 /TxD))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.72 1.72) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 /RxD))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916655)
    (at 188.5 43)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R02 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916681)
    (at 188.5 97)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R04 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 56916634)
    (at 103 43)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference R01 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 56A4B02B)
    (at 157.353 43.053 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at -1.8415 0 270) (layer F.SilkS))
    (fp_text value 100nF (at -1.905 -2.7305 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 +15V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 GNDA))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 56A4B034)
    (at 157.353 50.292 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at -2.032 0.0635 90) (layer F.SilkS))
    (fp_text value 100nF (at -0.508 3.683 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 116 +5VA))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 GNDA))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57B5C5FF)
    (at 128.7145 85.344 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at -2.2352 -0.0762 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57B5D619)
    (at 128.7145 98.044 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 4.5212 0.3429 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 56953D39)
    (at 117.221 75.311 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 4.3815 0.127 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57B6BF8E)
    (at 157.8356 90.4748 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at -2.4892 -0.0508 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.2192 -0.0889 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5735E204)
    (at 176.8094 93.1418)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at -0.0762 -0.1778 90) (layer F.SilkS))
    (fp_text value ADuM1251BR (at 0 3.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /I2C_SDA2))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /I2C_SCL2))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C10-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /I2C_SCL))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /I2C_SDA))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C10-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 57B5C3E6)
    (at 101.854 76.7715 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 -2.6035 180) (layer F.SilkS))
    (fp_text value RS232 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(P9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(P9-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(P9-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(P9-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 56A659DF)
    (at 142.461 62.992)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U10 (at 5.4305 2.032) (layer B.SilkS))
    (fp_text value MCP2562 (at 0 -3.5) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 /CANTX))
    (pad 2 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (pad 4 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 /CANRX))
    (pad 5 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(P5-Pad2)"))
    (pad 7 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(R1-Pad1)"))
    (pad 8 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:mdip_8 (layer B.Cu) (tedit 58983F18)
    (at 158.877 69.215 90)
    (descr "SMD DIL8 x 0,3\"")
    (tags "SMD DIL")
    (fp_text reference U12 (at 6.2484 0.4064 180) (layer B.SilkS))
    (fp_text value ISO1050 (at -0.508 1.016 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 -4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -1.27 -4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 45 /CANRX))
    (pad 3 smd rect (at 1.27 -4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 44 /CANTX))
    (pad 4 smd rect (at 3.81 -4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.81 4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 14 GNDA))
    (pad 6 smd rect (at 1.27 4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 63 /CANL))
    (pad 7 smd rect (at -1.27 4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 64 /CANH))
    (pad 8 smd rect (at -3.81 4.5 90) (size 1.8 3) (layers B.Cu B.Paste B.Mask)
      (net 116 +5VA))
    (model walter/smd_dil/mdip_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B5CC3D)
    (at 141.986 94.1705 90)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 0 0 90) (layer F.SilkS))
    (fp_text value 270 (at 0 2.032 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B5CC18)
    (at 142.0495 84.0105 90)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 270 (at 0 2.032 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B5CFF3)
    (at 145.161 82.931 270)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R13 (at 0 0 270) (layer F.SilkS))
    (fp_text value 1k (at 0 2.032 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(P31-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B58936)
    (at 123.6345 91.694)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R9 (at 0 0) (layer F.SilkS))
    (fp_text value 1k5 (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /CLOCK))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B6BFA7)
    (at 113.9825 89.5985)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 0 0) (layer F.SilkS))
    (fp_text value 390 (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(R6-Pad2)"))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B5892A)
    (at 123.6345 89.5985)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R8 (at 0 0) (layer F.SilkS))
    (fp_text value 1k5 (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LOAD))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B588F4)
    (at 113.9825 91.694 180)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1k5 (at 0 2.032 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /RESET))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B61431)
    (at 110.49 72.7075 90)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 270 (at 0 2.032 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57B61418)
    (at 113.03 72.7075 90)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.032 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GPIO4))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 589672AB)
    (at 164 79.502 270)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R15 (at 0 0 270) (layer F.SilkS))
    (fp_text value 1K5 (at 0 2.032 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P11-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(D1-Pad1)"))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-6-3,5-h (layer F.Cu) (tedit 58987578)
    (at 116.84 96.52)
    (descr "6-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P6 (at 0.127 -2.7305) (layer F.SilkS))
    (fp_text value S88 (at -14.8336 -8.4836) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5.25 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (pad 1 thru_hole rect (at 8.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 16 /DATA))
    (pad 3 thru_hole circle (at 1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 17 /CLOCK))
    (pad 4 thru_hole circle (at -1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LOAD))
    (pad 5 thru_hole circle (at -5.25 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 19 /RESET))
    (pad 6 thru_hole circle (at -8.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (model walter/conn_pt-1_5/pt_1,5-6-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-2-3,5-h (layer F.Cu) (tedit 57DFA822)
    (at 149.5425 106.553 180)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P15 (at -0.0075 1.353 180) (layer F.SilkS))
    (fp_text value POWER (at 4.3425 0.403 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at -1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(P15-Pad2)"))
    (pad 1 thru_hole rect (at 1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 51 /CB4))
    (model walter/conn_pt-1_5/pt_1,5-2-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-5-3,5-h (layer F.Cu) (tedit 589872F4)
    (at 172.085 62.23 90)
    (descr "5-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P12 (at 9.525 -0.127 180) (layer F.SilkS))
    (fp_text value CAN-Bus (at -5.1308 -12.2682 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 GNDA))
    (pad 1 thru_hole rect (at 7 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 +15V))
    (pad 3 thru_hole circle (at 0 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 116 +5VA))
    (pad 4 thru_hole circle (at -3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 63 /CANL))
    (pad 5 thru_hole circle (at -7 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 64 /CANH))
    (model walter/conn_pt-1_5/pt_1,5-5-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-5-3,5-h (layer F.Cu) (tedit 57DFAB22)
    (at 156.591 124.333 90)
    (descr "5-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P14 (at -11.8364 -4.7752 90) (layer F.SilkS))
    (fp_text value CAN-Bus (at 9.883 -0.441 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 51 /CB4))
    (pad 1 thru_hole rect (at 7 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 56 /CVCC))
    (pad 3 thru_hole circle (at 0 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 133 /CB6'))
    (pad 4 thru_hole circle (at -3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 54 /CB7))
    (pad 5 thru_hole circle (at -7 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 55 /CB8))
    (model walter/conn_pt-1_5/pt_1,5-5-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 569249C2)
    (at 163.322 53.594 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P19 (at -0.1778 -2.4638 90) (layer F.SilkS))
    (fp_text value TERM (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /CANL))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(P19-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 58984FB8)
    (at 150.495 60.579 90)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value R (at 0 2.032 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P5-Pad1)"))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 58984C49)
    (at 159.131 60.452)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R21 (at 0 0) (layer F.SilkS))
    (fp_text value 0 (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 64 /CANH))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 58984C4F)
    (at 159.131 58.42)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R22 (at 0 0) (layer F.SilkS))
    (fp_text value 0 (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(P5-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 63 /CANL))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-6-3,5-h (layer F.Cu) (tedit 5696581A)
    (at 196.85 121.412 90)
    (descr "6-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P2 (at -11.811 -3.4036 180) (layer F.SilkS))
    (fp_text value S88 (at 11.684 -5.461 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5.25 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(P2-Pad2)"))
    (pad 1 thru_hole rect (at 8.75 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(P2-Pad1)"))
    (pad 3 thru_hole circle (at 1.75 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(P2-Pad3)"))
    (pad 4 thru_hole circle (at -1.75 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(P2-Pad4)"))
    (pad 5 thru_hole circle (at -5.25 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(P2-Pad5)"))
    (pad 6 thru_hole circle (at -8.75 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(P2-Pad6)"))
    (model walter/conn_pt-1_5/pt_1,5-6-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5896676B)
    (at 139.9358 48.3262 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P21 (at -0.0027 -2.4312 270) (layer F.SilkS))
    (fp_text value "RS232 Con" (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /TxD))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /RxD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "abort_edge:abort edge" (layer F.Cu) (tedit 56916806)
    (at 159.2 121.4 90)
    (fp_text reference E01 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value "abort edge" (at 0 -0.5 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.25 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.75 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.5 1.25 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module w_conn_pc:megb8-8 (layer F.Cu) (tedit 56924562)
    (at 178.308 106.553 180)
    (descr "RJ45 + led indicators, Wiznet P/N RB1-125BAG1A")
    (fp_text reference J4 (at 0.381 -0.635 180) (layer F.SilkS))
    (fp_text value RJ45 (at 0.254 1.651 360) (layer F.SilkS))
    (pad 3 thru_hole circle (at -1.905 -6.34 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 65 /S88_3))
    (pad 1 thru_hole circle (at -4.445 -6.34 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 /S88_1))
    (pad 2 thru_hole circle (at -3.175 -8.88 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 /S88_2))
    (pad 4 thru_hole circle (at -0.635 -8.88 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 /S88_4))
    (pad 5 thru_hole circle (at 0.635 -6.34 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 /S88_5))
    (pad 6 thru_hole circle (at 1.905 -8.88 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 /S88_6))
    (pad 7 thru_hole circle (at 3.175 -6.34 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 71 /S88_7))
    (pad 8 thru_hole circle (at 4.445 -8.88 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 /S88_8))
    (pad 13 thru_hole circle (at -7.75 -3.05 180) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 7.75 -3.05 180) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5.715 0 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
  )
  (module w_conn_pc:megb8-8 (layer F.Cu) (tedit 5692455A)
    (at 178.181 136.398)
    (descr "RJ45 + led indicators, Wiznet P/N RB1-125BAG1A")
    (fp_text reference J3 (at 0.635 -0.381) (layer F.SilkS))
    (fp_text value RJ45 (at 0.254 2.032 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at -1.905 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 65 /S88_3))
    (pad 1 thru_hole circle (at -4.445 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 /S88_1))
    (pad 2 thru_hole circle (at -3.175 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 /S88_2))
    (pad 4 thru_hole circle (at -0.635 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 /S88_4))
    (pad 5 thru_hole circle (at 0.635 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 /S88_5))
    (pad 6 thru_hole circle (at 1.905 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 /S88_6))
    (pad 7 thru_hole circle (at 3.175 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 71 /S88_7))
    (pad 8 thru_hole circle (at 4.445 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 /S88_8))
    (pad 13 thru_hole circle (at -7.75 -3.05) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 7.75 -3.05) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5.715 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
  )
  (module w_conn_pc:megb8-8 (layer F.Cu) (tedit 569245B5)
    (at 141 136.8)
    (descr "RJ45 + led indicators, Wiznet P/N RB1-125BAG1A")
    (fp_text reference J2 (at 0.5796 -0.275) (layer F.SilkS))
    (fp_text value RJ45 (at 0.351 1.884) (layer F.SilkS))
    (pad 3 thru_hole circle (at -1.905 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 /CB3))
    (pad 1 thru_hole circle (at -4.445 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 /CB1))
    (pad 2 thru_hole circle (at -3.175 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 /CB2))
    (pad 4 thru_hole circle (at -0.635 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 /CB4))
    (pad 5 thru_hole circle (at 0.635 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 /CB5))
    (pad 6 thru_hole circle (at 1.905 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 /CB6))
    (pad 7 thru_hole circle (at 3.175 -6.34) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 /CB7))
    (pad 8 thru_hole circle (at 4.445 -8.88) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 /CB8))
    (pad 13 thru_hole circle (at -7.75 -3.05) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 7.75 -3.05) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5.715 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu))
  )
  (module Pin_Headers:Pin_Header_Straight_2x08 (layer F.Cu) (tedit 56965830)
    (at 188.595 112.522)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P20 (at -0.0762 20.1676) (layer F.SilkS))
    (fp_text value "S88 CONN" (at -2.794 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 /S88_1))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(P2-Pad6)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /S88_2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(P2-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 /S88_3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(P2-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /S88_4))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(P2-Pad3)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /S88_5))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(P20-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /S88_6))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(P2-Pad4)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 /S88_7))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(P2-Pad5)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 /S88_8))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(P20-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5696584E)
    (at 166.37 115.443)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P22 (at -0.0508 15.3416) (layer F.SilkS))
    (fp_text value S88 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(P2-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 78xx:TO-220-78xx (layer F.Cu) (tedit 56A4B021)
    (at 160.528 46.609 270)
    (descr "TO-220, Bipolar-BCE, Horizontal,")
    (tags "TO-220, Bipolar-BCE, Horizontal,")
    (fp_text reference U2 (at -4.826 -2.413 360) (layer F.SilkS))
    (fp_text value LM7805 (at -4.1275 -8.509 540) (layer F.Fab))
    (pad GND thru_hole oval (at 0 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 GNDA))
    (pad VI thru_hole oval (at -2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 +15V))
    (pad VO thru_hole oval (at 2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 116 +5VA))
    (pad "" np_thru_hole circle (at 0 -16.764) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
  )
  (module w_smd_dil:ssop-16 (layer B.Cu) (tedit 0)
    (at 103.632 55.626)
    (descr SSOP-16)
    (fp_text reference U13 (at 0 -0.508) (layer B.SilkS))
    (fp_text value FT230XS (at 0 1.143) (layer B.SilkS))
    (pad 4 smd rect (at -0.3175 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 10 /TxD))
    (pad 5 smd rect (at 0.3175 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.9525 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(U13-Pad6)"))
    (pad 7 smd rect (at 1.5875 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 129 /RxLED))
    (pad 16 smd rect (at -2.2225 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(U13-Pad16)"))
    (pad 1 smd rect (at -2.2225 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 11 /RxD))
    (pad 2 smd rect (at -1.5875 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(U13-Pad2)"))
    (pad 3 smd rect (at -0.9525 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(C20-Pad1)"))
    (pad 9 smd rect (at 2.2225 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(R16-Pad1)"))
    (pad 10 smd rect (at 1.5875 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(C20-Pad1)"))
    (pad 11 smd rect (at 0.9525 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(C20-Pad1)"))
    (pad 12 smd rect (at 0.3175 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 117 VCOM))
    (pad 13 smd rect (at -0.3175 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -0.9525 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 130 /TxLED))
    (pad 8 smd rect (at 2.2225 -2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(R17-Pad1)"))
    (pad 15 smd rect (at -1.5875 2.667) (size 0.4064 1.651) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(U13-Pad15)"))
    (model walter/smd_dil/ssop-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5779FB83)
    (at 175.5775 98.171 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at -0.2286 -2.5019 90) (layer F.SilkS))
    (fp_text value I2C-Bus (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /I2C_SDA))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /I2C_SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(C10-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-3-3,5-h (layer F.Cu) (tedit 56A4B29E)
    (at 168.91 85.852 90)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P8 (at -2.286 -7.0485 90) (layer F.SilkS))
    (fp_text value RS485 (at -2.9972 -5.0546 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(P8-Pad2)"))
    (pad 1 thru_hole rect (at 3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(P8-Pad1)"))
    (pad 3 thru_hole circle (at -3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model walter/conn_pt-1_5/pt_1,5-3-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-2-3,5-h (layer F.Cu) (tedit 589876AD)
    (at 168.91 76.835 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P11 (at -0.1397 1.3589 270) (layer F.SilkS))
    (fp_text value SNIFFER (at 4.7752 -10.9982 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at -1.75 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 1.75 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P11-Pad1)"))
    (model walter/conn_pt-1_5/pt_1,5-2-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57B61C15)
    (at 149.098 82.844 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C21 (at -2.0955 -0.0635 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x09 (layer F.Cu) (tedit 5779FBFA)
    (at 134.239 53.34 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at -0.254 -3.429 90) (layer F.SilkS))
    (fp_text value SPI (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /MISO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(P10-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /SCLK))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /MOSI))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /PI14))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /CE0))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x09.wrl
      (at (xyz 0 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 58986463)
    (at 140.0175 56.3245 180)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R10 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1K5 (at 0 2.032 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(P10-Pad2)"))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 78xx:DCDC (layer F.Cu) (tedit 5735EA0C)
    (at 134.6708 117.2464 270)
    (descr "DC-DC Board")
    (tags DCDC)
    (fp_text reference P23 (at 1.8796 -5.8166 270) (layer F.SilkS))
    (fp_text value CONN_01X08 (at -3.683 -7.53 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at -6.604 -9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(P23-Pad1)"))
    (pad 2 thru_hole oval (at -4.064 -9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(P23-Pad1)"))
    (pad 3 thru_hole oval (at 4.064 -9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 /CB4))
    (pad 4 thru_hole oval (at 6.604 -9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 /CB4))
    (pad 5 thru_hole oval (at -6.604 9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 53 /CB6))
    (pad 6 thru_hole oval (at -4.064 9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 53 /CB6))
    (pad 7 thru_hole oval (at 4.064 9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 /CB4))
    (pad 8 thru_hole oval (at 6.604 9.271 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 /CB4))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57DFA813)
    (at 150.9268 112.2426)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P24 (at -3.4268 -0.8426) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(P15-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(P23-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /CVCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 56A4B0C8)
    (at 187.325 48.641)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at -1.143 -2.0955) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 GNDA))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 0)
    (at 186.055 52.451 180)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R12 (at 0 0 180) (layer F.SilkS))
    (fp_text value 220 (at 0 2.032 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 116 +5VA))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 131.699 73.8505 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C12 (at 1.25 -3.8 90) (layer F.SilkS))
    (fp_text value 10uf (at 1.25 3.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(C12-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 56A63046)
    (at 182.626 43.434 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 0.3175 -1.8415 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 14 GNDA))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 58986A66)
    (at 110.0074 63.2714 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 2.7686 -0.9906 180) (layer F.SilkS))
    (fp_text value LED (at -3.2385 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C20-Pad1)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 58986A63)
    (at 110.0074 65.3288 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 2.7432 -0.9652 180) (layer F.SilkS))
    (fp_text value LED (at -3.2385 0.0635 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C20-Pad1)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B5830A)
    (at 109.855 58.928 180)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C22 (at -4.1275 -1.4605 180) (layer B.SilkS))
    (fp_text value 10nF (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 180) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B582C8)
    (at 109.9185 61.1505 180)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference F1 (at -2.794 -0.508 180) (layer B.SilkS))
    (fp_text value Ferrit (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 180) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 117 VCOM))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 58985CF3)
    (at 147.574 62.4332 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C16 (at -1.0287 -2.0955 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 54189DEE)
    (at 137.6426 63.0428 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 589866FB)
    (at 167.1828 68.6308 90)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C19 (at 3.302 -0.0508 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 116 +5VA))
    (pad 2 smd rect (at 1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 GNDA))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 5898671E)
    (at 151.257 71.6788 90)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C18 (at 3.2004 -0.0254 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B58300)
    (at 103.4415 61.849 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C26 (at 3.302 -0.254 270) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 117 VCOM))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B582F4)
    (at 101.4095 61.849 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C25 (at -3.175 0.762 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 117 VCOM))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B5831A)
    (at 112.776 57.785 90)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 27 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(C23-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B58314)
    (at 106.9975 55.626 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C23 (at -2.9845 0.127 270) (layer B.SilkS))
    (fp_text value 47pf (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 56A64E42)
    (at 109.093 52.1335)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0.254 -1.651) (layer B.SilkS))
    (fp_text value 27 (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 128 "Net-(C24-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 56A64F0A)
    (at 102.616 49.102 90)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C20 (at 0.08 -1.651 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 1.05 0 90) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 56A64E39)
    (at 112.7125 53.1495 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C24 (at 1.27 -1.8415 270) (layer B.SilkS))
    (fp_text value 47pf (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 128 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B582CF)
    (at 109.9312 65.3288)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 4.318 -0.0635) (layer B.SilkS))
    (fp_text value 220 (at 0 -4.699) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 130 /TxLED))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer B.Cu) (tedit 57B582E9)
    (at 109.982 63.2714)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 4.445 0) (layer B.SilkS))
    (fp_text value 220 (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 129 /RxLED))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer F.Cu) (tedit 5898763A)
    (at 183.007 91.186)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C10 (at 3.7338 -0.3556) (layer F.SilkS))
    (fp_text value 100nF (at -0.0508 -0.0254) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer F.Cu) (tedit 5898763E)
    (at 183.007 93.218)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 3.8354 -1.0414) (layer F.SilkS))
    (fp_text value 3k3 (at -0.0254 0.0254) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /I2C_SDA))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer F.Cu) (tedit 58987637)
    (at 183.007 95.25)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 3.7846 -1.6764) (layer F.SilkS))
    (fp_text value 3k3 (at -0.0762 0.1524) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /I2C_SCL))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer F.Cu) (tedit 57B6BF85)
    (at 170.0784 92.456 180)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C9 (at 2.7559 0.0635 180) (layer F.SilkS))
    (fp_text value 100nF (at -0.0381 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer F.Cu) (tedit 5735E224)
    (at 170.7515 95.377 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 3.2385 -0.0635 270) (layer F.SilkS))
    (fp_text value 3K3 (at 0.0254 -0.1397 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /I2C_SDA2))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer F.Cu) (tedit 5735E22A)
    (at 168.656 95.377 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 3.2385 -0.0635 270) (layer F.SilkS))
    (fp_text value 3k3 (at -0.0254 -0.0254 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /I2C_SCL2))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering_II (layer F.Cu) (tedit 54189DEE)
    (at 182.626 47.244 270)
    (descr "Resistor SMD 0805, hand soldering (little msmaller)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 220 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.05 0 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 116 +5VA))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_copper_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 116.0145 121.0945)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference G*** (at 0.3 -1.4) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.3 0.5) (layer F.SilkS) hide)
  )
  (module w_pth_circuits:dil_16-300_socket (layer F.Cu) (tedit 56A64FEC)
    (at 124 65 90)
    (descr "IC, DIL16 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U9 (at 0 -6.35 90) (layer F.SilkS))
    (fp_text value MAX3232 (at 0 6.604 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -8.89 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(C12-Pad1)"))
    (pad 2 thru_hole oval (at -6.35 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(C14-Pad1)"))
    (pad 3 thru_hole oval (at -3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(C12-Pad2)"))
    (pad 4 thru_hole oval (at -1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(C13-Pad1)"))
    (pad 5 thru_hole oval (at 1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(C13-Pad2)"))
    (pad 6 thru_hole oval (at 3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(C15-Pad2)"))
    (pad 7 thru_hole oval (at 6.35 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(P9-Pad2)"))
    (pad 8 thru_hole oval (at 8.89 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(P9-Pad4)"))
    (pad 9 thru_hole oval (at 8.89 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CTS2))
    (pad 10 thru_hole oval (at 6.35 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 36 /RTS2))
    (pad 11 thru_hole oval (at 3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 32 /TXD2))
    (pad 12 thru_hole oval (at 1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 31 /RXD2))
    (pad 13 thru_hole oval (at -1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(P9-Pad3)"))
    (pad 14 thru_hole oval (at -3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(P9-Pad1)"))
    (pad 15 thru_hole oval (at -6.35 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole oval (at -8.89 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model walter/pth_circuits/dil_16-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 57B6C339)
    (at 135.509 84.0105 90)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U4 (at 0.0635 0.0635 90) (layer F.SilkS))
    (fp_text value 6N137 (at 3.175 0.762 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(R3-Pad1)"))
    (pad 3 thru_hole oval (at 1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO2))
    (pad 4 thru_hole oval (at 3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (pad 6 thru_hole oval (at 1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LOAD))
    (pad 7 thru_hole oval (at -1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 8 thru_hole oval (at -3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 57B5D627)
    (at 135.509 94.1705 90)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U5 (at 0.0635 0.0635 90) (layer F.SilkS))
    (fp_text value 6N137 (at 3.8481 0.0762 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R4-Pad1)"))
    (pad 3 thru_hole oval (at 1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 /GPIO3))
    (pad 4 thru_hole oval (at 3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (pad 6 thru_hole oval (at 1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 /CLOCK))
    (pad 7 thru_hole oval (at -1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (pad 8 thru_hole oval (at -3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 57B61C1B)
    (at 151.638 94.3356 270)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U8 (at 0.0635 0.0635 270) (layer F.SilkS))
    (fp_text value MAX3072E (at -6.0706 -0.1905 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 26 /UART3_RX))
    (pad 2 thru_hole oval (at -1.27 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PH2))
    (pad 3 thru_hole oval (at 1.27 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PH2))
    (pad 4 thru_hole oval (at 3.81 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 25 /UART3_TX))
    (pad 5 thru_hole oval (at 3.81 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 1.27 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(P8-Pad1)"))
    (pad 7 thru_hole oval (at -1.27 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(P8-Pad2)"))
    (pad 8 thru_hole oval (at -3.81 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 58985CBE)
    (at 155.81 80.137 90)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U11 (at 0.0635 0.0635 90) (layer F.SilkS))
    (fp_text value 6N137 (at 6.17728 -1.48976 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 1.27 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at 3.81 3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(P31-Pad2)"))
    (pad 7 thru_hole oval (at -1.27 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 8 thru_hole oval (at -3.81 -3.81 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 589873FB)
    (at 141.859 62.992)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U1 (at 0.0635 0.0635) (layer F.SilkS))
    (fp_text value MCP2562 (at 6.2484 1.397 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 44 /CANTX))
    (pad 2 thru_hole oval (at -1.27 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 1.27 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 3.81 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 45 /CANRX))
    (pad 5 thru_hole oval (at 3.81 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 6 thru_hole oval (at 1.27 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(P5-Pad2)"))
    (pad 7 thru_hole oval (at -1.27 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(R1-Pad1)"))
    (pad 8 thru_hole oval (at -3.81 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_copper_CC-BY-SA_10x4.5mm (layer B.Cu) (tedit 0)
    (at 168.5925 43.2435 180)
    (descr "CC BY-SA logo, 10x4.5mm")
    (fp_text reference G*** (at 1.9 -0.5 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 1.9 1.7 180) (layer B.SilkS) hide)
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 575AE9B5)
    (at 166.7256 59.69 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R20 (at 0.254 -2.032 270) (layer B.SilkS))
    (fp_text value 120 (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(P19-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 64 /CANH))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_av:minidin-10 (layer F.Cu) (tedit 57B590B1)
    (at 104.8258 121.3612 270)
    (descr "MiniDin 10 Maerklin")
    (fp_text reference P16 (at 3.8608 3.4163 270) (layer F.SilkS))
    (fp_text value CAN (at 9.8298 -4.2926 270) (layer F.SilkS))
    (pad 7 thru_hole circle (at -3.95 -2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 96 "Net-(P16-Pad7)"))
    (pad 1 thru_hole circle (at 2.3 -2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 56 /CVCC))
    (pad 11 thru_hole circle (at -7.25 1 270) (size 3.5 3.5) (drill 2.2) (layers *.Cu))
    (pad 13 thru_hole circle (at 7.25 1 270) (size 3.5 3.5) (drill 2.2) (layers *.Cu))
    (pad 3 thru_hole circle (at -1.7 -2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 94 "Net-(P16-Pad3)"))
    (pad 2 thru_hole circle (at 0.3 -2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 51 /CB4))
    (pad 4 thru_hole circle (at 3.95 -2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 55 /CB8))
    (pad 6 thru_hole circle (at 0 -4.5 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 97 "Net-(P16-Pad6)"))
    (pad 5 thru_hole circle (at 2 -4.50088 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 99 "Net-(P16-Pad5)"))
    (pad 10 thru_hole circle (at -3.95 -4.5 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 95 "Net-(P16-Pad10)"))
    (pad 9 thru_hole circle (at -2 -4.5 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 98 "Net-(P16-Pad9)"))
    (pad 8 thru_hole circle (at 3.95 -4.50088 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 54 /CB7))
    (pad 12 thru_hole circle (at 0 1.8 270) (size 3.5 3.5) (drill 2.5) (layers *.Cu))
    (model walter/conn_av/minidin-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_av:minidin-10 (layer F.Cu) (tedit 57B59114)
    (at 116.2812 107.3912 180)
    (descr "MiniDin 10 Maerklin")
    (fp_text reference P17 (at -4.0513 3.1242 180) (layer F.SilkS))
    (fp_text value CAN (at -0.1524 -7.747 180) (layer F.SilkS))
    (pad 7 thru_hole circle (at -3.95 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 59 "Net-(P17-Pad7)"))
    (pad 1 thru_hole circle (at 2.3 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 56 /CVCC))
    (pad 11 thru_hole circle (at -7.25 1 180) (size 3.5 3.5) (drill 2.2) (layers *.Cu))
    (pad 13 thru_hole circle (at 7.25 1 180) (size 3.5 3.5) (drill 2.2) (layers *.Cu))
    (pad 3 thru_hole circle (at -1.7 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 57 "Net-(P17-Pad3)"))
    (pad 2 thru_hole circle (at 0.3 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 51 /CB4))
    (pad 4 thru_hole circle (at 3.95 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 55 /CB8))
    (pad 6 thru_hole circle (at 0 -4.5 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 60 "Net-(P17-Pad6)"))
    (pad 5 thru_hole circle (at 2 -4.50088 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 62 "Net-(P17-Pad5)"))
    (pad 10 thru_hole circle (at -3.95 -4.5 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 58 "Net-(P17-Pad10)"))
    (pad 9 thru_hole circle (at -2 -4.5 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 61 "Net-(P17-Pad9)"))
    (pad 8 thru_hole circle (at 3.95 -4.50088 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 54 /CB7))
    (pad 12 thru_hole circle (at 0 1.8 180) (size 3.5 3.5) (drill 2.5) (layers *.Cu))
    (model walter/conn_av/minidin-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_av:minidin-10 (layer F.Cu) (tedit 57B5905C)
    (at 135.3312 107.3912 180)
    (descr "MiniDin 10 Maerklin")
    (fp_text reference P18 (at -3.9878 3.3147 180) (layer F.SilkS))
    (fp_text value CAN (at -0.3556 -7.8232 180) (layer F.SilkS))
    (pad 7 thru_hole circle (at -3.95 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 102 "Net-(P18-Pad7)"))
    (pad 1 thru_hole circle (at 2.3 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 56 /CVCC))
    (pad 11 thru_hole circle (at -7.25 1 180) (size 3.5 3.5) (drill 2.2) (layers *.Cu))
    (pad 13 thru_hole circle (at 7.25 1 180) (size 3.5 3.5) (drill 2.2) (layers *.Cu))
    (pad 3 thru_hole circle (at -1.7 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 100 "Net-(P18-Pad3)"))
    (pad 2 thru_hole circle (at 0.3 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 51 /CB4))
    (pad 4 thru_hole circle (at 3.95 -2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 55 /CB8))
    (pad 6 thru_hole circle (at 0 -4.5 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 103 "Net-(P18-Pad6)"))
    (pad 5 thru_hole circle (at 2 -4.50088 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 105 "Net-(P18-Pad5)"))
    (pad 10 thru_hole circle (at -3.95 -4.5 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 101 "Net-(P18-Pad10)"))
    (pad 9 thru_hole circle (at -2 -4.5 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 104 "Net-(P18-Pad9)"))
    (pad 8 thru_hole circle (at 3.95 -4.50088 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.SilkS *.Mask)
      (net 54 /CB7))
    (pad 12 thru_hole circle (at 0 1.8 180) (size 3.5 3.5) (drill 2.5) (layers *.Cu))
    (model walter/conn_av/minidin-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57B5C4A4)
    (at 101.981 98.044 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P26 (at -0.254 6.1595 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GNDD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5VD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57DFA9E4)
    (at 147.4 124 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P27 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value POWER (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /CB6))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 133 /CB6'))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57DFA9DD)
    (at 147.4 120.5 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P28 (at -0.15 -6.35 180) (layer F.SilkS))
    (fp_text value POWER (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /CB6))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /CVCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57DFACF5)
    (at 157.5 111.7 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P29 (at -0.05 -3.25 270) (layer F.SilkS) hide)
    (fp_text value POWER (at 0.1 -3.25 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /CVCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(P15-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_S4B-PH-K (layer F.Cu) (tedit 55F6C32A)
    (at 159.322 96.3168)
    (descr "JST PH series connector, S4B-PH-K")
    (tags "connector jst ph")
    (fp_text reference P25 (at 2.984 3.3528) (layer F.SilkS))
    (fp_text value I2C-Bus (at 3 7.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 23 /I2C_SDA2))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 24 /I2C_SCL2))
    (model walter/conn_jst-ph/s4b-ph-kl.wrl
      (at (xyz 0.119 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 148.844 80.264 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P31 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PH2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(P31-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /PI3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_pth_diodes:diode_do35 (layer F.Cu) (tedit 58967370)
    (at 162 79.5 90)
    (descr "Diode, DO-35 package")
    (fp_text reference D1 (at -0.25 0 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 -2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(D1-Pad2)"))
    (model walter/pth_diodes/diode_do35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 589723DD)
    (at 187.7568 59.0296)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D6 (at 4.8006 -0.7874) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab) hide)
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 138 /GND_))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 137 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 5898426D)
    (at 188.976 62.4332 180)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R14 (at 0 0 180) (layer F.SilkS))
    (fp_text value 8k2 (at 0 2.032 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 137 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 141 /VCC_))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 589723C4)
    (at 190.8048 85.09 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P30 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 139 /rt_))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 140 /br_))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_capacitors:cnp_3mm_disc (layer F.Cu) (tedit 58985CD9)
    (at 150.20544 71.59752 90)
    (descr "Small ceramic capacitor")
    (tags C)
    (fp_text reference C27 (at -0.51816 -2.09296 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 -2.286 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model walter/capacitors/cnp_3mm_disc.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:cnp_3mm_disc (layer F.Cu) (tedit 589876A6)
    (at 167.64 72.1868)
    (descr "Small ceramic capacitor")
    (tags C)
    (fp_text reference C28 (at -4.064 -1.5748) (layer F.SilkS))
    (fp_text value 100nF (at 0 -2.286) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 116 +5VA))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 GNDA))
    (model walter/capacitors/cnp_3mm_disc.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 58985033)
    (at 164.719 59.563 270)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R28 (at 0 0 270) (layer F.SilkS))
    (fp_text value 120 (at 0 2.032 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(P19-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 64 /CANH))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RTS (at 104.6734 74.3458) (layer F.SilkS))
  (gr_text CTS (at 104.5972 69.2404) (layer F.SilkS))
  (gr_text RxD (at 104.6734 71.7296) (layer F.SilkS))
  (gr_text TxD (at 104.8004 76.8604) (layer F.SilkS))
  (gr_text GND (at 104.775 66.6496) (layer F.SilkS))
  (gr_text CAN-Term (at 161.1376 51.562) (layer F.SilkS))
  (gr_text "Gerhard Bertelsmann" (at 197 72 90) (layer B.Cu))
  (gr_text "V1.5 02/17" (at 196 72 90) (layer B.Cu))
  (gr_text GND (at 183.7944 76.0984) (layer F.SilkS))
  (gr_text "VCC\n" (at 183.8706 70.9422) (layer F.SilkS))
  (gr_text CANL (at 183.769 68.3768) (layer F.SilkS))
  (gr_text CANH (at 183.9214 65.8114) (layer F.SilkS))
  (gr_text br (at 190.8556 82.2452 90) (layer F.SilkS))
  (gr_text rt (at 188.0616 82.4484 90) (layer F.SilkS))
  (gr_text PH2 (at 146.812 80.264 90) (layer F.SilkS))
  (gr_text PI3 (at 146.558 74.93 90) (layer F.SilkS))
  (gr_line (start 176 58.5) (end 176 55.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176 69.5) (end 176 65.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179 65.75) (end 179 78.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 58.5) (end 177.5 60) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 65.75) (end 177.5 64.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 65.75) (end 176 65.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.5 78.25) (end 172.5 72.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.5 79.75) (end 174 79.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174 84) (end 177.5 84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.5 88.5) (end 172.5 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174 78.25) (end 174 79.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 78.25) (end 179 78.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174 85.5) (end 172.5 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 85.5) (end 177.5 84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 58.5) (end 179 58.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 58.5) (end 200 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.5 57) (end 198.5 57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.5 87) (end 198.5 87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180.5 85.5) (end 180.5 87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 198.5 85.5) (end 200 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 198.5 58.5) (end 198.5 57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180.5 58.5) (end 179 58.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text RxD (at 113.792 63.5254) (layer F.SilkS))
  (gr_text 5V (at 104.7115 95.8215) (layer F.SilkS))
  (gr_text GND (at 101.7905 95.8215) (layer F.SilkS))
  (gr_text SDA (at 178.054 96.393) (layer F.SilkS))
  (gr_text SCL (at 180.848 96.393) (layer F.SilkS))
  (gr_text G (at 184.7596 96.774) (layer F.SilkS))
  (gr_text V (at 176.022 96.3168) (layer F.SilkS))
  (gr_text VCC (at 151.1046 119.3292) (layer F.SilkS))
  (gr_text GND (at 151.3332 121.7168) (layer F.SilkS))
  (gr_text 5V (at 151.95 124.65) (layer F.SilkS))
  (gr_text CANL (at 151.0538 127.889) (layer F.SilkS))
  (gr_text CANH (at 151.1046 131.3942) (layer F.SilkS))
  (gr_text 3V3 (at 161.3408 93.98 90) (layer F.SilkS))
  (gr_text SCL (at 165.4048 94.1324 90) (layer F.SilkS))
  (gr_text SDA (at 163.4236 93.8784 90) (layer F.SilkS))
  (gr_text GND (at 159.5628 93.8276 90) (layer F.SilkS))
  (gr_text TxD (at 113.5634 65.5828) (layer F.SilkS))
  (gr_text "V1.5 02/17" (at 168.5925 46.228) (layer B.Cu))
  (gr_text "Gerhard Bertelsmann" (at 115.5065 124.714) (layer F.Cu))
  (gr_text "V1.5 02/17" (at 115.5065 123.698) (layer F.Cu))
  (gr_text "V1.5 02/17" (at 190.1825 138.4935) (layer F.Cu))
  (gr_text "Gerhard Bertelsmann" (at 190.6905 139.319) (layer F.Cu))
  (gr_text "Gerhard Bertelsmann" (at 168.656 47.3075) (layer B.Cu))
  (gr_text VCC (at 166.878 55.753) (layer F.SilkS))
  (dimension 2.667 (width 0.3) (layer Dwgs.User)
    (gr_text "2.667 mm" (at 92.8078 41.3385 270) (layer Dwgs.User))
    (feature1 (pts (xy 109.6264 42.672) (xy 91.4578 42.672)))
    (feature2 (pts (xy 109.6264 40.005) (xy 91.4578 40.005)))
    (crossbar (pts (xy 94.1578 40.005) (xy 94.1578 42.672)))
    (arrow1a (pts (xy 94.1578 42.672) (xy 93.571379 41.545496)))
    (arrow1b (pts (xy 94.1578 42.672) (xy 94.744221 41.545496)))
    (arrow2a (pts (xy 94.1578 40.005) (xy 93.571379 41.131504)))
    (arrow2b (pts (xy 94.1578 40.005) (xy 94.744221 41.131504)))
  )
  (gr_text GND (at 166.9034 58.8518) (layer F.SilkS))
  (gr_text 5V (at 166.624 62.1665) (layer F.SilkS))
  (gr_text CANH (at 166.497 69.1515) (layer F.SilkS))
  (gr_text CANL (at 166.497 65.9765) (layer F.SilkS))
  (gr_text GND (at 140.1572 50.6984) (layer F.SilkS))
  (gr_text RxD (at 134.747 50.673) (layer F.SilkS))
  (gr_text TxD (at 137.5664 50.7492) (layer F.SilkS))
  (dimension 12 (width 0.3) (layer Dwgs.User)
    (gr_text "12.000 mm" (at 149 37.4) (layer Dwgs.User))
    (feature1 (pts (xy 155 42.5) (xy 155 36.05)))
    (feature2 (pts (xy 143 42.5) (xy 143 36.05)))
    (crossbar (pts (xy 143 38.75) (xy 155 38.75)))
    (arrow1a (pts (xy 155 38.75) (xy 153.873496 39.336421)))
    (arrow1b (pts (xy 155 38.75) (xy 153.873496 38.163579)))
    (arrow2a (pts (xy 143 38.75) (xy 144.126504 39.336421)))
    (arrow2b (pts (xy 143 38.75) (xy 144.126504 38.163579)))
  )
  (gr_line (start 148.25 100) (end 172.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141 100) (end 114.75 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.75 103) (end 141 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 141 101.5) (end 141 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 141 101.5) (end 142.5 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.5 100) (end 107.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.5 103) (end 107.5 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.25 101.5) (end 146.75 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.25 103) (end 158.5 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.25 101.5) (end 148.25 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174 90) (end 190 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.5 54) (end 190 54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174 71) (end 174.5 71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174.5 69.5) (end 176 69.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174 72.5) (end 172.5 72.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.5 117.5) (end 163 117.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.5 124.5) (end 161.5 123) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163 124.5) (end 163 138.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163 104.5) (end 163 117.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160 124.5) (end 160 138.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160 104.5) (end 160 117.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.5 124.5) (end 160 124.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.5 117.5) (end 161.5 119) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.5 103) (end 172.5 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.5 140) (end 198.5 140) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 164.5 138.5) (end 164.5 140) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.5 138.5) (end 160 138.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 164.5 104.5) (end 163 104.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.5 104.5) (end 158.5 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 91.5 (width 0.3) (layer Dwgs.User)
    (gr_text "91.500 mm" (at 145.75 29.65) (layer Dwgs.User))
    (feature1 (pts (xy 191.5 46) (xy 191.5 28.3)))
    (feature2 (pts (xy 100 46) (xy 100 28.3)))
    (crossbar (pts (xy 100 31) (xy 191.5 31)))
    (arrow1a (pts (xy 191.5 31) (xy 190.373496 31.586421)))
    (arrow1b (pts (xy 191.5 31) (xy 190.373496 30.413579)))
    (arrow2a (pts (xy 100 31) (xy 101.126504 31.586421)))
    (arrow2b (pts (xy 100 31) (xy 101.126504 30.413579)))
  )
  (dimension 60 (width 0.3) (layer Dwgs.User)
    (gr_text "60.000 mm" (at 200.85 70 270) (layer Dwgs.User))
    (feature1 (pts (xy 187 100) (xy 202.2 100)))
    (feature2 (pts (xy 187 40) (xy 202.2 40)))
    (crossbar (pts (xy 199.5 40) (xy 199.5 100)))
    (arrow1a (pts (xy 199.5 100) (xy 198.913579 98.873496)))
    (arrow1b (pts (xy 199.5 100) (xy 200.086421 98.873496)))
    (arrow2a (pts (xy 199.5 40) (xy 198.913579 41.126504)))
    (arrow2b (pts (xy 199.5 40) (xy 200.086421 41.126504)))
  )
  (dimension 43 (width 0.3) (layer Dwgs.User)
    (gr_text "43.000 mm" (at 121.5 35.15) (layer Dwgs.User))
    (feature1 (pts (xy 100 43) (xy 100 33.8)))
    (feature2 (pts (xy 143 43) (xy 143 33.8)))
    (crossbar (pts (xy 143 36.5) (xy 100 36.5)))
    (arrow1a (pts (xy 100 36.5) (xy 101.126504 35.913579)))
    (arrow1b (pts (xy 100 36.5) (xy 101.126504 37.086421)))
    (arrow2a (pts (xy 143 36.5) (xy 141.873496 35.913579)))
    (arrow2b (pts (xy 143 36.5) (xy 141.873496 37.086421)))
  )
  (dimension 100 (width 0.3) (layer Dwgs.User)
    (gr_text "100.000 mm" (at 150 146.85) (layer Dwgs.User))
    (feature1 (pts (xy 200 137.5) (xy 200 148.2)))
    (feature2 (pts (xy 100 137.5) (xy 100 148.2)))
    (crossbar (pts (xy 100 145.5) (xy 200 145.5)))
    (arrow1a (pts (xy 200 145.5) (xy 198.873496 146.086421)))
    (arrow1b (pts (xy 200 145.5) (xy 198.873496 144.913579)))
    (arrow2a (pts (xy 100 145.5) (xy 101.126504 146.086421)))
    (arrow2b (pts (xy 100 145.5) (xy 101.126504 144.913579)))
  )
  (dimension 100 (width 0.3) (layer Dwgs.User)
    (gr_text "100.000 mm" (at 95.15 90 90) (layer Dwgs.User))
    (feature1 (pts (xy 103 40) (xy 93.8 40)))
    (feature2 (pts (xy 103 140) (xy 93.8 140)))
    (crossbar (pts (xy 96.5 140) (xy 96.5 40)))
    (arrow1a (pts (xy 96.5 40) (xy 97.086421 41.126504)))
    (arrow1b (pts (xy 96.5 40) (xy 95.913579 41.126504)))
    (arrow2a (pts (xy 96.5 140) (xy 97.086421 138.873496)))
    (arrow2b (pts (xy 96.5 140) (xy 95.913579 138.873496)))
  )
  (gr_arc (start 114.75 101.5) (end 114.75 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 114.75 101.5) (end 113.25 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.5 101.5) (end 172.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.5 101.5) (end 174 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.5 101.5) (end 179.5 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.5 101.5) (end 178 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190 100) (end 179.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.5 103) (end 179.5 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107.5 101.5) (end 109 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107.5 101.5) (end 107.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 198.5 138.5) (end 200 138.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 198.5 104.5) (end 198.5 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 101.5 104.5) (end 100 104.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 101.5 138.5) (end 101.5 140) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 104.5) (end 100 138.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 104.5) (end 200 138.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.5 140) (end 158.5 140) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 190 91.5) (end 190 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174 88.5) (end 174 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 55.5) (end 176 55.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 190 52.5) (end 191.5 52.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.5 41.5) (end 191.5 52.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 141.5 41.5) (end 141.5 40) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 156.5 41.5) (end 155 41.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.5 50) (end 155 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.5 50) (end 144.5 51.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.5 51.5) (end 153.5 51.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143 41.5) (end 143 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155 41.5) (end 155 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190 40) (end 156.5 40) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 41.5) (end 100 98.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.5 91.5) (end 191.5 98.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 190 41.5) (end 190 40) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 190 98.5) (end 191.5 98.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 101.5 98.5) (end 101.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 101.5 41.5) (end 100 41.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.5 40) (end 141.5 40) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 22) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.334 99.6823) (xy 99.403 99.6688) (xy 99.441 84.963) (xy 125.73 84.963) (xy 127.8636 82.3722)
        (xy 127.889 82.3595) (xy 130.2385 79.4385) (xy 130.7465 78.994) (xy 132.842 78.994) (xy 133.731 80.01)
        (xy 133.731 99.695)
      )
    )
  )
  (zone (net 51) (net_name /CB4) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.403 140.38) (xy 159.768 140.4435) (xy 159.768 140.38) (xy 160.403 140.38)
      )
    )
  )
  (zone (net 51) (net_name /CB4) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.7045 140.38) (xy 99.403 140.38) (xy 99.4284 103.2436) (xy 159.7299 103.2436) (xy 159.7045 140.38)
      )
    )
  )
  (zone (net 118) (net_name "Net-(C10-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 99.949) (xy 177.165 99.949) (xy 177.165 89.916) (xy 191.77 89.916) (xy 191.77 99.949)
      )
    )
  )
  (zone (net 118) (net_name "Net-(C10-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 99.949) (xy 177.165 99.949) (xy 177.165 89.916) (xy 191.77 89.916) (xy 191.77 99.949)
      )
    )
  )
  (zone (net 14) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.516 53.975) (xy 176.149 53.975) (xy 176.149 71.12) (xy 173.482 71.12) (xy 172.593 72.136)
        (xy 172.593 79.756) (xy 164.973 79.756) (xy 159.512 74.676) (xy 159.512 51.562) (xy 155.0416 48.3616)
        (xy 154.94 40.005) (xy 191.516 40.005) (xy 191.516 53.975)
      )
    )
  )
  (zone (net 14) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.516 53.975) (xy 176.149 53.975) (xy 176.149 71.12) (xy 173.482 71.12) (xy 172.593 72.136)
        (xy 172.593 79.756) (xy 164.973 79.756) (xy 159.512 74.676) (xy 159.512 51.562) (xy 154.9908 48.3108)
        (xy 155.067 40.005) (xy 191.516 40.005) (xy 191.516 53.975)
      )
    )
  )
  (zone (net 65) (net_name /S88_3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.025 140.208) (xy 163.3855 139.954) (xy 163.3855 102.87) (xy 200.279 102.87) (xy 200.025 140.208)
      )
    )
  )
  (zone (net 65) (net_name /S88_3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.025 140.208) (xy 163.3855 140.208) (xy 163.3855 102.87) (xy 200.279 102.87) (xy 200.025 140.208)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.511 51.054) (xy 154.051 51.054) (xy 154.051 54.61) (xy 157.099 57.404) (xy 157.099 73.4568)
        (xy 153.035 75.692) (xy 153.035 83.312) (xy 154.7622 83.2866) (xy 158.115 86.868) (xy 162.687 86.868)
        (xy 165.989 81.788) (xy 172.339 81.788) (xy 172.339 88.646) (xy 174.625 90.424) (xy 175.387 91.186)
        (xy 175.387 96.012) (xy 173.609 96.012) (xy 171.2722 99.5934) (xy 137.3505 99.6315) (xy 137.3505 79.502)
        (xy 134.5565 77.1525) (xy 125.6665 77.1525) (xy 121.92 81.026) (xy 99.695 81.026) (xy 99.695 39.624)
        (xy 143.256 39.624) (xy 143.256 51.054)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.4475 51.054) (xy 153.9875 51.054) (xy 153.9875 54.61) (xy 157.0355 57.404) (xy 157.0355 73.3552)
        (xy 152.9715 75.692) (xy 152.9715 83.312) (xy 154.6987 83.2866) (xy 158.0515 86.868) (xy 162.6235 86.868)
        (xy 165.9255 81.788) (xy 172.2755 81.788) (xy 172.2755 88.646) (xy 175.3235 91.186) (xy 175.3235 96.012)
        (xy 173.5455 96.012) (xy 171.2849 99.568) (xy 137.3505 99.6315) (xy 137.3505 79.502) (xy 134.493 77.1525)
        (xy 125.603 77.1525) (xy 121.92 81.026) (xy 99.695 81.026) (xy 99.695 39.624) (xy 143.1925 39.624)
        (xy 143.1925 51.054)
      )
    )
  )
  (zone (net 22) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.334 99.6823) (xy 99.403 99.6688) (xy 99.441 84.963) (xy 125.73 84.963) (xy 127.8636 82.3722)
        (xy 127.889 82.3595) (xy 130.2385 79.4385) (xy 130.7465 78.994) (xy 132.842 78.994) (xy 133.731 80.01)
        (xy 133.731 99.695)
      )
    )
  )
  (zone (net 51) (net_name /CB4) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.403 140.38) (xy 99.403 103.269) (xy 159.7045 103.269) (xy 159.7045 140.3165) (xy 99.403 140.38)
      )
    )
  )
  (zone (net 138) (net_name /GND_) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179 57) (xy 200 57) (xy 200 87) (xy 179 87)
      )
    )
  )
  (zone (net 138) (net_name /GND_) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179 57) (xy 200 57) (xy 200 87) (xy 179 87)
      )
    )
  )
)
