<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<circle x="0" y="0" locked="yes" radius="24" width="0.1524" layer="20"/>
<text>Desc: 1930 Breakout
Part #: ZRT-2020-00006-A
Date: 2020/08/31</text>
<text>J1.1 = J2.8-10 = GND
J1.2 = +5.0V
J1.3 = J2.16 = RESERVED
J1.4 = J2.6 = TXTD_UNC
J1.5 = J2.15 = RXTD_UNC
J1.6 = J2.5 = RESET
J1.7 = J2.14 = NOUTPUT_DIS_MODE_SEL_UNC
J1.8 = J2.4 = NIBIT
J1.9 = J2.13 = SER_DATA_OUT_H
J1.10 = J2.3 = SER_DATA_OUT_L
J1.11 = J2.12 = DATA_SYNC_OUT_IN_L_UNC
J1.12 = J2.2 = DATA_SYNC_OUT_IN_H_UNC
J1.13 = J2.11 = XMT_RCV_CLK_H
J1.14 = J2.1 = XMR_RCV_CLK_L</text>
</plain>
<libraries>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="KTDELMS112QHRH2526E6">
<description>&lt;b&gt;KT DELMS1.12-QHRH-25-26E6-4&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CAPC2012X145N">
<description>&lt;b&gt;CC0805 1.45T CASE EB&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="RESC1608X55N">
<description>&lt;b&gt;RC0603&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="RectangularConnectors_Harwin">
<packages>
<package name="M80-5022042">
</package>
</packages>
</library>
<library name="MountingHole_SAE">
<packages>
<package name="CAPSCREW_NC_2-56">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.5 mm with drill center</description>
</package>
</packages>
</library>
<library name="RectangularConnectors_Samtec">
<packages>
<package name="CLT-107-YY-XX">
<description>&lt;b&gt;CLT-107-YY-XX-D&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="RectangularConnectors_Harwin" package="M80-5022042" value="M80-5022042">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SamacSys_Parts" package="KTDELMS112QHRH2526E6" value="KT_DELMS1.12-QHRH-25-26E6">
<attribute name="DESCRIPTION" value="Standard LEDs - SMD True Green TOPLED E 1608"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="OSRAM"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="KT DELMS1.12-QHRH-25-26E6"/>
<attribute name="MOUSER_PART_NUMBER" value="720-KTDELMS112A5167"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/OSRAM-Opto-Semiconductors/KT-DELMS112-QHRH-25-26E6?qs=XeJtXLiO41TGvurUVIwLkg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="MountingHole_SAE" package="CAPSCREW_NC_2-56" value="CAPSCREW_NC_2-56"/>
<element name="H2" library="MountingHole_SAE" package="CAPSCREW_NC_2-56" value="CAPSCREW_NC_2-56"/>
<element name="H3" library="MountingHole_SAE" package="CAPSCREW_NC_2-56" value="CAPSCREW_NC_2-56"/>
<element name="H4" library="MountingHole_SAE" package="CAPSCREW_NC_2-56" value="CAPSCREW_NC_2-56"/>
<element name="J1" library="RectangularConnectors_Samtec" package="CLT-107-YY-XX" value="CLT-107-01-F-D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SamacSys_Parts" package="CAPC2012X145N" value="CC0805KKX7R7BB106">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT 10uF 16V 10% Ceramic Capacitor"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO (PHYCOMP)"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CC0805KKX7R7BB106"/>
<attribute name="MOUSER_PART_NUMBER" value="603-CC0805KKX77BB106"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Yageo/CC0805KKX7R7BB106?qs=UgE%2F0m3bTsbyPftnSvLmPQ%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SamacSys_Parts" package="RESC1608X55N" value="RC0603FR-13200RL">
<attribute name="DESCRIPTION" value="Thick Film Resistors - SMD 200 OHM 1%"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO (PHYCOMP)"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RC0603FR-13200RL"/>
<attribute name="MOUSER_PART_NUMBER" value="603-RC0603FR-13200RL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Yageo/RC0603FR-13200RL?qs=J1R1puj4KiHFcttXMMFd8A%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SamacSys_Parts" package="CAPC2012X145N" value="CC0805KKX7R7BB106">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT 10uF 16V 10% Ceramic Capacitor"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO (PHYCOMP)"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CC0805KKX7R7BB106"/>
<attribute name="MOUSER_PART_NUMBER" value="603-CC0805KKX77BB106"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Yageo/CC0805KKX7R7BB106?qs=UgE%2F0m3bTsbyPftnSvLmPQ%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$4">
<contactref element="LED1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="8"/>
<contactref element="J2" pad="10"/>
<contactref element="J2" pad="9"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="18"/>
<contactref element="J2" pad="19"/>
<contactref element="J2" pad="20"/>
<contactref element="C2" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="RESERVED">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="16"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="NIBIT">
<contactref element="J1" pad="8"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="SER_DATA_OUT_H">
<contactref element="J1" pad="9"/>
<contactref element="J2" pad="13"/>
</signal>
<signal name="SER_DATA_OUT_L">
<contactref element="J1" pad="10"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="XMT_RCV_CLK_H">
<contactref element="J1" pad="13"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="XMT_RCV_CLK_L">
<contactref element="J1" pad="14"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="TXTD_UNC">
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="RXTD_UNC">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="15"/>
</signal>
<signal name="NOUTPUT_DIS_MODE_SEL_UNC">
<contactref element="J1" pad="7"/>
<contactref element="J2" pad="14"/>
</signal>
<signal name="DATA_SYNC_OUT_IN_H_UNC">
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="DATA_SYNC_OUT_IN_L_UNC">
<contactref element="J1" pad="11"/>
<contactref element="J2" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
