(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 12)
    (zones 0)
    (modules 4)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 113.03 97.663)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /jack_sleeve)
  (net 2 /tip_normal)
  (net 3 /jack_tip)
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /jack_sleeve)
    (add_net /jack_tip)
    (add_net /tip_normal)
  )
  (module zzzzzzzz:PinHeader_1x03_P2.54mm_Vertical_Castellated_RH (layer F.Cu) (tedit 609EEA71)
    (at 130.81 99.568)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, castellated, right-hand side")
    (tags "Through hole pin header THT 1x03 2.54mm castellated right-hand")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /tip_normal))
    (pad 2 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /jack_sleeve))
    (pad 1 thru_hole rect (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /jack_tip))
    (pad 3 thru_hole oval (at 0 5.08) (size 4.24 1.7) (drill 1 (offset 1.27 0)) (layers *.Cu *.Mask)
      (net 2 /tip_normal))
    (pad 2 thru_hole oval (at 0 2.54) (size 4.24 1.7) (drill 1 (offset 1.27 0)) (layers *.Cu *.Mask)
      (net 1 /jack_sleeve))
    (pad 1 thru_hole rect (at 0 0) (size 4.24 1.7) (drill 1 (offset 1.27 0)) (layers *.Cu *.Mask)
      (net 3 /jack_tip))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module zzzzzzzz:PinHeader_1x03_P2.54mm_Vertical_Castellated_LH (layer F.Cu) (tedit 609EEA87)
    (at 110.49 99.568)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, castellated left-hand side")
    (tags "Through hole pin header THT 1x03 2.54mm castellated left hand")
    (fp_text reference J2 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /tip_normal))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /jack_sleeve))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /jack_tip))
    (pad 3 thru_hole oval (at 2.54 5.08) (size 4.24 1.7) (drill 1 (offset -1.27 0)) (layers *.Cu *.Mask)
      (net 2 /tip_normal))
    (pad 2 thru_hole oval (at 2.54 2.54) (size 4.24 1.7) (drill 1 (offset -1.27 0)) (layers *.Cu *.Mask)
      (net 1 /jack_sleeve))
    (pad 1 thru_hole rect (at 2.54 0) (size 4.24 1.7) (drill 1 (offset -1.27 0)) (layers *.Cu *.Mask)
      (net 3 /jack_tip))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module zzzzzzzz:zzzzzzzz_back_no_cu (layer F.Cu) (tedit 607A6312)
    (at 121.539 101.346)
    (fp_text reference Ref** (at 0 0) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 0) (layer F.SilkS) hide)
  )
  (module AudioJacks:Jack_3.5mm_QingPu_WQP-PJ301BM_Vertical (layer F.Cu) (tedit 605714FA)
    (at 121.92 102.108)
    (fp_text reference J1 (at 0 0) (layer F.SilkS))
    (fp_text value AudioJack2_SwitchT (at 3.7 -6.4) (layer F.Fab))
    (pad S thru_hole oval (at 4.7 0.6 90) (size 4 3) (drill oval 2 1) (layers *.Cu *.Mask)
      (net 1 /jack_sleeve))
    (pad S thru_hole oval (at -4.7 0 90) (size 4.5 3) (drill oval 2.5 1) (layers *.Cu *.Mask)
      (net 1 /jack_sleeve))
    (pad TN thru_hole oval (at 0 3.3) (size 4 2) (drill oval 2.5 0.5) (layers *.Cu *.Mask)
      (net 2 /tip_normal))
    (pad T thru_hole oval (at 0 -4.8) (size 4 2) (drill oval 2.5 0.5) (layers *.Cu *.Mask)
      (net 3 /jack_tip))
    (model ${KISYS3DMOD}/AudioJacks.3dshapes/PJ301BM.step
      (offset (xyz 0 0 2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/AudioJacks.3dshapes/PJ301BM_Hex_nut.step
      (offset (xyz 0 0 2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/AudioJacks.3dshapes/PJ301BM_Knurl_nut.step
      (offset (xyz 0 0 2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 113.03 97.663) (end 113.03 95.123) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.03 106.553) (end 110.49 106.553) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 130.81 106.553) (end 130.81 109.093) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 130.81 97.663) (end 133.35 97.663) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.03 109.093) (end 130.81 109.093) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.49 97.663) (end 110.49 106.553) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.81 95.123) (end 113.03 95.123) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.35 106.553) (end 133.35 97.663) (layer Edge.Cuts) (width 0.05))
  (dimension 5.08 (width 0.15) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 115.57 86.203) (layer Dwgs.User))
    (feature1 (pts (xy 113.03 89.408) (xy 113.03 86.916579)))
    (feature2 (pts (xy 118.11 89.408) (xy 118.11 86.916579)))
    (crossbar (pts (xy 118.11 87.503) (xy 113.03 87.503)))
    (arrow1a (pts (xy 113.03 87.503) (xy 114.156504 86.916579)))
    (arrow1b (pts (xy 113.03 87.503) (xy 114.156504 88.089421)))
    (arrow2a (pts (xy 118.11 87.503) (xy 116.983496 86.916579)))
    (arrow2b (pts (xy 118.11 87.503) (xy 116.983496 88.089421)))
  )
  (dimension 5.08 (width 0.15) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 128.27 86.203) (layer Dwgs.User))
    (feature1 (pts (xy 130.81 89.408) (xy 130.81 86.916579)))
    (feature2 (pts (xy 125.73 89.408) (xy 125.73 86.916579)))
    (crossbar (pts (xy 125.73 87.503) (xy 130.81 87.503)))
    (arrow1a (pts (xy 130.81 87.503) (xy 129.683496 88.089421)))
    (arrow1b (pts (xy 130.81 87.503) (xy 129.683496 86.916579)))
    (arrow2a (pts (xy 125.73 87.503) (xy 126.856504 88.089421)))
    (arrow2b (pts (xy 125.73 87.503) (xy 126.856504 86.916579)))
  )
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "0.3000 in" (at 121.92 82.393) (layer Dwgs.User))
    (feature1 (pts (xy 118.11 89.408) (xy 118.11 83.106579)))
    (feature2 (pts (xy 125.73 89.408) (xy 125.73 83.106579)))
    (crossbar (pts (xy 125.73 83.693) (xy 118.11 83.693)))
    (arrow1a (pts (xy 118.11 83.693) (xy 119.236504 83.106579)))
    (arrow1b (pts (xy 118.11 83.693) (xy 119.236504 84.279421)))
    (arrow2a (pts (xy 125.73 83.693) (xy 124.603496 83.106579)))
    (arrow2b (pts (xy 125.73 83.693) (xy 124.603496 84.279421)))
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.985 110.998) (xy 109.855 110.998) (xy 109.855 92.583) (xy 133.985 92.583)
      )
    )
  )
)
