(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 122.124999 106.574999 128.775001 113.475001)
    (thickness 1.6)
    (drawings 5)
    (tracks 50)
    (zones 0)
    (modules 19)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 576B8F0F)
    (at 126.4 110.3 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0.95 -1.636 180) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x08 (at 1.6 -2.186 180) (layer F.Fab))
    (pad 1 connect rect (at 0 -1.516 180) (size 0.4 0.4) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 -1.016 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -0.516 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0 -0.016 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 0.484 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0 0.984 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0 1.484 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 1.984 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.01 0))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 90))
    )
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 127.85 112.4 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D8162)
    (at 127.85 110.95 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 -0.25 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 127.85 108.8 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D813F)
    (at 127.85 107.25 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 -0.35 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 127.85 110 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 126.65 112.75 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 125.45 112.75 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 124.25 112.75 180)
    (fp_text reference REF** (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 126.65 107.3)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 125.45 107.3)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 124.25 107.3)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 123.05 110.05)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D813F)
    (at 123.05 112.8)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 -0.35) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 123.05 111.25)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D8162)
    (at 123.05 109.1)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 -0.25) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "1x1 pad" (layer B.Cu) (tedit 576D7BE9)
    (at 123.05 107.65)
    (fp_text reference REF** (at 0 -0.254) (layer B.SilkS))
    (fp_text value ".8 pad" (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module "silicon chip" (layer B.Cu) (tedit 576C2481)
    (at 125.2 110.15)
    (fp_text reference REF** (at -1.016 1.016) (layer B.SilkS))
    (fp_text value "silicon chip" (at -0.508 1.524) (layer B.Fab))
    (pad 9 smd rect (at 0.25 -0.13) (size 3 4) (layers B.Cu B.Paste B.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 576B8F0F)
    (at 124.5 109.75)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0.95 -1.636) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x08 (at 1.6 -2.186) (layer F.Fab))
    (pad 1 connect rect (at 0 -1.516) (size 0.4 0.4) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 -1.016) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -0.516) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0 -0.016) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 0.484) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0 0.984) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0 1.484) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 1.984) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.01 0))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 122.2 113.4) (end 122.2 106.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.25 113.4) (end 122.2 113.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.7 113.4) (end 122.25 113.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.7 106.65) (end 128.7 113.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.2 106.65) (end 128.7 106.65) (angle 90) (layer Edge.Cuts) (width 0.15))
)
