(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 186)
    (no_connects 0)
    (area 130.734999 69.774999 170.255001 135.330001)
    (thickness 1.6)
    (drawings 29)
    (tracks 1231)
    (zones 0)
    (modules 45)
    (nets 84)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.375)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFCFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VBUS)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 +3V3)
  (net 8 VCC)
  (net 9 "Net-(C8-Pad1)")
  (net 10 /1V8)
  (net 11 VSPI)
  (net 12 /SW)
  (net 13 "Net-(L1-Pad1)")
  (net 14 /TCK)
  (net 15 /TDO)
  (net 16 /TMS)
  (net 17 /~RST)
  (net 18 /TDI)
  (net 19 /UDM)
  (net 20 /UDP)
  (net 21 /USB_ID)
  (net 22 /AMISO)
  (net 23 /ASCK)
  (net 24 /AMOSI)
  (net 25 /A18)
  (net 26 /A16)
  (net 27 /A15)
  (net 28 /A12)
  (net 29 /A7)
  (net 30 /A6)
  (net 31 /A5)
  (net 32 /A4)
  (net 33 /A3)
  (net 34 /A2)
  (net 35 /A1)
  (net 36 /A0)
  (net 37 /D0)
  (net 38 /D1)
  (net 39 /D2)
  (net 40 /~WR)
  (net 41 /A17)
  (net 42 /A14)
  (net 43 /A13)
  (net 44 /A8)
  (net 45 /A9)
  (net 46 /A11)
  (net 47 /~RD)
  (net 48 /A10)
  (net 49 /~CE)
  (net 50 /D7)
  (net 51 /D6)
  (net 52 /D5)
  (net 53 /D4)
  (net 54 /D3)
  (net 55 /QMOSI)
  (net 56 /~QCS)
  (net 57 /QSCK)
  (net 58 ~ESPI_EN)
  (net 59 ESPI_BUF)
  (net 60 "Net-(R17-Pad2)")
  (net 61 "Net-(R18-Pad2)")
  (net 62 /ICK)
  (net 63 /~ESPI_HD)
  (net 64 /~ESPI_WP)
  (net 65 /~ICS)
  (net 66 /ESPI_MOSI)
  (net 67 /ESPI_CK)
  (net 68 /ESPI_MISO)
  (net 69 /~ESPI_CS)
  (net 70 /IMISO)
  (net 71 /IMOSI)
  (net 72 /QMISO)
  (net 73 /~QWP)
  (net 74 /~QHD)
  (net 75 /LD1)
  (net 76 /LD2)
  (net 77 /~HWB)
  (net 78 /VSPI_ADC)
  (net 79 "Net-(RP5-Pad8)")
  (net 80 "Net-(RP5-Pad7)")
  (net 81 "Net-(RP5-Pad6)")
  (net 82 /LR1)
  (net 83 /LR2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /1V8)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AMISO)
    (add_net /AMOSI)
    (add_net /ASCK)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /ESPI_CK)
    (add_net /ESPI_MISO)
    (add_net /ESPI_MOSI)
    (add_net /ICK)
    (add_net /IMISO)
    (add_net /IMOSI)
    (add_net /LD1)
    (add_net /LD2)
    (add_net /LR1)
    (add_net /LR2)
    (add_net /QMISO)
    (add_net /QMOSI)
    (add_net /QSCK)
    (add_net /SW)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /UDM)
    (add_net /UDP)
    (add_net /USB_ID)
    (add_net /VBUS)
    (add_net /VSPI_ADC)
    (add_net /~CE)
    (add_net /~ESPI_CS)
    (add_net /~ESPI_HD)
    (add_net /~ESPI_WP)
    (add_net /~HWB)
    (add_net /~ICS)
    (add_net /~QCS)
    (add_net /~QHD)
    (add_net /~QWP)
    (add_net /~RD)
    (add_net /~RST)
    (add_net /~WR)
    (add_net ESPI_BUF)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(RP5-Pad6)")
    (add_net "Net-(RP5-Pad7)")
    (add_net "Net-(RP5-Pad8)")
    (add_net VCC)
    (add_net VSPI)
    (add_net ~ESPI_EN)
  )
  (module Connect:USB_Micro-B (layer F.Cu) (tedit 58F7730C)
    (at 150.495 132.08)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P2 (at 0 -3.24) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at 0 5.01) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /VBUS))
    (pad 2 smd rect (at -0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /UDM))
    (pad 3 smd rect (at 0 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /UDP))
    (pad 4 smd rect (at 0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /USB_ID))
    (pad 5 smd rect (at 1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.5 -1.35 90) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.5 -1.35 90) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -3.5 1.35 90) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 3.5 1.35 90) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 161.417 75.311 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Power_Integrations:PDIP-8 (layer F.Cu) (tedit 58F73BEA)
    (at 150.495 72.39)
    (descr "PDIP-8 Standard 300mil 8pin Dual In Line Package")
    (tags "Power Integrations P Package")
    (fp_text reference U6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value DIL8 (at 0 1.524) (layer F.Fab))
    (pad 1 smd rect (at -3.81 0) (size 1.905 3.81) (layers B.Cu B.Paste B.Mask)
      (net 69 /~ESPI_CS))
    (pad 2 smd rect (at -1.27 0) (size 1.905 3.81) (layers B.Cu B.Paste B.Mask)
      (net 68 /ESPI_MISO))
    (pad 3 smd rect (at 1.27 0) (size 1.905 3.81) (layers B.Cu B.Paste B.Mask)
      (net 64 /~ESPI_WP))
    (pad 4 smd rect (at 3.81 0) (size 1.905 3.81) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.81 0) (size 1.905 3.81) (layers F.Cu F.Paste F.Mask)
      (net 66 /ESPI_MOSI))
    (pad 6 smd trapezoid (at 1.27 0) (size 1.905 3.81) (layers F.Cu F.Paste F.Mask)
      (net 67 /ESPI_CK))
    (pad 7 smd rect (at -1.27 0) (size 1.905 3.81) (layers F.Cu F.Paste F.Mask)
      (net 63 /~ESPI_HD))
    (pad 8 smd rect (at -3.81 0) (size 1.905 3.81) (layers F.Cu F.Paste F.Mask)
      (net 11 VSPI))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58F73B56)
    (at 137.795 127.635 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.75 270) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /VBUS))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58F73BE2)
    (at 159.385 92.075 315)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.25 315) (layer B.SilkS) hide)
    (fp_text value 22p (at 0 -1.5 315) (layer B.Fab))
    (fp_text user %R (at 0 1.25 315) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 315) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 315) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58F73BD8)
    (at 162.56 95.25 135)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.25 135) (layer B.SilkS) hide)
    (fp_text value 22p (at 0 -1.5 135) (layer B.Fab))
    (fp_text user %R (at 0 1.25 135) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 135) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 135) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58F73BB3)
    (at 156.845 114.935 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58F73BC2)
    (at 146.05 114.935)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58F73B5E)
    (at 142.875 127.635 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 1.75 90) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58F73BC9)
    (at 140.335 109.855 315)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 315) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.75 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 315) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 315) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1.25 0 315) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58F73BFE)
    (at 139.065 79.375 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58F73B86)
    (at 136.525 76.2 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 1.75 270) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 /1V8))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58F73B89)
    (at 143.51 78.105 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -1.75 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 VSPI))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58F73B6C)
    (at 161.29 123.825 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 82 /LR1))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58F73B69)
    (at 163.83 123.825 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 83 /LR2))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58F73B4A)
    (at 137.16 130.81 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value SMD (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 58F73B66)
    (at 162.56 130.175 180)
    (fp_text reference JP1 (at 0 -0.762 180) (layer F.SilkS) hide)
    (fp_text value Button (at 0 1.016 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 /SW))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 /SW))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58F73B62)
    (at 140.97 130.81)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 1.7) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm (layer F.Cu) (tedit 58F73B76)
    (at 144.145 118.745 270)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference P1 (at 0.635 -1.695 270) (layer F.SilkS) hide)
    (fp_text value AVR_JTAG (at 0.635 6.775 270) (layer F.Fab))
    (fp_text user %R (at 0.635 -1.695 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /TCK))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 /TDO))
    (pad 4 thru_hole oval (at 1.27 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 5 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /TMS))
    (pad 6 thru_hole oval (at 1.27 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /~RST))
    (pad 7 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 1.27 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /TDI))
    (pad 10 thru_hole oval (at 1.27 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58F73B6F)
    (at 161.29 119.38 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value BOOT/ALE (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /~HWB))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 58F73B72)
    (at 154.94 118.11 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P4 (at 1.27 -2.33 270) (layer F.SilkS) hide)
    (fp_text value AVRISP (at 1.27 7.41 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /AMISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /ASCK))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /AMOSI))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /~RST))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm locked (layer F.Cu) (tedit 58F73B7F)
    (at 134.62 80.01)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value UL (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A18))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /A16))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /A15))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /A12))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /A7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /A6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /A5))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /A4))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm locked (layer F.Cu) (tedit 58F73B7A)
    (at 134.62 106.68)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P6 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value DL (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /A3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /A1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /A0))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /D0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /D1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /D2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm locked (layer F.Cu) (tedit 58F73BAC)
    (at 166.37 80.01)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P7 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value UR (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /~WR))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /A17))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /A14))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /A13))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /A8))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /A9))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /A11))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm locked (layer F.Cu) (tedit 58F73BAF)
    (at 166.37 101.6)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P8 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value DR (at -1.1811 16.9164) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /~RD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /A10))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /~CE))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /D7))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /D6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /D5))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /D4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /D3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58F73BA6)
    (at 163.1315 85.09 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 1k5 (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer B.Cu) (tedit 58F73C07)
    (at 138.43 95.885 270)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R8 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value 8R2 (at 0 -2.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -3.95 0 270) (size 2.7 3.2) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 3.95 0 270) (size 2.7 3.2) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F73BA4)
    (at 159.385 85.09 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 ~ESPI_EN))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F73BA9)
    (at 158.115 78.105 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 ESPI_BUF))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 VSPI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F73BB7)
    (at 152.4 126.365 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value 22 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /UDM))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F73BBF)
    (at 154.94 126.365 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value 22 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /UDP))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 58F73B98)
    (at 150.495 86.36 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP1 (at 0 -2.6 180) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 VSPI))
    (pad 3 smd rect (at -0.85 0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 VSPI))
    (pad 1 smd rect (at -0.85 -1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.85 1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 VSPI))
    (pad 8 smd rect (at 0.85 -1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 62 /ICK))
    (pad 7 smd rect (at 0.85 -0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 63 /~ESPI_HD))
    (pad 6 smd rect (at 0.85 0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 64 /~ESPI_WP))
    (pad 5 smd rect (at 0.85 1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 65 /~ICS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 58F73B9C)
    (at 150.495 82.55 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP2 (at 0 -2.6 270) (layer F.SilkS) hide)
    (fp_text value 49R9 (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 66 /ESPI_MOSI))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 67 /ESPI_CK))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 /ESPI_MISO))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 /~ESPI_CS))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 /IMISO))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 71 /IMOSI))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 62 /ICK))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 65 /~ICS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer B.Cu) (tedit 58F73B5A)
    (at 140.335 127.635 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value LM3671MF-3.3/NOPB (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 /VBUS))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 /VBUS))
    (pad 4 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 5 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(L1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-64_14x14mm_Pitch0.8mm (layer F.Cu) (tedit 58F73BC7)
    (at 150.495 103.505 135)
    (descr "64-Lead Plastic Thin Quad Flatpack (PF) - 14x14x1 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 -9.45 135) (layer F.SilkS) hide)
    (fp_text value AT90USB646-AU (at 0 9.45 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -7.7 -6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /A18))
    (pad 2 smd rect (at -7.7 -5.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /SW))
    (pad 3 smd rect (at -7.7 -4.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /VBUS))
    (pad 4 smd rect (at -7.7 -3.6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R17-Pad2)"))
    (pad 5 smd rect (at -7.7 -2.8 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R18-Pad2)"))
    (pad 6 smd rect (at -7.7 -2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -7.7 -1.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 8 smd rect (at -7.7 -0.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /VBUS))
    (pad 9 smd rect (at -7.7 0.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /USB_ID))
    (pad 10 smd rect (at -7.7 1.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /A0))
    (pad 11 smd rect (at -7.7 2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /ASCK))
    (pad 12 smd rect (at -7.7 2.8 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /AMOSI))
    (pad 13 smd rect (at -7.7 3.6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /AMISO))
    (pad 14 smd rect (at -7.7 4.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /A4))
    (pad 15 smd rect (at -7.7 5.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /A5))
    (pad 16 smd rect (at -7.7 6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /A6))
    (pad 17 smd rect (at -6 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /A7))
    (pad 18 smd rect (at -5.2 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /A16))
    (pad 19 smd rect (at -4.4 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /A17))
    (pad 20 smd rect (at -3.6 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /~RST))
    (pad 21 smd rect (at -2.8 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 22 smd rect (at -2 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -1.2 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 24 smd rect (at -0.4 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 25 smd rect (at 0.4 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 58 ~ESPI_EN))
    (pad 26 smd rect (at 1.2 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 59 ESPI_BUF))
    (pad 27 smd rect (at 2 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 72 /QMISO))
    (pad 28 smd rect (at 2.8 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(RP5-Pad6)"))
    (pad 29 smd rect (at 3.6 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(RP5-Pad7)"))
    (pad 30 smd rect (at 4.4 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(RP5-Pad8)"))
    (pad 31 smd rect (at 5.2 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 /~QWP))
    (pad 32 smd rect (at 6 7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 74 /~QHD))
    (pad 33 smd rect (at 7.7 6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /~WR))
    (pad 34 smd rect (at 7.7 5.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 /~RD))
    (pad 35 smd rect (at 7.7 4.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 /A8))
    (pad 36 smd rect (at 7.7 3.6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /A9))
    (pad 37 smd rect (at 7.7 2.8 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 /A10))
    (pad 38 smd rect (at 7.7 2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /A11))
    (pad 39 smd rect (at 7.7 1.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /A12))
    (pad 40 smd rect (at 7.7 0.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 /A13))
    (pad 41 smd rect (at 7.7 -0.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 /A14))
    (pad 42 smd rect (at 7.7 -1.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /A15))
    (pad 43 smd rect (at 7.7 -2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 77 /~HWB))
    (pad 44 smd rect (at 7.7 -2.8 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 /D7))
    (pad 45 smd rect (at 7.7 -3.6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 /D6))
    (pad 46 smd rect (at 7.7 -4.4 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 52 /D5))
    (pad 47 smd rect (at 7.7 -5.2 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 53 /D4))
    (pad 48 smd rect (at 7.7 -6 135) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 /D3))
    (pad 49 smd rect (at 6 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /D2))
    (pad 50 smd rect (at 5.2 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /D1))
    (pad 51 smd rect (at 4.4 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /D0))
    (pad 52 smd rect (at 3.6 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 53 smd rect (at 2.8 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 54 smd rect (at 2 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /TDI))
    (pad 55 smd rect (at 1.2 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /TDO))
    (pad 56 smd rect (at 0.4 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /TMS))
    (pad 57 smd rect (at -0.4 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /TCK))
    (pad 58 smd rect (at -1.2 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 76 /LD2))
    (pad 59 smd rect (at -2 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 75 /LD1))
    (pad 60 smd rect (at -2.8 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 /~CE))
    (pad 61 smd rect (at -3.6 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 78 /VSPI_ADC))
    (pad 62 smd rect (at -4.4 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 63 smd rect (at -5.2 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 64 smd rect (at -6 -7.7 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Housings_QFP.3dshapes/TQFP-64_14x14mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer B.Cu) (tedit 58F73B8B)
    (at 139.065 76.2 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0 2.9 90) (layer B.SilkS) hide)
    (fp_text value MCP1824T-1802E/OT (at 0 -2.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 10 /1V8))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-N (layer B.Cu) (tedit 58F73B95)
    (at 144.145 85.09 180)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 0.127 1.27 180) (layer B.SilkS) hide)
    (fp_text value 74AVC4T245D (at 0 -1.27 180) (layer B.Fab))
    (pad 16 smd rect (at -4.445 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 11 VSPI))
    (pad 14 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 65 /~ICS))
    (pad 12 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 62 /ICK))
    (pad 11 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 64 /~ESPI_WP))
    (pad 10 smd rect (at 3.175 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 63 /~ESPI_HD))
    (pad 9 smd rect (at 4.445 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 4.445 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.175 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 74 /~QHD))
    (pad 6 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 73 /~QWP))
    (pad 5 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 57 /QSCK))
    (pad 4 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 56 /~QCS))
    (pad 3 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.175 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 1 smd rect (at -4.445 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 15 smd rect (at -3.175 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 58 ~ESPI_EN))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-N (layer B.Cu) (tedit 58F73B9F)
    (at 156.21 85.09 180)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U5 (at 0.127 1.27 180) (layer B.SilkS) hide)
    (fp_text value 74AVC4T245D (at 0 -1.27 180) (layer B.Fab))
    (pad 16 smd rect (at -4.445 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 11 VSPI))
    (pad 14 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 71 /IMOSI))
    (pad 12 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 71 /IMOSI))
    (pad 11 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 70 /IMISO))
    (pad 10 smd rect (at 3.175 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 70 /IMISO))
    (pad 9 smd rect (at 4.445 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 4.445 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.175 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 72 /QMISO))
    (pad 6 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 72 /QMISO))
    (pad 5 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 55 /QMOSI))
    (pad 4 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 55 /QMOSI))
    (pad 3 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.175 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 1 smd rect (at -4.445 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 15 smd rect (at -3.175 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 58 ~ESPI_EN))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58F73BDC)
    (at 157.204319 93.704319 315)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.44 -3.525 315) (layer F.SilkS) hide)
    (fp_text value 16M (at 2.44 3.525 315) (layer F.Fab))
    (fp_text user %R (at 2.44 0 315) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 315) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 315) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58F73B4D)
    (at 140.97 133.35 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value JUMPER3 (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VBUS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58F73B8E)
    (at 140.97 71.755 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value JUMPER3 (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VSPI))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /1V8))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 58F73B91)
    (at 146.685 79.375 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference P9 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ISP (at 1.27 9.95 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VSPI))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /~ESPI_CS))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /ESPI_CK))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /ESPI_MOSI))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /ESPI_MISO))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 ESPI_BUF))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer B.Cu) (tedit 58F73BCF)
    (at 148.59 98.552 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP3 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 2 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (pad 3 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 11 VSPI))
    (pad 1 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (pad 4 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 77 /~HWB))
    (pad 7 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 17 /~RST))
    (pad 6 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 78 /VSPI_ADC))
    (pad 5 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 78 /VSPI_ADC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer B.Cu) (tedit 58F73BCC)
    (at 150.4315 108.712 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP4 (at 0 2.6 180) (layer B.SilkS) hide)
    (fp_text value 2k2 (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 2 smd rect (at -0.85 0.4 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 24 /AMOSI))
    (pad 3 smd rect (at -0.85 -0.4 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 23 /ASCK))
    (pad 1 smd rect (at -0.85 1.2 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 22 /AMISO))
    (pad 4 smd rect (at -0.85 -1.2 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 82 /LR1))
    (pad 8 smd rect (at 0.85 1.2 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 33 /A3))
    (pad 7 smd rect (at 0.85 0.4 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 34 /A2))
    (pad 6 smd rect (at 0.85 -0.4 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 35 /A1))
    (pad 5 smd rect (at 0.85 -1.2 180) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 75 /LD1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer B.Cu) (tedit 58F73BD3)
    (at 152.273 97.536 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP5 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value 2k2 (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 2 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 56 /~QCS))
    (pad 3 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 55 /QMOSI))
    (pad 1 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 57 /QSCK))
    (pad 4 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 83 /LR2))
    (pad 8 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(RP5-Pad8)"))
    (pad 7 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(RP5-Pad7)"))
    (pad 6 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(RP5-Pad6)"))
    (pad 5 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 76 /LD2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text -170419- (at 162.56 71.755) (layer F.Mask))
  (gr_text GND (at 156.464 72.39 90) (layer B.SilkS))
  (gr_text JTAG (at 141.478 116.586) (layer F.SilkS))
  (gr_text ~HWB (at 158.877 119.38 90) (layer F.SilkS))
  (gr_text GND (at 138.049 124.46) (layer F.SilkS))
  (gr_text VCC (at 163.449 80.137) (layer F.SilkS))
  (gr_text VCC (at 138.43 128.651) (layer F.SilkS))
  (gr_text VSPI (at 138.43 77.089) (layer F.SilkS))
  (gr_text 2 (at 165.1 123.825) (layer F.SilkS))
  (gr_text 1 (at 159.893 123.825) (layer F.SilkS))
  (gr_text 5V0 (at 140.97 130.937) (layer F.SilkS))
  (gr_text 3V3 (at 133.096 130.937) (layer F.SilkS))
  (gr_text 3V3 (at 140.843 74.295) (layer F.SilkS))
  (gr_text 1V8 (at 135.89 74.295) (layer F.SilkS))
  (gr_text VSPI (at 144.653 72.39 90) (layer F.SilkS))
  (gr_line (start 167.64 135.255) (end 170.18 132.715) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 132.715) (end 133.35 135.255) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 72.39) (end 133.35 69.85) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 69.85) (end 170.18 72.39) (layer Edge.Cuts) (width 0.15))
  (dimension 65.405 (width 0.3) (layer Dwgs.User)
    (gr_text "65.405 mm" (at 123.745 102.5525 270) (layer Dwgs.User))
    (feature1 (pts (xy 130.81 135.255) (xy 122.395 135.255)))
    (feature2 (pts (xy 130.81 69.85) (xy 122.395 69.85)))
    (crossbar (pts (xy 125.095 69.85) (xy 125.095 135.255)))
    (arrow1a (pts (xy 125.095 135.255) (xy 124.508579 134.128496)))
    (arrow1b (pts (xy 125.095 135.255) (xy 125.681421 134.128496)))
    (arrow2a (pts (xy 125.095 69.85) (xy 124.508579 70.976504)))
    (arrow2b (pts (xy 125.095 69.85) (xy 125.681421 70.976504)))
  )
  (dimension 39.37 (width 0.3) (layer Dwgs.User)
    (gr_text "39.370 mm" (at 150.495 142.955) (layer Dwgs.User))
    (feature1 (pts (xy 170.18 135.255) (xy 170.18 144.305)))
    (feature2 (pts (xy 130.81 135.255) (xy 130.81 144.305)))
    (crossbar (pts (xy 130.81 141.605) (xy 170.18 141.605)))
    (arrow1a (pts (xy 170.18 141.605) (xy 169.053496 142.191421)))
    (arrow1b (pts (xy 170.18 141.605) (xy 169.053496 141.018579)))
    (arrow2a (pts (xy 130.81 141.605) (xy 131.936504 142.191421)))
    (arrow2b (pts (xy 130.81 141.605) (xy 131.936504 141.018579)))
  )
  (gr_line (start 130.81 72.39) (end 130.81 132.715) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 69.85) (end 133.35 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 132.715) (end 170.18 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 135.255) (end 167.64 135.255) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 135.255) (xy 167.64 135.255) (xy 170.18 132.715) (xy 170.18 72.39) (xy 167.64 69.85)
        (xy 133.35 69.85) (xy 130.81 72.39) (xy 130.81 132.715)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 135.255) (xy 167.64 135.255) (xy 170.18 132.715) (xy 170.18 72.39) (xy 167.64 69.85)
        (xy 133.35 69.85) (xy 130.81 72.39) (xy 130.81 132.715)
      )
    )
  )
)
