(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 8)
    (zones 0)
    (modules 24)
    (nets 9)
  )
  (page A)
  (title_block
    (title "YSK900 Adapter")
    (date 2019-03-12)
    (rev A)
    (company "Martin Held")
    (comment 1 "Design by Martin Held, AE7EU")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (user_via 0.635 0.381)
    (user_via 0.635 0.381)
    (user_via 0.889 0.635)
    (user_via 0.889 0.635)
    (user_via 1.27 0.889)
    (user_via 1.27 0.889)
    (user_via 1.905 1.524)
    (user_via 1.905 1.524)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1.27 1.27)
    (mod_text_width 0.254)
    (pad_size 0.635 0.635)
    (pad_drill 0.381)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U11-Pad1)")
  (net 3 "Net-(U13-Pad1)")
  (net 4 "Net-(U15-Pad1)")
  (net 5 "Net-(U17-Pad1)")
  (net 6 "Net-(U19-Pad1)")
  (net 7 "Net-(U21-Pad1)")
  (net 8 "Net-(U23-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U11-Pad1)")
    (add_net "Net-(U13-Pad1)")
    (add_net "Net-(U15-Pad1)")
    (add_net "Net-(U17-Pad1)")
    (add_net "Net-(U19-Pad1)")
    (add_net "Net-(U21-Pad1)")
    (add_net "Net-(U23-Pad1)")
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 57.15 45.72)
    (fp_text reference U1 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)"))
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 54.61 43.18)
    (fp_text reference U2 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 "Net-(U11-Pad1)"))
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 57.15 40.64)
    (fp_text reference U3 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 "Net-(U13-Pad1)"))
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 54.61 38.1)
    (fp_text reference U4 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 4 "Net-(U15-Pad1)"))
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 57.15 35.56)
    (fp_text reference U5 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 5 "Net-(U17-Pad1)"))
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 54.61 33.02)
    (fp_text reference U6 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 6 "Net-(U19-Pad1)"))
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 57.15 30.48)
    (fp_text reference U7 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 7 "Net-(U21-Pad1)"))
  )
  (module mheld_std:TP_SPRING (layer F.Cu) (tedit 54B6C308)
    (at 54.61 27.94)
    (fp_text reference U8 (at 0.11 -1.16) (layer F.SilkS) hide)
    (fp_text value TP (at 0.52 1.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 8 "Net-(U23-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 45.72)
    (fp_text reference U9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C885558)
    (at 48.26 45.72)
    (fp_text reference U10 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 43.18)
    (fp_text reference U11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U11-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C885556)
    (at 48.26 43.18)
    (fp_text reference U12 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(U11-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 40.64)
    (fp_text reference U13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U13-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C885554)
    (at 48.26 40.64)
    (fp_text reference U14 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(U13-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 38.1)
    (fp_text reference U15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U15-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C885551)
    (at 48.26 38.1)
    (fp_text reference U16 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(U15-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 35.56)
    (fp_text reference U17 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U17-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C88554F)
    (at 48.26 35.56)
    (fp_text reference U18 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(U17-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 33.02)
    (fp_text reference U19 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U19-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C88554D)
    (at 48.26 33.02)
    (fp_text reference U20 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(U19-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 30.48)
    (fp_text reference U21 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U21-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C88554A)
    (at 48.26 30.48)
    (fp_text reference U22 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(U21-Pad1)"))
  )
  (module mheld_std:PAD_70_300 (layer F.Cu) (tedit 5C3CFC79)
    (at 54.61 27.94)
    (fp_text reference U23 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 7.62 1.778) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U23-Pad1)"))
  )
  (module mheld_std:TP_40mil (layer F.Cu) (tedit 5C885548)
    (at 48.26 27.94)
    (fp_text reference U24 (at -2.794 0.254) (layer F.SilkS) hide)
    (fp_text value TP (at 0.5 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(U23-Pad1)"))
  )
  (gr_text "AE7EU\nYay-su FT900\nYSK900 Interface PCB" (at 40.64 36.83 90) (layer F.SilkS))
  (dimension 6.35 (width 0.3) (layer F.SilkS)
    (gr_text "0.2500 in" (at 40.005 15.045) (layer F.SilkS))
    (feature1 (pts (xy 43.18 26.035) (xy 43.18 16.558579)))
    (feature2 (pts (xy 36.83 26.035) (xy 36.83 16.558579)))
    (crossbar (pts (xy 36.83 17.145) (xy 43.18 17.145)))
    (arrow1a (pts (xy 43.18 17.145) (xy 42.053496 17.731421)))
    (arrow1b (pts (xy 43.18 17.145) (xy 42.053496 16.558579)))
    (arrow2a (pts (xy 36.83 17.145) (xy 37.956504 17.731421)))
    (arrow2b (pts (xy 36.83 17.145) (xy 37.956504 16.558579)))
  )
  (dimension 1.905 (width 0.3) (layer Dwgs.User)
    (gr_text "0.0750 in" (at 60.0075 16.95) (layer Dwgs.User))
    (feature1 (pts (xy 59.055 27.94) (xy 59.055 18.463579)))
    (feature2 (pts (xy 60.96 27.94) (xy 60.96 18.463579)))
    (crossbar (pts (xy 60.96 19.05) (xy 59.055 19.05)))
    (arrow1a (pts (xy 59.055 19.05) (xy 60.181504 18.463579)))
    (arrow1b (pts (xy 59.055 19.05) (xy 60.181504 19.636421)))
    (arrow2a (pts (xy 60.96 19.05) (xy 59.833496 18.463579)))
    (arrow2b (pts (xy 60.96 19.05) (xy 59.833496 19.636421)))
  )
  (dimension 21.59 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8500 in" (at 67.505 36.83 270) (layer Dwgs.User))
    (feature1 (pts (xy 61.595 47.625) (xy 65.991421 47.625)))
    (feature2 (pts (xy 61.595 26.035) (xy 65.991421 26.035)))
    (crossbar (pts (xy 65.405 26.035) (xy 65.405 47.625)))
    (arrow1a (pts (xy 65.405 47.625) (xy 64.818579 46.498496)))
    (arrow1b (pts (xy 65.405 47.625) (xy 65.991421 46.498496)))
    (arrow2a (pts (xy 65.405 26.035) (xy 64.818579 27.161504)))
    (arrow2b (pts (xy 65.405 26.035) (xy 65.991421 27.161504)))
  )
  (dimension 24.13 (width 0.3) (layer Dwgs.User)
    (gr_text "0.9500 in" (at 48.895 20.76) (layer Dwgs.User))
    (feature1 (pts (xy 36.83 26.035) (xy 36.83 22.273579)))
    (feature2 (pts (xy 60.96 26.035) (xy 60.96 22.273579)))
    (crossbar (pts (xy 60.96 22.86) (xy 36.83 22.86)))
    (arrow1a (pts (xy 36.83 22.86) (xy 37.956504 22.273579)))
    (arrow1b (pts (xy 36.83 22.86) (xy 37.956504 23.446421)))
    (arrow2a (pts (xy 60.96 22.86) (xy 59.833496 22.273579)))
    (arrow2b (pts (xy 60.96 22.86) (xy 59.833496 23.446421)))
  )
  (gr_line (start 36.83 26.035) (end 60.96 26.035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.83 47.625) (end 36.83 26.035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.96 47.625) (end 36.83 47.625) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.96 26.035) (end 60.96 47.625) (layer Edge.Cuts) (width 0.1))
)
