(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 4)
    (no_connects 0)
    (area 153.902999 106.325 169.693001 129.815001)
    (thickness 1.6)
    (drawings 11)
    (tracks 11)
    (zones 0)
    (modules 2)
    (nets 17)
  )
  (page A4)
  (title_block
    (title "ELEC-0126 A4988 adapter board")
    (date 2017-04-10)
    (rev 2)
    (company "Marginally Clever Robots, Ltd.")
    (comment 1 "Dan Royer (dan@marginallyclever.com)")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad3)")
  (net 2 "Net-(U1-Pad2)")
  (net 3 "Net-(U1-Pad3)")
  (net 4 "Net-(U1-Pad4)")
  (net 5 "Net-(U1-Pad5)")
  (net 6 "Net-(U1-Pad6)")
  (net 7 "Net-(U1-Pad8)")
  (net 8 "Net-(U1-Pad10)")
  (net 9 "Net-(U1-Pad11)")
  (net 10 "Net-(U1-Pad12)")
  (net 11 "Net-(U1-Pad13)")
  (net 12 "Net-(U1-Pad14)")
  (net 13 GND)
  (net 14 "Net-(P1-Pad4)")
  (net 15 "Net-(P1-Pad2)")
  (net 16 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
  )
  (module a4988:a4988 (layer F.Cu) (tedit 58BDB267)
    (at 161.798 119.38 180)
    (fp_text reference U1 (at 0 11.93 180) (layer F.SilkS))
    (fp_text value A4988 (at -2.286 8.636 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.35 -8.89 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 -6.35 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -6.35 -3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -6.35 -1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at -6.35 1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at -6.35 3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at -6.35 6.35 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 8 thru_hole circle (at -6.35 8.89 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 6.35 8.89 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P1-Pad4)"))
    (pad 10 thru_hole circle (at 6.35 6.35 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at 6.35 3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 6.35 1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at 6.35 -1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 6.35 -3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at 6.35 -6.35 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad3)"))
    (pad 16 thru_hole circle (at 6.35 -8.89 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P1-Pad2)"))
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_4pol (layer F.Cu) (tedit 58BDE2EC)
    (at 160.02 123.952 90)
    (descr "4-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P1 (at -3.048 0 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.08 -2.032 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad4)"))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "G  D  S  E" (at 166.116 118.872 90) (layer F.SilkS))
  (gr_text GND (at 165.608 113.03) (layer B.SilkS))
  (gr_text EN (at 157.734 110.49) (layer B.SilkS))
  (gr_text GND (at 165.354 128.27) (layer B.SilkS))
  (gr_text STEP (at 158.496 125.73) (layer B.SilkS))
  (gr_text DIR (at 157.988 128.27) (layer B.SilkS))
  (gr_line (start 169.164 109.474) (end 169.164 129.286) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.432 109.474) (end 169.164 109.474) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.432 129.286) (end 154.432 109.474) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.164 129.286) (end 154.432 129.286) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Marginally\nClever.com\n2017-03-06 ELEC-0126" (at 164.084 119.888 270) (layer B.SilkS))
)
