(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~90~ubuntu21.04.1)
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 41)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page USLetter)
  (title_block
    (title "DS1x00 SOIC8 to DS1000 DIP14 adapter")
    (date 2021-10-17)
    (rev 001)
    (company "Bran. K. White - b.kenyon.w@gmail.com")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.6)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.3)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 2)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 0 0)
    (grid_origin 136.03 103.81)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_DS1000_DIP14_001"))
  )
  (net 0 "")
  (net 1 /IN)
  (net 2 /TAP2)
  (net 3 /TAP4)
  (net 4 GND)
  (net 5 /TAP5)
  (net 6 /TAP3)
  (net 7 /TAP1)
  (net 8 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6)
    (uvia_drill 0.3)
    (add_net /IN)
    (add_net /TAP1)
    (add_net /TAP2)
    (add_net /TAP3)
    (add_net /TAP4)
    (add_net /TAP5)
    (add_net GND)
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad9)")
    (add_net VCC)
  )
  (module 000_LOCAL:DIP14_0.3_pcb_sil_pins (layer F.Cu) (tedit 616BF2BF)
    (at 136.03 103.81)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference J1 (at 0 0 -90) (layer F.SilkS) hide)
    (fp_text value DS1000 (at -1.5 0 -90) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -3.81 -7.62) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 /IN))
    (pad 2 thru_hole circle (at -3.81 -5.08) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -3.81 -2.54) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 /TAP2))
    (pad 5 thru_hole circle (at -3.81 2.54) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -3.81 5.08) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 /TAP4))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 3.81 7.62) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 /TAP5))
    (pad 9 thru_hole circle (at 3.81 5.08) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 3.81 2.54) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 /TAP3))
    (pad 11 thru_hole circle (at 3.81 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 3.81 -2.54) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 /TAP1))
    (pad 13 thru_hole circle (at 3.81 -5.08) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 3.81 -7.62) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIP14_legs.step_
      (offset (xyz -3.81 7.62 -1.6002))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIP14_legs_solder.step
      (offset (xyz -3.81 7.62 -1.80086))
      (scale (xyz 1 1 1.1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 000_LOCAL:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 616BBA34)
    (at 136.03 103.81 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -0.635 0) (layer F.SilkS))
    (fp_text value DS1100 (at 0.6985 0) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.6 -1.905 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VCC))
    (pad 7 smd roundrect (at 2.6 -0.635 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /TAP1))
    (pad 6 smd roundrect (at 2.6 0.635 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /TAP3))
    (pad 5 smd roundrect (at 2.6 1.905 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /TAP5))
    (pad 4 smd roundrect (at -2.6 1.905 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 3 smd roundrect (at -2.6 0.635 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /TAP4))
    (pad 2 smd roundrect (at -2.6 -0.635 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /TAP2))
    (pad 1 smd roundrect (at -2.6 -1.905 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /IN))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/SOIC-8_3.9x4.9mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:NPTH_0.1 locked (layer F.Cu) (tedit 5F9F8E45)
    (at 136.03 95.555)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value NPTH_0.1 (at 0 -2.54) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
  )
  (gr_text github.com/bkw777/aDIPters (at 138.1255 103.81 90) (layer B.SilkS))
  (gr_text DS1000 (at 136.03 97.7775) (layer F.SilkS))
  (gr_line (start 131.585 112.065) (end 131.585 95.555) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.475 95.555) (end 140.475 112.065) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.585 95.555) (end 140.475 95.555) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.585 112.065) (end 140.475 112.065) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 140.475 112.065) (xy 131.585 112.065) (xy 131.585 95.555) (xy 140.475 95.555)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 140.475 112.065) (xy 131.585 112.065) (xy 131.585 95.555) (xy 140.475 95.555)
      )
    )
  )
)
