(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-c78a2ba~59~ubuntu16.10.1)
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 447)
    (zones 0)
    (modules 37)
    (nets 74)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.152)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 /IM0)
  (net 3 GND)
  (net 4 /IM1)
  (net 5 /IM2)
  (net 6 /IM3)
  (net 7 "Net-(J5-Pad4)")
  (net 8 "Net-(J5-Pad3)")
  (net 9 "Net-(J5-Pad2)")
  (net 10 "Net-(J5-Pad1)")
  (net 11 /TE)
  (net 12 /CS)
  (net 13 /RS)
  (net 14 /WR)
  (net 15 /RD)
  (net 16 /SDI)
  (net 17 /SDO)
  (net 18 "Net-(J6-Pad32)")
  (net 19 "Net-(J6-Pad31)")
  (net 20 "Net-(J6-Pad30)")
  (net 21 "Net-(J6-Pad29)")
  (net 22 "Net-(J6-Pad28)")
  (net 23 "Net-(J6-Pad27)")
  (net 24 "Net-(J6-Pad26)")
  (net 25 "Net-(J6-Pad25)")
  (net 26 "Net-(J6-Pad24)")
  (net 27 "Net-(J6-Pad23)")
  (net 28 "Net-(J6-Pad22)")
  (net 29 "Net-(J6-Pad21)")
  (net 30 "Net-(J6-Pad20)")
  (net 31 "Net-(J6-Pad19)")
  (net 32 "Net-(J6-Pad18)")
  (net 33 "Net-(J6-Pad17)")
  (net 34 "Net-(J6-Pad16)")
  (net 35 "Net-(J6-Pad15)")
  (net 36 "Net-(J6-Pad14)")
  (net 37 "Net-(J6-Pad13)")
  (net 38 "Net-(J6-Pad12)")
  (net 39 "Net-(J6-Pad11)")
  (net 40 /RESET)
  (net 41 "Net-(J6-Pad5)")
  (net 42 "Net-(J6-Pad4)")
  (net 43 "Net-(J6-Pad3)")
  (net 44 "Net-(J6-Pad2)")
  (net 45 "Net-(J9-Pad40)")
  (net 46 "Net-(J9-Pad38)")
  (net 47 /R4)
  (net 48 /G2)
  (net 49 /G5)
  (net 50 "Net-(J9-Pad33)")
  (net 51 "Net-(J9-Pad32)")
  (net 52 /B0)
  (net 53 "Net-(J9-Pad29)")
  (net 54 /DE)
  (net 55 /DOTCLK)
  (net 56 /B1)
  (net 57 /B2)
  (net 58 /B5)
  (net 59 /R3)
  (net 60 /B3)
  (net 61 /B4)
  (net 62 /R2)
  (net 63 /R1)
  (net 64 /R0)
  (net 65 /R5)
  (net 66 /G4)
  (net 67 /G3)
  (net 68 /G1)
  (net 69 /G0)
  (net 70 "Net-(J9-Pad7)")
  (net 71 /HSYNC)
  (net 72 +5V)
  (net 73 /VSYNC)
  (net_class Default "This is the default net class."
    (clearance 0.152)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /B0)
    (add_net /B1)
    (add_net /B2)
    (add_net /B3)
    (add_net /B4)
    (add_net /B5)
    (add_net /CS)
    (add_net /DE)
    (add_net /DOTCLK)
    (add_net /G0)
    (add_net /G1)
    (add_net /G2)
    (add_net /G3)
    (add_net /G4)
    (add_net /G5)
    (add_net /HSYNC)
    (add_net /IM0)
    (add_net /IM1)
    (add_net /IM2)
    (add_net /IM3)
    (add_net /R0)
    (add_net /R1)
    (add_net /R2)
    (add_net /R3)
    (add_net /R4)
    (add_net /R5)
    (add_net /RD)
    (add_net /RESET)
    (add_net /RS)
    (add_net /SDI)
    (add_net /SDO)
    (add_net /TE)
    (add_net /VSYNC)
    (add_net /WR)
    (add_net GND)
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J6-Pad11)")
    (add_net "Net-(J6-Pad12)")
    (add_net "Net-(J6-Pad13)")
    (add_net "Net-(J6-Pad14)")
    (add_net "Net-(J6-Pad15)")
    (add_net "Net-(J6-Pad16)")
    (add_net "Net-(J6-Pad17)")
    (add_net "Net-(J6-Pad18)")
    (add_net "Net-(J6-Pad19)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad20)")
    (add_net "Net-(J6-Pad21)")
    (add_net "Net-(J6-Pad22)")
    (add_net "Net-(J6-Pad23)")
    (add_net "Net-(J6-Pad24)")
    (add_net "Net-(J6-Pad25)")
    (add_net "Net-(J6-Pad26)")
    (add_net "Net-(J6-Pad27)")
    (add_net "Net-(J6-Pad28)")
    (add_net "Net-(J6-Pad29)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad30)")
    (add_net "Net-(J6-Pad31)")
    (add_net "Net-(J6-Pad32)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J9-Pad29)")
    (add_net "Net-(J9-Pad32)")
    (add_net "Net-(J9-Pad33)")
    (add_net "Net-(J9-Pad38)")
    (add_net "Net-(J9-Pad40)")
    (add_net "Net-(J9-Pad7)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 157.83 67.11 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FFC_FH34S-50 (layer B.Cu) (tedit 5987CB2F)
    (at 137.179459 71.478)
    (descr "FFC connector 40-pin, Hirose FH34S-32, http://www.hirose.co.jp/cataloge_hp/ed_FH34S_20140305.pdf")
    (tags FFC)
    (fp_text reference J6 (at 0 -2.25) (layer B.SilkS))
    (fp_text value ER-TFT026-1 (at 0 -1) (layer B.Fab))
    (pad 0 smd rect (at 15 -1.45) (size 2 2) (layers B.Cu B.Paste B.Mask))
    (pad 40 smd rect (at 7.553003 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 39 smd rect (at 7.052926 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 11 /TE))
    (pad 38 smd rect (at 6.552849 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 12 /CS))
    (pad 37 smd rect (at 6.052772 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 13 /RS))
    (pad 36 smd rect (at 5.552695 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 14 /WR))
    (pad 35 smd rect (at 5.052618 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 /RD))
    (pad 34 smd rect (at 4.552541 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDI))
    (pad 33 smd rect (at 4.052464 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 17 /SDO))
    (pad 32 smd rect (at 3.552387 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J6-Pad32)"))
    (pad 31 smd rect (at 3.05231 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J6-Pad31)"))
    (pad 30 smd rect (at 2.552233 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J6-Pad30)"))
    (pad 29 smd rect (at 2.052156 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J6-Pad29)"))
    (pad 28 smd rect (at 1.552079 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J6-Pad28)"))
    (pad 27 smd rect (at 1.052002 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J6-Pad27)"))
    (pad 26 smd rect (at 0.551925 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J6-Pad26)"))
    (pad 25 smd rect (at 0.051848 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J6-Pad25)"))
    (pad 24 smd rect (at -0.448229 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J6-Pad24)"))
    (pad 23 smd rect (at -0.948306 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J6-Pad23)"))
    (pad 22 smd rect (at -1.448383 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J6-Pad22)"))
    (pad 21 smd rect (at -1.94846 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(J6-Pad21)"))
    (pad 20 smd rect (at -2.448537 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J6-Pad20)"))
    (pad 19 smd rect (at -2.948614 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J6-Pad19)"))
    (pad 18 smd rect (at -3.448691 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J6-Pad18)"))
    (pad 17 smd rect (at -3.948768 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J6-Pad17)"))
    (pad 16 smd rect (at -4.448845 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J6-Pad16)"))
    (pad 15 smd rect (at -4.948922 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J6-Pad15)"))
    (pad 14 smd rect (at -5.448999 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J6-Pad14)"))
    (pad 13 smd rect (at -5.949076 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J6-Pad13)"))
    (pad 12 smd rect (at -6.449153 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J6-Pad12)"))
    (pad 11 smd rect (at -6.94923 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J6-Pad11)"))
    (pad 10 smd rect (at -7.449307 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 40 /RESET))
    (pad 9 smd rect (at -7.949384 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 /IM3))
    (pad 8 smd rect (at -8.449461 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 /IM2))
    (pad 7 smd rect (at -8.949538 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 /IM1))
    (pad 6 smd rect (at -9.449615 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 /IM0))
    (pad 5 smd rect (at -9.949692 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J6-Pad5)"))
    (pad 4 smd rect (at -10.449769 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J6-Pad4)"))
    (pad 3 smd rect (at -10.949846 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at -11.449923 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J6-Pad2)"))
    (pad 1 smd rect (at -11.95 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 50 smd rect (at 13.053773 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 41 smd rect (at 8.05308 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 43 smd rect (at 9.053157 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 43 smd rect (at 9.553234 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 46 smd rect (at 11.053465 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J5-Pad2)"))
    (pad 47 smd rect (at 11.553542 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J5-Pad1)"))
    (pad 44 smd rect (at 10.053311 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J5-Pad4)"))
    (pad 45 smd rect (at 10.553388 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J5-Pad3)"))
    (pad 48 smd rect (at 12.053619 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 49 smd rect (at 12.553696 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 42 smd rect (at 8.55 0.15) (size 0.27 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 0 smd rect (at -13.7 -1.5) (size 2 2) (layers B.Cu B.Paste B.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5987E1AB)
    (at 181.102 68.8485 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value IM0 (at 0.102 -2.3915 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /IM0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5987E1A8)
    (at 177.037998 68.8485 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value IM1 (at -0.042002 -2.3915 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /IM1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5987E1A4)
    (at 172.635332 68.8485 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value IM2 (at -0.064668 -2.4615 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /IM2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5987E19F)
    (at 168.232666 68.8485 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value IM3 (at -0.097334 -2.4615 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /IM3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 174.4 122.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value RESET (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /RESET))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5987E1B2)
    (at 173.228 74.168)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value SERIAL (at -2.032 20.32) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SDO))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SDI))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /RD))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /WR))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /RS))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /TE))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 5987E1AF)
    (at 178.308 74.168)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J9 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value RPI_DPI (at 1.27 50.59) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 90) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J9-Pad40)"))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J9-Pad38)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /R4))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /G2))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /G5))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J9-Pad33)"))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J9-Pad32)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /B0))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J9-Pad29)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /DE))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /DOTCLK))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /B1))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /B2))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /B5))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /R3))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /B3))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /B4))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /R2))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /R1))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /R0))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /R5))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /G4))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /G3))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /G1))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /G0))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J9-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /HSYNC))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /VSYNC))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5987AF1E)
    (at 125 75.35 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7 270) (layer B.SilkS) hide)
    (fp_text value 5.6 (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59877060)
    (at 125.5 81.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 270) (layer B.SilkS) hide)
    (fp_text value 5.6 (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59877068)
    (at 127.52 81.49 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7 270) (layer B.SilkS) hide)
    (fp_text value 5.6 (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J6-Pad4)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59877071)
    (at 128 75.35 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7 270) (layer B.SilkS) hide)
    (fp_text value 5.6 (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J6-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875B86)
    (at 158.718701 120.875193)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J6-Pad11)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 73 /VSYNC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875C54)
    (at 158.758701 118.925479)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.7) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 71 /HSYNC))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J6-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875C5C)
    (at 158.758701 116.975765)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.7) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J6-Pad13)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 /DOTCLK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875C65)
    (at 158.758701 115.026051)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.7) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J6-Pad14)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 54 /DE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5987651B)
    (at 158.718701 78.457193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 52 /B0))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J6-Pad32)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59876520)
    (at 158.718701 80.489193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 /B1))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J6-Pad31)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59876529)
    (at 158.718701 82.521193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J6-Pad30)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 57 /B2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59876530)
    (at 158.7284 84.5312 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 60 /B3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J6-Pad29)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59876539)
    (at 158.718701 86.585193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J6-Pad28)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 61 /B4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59876547)
    (at 158.718701 88.617193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at -0.641001 -0.3725 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J6-Pad27)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 /B5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5987654F)
    (at 158.718701 90.649193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 69 /G0))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J6-Pad26)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59876557)
    (at 158.718701 92.681193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J6-Pad25)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 68 /G1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5987655A)
    (at 158.718701 94.713193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at -2.032 3.048 90) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 48 /G2))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J6-Pad24)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875D09)
    (at 158.718701 96.745193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J6-Pad23)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 67 /G3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875D0D)
    (at 158.718701 98.777193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 66 /G4))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J6-Pad22)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875D04)
    (at 158.718701 100.809193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(J6-Pad21)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 49 /G5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875CF9)
    (at 158.718701 102.841193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 64 /R0))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J6-Pad20)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875CFD)
    (at 158.758701 104.873193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J6-Pad19)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 63 /R1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875CEB)
    (at 158.758701 106.905193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 62 /R2))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J6-Pad18)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875CDF)
    (at 158.758701 108.937193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J6-Pad17)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 /R3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875CD3)
    (at 158.758701 110.969193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 47 /R4))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J6-Pad16)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59875C6F)
    (at 158.758701 113.001193 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J6-Pad15)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 65 /R5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5987E1B6)
    (at 169.164 74.168)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value SERIAL2 (at 0 20.11) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SDO))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SDI))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /RD))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /WR))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /RS))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /TE))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 162.79 66.94 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.25 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Rev.1 (at 126.72 65.64) (layer F.SilkS))
  (gr_text PizzaArcade (at 130.48 62.94) (layer F.SilkS))
  (gr_text RST (at 170.34 122.45) (layer F.SilkS))
  (gr_text GND (at 165.29 92.01) (layer F.SilkS))
  (gr_text SDO (at 165.25 89.41) (layer F.SilkS))
  (gr_text SDI (at 165.76 86.87) (layer F.SilkS))
  (gr_text RD (at 166.17 84.27) (layer F.SilkS))
  (gr_text "WR\n" (at 166.09 81.85) (layer F.SilkS))
  (gr_text RS (at 166.23 79.25) (layer F.SilkS))
  (gr_text CS (at 166.25 76.85) (layer F.SilkS))
  (gr_text "TE\n" (at 166.19 74.3) (layer F.SilkS))
  (gr_line (start 121.92 60.45) (end 121.92 60.45) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 60.46) (end 121.92 60.45) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 91.95) (end 121.92 60.46) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.896 126.492) (end 183.896 60.452) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 126.492) (end 183.896 126.492) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 91.948) (end 156.464 126.492) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.896 60.452) (end 121.92 60.452) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.71 59.88) (xy 184.29 59.88) (xy 184.29 126.8) (xy 156.32 126.8) (xy 121.71 92.19)
        (xy 121.71 59.91)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.3 67.83) (xy 153.79 67.83) (xy 153.79 73.06) (xy 152.93 73.92) (xy 145.89 73.92)
        (xy 144.86 72.89)
      )
    )
  )
)
