(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/DATAIN")
	(net 2 "/GND")
	(net 3 "/DATAOUT")
	(net 4 "unconnected-(J3-Pin_19-Pad19)")
	(net 5 "unconnected-(J3-Pin_13-Pad13)")
	(net 6 "/PC4")
	(net 7 "unconnected-(J3-Pin_17-Pad17)")
	(net 8 "unconnected-(J3-Pin_15-Pad15)")
	(net 9 "unconnected-(J3-Pin_9-Pad9)")
	(net 10 "/TIN")
	(net 11 "unconnected-(J3-Pin_11-Pad11)")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 148 73.1 180)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05_Pin"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "ECB_TAPE_CARD_EDGE_JACKS.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "/DATAIN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "/DATAOUT")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 10 "/TIN")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "/PC4")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CinchEdge:TI-H421021-10-3"
		(layer "F.Cu")
		(at 148 98.9)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "J3"
			(at 15 -4.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 0 7.62 180)
			(layer "F.Fab")
		)
		(property "Footprint" "CinchEdge:TI-H421021-10-3"
			(at -11.43 -1.27 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -11.43 -1.27 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at -11.43 -1.27 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "ECB_TAPE_CARD_EDGE_JACKS.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.12 1.36 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -11.43 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "/DATAIN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -11.43 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -8.89 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "/DATAOUT")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -8.89 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -6.35 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 10 "/TIN")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -6.35 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at -3.81 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "/PC4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at -3.81 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at -1.27 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 9 "unconnected-(J3-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole oval
			(at -1.27 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 1.27 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 11 "unconnected-(J3-Pin_11-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive+no_connect")
		)
		(pad "12" thru_hole oval
			(at 1.27 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 3.81 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "unconnected-(J3-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole oval
			(at 3.81 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 6.35 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "unconnected-(J3-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole oval
			(at 6.35 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 8.89 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "unconnected-(J3-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
		)
		(pad "18" thru_hole oval
			(at 8.89 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 11.43 -1.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 4 "unconnected-(J3-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole oval
			(at 11.43 3.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(model "C:/Users/kb0iic/Documents/KiCad/8.0/3dmodels/card-edge-connector-slot-1.snapshot.5/A edge connector 20 pins.STEP"
			(offset
				(xyz -11.5 23 -7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Connector_Audio:Jack_3.5mm_CUI_SJ1-3525N_Horizontal"
		(layer "F.Cu")
		(at 157 66 180)
		(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
		(tags "TRS audio jack stereo horizontal")
		(property "Reference" "J2"
			(at -6.1 -8.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "AudioJack3"
			(at 0 -10 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Audio:Jack_3.5mm_CUI_SJ1-3525N_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "Root")
		(sheetfile "ECB_TAPE_CARD_EDGE_JACKS.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(fp_line
			(start 2.2 4.5)
			(end 6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.2 3.5)
			(end 2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 1.8 3.1)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 4.5)
			(end -6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 3.5)
			(end -2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 1.8 3.1)
			(mid 2.082843 3.217157)
			(end 2.2 3.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -2.2 3.5)
			(mid -2.082842 3.217158)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_text user "PCB edge"
			(at 0 3.65 180)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at -5 2.5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0 -5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 5 2.5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "R" thru_hole oval
			(at -5 -5 180)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "/DATAOUT")
			(pintype "passive")
		)
		(pad "RN" thru_hole oval
			(at -2.5 -5 180)
			(size 1.6 2.3)
			(drill oval 0.8 1.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
		)
		(pad "S" thru_hole oval
			(at 0 0 180)
			(size 2.2 1.2)
			(drill oval 1.4 0.4)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 5 -5)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "/DATAOUT")
			(pintype "passive")
		)
		(pad "TN" thru_hole oval
			(at 2.5 -5)
			(size 1.6 2.5)
			(drill oval 0.8 1.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3525N_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Audio:Jack_3.5mm_CUI_SJ1-3525N_Horizontal"
		(layer "F.Cu")
		(at 139 66 180)
		(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
		(tags "TRS audio jack stereo horizontal")
		(property "Reference" "J1"
			(at 6.1 -8.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "AudioJack3"
			(at 0 -10 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Audio:Jack_3.5mm_CUI_SJ1-3525N_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "Root")
		(sheetfile "ECB_TAPE_CARD_EDGE_JACKS.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(fp_line
			(start 2.2 4.5)
			(end 6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.2 3.5)
			(end 2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 1.8 3.1)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 4.5)
			(end -6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 3.5)
			(end -2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 1.8 3.1)
			(mid 2.082843 3.217157)
			(end 2.2 3.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -2.2 3.5)
			(mid -2.082842 3.217158)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_text user "PCB edge"
			(at 0 3.65 180)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at -5 2.5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0 -5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 5 2.5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "R" thru_hole oval
			(at -5 -5 180)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "/DATAIN")
			(pintype "passive")
		)
		(pad "RN" thru_hole oval
			(at -2.5 -5 180)
			(size 1.6 2.3)
			(drill oval 0.8 1.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
		)
		(pad "S" thru_hole oval
			(at 0 0 180)
			(size 2.2 1.2)
			(drill oval 1.4 0.4)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "/GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 5 -5)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "/DATAIN")
			(pintype "passive")
		)
		(pad "TN" thru_hole oval
			(at 2.5 -5)
			(size 1.6 2.5)
			(drill oval 0.8 1.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3525N_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 163.5 61.5)
		(mid 163.853553 61.646447)
		(end 164 62)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132 105.25)
		(end 164 105.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 132 62)
		(mid 132.146447 61.646447)
		(end 132.5 61.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132 62)
		(end 132 105.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164 105.25)
		(end 164 62)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.5 61.5)
		(end 150.5 61.5)
		(layer "Edge.Cuts")
	)
	(gr_text "DATAOUT"
		(at 162 76.1 0)
		(layer "B.SilkS")
	)
	(gr_text "G\n\n7\n\n5\n\n3\n\n1"
		(at 150.4 73.5 0)
		(layer "B.SilkS")
	)
	(gr_text "NOT CONNECTED"
		(at 159.3 94.6 0)
		(layer "B.SilkS")
	)
	(gr_text "7  5  3  1"
		(at 144.6 94.5 0)
		(layer "B.SilkS")
	)
	(gr_text "DATAIN\n\nDATAOUT\n\nTIN\n\nPC4\n"
		(at 144.8 92.4 90)
		(layer "B.SilkS")
	)
	(gr_text "See table 8-2\nof ECB manual"
		(at 134.4 83 90)
		(layer "B.SilkS")
	)
	(gr_text "DATAIN"
		(at 142.9 76.1 0)
		(layer "B.SilkS")
	)
	(gr_text "BERZERKULA.ORG\nECB TAPE J2\nCARD EDGE CONN"
		(at 162.9 91.9 0)
		(layer "B.SilkS")
	)
	(gr_text "TIN - TIMER INPUT TO PI/T\n      EXT CLK OR CLK EN\n\nPC4 - PI/T PORTC BIT 4"
		(at 163.9 82.8 0)
		(layer "B.SilkS")
	)
	(gr_text "1  3  5  7"
		(at 136.1 94.5 0)
		(layer "F.SilkS")
	)
	(gr_text "DATAIN\n\nDATAOUT\n\nTIN\n\nPC4"
		(at 144.8 92.4 90)
		(layer "F.SilkS")
	)
	(gr_text "NOT CONNECTED"
		(at 146.8 94.6 0)
		(layer "F.SilkS")
	)
	(gr_text "DATAIN"
		(at 135.1 76.1 0)
		(layer "F.SilkS")
	)
	(gr_text "G\n\n7\n\n5\n\n3\n\n1"
		(at 149.5 73.5 0)
		(layer "F.SilkS")
	)
	(gr_text "See table 8-2\nof ECB manual"
		(at 134.4 92.3 90)
		(layer "F.SilkS")
	)
	(gr_text "DATAOUT"
		(at 152 76.1 0)
		(layer "F.SilkS")
	)
	(gr_text "TIN - TIMER INPUT TO PI/T\n      EXT CLK OR CLK EN\n\nPC4 - PI/T PORTC BIT 4"
		(at 146.9 82.9 0)
		(layer "F.SilkS")
	)
	(gr_text "BERZERKULA.ORG\nECB TAPE J2\nCARD EDGE CONN"
		(at 152.3 91.9 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "/GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.75 50) (xy 185.25 50.25) (xy 185 109.5) (xy 112.75 109.5)
			)
		)
	)
)
