(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6002)
    (drawings 7)
    (tracks 75)
    (zones 0)
    (modules 7)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.127)
    (segment_width 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.25)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 148.59 105.41)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /Anode)
  (net 4 /HV6)
  (net 5 /HV5)
  (net 6 /HV4)
  (net 7 /HV9)
  (net 8 /HV3)
  (net 9 /HV8)
  (net 10 /HV2)
  (net 11 /HV7)
  (net 12 /HV1)
  (net 13 /Din)
  (net 14 "Net-(J1-Pad4)")
  (net 15 "Net-(LED1-Pad1-DOUT)")
  (net 16 /HV0)
  (net 17 "Net-(J1-Pad6)")
  (net 18 "Net-(NX1-PadP$9)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV0)
    (add_net /HV1)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(LED1-Pad1-DOUT)")
    (add_net "Net-(NX1-PadP$9)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 148.59 97.79)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at -0.127 -1.524) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 158.59 87.91 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 2.33 90) (layer B.SilkS) hide)
    (fp_text value Nixie (at 1.27 -22.65 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -10.16) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV6))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV5))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV4))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /HV0))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV3))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV9))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV2))
    (pad 12 thru_hole oval (at 2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV8))
    (pad 13 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV1))
    (pad 14 thru_hole oval (at 2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV7))
    (pad 15 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Din))
    (pad 16 thru_hole oval (at 2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Din))
    (pad 17 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 18 thru_hole oval (at 2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 200000)
    (at 148.59 101.6 270)
    (attr smd)
    (fp_text reference LED1 (at 3.175 -0.254) (layer F.SilkS) hide)
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54 90) (layer F.SilkS) hide)
    (pad 4-VDD smd rect (at -1.74752 0.87376) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3-DIN smd rect (at -1.74752 -0.87376) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 13 /Din))
    (pad 2-GND smd rect (at 1.74752 -0.87376) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1-DOUT smd rect (at 1.74752 0.87376) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(LED1-Pad1-DOUT)"))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 159.09 113.91 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 148.59 119.7)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module mynixies:mynixies-CK1806 (layer F.Cu) (tedit 200000)
    (at 148.59 105.41)
    (attr virtual)
    (fp_text reference NX1 (at 0 2.54) (layer F.SilkS))
    (fp_text value CK8650D-SUB (at 0 0) (layer Dwgs.User))
    (pad P$11 thru_hole circle (at 2.5781 0) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 8 /HV3))
    (pad P$10 thru_hole circle (at -2.5781 0) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 9 /HV8))
    (pad P$9 thru_hole circle (at 3.48234 -4.79298) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 18 "Net-(NX1-PadP$9)"))
    (pad P$8 thru_hole circle (at 5.63372 -1.8288) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 10 /HV2))
    (pad P$7 thru_hole circle (at 5.63372 1.8288) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 6 /HV4))
    (pad P$6 thru_hole circle (at 3.48234 4.79298) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 5 /HV5))
    (pad P$5 thru_hole circle (at 0 5.92328) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 12 /HV1))
    (pad P$4 thru_hole circle (at -3.48234 4.79298) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 4 /HV6))
    (pad P$3 thru_hole circle (at -5.63372 1.8288) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 11 /HV7))
    (pad P$2 thru_hole circle (at -5.63372 -1.8288) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 7 /HV9))
    (pad P$1 thru_hole circle (at -3.48234 -4.79298) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 16 /HV0))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 158.59 92.075 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 90) (layer Dwgs.User))
    (fp_text value 11k (at 0 -1.75 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /Anode))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(NX1-PadP$9)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 140.59 118.41) (end 135.59 118.41) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 156.59 118.41) (end 156.59 123.41) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 161.59 82.41) (end 135.59 82.41) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 161.59 118.41) (end 161.59 82.41) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 140.59 123.41) (end 156.59 123.41) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 135.59 82.41) (end 135.59 118.41) (layer Edge.Cuts) (width 0.127))
  (gr_text "nixies.us\nCK8650" (at 157.84 114.41) (layer B.Mask))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 133.59 80.41) (xy 163.59 80.41) (xy 163.59 125.41) (xy 133.59 125.41)
      )
    )
  )
)
