(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 185)
    (zones 0)
    (modules 9)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Exports/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad20)")
  (net 2 "Net-(J1-Pad19)")
  (net 3 "Net-(J1-Pad18)")
  (net 4 "Net-(J1-Pad17)")
  (net 5 "Net-(J1-Pad16)")
  (net 6 "Net-(J1-Pad15)")
  (net 7 "Net-(J1-Pad14)")
  (net 8 "Net-(J1-Pad13)")
  (net 9 "Net-(J1-Pad12)")
  (net 10 "Net-(J1-Pad11)")
  (net 11 "Net-(J1-Pad10)")
  (net 12 "Net-(J1-Pad9)")
  (net 13 "Net-(J1-Pad8)")
  (net 14 "Net-(J1-Pad7)")
  (net 15 "Net-(J1-Pad6)")
  (net 16 "Net-(J1-Pad5)")
  (net 17 "Net-(J1-Pad4)")
  (net 18 "Net-(J1-Pad3)")
  (net 19 "Net-(J1-Pad2)")
  (net 20 "Net-(J1-Pad1)")
  (net 21 "Net-(J3-Pad6)")
  (net 22 "Net-(J3-Pad5)")
  (net 23 "Net-(J3-Pad4)")
  (net 24 "Net-(J3-Pad3)")
  (net 25 "Net-(J3-Pad2)")
  (net 26 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
  )
  (module Gallant_Harwin:Harwin_20_vert (layer F.Cu) (tedit 5D30A11A)
    (at 123.77 128.875 270)
    (fp_text reference J1 (at -0.762 -5.596 90) (layer F.Fab))
    (fp_text value Conn_02x10_Top_Bottom (at 0 6.604 90) (layer F.Fab))
    (pad 20 smd rect (at 5.625 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad20)"))
    (pad 19 smd rect (at 4.375 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad19)"))
    (pad 18 smd rect (at 3.125 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad18)"))
    (pad 17 smd rect (at 1.875 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad17)"))
    (pad 16 smd rect (at 0.625 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad16)"))
    (pad 15 smd rect (at -0.625 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad15)"))
    (pad 14 smd rect (at -1.875 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad14)"))
    (pad 13 smd rect (at -3.125 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad13)"))
    (pad 12 smd rect (at -4.375 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 11 smd rect (at -5.625 1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad11)"))
    (pad 10 smd rect (at 5.625 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at 4.375 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at 3.125 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad8)"))
    (pad 7 smd rect (at 1.875 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at 0.625 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at -0.625 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad5)"))
    (pad 4 smd rect (at -1.875 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at -3.125 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -4.375 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -5.625 -1.85 270) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x03_P3.175mm_Drill0.8mm (layer F.Cu) (tedit 5AEE57A0)
    (at 137.795 122.555)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J9 (at -3.175 1.27) (layer F.Fab))
    (fp_text value DAC1 (at -3.81 0) (layer F.SilkS))
    (fp_text user %R (at 3.175 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 6.35 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad10)"))
    (pad 2 thru_hole circle (at 3.175 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad8)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad9)"))
  )
  (module Connector_Wire:SolderWirePad_1x03_P3.175mm_Drill0.8mm (layer F.Cu) (tedit 5AEE57A0)
    (at 137.795 135.255)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J8 (at -5.08 -1.905) (layer F.Fab))
    (fp_text value DAC0 (at -3.81 0) (layer F.SilkS))
    (fp_text user %R (at 3.175 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad18)"))
    (pad 2 thru_hole circle (at 3.175 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad17)"))
    (pad 3 thru_hole circle (at 6.35 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad19)"))
  )
  (module Gallant_Redstone:SM04B-XSRS-ETB (layer F.Cu) (tedit 5D31D3A9)
    (at 125.73 102.295 180)
    (fp_text reference Mic.3 (at -5.08 0.695) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 2.286) (layer F.Fab))
    (pad 0 smd rect (at 2.05 0.575 180) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at -2.05 0.575 180) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.9 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0.3 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at -0.3 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad6)"))
    (pad 1 smd rect (at -0.9 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad1)"))
  )
  (module Gallant_Redstone:SM04B-XSRS-ETB (layer F.Cu) (tedit 5D31D3A9)
    (at 143.02 102.4 180)
    (fp_text reference Mic.2 (at 5.225 0.8) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 2.286) (layer F.Fab))
    (pad 0 smd rect (at 2.05 0.575 180) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at -2.05 0.575 180) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.9 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0.3 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at -0.3 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad5)"))
    (pad 1 smd rect (at -0.9 -0.8 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad1)"))
  )
  (module Gallant_Redstone:SM04B-XSRS-ETB (layer F.Cu) (tedit 5D31D3A9)
    (at 125.73 107.95)
    (fp_text reference Mic.1 (at 5.08 0.635) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 2.286) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -0.3 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad4)"))
    (pad 3 smd rect (at 0.3 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 4 smd rect (at 0.9 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 0 smd rect (at -2.05 0.575) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 2.05 0.575) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
  )
  (module Gallant_Redstone:SM04B-XSRS-ETB (layer F.Cu) (tedit 5D31D3A9)
    (at 143.02 107.95)
    (fp_text reference Mic.0 (at -5.225 0.635) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 2.286) (layer F.Fab))
    (pad 0 smd rect (at 2.05 0.575) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at -2.05 0.575) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.9 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0.3 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at -0.3 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad3)"))
    (pad 1 smd rect (at -0.9 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad1)"))
  )
  (module Gallant_Redstone:SM06B-XSRS-ETB (layer F.Cu) (tedit 5D31D415)
    (at 134.62 105.41)
    (fp_text reference OUT (at 0 -2.54) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 -2.54 180) (layer F.Fab))
    (pad 6 smd rect (at 1.5 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad6)"))
    (pad 5 smd rect (at 0.9 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad5)"))
    (pad 0 smd rect (at 2.65 0.575) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at -2.65 0.575) (size 0.7 1.05) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.3 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad4)"))
    (pad 3 smd rect (at -0.3 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at -0.9 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.8) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad1)"))
  )
  (module Gallant_Redstone:SM06B-XSRS-ETB (layer B.Cu) (tedit 5D31D415)
    (at 144.78 129.54 270)
    (fp_text reference J2 (at 2.54 2.794 270) (layer B.SilkS))
    (fp_text value Conn_01x06 (at 0 -2.286 270) (layer B.Fab))
    (pad 6 smd rect (at 1.5 0.8 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad 5 smd rect (at 0.9 0.8 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad5)"))
    (pad 0 smd rect (at 2.65 -0.575 270) (size 0.7 1.05) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at -2.65 -0.575 270) (size 0.7 1.05) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 0.3 0.8 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -0.3 0.8 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.9 0.8 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 1 smd rect (at -1.5 0.8 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad14)"))
  )
  (gr_text "+ G -" (at 140.97 132.715) (layer F.SilkS))
  (gr_text "+ G -" (at 140.97 125.095) (layer F.SilkS))
  (gr_line (start 147.32 120.65) (end 116.84 120.65) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 147.32 137.16) (end 147.32 120.65) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 116.84 137.16) (end 147.32 137.16) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 116.84 120.65) (end 116.84 137.16) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 116.488984 105.410001) (end 119.638984 105.41) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 115.309492 99.668167) (end 152.309492 99.668167) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 147.98 108.111852) (end 147.98 105.41) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 115.309491 104.668167) (end 115.309492 99.668167) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.28 105.41) (end 154.279999 108.111852) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 116.488984 105.41) (end 116.488983 102.26) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 115.309492 106.151833) (end 110.309492 106.151833) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 152.309492 106.151834) (end 152.309492 111.151833) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.309492 106.151833) (end 110.309492 104.668167) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 152.309492 111.151833) (end 115.309492 111.151833) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 157.309492 104.668167) (end 157.309492 106.151833) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 116.488984 105.410001) (end 113.338984 105.41) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 151.13 105.41) (end 147.98 108.111852) (angle -98.7586) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 116.488984 105.41) (end 116.488983 108.56) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 152.309492 104.668167) (end 157.309492 104.668167) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 151.13 105.41) (end 154.28 105.41) (angle -180) (layer Edge.Cuts) (width 0.2))
)
