(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 19)
    (no_connects 0)
    (area 141.656999 84.252999 175.843001 110.819001)
    (thickness 1.6)
    (drawings 16)
    (tracks 87)
    (zones 0)
    (modules 6)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 A)
  (net 2 B)
  (net 3 GND)
  (net 4 C)
  (net 5 D)
  (net 6 5B)
  (net 7 5A)
  (net 8 5D)
  (net 9 5C)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class Signal ""
    (clearance 0.15)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5A)
    (add_net 5B)
    (add_net 5C)
    (add_net 5D)
    (add_net A)
    (add_net B)
    (add_net C)
    (add_net D)
  )
  (module RJ45:EJ45_RJHSE-5080 (layer F.Cu) (tedit 58771648)
    (at 143.891 93.98)
    (fp_text reference J1 (at 6.51002 3.79476) (layer F.SilkS))
    (fp_text value RJ45 (at 6.62178 -8.3312) (layer F.Fab))
    (fp_text user RJ45 (at 6.35 1.905) (layer F.SilkS))
    (pad 8 thru_hole circle (at 2.794 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole circle (at 3.81 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 7 5A))
    (pad 6 thru_hole circle (at 4.826 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 A))
    (pad 4 thru_hole circle (at 6.858 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 B))
    (pad 2 thru_hole circle (at 8.89 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 5B))
    (pad 5 thru_hole circle (at 5.842 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 B))
    (pad 3 thru_hole circle (at 7.874 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 A))
    (pad 1 thru_hole circle (at 9.906 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad "" thru_hole circle (at 0 0) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module RJ45:EJ45_RJHSE-5080 (layer F.Cu) (tedit 58771648)
    (at 160.782 93.98)
    (fp_text reference J2 (at 6.51002 3.79476) (layer F.SilkS))
    (fp_text value RJ45 (at 6.62178 -8.3312) (layer F.Fab))
    (fp_text user RJ45 (at 6.35 1.905) (layer F.SilkS))
    (pad 8 thru_hole circle (at 2.794 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole circle (at 3.81 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 5C))
    (pad 6 thru_hole circle (at 4.826 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 C))
    (pad 4 thru_hole circle (at 6.858 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 D))
    (pad 2 thru_hole circle (at 8.89 -4.318) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 5D))
    (pad 5 thru_hole circle (at 5.842 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 D))
    (pad 3 thru_hole circle (at 7.874 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 C))
    (pad 1 thru_hole circle (at 9.906 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad "" thru_hole circle (at 0 0) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 587883C1)
    (at 147.32 104.14)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference A (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 A))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 5A))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 587883C9)
    (at 154.94 104.14)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference B (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 B))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 5B))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 587883CE)
    (at 162.56 104.14)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference C (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 C))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 5C))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 587883D2)
    (at 170.18 104.14)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference D (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 D))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 5D))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text -> (at 143.87 102.108 270) (layer F.SilkS))
  (gr_text -> (at 151.07 102.108 270) (layer F.SilkS))
  (gr_text OTHER (at 142.13 100.584) (layer F.SilkS))
  (gr_text "4x Any Signal -> RJ45\nv0.1" (at 158.5976 98.5774) (layer B.SilkS))
  (gr_text RELAYS (at 151.12 100.584) (layer F.SilkS))
  (gr_text Rev (at 151.12 106.68) (layer F.SilkS))
  (gr_text Fwd (at 151.14 104.14) (layer F.SilkS))
  (gr_text Gnd (at 151.1 109.22) (layer F.SilkS))
  (gr_text Sig (at 143.76 103.886) (layer F.SilkS))
  (gr_text 5V (at 143.84 106.68) (layer F.SilkS))
  (gr_text Gnd (at 143.71 109.22) (layer F.SilkS))
  (gr_text FRC2168 (at 158.75 86.106) (layer B.SilkS))
  (gr_line (start 175.768 110.744) (end 175.768 84.328) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.732 110.744) (end 175.768 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.732 84.328) (end 141.732 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 84.328) (end 141.732 84.328) (angle 90) (layer Edge.Cuts) (width 0.15))
)
