(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 34)
    (no_connects 0)
    (area 114.372 74.239047 185.034762 131.806571)
    (thickness 1.6)
    (drawings 12)
    (tracks 218)
    (zones 0)
    (modules 22)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.4)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 163.376 117.824)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D3-Pad1)")
  (net 7 "Net-(D4-Pad1)")
  (net 8 "Net-(D5-Pad1)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(R6-Pad2)")
  (net 11 "Net-(Q1-Pad1)")
  (net 12 "Net-(Q1-Pad3)")
  (net 13 "Net-(SW2-Pad2)")
  (net 14 "Net-(CLR1-Pad1)")
  (net 15 "Net-(DAT1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(CLR1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(DAT1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(SW2-Pad2)")
  )
  (net_class Mine ""
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.508)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module MyStuff:Switch_CL-SB-12C-01 (layer F.Cu) (tedit 5AB47995)
    (at 166 110 64)
    (fp_text reference SW1 (at 3.960127 12.39438 64) (layer F.SilkS) hide)
    (fp_text value SW_SPDT (at 5.538529 11.06824 64) (layer F.Fab) hide)
    (fp_text user SW (at -5.633016 1.0518 64) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.5 -1.65 64) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.5 -1.65 64) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 0 1.65 64) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AB47976)
    (at 154.178 114.554 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 4.47 -0.198 270) (layer F.SilkS))
    (fp_text value 4.7uf (at 15.07 -9.948 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 148 115 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 4.7uf (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5AB47972)
    (at 157.48 113.792 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 4.432 -0.196 270) (layer F.SilkS))
    (fp_text value LED (at 15.582 -9.396 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5AB4796D)
    (at 160.782 113.792 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 4.232 -0.094 270) (layer F.SilkS))
    (fp_text value 220 (at 15.832 -7.844 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5AB479A3)
    (at 158 93.5 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -4.276 0.024 270) (layer F.SilkS))
    (fp_text value 220 (at -0.376 -16.376 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Mask)
      (net 8 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Mask)
      (net 12 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5AB4799E)
    (at 163.068 97.282)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 4.408 0.042) (layer F.SilkS))
    (fp_text value 1K (at 17.308 -1.158) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Mask)
      (net 10 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AA9C368)
    (at 162.5 92.5 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 0.95 -1.86 270) (layer F.SilkS))
    (fp_text value 220 (at 0.874 -13.376 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyStuff:DPACK (layer F.Cu) (tedit 5AA9C408)
    (at 145.288 97.028)
    (fp_text reference U1 (at 0.088 -4.154) (layer F.SilkS))
    (fp_text value AP1117-50 (at -6.912 -17.904) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 5.8 6.2) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.1 7.2) (size 1.6 3) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.1 7.2) (size 1.6 3) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5AA9C3A2)
    (at 146.558 89.408 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value BSS138 (at 12.034 -1.432 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 12 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5AA9C41E)
    (at 140.462 110.998)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -3.5) (layer F.SilkS))
    (fp_text value PIC16F15313 (at -20.836 1.126) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Mask))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Mask))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 14 "Net-(CLR1-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 13 "Net-(SW2-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 15 "Net-(DAT1-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyStuff:KingbrightSideMountLed (layer F.Cu) (tedit 5AB54070)
    (at 151 85)
    (fp_text reference D4 (at 2.876 1.824) (layer F.SilkS))
    (fp_text value LD271 (at 0.2 -3.5) (layer F.Fab))
    (pad 2 smd rect (at -1.75 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at 1.75 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 3 smd rect (at 0 0.65) (size 0.9 0.9) (layers F.Cu F.Mask))
  )
  (module MyStuff:KingbrightSideMountLed (layer F.Cu) (tedit 5AB5407E)
    (at 169 103 270)
    (fp_text reference D5 (at 4.324 0.124 270) (layer F.SilkS))
    (fp_text value LD271 (at 0.2 -3.5 270) (layer F.Fab))
    (pad 2 smd rect (at -1.75 0 270) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 1 smd rect (at 1.75 0 270) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 8 "Net-(D5-Pad1)"))
    (pad 3 smd rect (at 0 0.65 270) (size 0.9 0.9) (layers F.Cu F.Mask))
  )
  (module MyStuff:KingbrightSideMountLed (layer F.Cu) (tedit 5AB54086)
    (at 133 103 90)
    (fp_text reference D3 (at -3.324 1.876 90) (layer F.SilkS))
    (fp_text value LD271 (at 0.2 -3.5 90) (layer F.Fab))
    (pad 2 smd rect (at -1.75 0 90) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at 1.75 0 90) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad "" smd rect (at 0 0.65 90) (size 0.9 0.9) (layers F.Cu F.Mask))
  )
  (module MyStuff:KingbrightSideMountLed (layer F.Cu) (tedit 5AB5408C)
    (at 151 121 180)
    (fp_text reference D2 (at 3.624 1.176 180) (layer F.SilkS))
    (fp_text value LD271 (at 0.2 -3.5 180) (layer F.Fab))
    (pad 2 smd rect (at -1.75 0 180) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at 1.75 0 180) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad "" smd rect (at 0 0.65 180) (size 0.9 0.9) (layers F.Cu F.Mask))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 5AB565BC)
    (at 134.376 94.824)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP5 (at -11.5 -3) (layer B.SilkS) hide)
    (fp_text value CLK (at 1.5 -1.5) (layer B.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(SW2-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AB565A1)
    (at 137.376 94.824)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP4 (at -17 -5) (layer B.SilkS) hide)
    (fp_text value GND (at 2.5 0) (layer B.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module MyStuff:9V_Bat_Clip_TH (layer F.Cu) (tedit 5AB54788)
    (at 151.13 102.87 90)
    (fp_text reference J1 (at 0 10.16 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -10.16 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 4.2 4.2) (drill 2.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 4.2 4.2) (drill 2.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AB565C7)
    (at 137.376 91.824)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CLR (at 2.5 0) (layer B.SilkS))
    (fp_text value TEST (at -11.25 -3.5) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(CLR1-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AB565C2)
    (at 137.376 97.824)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference DAT (at 2.5 0) (layer B.SilkS))
    (fp_text value TEST (at -17 -1.5) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 15 "Net-(DAT1-Pad1)"))
  )
  (module MyStuff:DIP-6_GullWing (layer F.Cu) (tedit 5AB54C8A)
    (at 159 103)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads")
    (attr smd)
    (fp_text reference SW2 (at 22.126 -5.376) (layer F.SilkS) hide)
    (fp_text value SW_DIP_x03 (at 21.376 13.324) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.31 -2.54) (size 2.44 1.13) (layers F.Cu F.Mask)
      (net 15 "Net-(DAT1-Pad1)"))
    (pad 4 smd rect (at 4.31 2.54) (size 2.44 1.13) (layers F.Cu F.Mask)
      (net 10 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at -4.31 0) (size 2.44 1.13) (layers F.Cu F.Mask)
      (net 13 "Net-(SW2-Pad2)"))
    (pad 5 smd rect (at 4.31 0) (size 2.44 1.13) (layers F.Cu F.Mask)
      (net 10 "Net-(R6-Pad2)"))
    (pad 3 smd rect (at -4.31 2.54) (size 2.44 1.13) (layers F.Cu F.Mask)
      (net 14 "Net-(CLR1-Pad1)"))
    (pad 6 smd rect (at 4.31 -2.54) (size 2.44 1.13) (layers F.Cu F.Mask)
      (net 10 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm_SMDSocket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AB565B8)
    (at 134.376 97.824)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference VDD (at 1.5 -1.5) (layer B.SilkS))
    (fp_text value TEST (at -13.25 -3.5) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (gr_text "Skye Sweeney" (at 151.376 119.324) (layer B.SilkS))
  (gr_text "IR Beacon V1.0" (at 151.126 86.824) (layer B.SilkS))
  (gr_circle (center 150.876 103.124) (end 169.676 110.724) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.376 85.324) (xy 159.876 86.824) (xy 163.876 89.824) (xy 166.876 93.824) (xy 168.876 98.824)
        (xy 169.376 103.824) (xy 168.876 107.324) (xy 165.876 113.324) (xy 163.876 115.824) (xy 160.376 118.324)
        (xy 155.876 120.324) (xy 149.876 120.824) (xy 146.876 120.324) (xy 142.376 118.324) (xy 138.876 115.824)
        (xy 135.376 110.824) (xy 133.876 106.324) (xy 133.376 101.324) (xy 133.876 98.324) (xy 134.876 95.324)
        (xy 137.376 91.824) (xy 139.376 89.324) (xy 142.876 86.824) (xy 146.876 85.324) (xy 150.876 84.824)
      )
    )
  )
)
