(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 62)
    (zones 0)
    (modules 9)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad14)")
  (net 14 "Net-(J1-Pad15)")
  (net 15 "Net-(J1-Pad17)")
  (net 16 "Net-(J1-Pad19)")
  (net 17 "Net-(J1-Pad20)")
  (net 18 "Net-(J2-Pad1)")
  (net 19 "Net-(J2-Pad4)")
  (net 20 "Net-(J2-Pad5)")
  (net 21 "Net-(J2-Pad6)")
  (net 22 "Net-(J3-Pad1)")
  (net 23 "Net-(J3-Pad6)")
  (net 24 "Net-(J3-Pad7)")
  (net 25 "Net-(J3-Pad8)")
  (net 26 "Net-(J3-Pad9)")
  (net 27 "Net-(J3-Pad11)")
  (net 28 "Net-(J3-Pad12)")
  (net 29 "Net-(J3-Pad14)")
  (net 30 "Net-(J3-Pad15)")
  (net 31 "Net-(J3-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad14)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad20)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
  )
  (module "TSL Footprints:PC104_Card_Fixed" (layer F.Cu) (tedit 604BE4B7)
    (at 125.73 62.23)
    (fp_text reference REF** (at 45.72 -1.27) (layer F.SilkS))
    (fp_text value "PC104 Card" (at 54.61 -1.27) (layer F.Fab))
    (pad "" thru_hole circle (at 85.09 90.81) (size 5 5) (drill 3.18) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.08 90.81) (size 5 5) (drill 3.18) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 82.55 5.08) (size 5 5) (drill 3.18) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 8.89 5.08) (size 5 5) (drill 3.18) (layers *.Cu *.Mask))
    (pad H2_1 thru_hole circle (at 13.97 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_2 thru_hole circle (at 13.97 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_3 thru_hole circle (at 16.51 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_4 thru_hole circle (at 16.51 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_5 thru_hole circle (at 19.05 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_6 thru_hole circle (at 19.05 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_7 thru_hole circle (at 21.59 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_8 thru_hole circle (at 21.59 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_9 thru_hole circle (at 24.13 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_10 thru_hole circle (at 24.13 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_11 thru_hole circle (at 26.67 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_12 thru_hole circle (at 26.67 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_13 thru_hole circle (at 29.21 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_14 thru_hole circle (at 29.21 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_15 thru_hole circle (at 31.75 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_16 thru_hole circle (at 31.75 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_17 thru_hole circle (at 34.29 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_18 thru_hole circle (at 34.29 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_19 thru_hole circle (at 36.83 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_20 thru_hole circle (at 36.83 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_21 thru_hole circle (at 39.37 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_22 thru_hole circle (at 39.37 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_23 thru_hole circle (at 41.91 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_24 thru_hole circle (at 41.91 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_25 thru_hole circle (at 44.45 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_26 thru_hole circle (at 44.45 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_27 thru_hole circle (at 46.99 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_28 thru_hole circle (at 46.99 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_29 thru_hole circle (at 49.53 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_30 thru_hole circle (at 49.53 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_31 thru_hole circle (at 52.07 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_32 thru_hole circle (at 52.07 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_33 thru_hole circle (at 54.61 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_34 thru_hole circle (at 54.61 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_35 thru_hole circle (at 57.15 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_36 thru_hole circle (at 57.15 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_37 thru_hole circle (at 59.69 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_38 thru_hole circle (at 59.69 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_39 thru_hole circle (at 62.23 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_40 thru_hole circle (at 62.23 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_41 thru_hole circle (at 64.77 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_42 thru_hole circle (at 64.77 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_43 thru_hole circle (at 67.31 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_44 thru_hole circle (at 67.31 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_45 thru_hole circle (at 69.85 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_46 thru_hole circle (at 69.85 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_47 thru_hole circle (at 72.39 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_48 thru_hole circle (at 72.39 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_49 thru_hole circle (at 74.93 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_50 thru_hole circle (at 74.93 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_51 thru_hole circle (at 77.47 7.54) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H2_52 thru_hole circle (at 77.47 5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_51 thru_hole circle (at 77.47 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_41 thru_hole circle (at 64.77 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_40 thru_hole circle (at 62.23 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_42 thru_hole circle (at 64.77 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_44 thru_hole circle (at 67.31 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_43 thru_hole circle (at 67.31 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_45 thru_hole circle (at 69.85 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_46 thru_hole circle (at 69.85 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_47 thru_hole circle (at 72.39 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_48 thru_hole circle (at 72.39 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_49 thru_hole circle (at 74.93 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_50 thru_hole circle (at 74.93 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_1 thru_hole circle (at 13.97 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_23 thru_hole circle (at 41.91 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_24 thru_hole circle (at 41.91 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_7 thru_hole circle (at 21.59 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_10 thru_hole circle (at 24.13 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_25 thru_hole circle (at 44.45 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_26 thru_hole circle (at 44.45 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_17 thru_hole circle (at 34.29 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_19 thru_hole circle (at 36.83 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_20 thru_hole circle (at 36.83 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_3 thru_hole circle (at 16.51 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_6 thru_hole circle (at 19.05 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_15 thru_hole circle (at 31.75 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_21 thru_hole circle (at 39.37 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_13 thru_hole circle (at 29.21 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_18 thru_hole circle (at 34.29 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_2 thru_hole circle (at 13.97 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_4 thru_hole circle (at 16.51 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_9 thru_hole circle (at 24.13 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_22 thru_hole circle (at 39.37 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_12 thru_hole circle (at 26.67 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_14 thru_hole circle (at 29.21 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_16 thru_hole circle (at 31.75 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_8 thru_hole circle (at 21.59 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_11 thru_hole circle (at 26.67 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_5 thru_hole circle (at 19.05 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_27 thru_hole circle (at 46.99 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_28 thru_hole circle (at 46.99 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_30 thru_hole circle (at 49.53 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_29 thru_hole circle (at 49.53 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_31 thru_hole circle (at 52.07 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_32 thru_hole circle (at 52.07 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_33 thru_hole circle (at 54.61 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_35 thru_hole circle (at 57.15 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_34 thru_hole circle (at 54.61 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_36 thru_hole circle (at 57.15 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_37 thru_hole circle (at 59.69 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_38 thru_hole circle (at 59.69 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_39 thru_hole circle (at 62.23 12.62) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
    (pad H1_52 thru_hole circle (at 77.47 10.08) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x10_Pitch2.00mm (layer F.Cu) (tedit 58CD5450)
    (at 163.83 83.82 90)
    (descr "Through hole straight socket strip, 2x10, 2.00mm pitch, double rows")
    (tags "Through hole socket strip THT 2x10 2.00mm double row")
    (fp_text reference J1 (at 4.1 -2 90) (layer F.SilkS))
    (fp_text value "OEM719 Main Header" (at 4.1 20 90) (layer F.Fab))
    (fp_text user %R (at 4.25 9) (layer F.Fab))
    (pad 20 thru_hole oval (at -2 18 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad20)"))
    (pad 19 thru_hole oval (at 0 18 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad19)"))
    (pad 18 thru_hole oval (at -2 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 17 thru_hole oval (at 0 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at -2 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 15 thru_hole oval (at 0 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at -2 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 12 thru_hole oval (at -2 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at -2 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at -2 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at -2 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at -2 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at -2 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x10_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 189.83 149.86)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 155.24 149.86)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 189.53 85.09)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 154.94 85.09)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Connector_USB:USB_Mini-B_Tensility_54-00023_Vertical (layer F.Cu) (tedit 5A24F112)
    (at 129.13 138.45 90)
    (descr http://www.tensility.com/pdffiles/54-00023.pdf)
    (tags "usb mini receptacle vertical")
    (fp_text reference J2 (at 1.6 -3.7 90) (layer F.SilkS))
    (fp_text value USB_B_Mini (at 1.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 1.5 -1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 0.8 -1.75 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 1.6 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 4 thru_hole circle (at 2.4 -1.75 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 3.2 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at -2.05 -0.875 90) (size 1.1 2.4) (drill oval 0.7 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad6)"))
    (pad 6 thru_hole oval (at 5.25 -0.875 90) (size 1.1 2.4) (drill oval 0.7 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad6)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Mini-B_Tensility_54-00023_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_Altech_AK300-2_P5.00mm (layer F.Cu) (tedit 59FF0306)
    (at 208.28 102.87 90)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference J4 (at -1.92 -6.99 90) (layer F.SilkS))
    (fp_text value "Power Terminal" (at 2.78 7.75 90) (layer F.Fab))
    (fp_text user %R (at 2.5 -2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x10_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 130.81 124.46 180)
    (descr "Through hole straight pin header, 2x10, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.00mm double row")
    (fp_text reference J3 (at 1 -2.06) (layer F.SilkS))
    (fp_text value "DF11-20DP-2DS(24)-TSL_Footprint_Library" (at 1 20.06) (layer F.Fab))
    (fp_text user %R (at 1 9 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 0 6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 2 6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad8)"))
    (pad 9 thru_hole oval (at 0 8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad9)"))
    (pad 10 thru_hole oval (at 2 8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad11)"))
    (pad 12 thru_hole oval (at 2 10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad12)"))
    (pad 13 thru_hole oval (at 0 12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 14 thru_hole oval (at 2 12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad14)"))
    (pad 15 thru_hole oval (at 0 14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad15)"))
    (pad 16 thru_hole oval (at 2 14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 17 thru_hole oval (at 0 16 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad17)"))
    (pad 18 thru_hole oval (at 2 16 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 19 thru_hole oval (at 0 18 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at 2 18 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad20)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x10_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 125.73 158.12) (end 125.73 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 215.9 158.13) (end 125.73 158.12) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 215.9 62.23) (end 215.9 158.13) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 62.23) (end 215.9 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_text "Novatel OEM719 GPS Interface Board" (at 171.45 64.77) (layer F.SilkS))
  (gr_text "USB Mini\n" (at 134.62 137.16 -90) (layer F.SilkS))
  (gr_text "GND\n" (at 210.82 92.71) (layer F.SilkS))
  (gr_text 3.3V+ (at 210.82 107.95) (layer F.SilkS))
  (gr_text "OEM719 Header\n" (at 172.72 80.01) (layer F.SilkS))
  (gr_text "CDH Connector\n" (at 134.62 114.3 270) (layer F.SilkS))
)
