(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.5422)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(3 "In3.Cu" signal)
		(4 "In4.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.1)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.5102)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.1)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 4"
				(type "core")
				(thickness 0.5102)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 5"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "manufacturing/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "FILAMENT_SW")
	(net 3 "+5V")
	(net 4 "SPI_2_SDI")
	(net 5 "SPI_2_SCLK")
	(net 6 "SPI_2_SDO")
	(net 7 "ADS1220_DRDY")
	(net 8 "USB_PULL_UP")
	(net 9 "+24V")
	(net 10 "unconnected-(U5-AIN3{slash}REFN1-Pad6)")
	(net 11 "unconnected-(U5-AIN2-Pad7)")
	(net 12 "Net-(D2-A)")
	(net 13 "FAN0_TACH")
	(net 14 "NRST")
	(net 15 "Net-(D5-A)")
	(net 16 "FAN1_TACH")
	(net 17 "FAN1_PWM")
	(net 18 "BOOT0")
	(net 19 "unconnected-(AC1-RESERVED_1-Pad3)")
	(net 20 "Net-(D6-A)")
	(net 21 "/OSC_IN")
	(net 22 "/OSC_OUT")
	(net 23 "/+5V_USB")
	(net 24 "SWD_IO")
	(net 25 "SW_CLK")
	(net 26 "unconnected-(AC1-NC-Pad10)")
	(net 27 "unconnected-(AC1-INT1-Pad8)")
	(net 28 "unconnected-(AC1-INT2-Pad9)")
	(net 29 "/FAN0_MOSFET_GND")
	(net 30 "USB_D+")
	(net 31 "USB_D-")
	(net 32 "Earth_Protective")
	(net 33 "+5VA")
	(net 34 "Net-(U2-PB3)")
	(net 35 "FAN0_PWM")
	(net 36 "+3V3")
	(net 37 "/AIN0")
	(net 38 "/AIN1")
	(net 39 "/LED_SDI")
	(net 40 "/FILAMENT_SW_V+")
	(net 41 "/FILAMENT_SW_GND")
	(net 42 "/FAN1_MOSFET_GND")
	(net 43 "/LOAD_CELL_IN+")
	(net 44 "/LOAD_CELL_REF-")
	(net 45 "/LOAD_CELL_IN-")
	(net 46 "/LOAD_CELL_REF+")
	(net 47 "SPI_1_SDI")
	(net 48 "SPI_1_SCLK")
	(net 49 "SPI_1_SDO")
	(net 50 "HEATBREAK_THERMISTOR")
	(net 51 "AMBIENT_THERMISTOR")
	(net 52 "/HEATBREAK_TH_VREF")
	(net 53 "/HEATBREAK_TH_GND")
	(net 54 "+5V5")
	(net 55 "unconnected-(VR1-BOOT-Pad7)")
	(net 56 "unconnected-(VR1-SW-Pad6)")
	(net 57 "Net-(VR1-VCC)")
	(net 58 "Net-(VR1-FB)")
	(net 59 "/LED_POWER")
	(net 60 "/LED_GND")
	(net 61 "Net-(D13-A)")
	(net 62 "Net-(D14-A)")
	(net 63 "/SW_HEATSINK")
	(net 64 "Net-(P1-CC1)")
	(net 65 "Net-(P1-CC2)")
	(net 66 "HOTEND_THERMISTOR")
	(net 67 "/HOTEND_TH_VREF")
	(net 68 "Net-(L4-Pad2)")
	(net 69 "Net-(L5-Pad1)")
	(net 70 "/LED_CLK")
	(net 71 "/+24V_INPUT")
	(net 72 "/+FANV_INPUT")
	(net 73 "unconnected-(D16-CKO-Pad2)")
	(net 74 "Net-(U2-PB13)")
	(net 75 "/FAN1_PWM_+5V")
	(net 76 "/FAN0_PWM_+5V")
	(net 77 "Net-(Q1-G)")
	(net 78 "Net-(Q2-G)")
	(net 79 "unconnected-(P1-SBU1-PadA8)")
	(net 80 "unconnected-(P1-SBU2-PadB8)")
	(net 81 "/HOTEND_TH_GND")
	(net 82 "unconnected-(U2-PA15-Pad38)")
	(net 83 "unconnected-(U2-PC15-Pad4)")
	(net 84 "unconnected-(U2-PB11-Pad22)")
	(net 85 "unconnected-(U2-PA0-Pad10)")
	(net 86 "unconnected-(U2-PC14-Pad3)")
	(net 87 "unconnected-(U2-PB12-Pad25)")
	(net 88 "unconnected-(U2-PB9-Pad46)")
	(net 89 "unconnected-(U2-PB10-Pad21)")
	(net 90 "unconnected-(U2-PA1-Pad11)")
	(net 91 "unconnected-(U2-PC13-Pad2)")
	(net 92 "unconnected-(P1-SHIELD-PadS1)")
	(net 93 "unconnected-(P1-SHIELD-PadS1)_1")
	(net 94 "unconnected-(P1-SHIELD-PadS1)_2")
	(net 95 "unconnected-(P1-SHIELD-PadS1)_3")
	(net 96 "unconnected-(U2-PB2-Pad20)")
	(net 97 "Net-(D17-A)")
	(net 98 "unconnected-(D16-SDO-Pad3)")
	(net 99 "RGB_LED_DATA")
	(net 100 "RGB_LED_CLOCK")
	(net 101 "/RGB_INDICATOR_SDO")
	(net 102 "/RGB_INDICATOR_CLK")
	(net 103 "DOTSTAR_LED_DATA")
	(net 104 "DOTSTAR_LED_CLOCK")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 37.1 50.1 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 17.2 3.6 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D6"
			(at 1.41 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RED LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS22-2005-077/LTST-C193KRKT-5A.PDF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LTST-C193KRKT-5A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/liteon/LTST-C193KRKT-5A/2356244"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On Inc."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C193KRKT-5A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "160-1830-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 38.9 41.4 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at -3 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0470_1x04-1MP_P1.50mm_Vertical"
		(layer "F.Cu")
		(at 4.8 29.2 90)
		(descr "Molex CLIK-Mate series connector, 505405-0470 (http://www.molex.com/pdm_docs/sd/5054050270_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex CLIK-Mate side entry")
		(property "Reference" "J8"
			(at 0 -0.635 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0 5.15 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0470_1x04-1MP_P1.50mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "Neopixel"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132250370/14122180"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132250370"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132250370-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.25 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "/LED_GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -0.75 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/LED_SDI")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 0.75 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "/LED_CLK")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at 2.25 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "/LED_POWER")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at -4.85 -2.3 90)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at 4.85 -2.3 90)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_505405-0470_1x04-1MP_P1.50mm_Vertical.stp"
			(offset
				(xyz 0 -2 9.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0470_1x04-1MP_P1.50mm_Vertical"
		(layer "F.Cu")
		(at 4.8 45.6 90)
		(descr "Molex CLIK-Mate series connector, 505405-0470 (http://www.molex.com/pdm_docs/sd/5054050270_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex CLIK-Mate side entry")
		(property "Reference" "J6"
			(at 0 -0.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0 5.15 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0470_1x04-1MP_P1.50mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "Load Cell"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132250470/14122220?s=N4IgjCBcoKxaBjKAzAhgGwM4FMA0IB7KAbRAGYAOAdgCYaBOEAXXwAcAXKEAZXYCcAlgDsA5iAC%2B%2BGhXggkkNFjyES5egwBsABmZtOkHv2FjJIDWVnzFOfEUikN9R4xYgOXXoNET8GjZZQMGxV7EAAWMHoyaN03fUMvE19GaDlApVtVMK0oqNj3A09jHxAKGVSrIOU7UhotMjANKnz4ou9TeggK9OCa8hpGmgtXAoTi0xoYGgCFKszQgZowsjCWjyN2-Gy4btmMkNIIEdaNpJAYMGnd62rVFfotaTXC05KL8sQe29Cycz84Y7rRJvDSra5zA7kS5UMIAvRA8b4GAUFKfPa9LJaGBaR7PMabMz0Zrg-Z9I7wl7Ajr1GY3eakCJUDQ0ZqAymI8BaChgtF0yHRMjqaZs-FnS7mWkQsl4tpixwWEkYn5UMowOFxBEEsBUB6S0mqKiUdWjWUlbWdPVK0hkbE6-wi02mc1XXlS1RgCg5GkO15OnU7V360IROhkVkU0Vmu2W761HFhagy334SIomP0kA6JgTLRgLqBq3gJNUqS5l1pdGxos%2BksgOoe9OQ7VhZnFjl1IaNvqUCg28ka9kEjs8it86U19va8uVIOHPEAEQIAFcAEbobAlAC0%2BdHboWw1Mm5HM8LnthrMPAd3s-IzEPxILVbA23oMFwnez4nEQA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132250470"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132250470-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.25 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/LOAD_CELL_REF+")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -0.75 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/LOAD_CELL_IN+")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 0.75 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/LOAD_CELL_IN-")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at 2.25 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/LOAD_CELL_REF-")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at -4.85 -2.3 90)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at 4.85 -2.3 90)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_505405-0470_1x04-1MP_P1.50mm_Vertical.stp"
			(offset
				(xyz 0 -2 9.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 45.4 32.2 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "R1kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(Q2-G)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "/FAN1_PWM_+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 23.4 3.6 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -1.4 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R2kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(D13-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "/+FANV_INPUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm_ThermalVias"
		(layer "F.Cu")
		(at 23.4 29.8)
		(descr "VSON, 8 Pin (https://www.ti.com/lit/ds/symlink/tlv767-q1.pdf#page=31), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "VSON NoLead")
		(property "Reference" "LDO3"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TPS7A21-Q1 5V @ 500mA"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm_ThermalVias"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a21-q1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "500mA, low-noise ultra-low-IQ high-PSRR low-dropout (LDO) voltage regulator DRB (Wettable flank VSON, 8)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.mouser.com/ProductDetail/Texas-Instruments/TPS7A2150PQWDRBRQ1?qs=ZcfC38r4PotpxWDbDIZdAw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "595-TPS7A2150PQWDRQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TPS7A2150PQWDRBRQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(zone_connect 2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 0)
			(size 1.33 1.93)
			(layers "F.Paste")
			(roundrect_rratio 0.18797)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.45 -0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "+5VA")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.45 -0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.45 0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.45 0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 1.45 0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "+5V5")
			(pinfunction "EN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 1.45 0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 1.45 -0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 1.45 -0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "+5V5")
			(pinfunction "VIN")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 -0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 0)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.65 2.4)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.65 2.4)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 -0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 0)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 17 14.8 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D5"
			(at 0 -1.4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RED LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS22-2005-077/LTST-C193KRKT-5A.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/liteon/LTST-C193KRKT-5A/2356244"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C193KRKT-5A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LTST-C193KRKT-5A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "160-1830-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 26.8 43 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "R47Ω"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U2-PB3)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "SPI_1_SCLK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 17 29.2 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D17"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RED LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS22-2005-077/LTST-C193KRKT-5A.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/liteon/LTST-C193KRKT-5A/2356244"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C193KRKT-5A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LTST-C193KRKT-5A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "160-1830-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "Net-(D17-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 23.4 9.8)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "AMBIENT_THERMISTOR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 41.6 19.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -1.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "R10kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "R-FBB / 50mW / 0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(VR1-FB)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNAL_TLVM23615RDNR:CONV_TLVM23615RDNR"
		(layer "F.Cu")
		(at 35.2 21 -90)
		(property "Reference" "VR1"
			(at 0 3.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "TLVM23615RDNR"
			(at 9.18 3.365 90)
			(layer "F.Fab")
		)
		(property "Footprint" "SNAL_TLVM23615RDNR:CONV_TLVM23615RDNR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlvm23615.pdf?ts=1734735328754"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Power Management Modules 3-V to 17-V input voltage, 3-A output, synchronous buck module with QFN package"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.mouser.com/ProductDetail/Texas-Instruments/TLVM23615RDNR"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "595-TLVM23615RDNR "
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments "
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TPSM861252RDXR"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN-FCMOD11_RDN_TEX")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(zone_connect 2)
		(attr smd)
		(pad "1" smd roundrect
			(at -1.3875 -1.96 270)
			(size 1.225 0.47)
			(layers "F.Cu")
			(roundrect_rratio 0.225)
			(net 1 "GND")
			(pinfunction "PGOOD")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.4 -1.15 270)
			(size 1.2 0.35)
			(layers "F.Cu")
			(roundrect_rratio 0.3)
			(net 9 "+24V")
			(pinfunction "EN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at -1.75 -0.65 270)
			(size 0.45 0.45)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 9 "+24V")
			(pinfunction "VIN")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.4 -0.65 270)
			(size 1.2 0.35)
			(layers "F.Cu")
			(roundrect_rratio 0.3)
			(net 9 "+24V")
			(pinfunction "VIN")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at -1.05 -0.65 270)
			(size 0.45 0.45)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 9 "+24V")
			(pinfunction "VIN")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -1.73 0.55 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 54 "+5V5")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -1.73 1.05 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 54 "+5V5")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -1.73 1.55 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 54 "+5V5")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd custom
			(at -1.2 0.995 270)
			(size 0.9 1)
			(layers "F.Cu")
			(net 54 "+5V5")
			(pinfunction "VOUT")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.7 1.075) (xy -0.705 1.075) (xy -0.71 1.074) (xy -0.716 1.074) (xy -0.721 1.073) (xy -0.726 1.072)
						(xy -0.731 1.07) (xy -0.736 1.068) (xy -0.741 1.066) (xy -0.745 1.064) (xy -0.75 1.062) (xy -0.754 1.059)
						(xy -0.759 1.056) (xy -0.763 1.053) (xy -0.767 1.049) (xy -0.771 1.046) (xy -0.774 1.042) (xy -0.778 1.038)
						(xy -0.781 1.034) (xy -0.784 1.029) (xy -0.787 1.025) (xy -0.789 1.02) (xy -0.791 1.016) (xy -0.793 1.011)
						(xy -0.795 1.006) (xy -0.797 1.001) (xy -0.798 0.996) (xy -0.799 0.991) (xy -0.799 0.985) (xy -0.8 0.98)
						(xy -0.8 0.975) (xy -0.8 -0.975) (xy -0.8 -0.98) (xy -0.799 -0.985) (xy -0.799 -0.991) (xy -0.798 -0.996)
						(xy -0.797 -1.001) (xy -0.795 -1.006) (xy -0.793 -1.011) (xy -0.791 -1.016) (xy -0.789 -1.02)
						(xy -0.787 -1.025) (xy -0.784 -1.029) (xy -0.781 -1.034) (xy -0.778 -1.038) (xy -0.774 -1.042)
						(xy -0.771 -1.046) (xy -0.767 -1.049) (xy -0.763 -1.053) (xy -0.759 -1.056) (xy -0.754 -1.059)
						(xy -0.75 -1.062) (xy -0.745 -1.064) (xy -0.741 -1.066) (xy -0.736 -1.068) (xy -0.731 -1.07) (xy -0.726 -1.072)
						(xy -0.721 -1.073) (xy -0.716 -1.074) (xy -0.71 -1.074) (xy -0.705 -1.075) (xy -0.7 -1.075) (xy 0.7 -1.075)
						(xy 0.705 -1.075) (xy 0.71 -1.074) (xy 0.716 -1.074) (xy 0.721 -1.073) (xy 0.726 -1.072) (xy 0.731 -1.07)
						(xy 0.736 -1.068) (xy 0.741 -1.066) (xy 0.745 -1.064) (xy 0.75 -1.062) (xy 0.754 -1.059) (xy 0.759 -1.056)
						(xy 0.763 -1.053) (xy 0.767 -1.049) (xy 0.771 -1.046) (xy 0.774 -1.042) (xy 0.778 -1.038) (xy 0.781 -1.034)
						(xy 0.784 -1.029) (xy 0.787 -1.025) (xy 0.789 -1.02) (xy 0.791 -1.016) (xy 0.793 -1.011) (xy 0.795 -1.006)
						(xy 0.797 -1.001) (xy 0.798 -0.996) (xy 0.799 -0.991) (xy 0.799 -0.985) (xy 0.8 -0.98) (xy 0.8 -0.975)
						(xy 0.8 0.975) (xy 0.8 0.98) (xy 0.799 0.985) (xy 0.799 0.991) (xy 0.798 0.996) (xy 0.797 1.001)
						(xy 0.795 1.006) (xy 0.793 1.011) (xy 0.791 1.016) (xy 0.789 1.02) (xy 0.787 1.025) (xy 0.784 1.029)
						(xy 0.781 1.034) (xy 0.778 1.038) (xy 0.774 1.042) (xy 0.771 1.046) (xy 0.767 1.049) (xy 0.763 1.053)
						(xy 0.759 1.056) (xy 0.754 1.059) (xy 0.75 1.062) (xy 0.745 1.064) (xy 0.741 1.066) (xy 0.736 1.068)
						(xy 0.731 1.07) (xy 0.726 1.072) (xy 0.721 1.073) (xy 0.716 1.074) (xy 0.71 1.074) (xy 0.705 1.075)
						(xy 0.7 1.075) (xy -0.7 1.075)
					)
					(width 0.01)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -0.78 0.59 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 54 "+5V5")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -0.78 1.41 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 54 "+5V5")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0.78 0.59 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 63 "/SW_HEATSINK")
			(pinfunction "SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0.78 1.41 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 63 "/SW_HEATSINK")
			(pinfunction "SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd custom
			(at 1.2 0.995 270)
			(size 0.9 1)
			(layers "F.Cu")
			(net 63 "/SW_HEATSINK")
			(pinfunction "SW")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.7 1.075) (xy 0.705 1.075) (xy 0.71 1.074) (xy 0.716 1.074) (xy 0.721 1.073) (xy 0.726 1.072)
						(xy 0.731 1.07) (xy 0.736 1.068) (xy 0.741 1.066) (xy 0.745 1.064) (xy 0.75 1.062) (xy 0.754 1.059)
						(xy 0.759 1.056) (xy 0.763 1.053) (xy 0.767 1.049) (xy 0.771 1.046) (xy 0.774 1.042) (xy 0.778 1.038)
						(xy 0.781 1.034) (xy 0.784 1.029) (xy 0.787 1.025) (xy 0.789 1.02) (xy 0.791 1.016) (xy 0.793 1.011)
						(xy 0.795 1.006) (xy 0.797 1.001) (xy 0.798 0.996) (xy 0.799 0.991) (xy 0.799 0.985) (xy 0.8 0.98)
						(xy 0.8 0.975) (xy 0.8 -0.975) (xy 0.8 -0.98) (xy 0.799 -0.985) (xy 0.799 -0.991) (xy 0.798 -0.996)
						(xy 0.797 -1.001) (xy 0.795 -1.006) (xy 0.793 -1.011) (xy 0.791 -1.016) (xy 0.789 -1.02) (xy 0.787 -1.025)
						(xy 0.784 -1.029) (xy 0.781 -1.034) (xy 0.778 -1.038) (xy 0.774 -1.042) (xy 0.771 -1.046) (xy 0.767 -1.049)
						(xy 0.763 -1.053) (xy 0.759 -1.056) (xy 0.754 -1.059) (xy 0.75 -1.062) (xy 0.745 -1.064) (xy 0.741 -1.066)
						(xy 0.736 -1.068) (xy 0.731 -1.07) (xy 0.726 -1.072) (xy 0.721 -1.073) (xy 0.716 -1.074) (xy 0.71 -1.074)
						(xy 0.705 -1.075) (xy 0.7 -1.075) (xy -0.7 -1.075) (xy -0.705 -1.075) (xy -0.71 -1.074) (xy -0.716 -1.074)
						(xy -0.721 -1.073) (xy -0.726 -1.072) (xy -0.731 -1.07) (xy -0.736 -1.068) (xy -0.741 -1.066)
						(xy -0.745 -1.064) (xy -0.75 -1.062) (xy -0.754 -1.059) (xy -0.759 -1.056) (xy -0.763 -1.053)
						(xy -0.767 -1.049) (xy -0.771 -1.046) (xy -0.774 -1.042) (xy -0.778 -1.038) (xy -0.781 -1.034)
						(xy -0.784 -1.029) (xy -0.787 -1.025) (xy -0.789 -1.02) (xy -0.791 -1.016) (xy -0.793 -1.011)
						(xy -0.795 -1.006) (xy -0.797 -1.001) (xy -0.798 -0.996) (xy -0.799 -0.991) (xy -0.799 -0.985)
						(xy -0.8 -0.98) (xy -0.8 -0.975) (xy -0.8 0.975) (xy -0.8 0.98) (xy -0.799 0.985) (xy -0.799 0.991)
						(xy -0.798 0.996) (xy -0.797 1.001) (xy -0.795 1.006) (xy -0.793 1.011) (xy -0.791 1.016) (xy -0.789 1.02)
						(xy -0.787 1.025) (xy -0.784 1.029) (xy -0.781 1.034) (xy -0.778 1.038) (xy -0.774 1.042) (xy -0.771 1.046)
						(xy -0.767 1.049) (xy -0.763 1.053) (xy -0.759 1.056) (xy -0.754 1.059) (xy -0.75 1.062) (xy -0.745 1.064)
						(xy -0.741 1.066) (xy -0.736 1.068) (xy -0.731 1.07) (xy -0.726 1.072) (xy -0.721 1.073) (xy -0.716 1.074)
						(xy -0.71 1.074) (xy -0.705 1.075) (xy -0.7 1.075) (xy 0.7 1.075)
					)
					(width 0.01)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 1.73 0.55 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 63 "/SW_HEATSINK")
			(pinfunction "SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 1.73 1.05 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 63 "/SW_HEATSINK")
			(pinfunction "SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 1.73 1.55 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 63 "/SW_HEATSINK")
			(pinfunction "SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 1.4 -0.65 270)
			(size 1.2 0.35)
			(layers "F.Cu")
			(roundrect_rratio 0.3)
			(net 56 "unconnected-(VR1-SW-Pad6)")
			(pinfunction "SW")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 1.4 -1.15 270)
			(size 1.2 0.35)
			(layers "F.Cu")
			(roundrect_rratio 0.3)
			(net 55 "unconnected-(VR1-BOOT-Pad7)")
			(pinfunction "BOOT")
			(pintype "power_in+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 1.425 -1.96 270)
			(size 1.15 0.47)
			(layers "F.Cu")
			(roundrect_rratio 0.225)
			(net 57 "Net-(VR1-VCC)")
			(pinfunction "VCC")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 0.5 -2.06 270)
			(size 0.35 0.9)
			(layers "F.Cu")
			(roundrect_rratio 0.3)
			(net 58 "Net-(VR1-FB)")
			(pinfunction "FB")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 0 -1.23 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 0 -0.23 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 0 -0.01 270)
			(size 0.35 5)
			(layers "F.Cu")
			(roundrect_rratio 0.3)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 0 0.77 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 0 1.77 270)
			(size 0.4 0.4)
			(drill 0.245)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -0.5 -2.06 270)
			(size 0.35 0.9)
			(layers "F.Cu")
			(roundrect_rratio 0.3)
			(net 1 "GND")
			(pinfunction "RT")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/ULTRA_TLVM23615RDNR/RDN0011A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 34.7 25.6)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D15"
			(at -4.2 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "40V, 1A, SMA"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/B120_B-B160_B.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "B140-13-F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/diodes-incorporated/B140-13-F/814934"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "B140-FDICT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 9 "+24V")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 23 "/+5V_USB")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 48.8 26.8 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "FAN0_TACH")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(locked yes)
		(layer "F.Cu")
		(at 56 56)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 15.5 44.3 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R240Ω"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/AIN1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(L5-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 21.4 3.6 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D13"
			(at 1.4 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RED LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS22-2005-077/LTST-C193KRKT-5A.PDF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/liteon/LTST-C193KRKT-5A/2356244"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On Inc."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C193KRKT-5A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LTST-C193KRKT-5A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "160-1830-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/FAN0_MOSFET_GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(D13-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 37 15.6 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 50V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 9 "+24V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 30.5 38.4 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(locked yes)
		(layer "F.Cu")
		(at 56 4)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H4"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 17 22 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -1.6 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RED LED"
			(at -0.1 -1.57 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS22-2005-077/LTST-C193KRKT-5A.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/liteon/LTST-C193KRKT-5A/2356244"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C193KRKT-5A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LTST-C193KRKT-5A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "160-1830-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 4.6 21.2 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at -3.809558 -0.020446 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 36V / 10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
		(layer "F.Cu")
		(at 20.3 50.9 180)
		(descr "Texas RSA VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/msp430g2001.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "Texas VQFN NoLead")
		(property "Reference" "U5"
			(at -2.6 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1220"
			(at 0 3.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1220.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low-power, quad-input, 24-bit analog to digital converter, integrated temperature sensor, SPI interface, TSSOP-16 package"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/texas-instruments/ADS1220IRVAR/4866973"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "296-48475-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ADS1220IRVAR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.9 -0.9 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.9 0 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.9 0.9 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0 -0.9 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0 0 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0 0.9 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.9 -0.9 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.9 0 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.9 0.9 180)
			(size 0.73 0.73)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.9625 -0.975 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "SPI_1_SCLK")
			(pinfunction "SCLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.9625 -0.325 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{CS}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.9625 0.325 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "CLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.9625 0.975 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "DGND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -0.975 1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AVSS")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -0.325 1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "unconnected-(U5-AIN3{slash}REFN1-Pad6)")
			(pinfunction "AIN3/REFN1")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 0.325 1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "unconnected-(U5-AIN2-Pad7)")
			(pinfunction "AIN2")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 0.975 1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "REFN0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 1.9625 0.975 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "+5VA")
			(pinfunction "REFP0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 1.9625 0.325 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/AIN1")
			(pinfunction "AIN1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 1.9625 -0.325 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/AIN0")
			(pinfunction "AIN0/REFP1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 1.9625 -0.975 180)
			(size 0.825 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "+5VA")
			(pinfunction "AVDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 0.975 -1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "DVDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 0.325 -1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "ADS1220_DRDY")
			(pinfunction "~{DRDY}")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -0.325 -1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "SPI_1_SDI")
			(pinfunction "DOUT/~{DRDY}")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -0.975 -1.9625 180)
			(size 0.35 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "SPI_1_SDO")
			(pinfunction "DIN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 2.7 2.7)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "THERMAL")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 17.375 39.275 90)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "J13"
			(at -2.63 2.67 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_2x4_P2.54mm"
			(at 1.27 7.41 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "BOOT0")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "SW_CLK")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "+3V3")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "SWD_IO")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_width 0.4)
			(thermal_gap 0.2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 19.4 9.8 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "R4.7kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "AMBIENT_THERMISTOR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AQ4020-01FTG:SOD2613X114N"
		(layer "F.Cu")
		(at 11.4 26.4)
		(descr "SOD323")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D4"
			(at 0 -1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "AQW05-01FTG"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AQ4020-01FTG:SOD2613X114N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/littelfuse_tvs_diode_array_aq3530-01ftg_datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30A 230pF AEC-Q101 Unidirectional 5V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AQW05-01FTG"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/AQW05-01FTG/22320797"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "18-AQW05-01FTGCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 90)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "/LED_CLK")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.15 0 90)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "AQ4020-01FTG.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical"
		(layer "F.Cu")
		(at 55.2 24 -90)
		(descr "Molex CLIK-Mate series connector, 505405-0370 (http://www.molex.com/pdm_docs/sd/5054050270_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex CLIK-Mate side entry")
		(property "Reference" "J1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 0 5.15 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "Hotend Fan"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132250370/14122180"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132250370"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132250370-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/FAN0_MOSFET_GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "FAN0_TACH")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 1.5 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "/+FANV_INPUT")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at -4.1 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at 4.1 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical.stp"
			(offset
				(xyz 0 -2 9.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 19.4 26.6)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -2.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R2kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "Net-(D17-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "+5VA")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "F.Cu")
		(at 14.2 3.6 180)
		(descr "SOT-363, SC-70-6, SC-88")
		(tags "SOT-363 SC-70-6 SC-88")
		(property "Reference" "U4"
			(at 0 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC2G17DSFR"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc2g17.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC BUFFER 2 CHANNEL NON-INVERT 5.5V 6SON"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6076"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "771-LVC1G17GV125"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nexperia/74LVC1G17GV125?qs=me8TqzrmIYX3DxU5Fpa8sQ%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Nexperia"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "74LVC1G17GV,125"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/nexperia-usa-inc/74LVC1G17GV-125/1231446"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "1727-6070-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSF6_TEX")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "RGB_LED_CLOCK")
			(pinfunction "1A")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.95 0 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "RGB_LED_DATA")
			(pinfunction "2A")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 102 "/RGB_INDICATOR_CLK")
			(pinfunction "2Y")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 0.95 0 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 101 "/RGB_INDICATOR_SDO")
			(pinfunction "1Y")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 18.3 46.7 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "+5VA")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 50.4 16 180)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L11"
			(at 2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 180)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "/HEATBREAK_TH_GND")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 180)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
		(layer "F.Cu")
		(at 33.3 44 90)
		(descr "QFN, 48 Pin (http://www.st.com/resource/en/datasheet/stm32f042k6.pdf#page=94), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead ST_UFQFPN48 Analog_CP-48-13 JEDEC_MO-220-WKKD-4")
		(property "Reference" "U2"
			(at -3 5.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32F103CBU6TR"
			(at 0 4.83 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103cb.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, 48UFQFPN"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/stmicroelectronics/STM32F103CBU6TR/5268215"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "497-18757-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "STM32F103CBU6TR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*7x7mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -2.1 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -2.1 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -2.1 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -2.1 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.7 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.7 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.7 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.7 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.7 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.7 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.7 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.7 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 2.1 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 2.1 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 2.1 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 2.1 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -3.4375 -2.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "VBAT")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -3.4375 -2.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "unconnected-(U2-PC13-Pad2)")
			(pinfunction "PC13")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -3.4375 -1.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "unconnected-(U2-PC14-Pad3)")
			(pinfunction "PC14")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -3.4375 -1.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "unconnected-(U2-PC15-Pad4)")
			(pinfunction "PC15")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -3.4375 -0.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/OSC_IN")
			(pinfunction "PD0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -3.4375 -0.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/OSC_OUT")
			(pinfunction "PD1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -3.4375 0.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "NRST")
			(pinfunction "NRST")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -3.4375 0.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSSA")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -3.4375 1.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "VDDA")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -3.4375 1.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 85 "unconnected-(U2-PA0-Pad10)")
			(pinfunction "PA0")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -3.4375 2.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 90 "unconnected-(U2-PA1-Pad11)")
			(pinfunction "PA1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -3.4375 2.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "HOTEND_THERMISTOR")
			(pinfunction "PA2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -2.75 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "FAN1_TACH")
			(pinfunction "PA3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -2.25 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "FAN0_TACH")
			(pinfunction "PA4")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -1.75 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "FAN1_PWM")
			(pinfunction "PA5")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -1.25 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "HEATBREAK_THERMISTOR")
			(pinfunction "PA6")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at -0.75 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "FILAMENT_SW")
			(pinfunction "PA7")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at -0.25 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "FAN0_PWM")
			(pinfunction "PB0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 0.25 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "AMBIENT_THERMISTOR")
			(pinfunction "PB1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 0.75 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 96 "unconnected-(U2-PB2-Pad20)")
			(pinfunction "PB2")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 1.25 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "unconnected-(U2-PB10-Pad21)")
			(pinfunction "PB10")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 1.75 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "unconnected-(U2-PB11-Pad22)")
			(pinfunction "PB11")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 2.25 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 2.75 3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 3.4375 2.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "unconnected-(U2-PB12-Pad25)")
			(pinfunction "PB12")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 3.4375 2.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(U2-PB13)")
			(pinfunction "PB13")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 3.4375 1.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "SPI_2_SDI")
			(pinfunction "PB14")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 3.4375 1.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "SPI_2_SDO")
			(pinfunction "PB15")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 3.4375 0.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "RGB_LED_CLOCK")
			(pinfunction "PA8")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 3.4375 0.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "RGB_LED_DATA")
			(pinfunction "PA9")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 3.4375 -0.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "USB_PULL_UP")
			(pinfunction "PA10")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 3.4375 -0.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "USB_D+")
			(pinfunction "PA11")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" smd roundrect
			(at 3.4375 -1.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "USB_D-")
			(pinfunction "PA12")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" smd roundrect
			(at 3.4375 -1.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "SWD_IO")
			(pinfunction "PA13")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" smd roundrect
			(at 3.4375 -2.25 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" smd roundrect
			(at 3.4375 -2.75 90)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" smd roundrect
			(at 2.75 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "SW_CLK")
			(pinfunction "PA14")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" smd roundrect
			(at 2.25 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "unconnected-(U2-PA15-Pad38)")
			(pinfunction "PA15")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" smd roundrect
			(at 1.75 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U2-PB3)")
			(pinfunction "PB3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" smd roundrect
			(at 1.25 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "SPI_1_SDI")
			(pinfunction "PB4")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "41" smd roundrect
			(at 0.75 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "SPI_1_SDO")
			(pinfunction "PB5")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "42" smd roundrect
			(at 0.25 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "DOTSTAR_LED_DATA")
			(pinfunction "PB6")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "43" smd roundrect
			(at -0.25 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "DOTSTAR_LED_CLOCK")
			(pinfunction "PB7")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "44" smd roundrect
			(at -0.75 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "BOOT0")
			(pinfunction "BOOT0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "45" smd roundrect
			(at -1.25 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "ADS1220_DRDY")
			(pinfunction "PB8")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "46" smd roundrect
			(at -1.75 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "unconnected-(U2-PB9-Pad46)")
			(pinfunction "PB9")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "47" smd roundrect
			(at -2.25 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "48" smd roundrect
			(at -2.75 -3.4375 90)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "49" smd rect
			(at 0 0 90)
			(size 5.6 5.6)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 54.7 29.9 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 2.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R20kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/FAN1_MOSFET_GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 19.4 12)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -2.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R2kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D5-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 34.4 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L9"
			(at 0.7 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "/LED_GND")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ADXL345:ADXL345"
		(layer "F.Cu")
		(at 41.8 54.6 180)
		(descr "CC-14-1")
		(tags "Accelerometer")
		(property "Reference" "AC1"
			(at 0 3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADXL345"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "ADXL345:ADXL345"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.analog.com/media/en/technical-documentation/data-sheets/ADXL345.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3-Axis Accelerometer IC Extended Temperature Range"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "N/A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/ADXL345?qs=5aG0NVq1C4y%252BItyqaAF9pQ%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ADXL345TCCZ-EP-RL7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/ADXL345TCCZ-EP-RL7/3043345"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "ADXL345TCCZ-EP-RL7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "505-ADXL345TCCZ-EP-RL7CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.0975 -2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "+3V3")
			(pinfunction "VDD_I/O")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -1.0975 -1.2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND_1")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -1.0975 -0.4 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "unconnected-(AC1-RESERVED_1-Pad3)")
			(pinfunction "RESERVED_1")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at -1.0975 0.4 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -1.0975 1.2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND_3")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at -1.0975 2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "+3V3")
			(pinfunction "VS")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at 0 2.0975 180)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "~{CS}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at 1.0975 2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "unconnected-(AC1-INT1-Pad8)")
			(pinfunction "INT1")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 1.0975 1.2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "unconnected-(AC1-INT2-Pad9)")
			(pinfunction "INT2")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at 1.0975 0.4 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "unconnected-(AC1-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at 1.0975 -0.4 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "RESERVED_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 1.0975 -1.2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SPI_2_SDI")
			(pinfunction "SDO/ALT_ADDRESS")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at 1.0975 -2 270)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "SPI_2_SDO")
			(pinfunction "SDA/SDI/SDIO")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at 0 -2.0975 180)
			(size 0.55 1.145)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SPI_2_SCLK")
			(pinfunction "SCL/SCLK")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/ADXL345/ADXL345.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 45.4 20.4 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "R1kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "Net-(Q1-G)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "/FAN0_PWM_+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 50.8 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 1.3 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/LOAD_CELL_REF+")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "+5VA")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 10.6 47.999 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L4"
			(at 2.4 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/LOAD_CELL_IN+")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "Net-(L4-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 27.6 3.6 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -1.4 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R2kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "Net-(D14-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "/+FANV_INPUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AQ4020-01FTG:SOD2613X114N"
		(layer "F.Cu")
		(at 43.5 11.2 180)
		(descr "SOD323")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D10"
			(at 3.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "AQ4020-01FTG-C"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AQ4020-01FTG:SOD2613X114N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/2/AQ4020-01FTG.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30A 2.5pF AEC-Q101 Bidirectional 3.3V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.14"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AQ4020-01FTG-C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/AQ4020-01FTG-C/7902198?s=N4IgTCBcDaIIIEUAsAGMKC0KCMAxAKgOIYDCIAugL5A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "F10395CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "USB_D-")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "AQ4020-01FTG.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AQ4020-01FTG:SOD2613X114N"
		(layer "F.Cu")
		(at 11.4 14)
		(descr "SOD323")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D11"
			(at 0 -1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "AQ4020-01FTG"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AQ4020-01FTG:SOD2613X114N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/2/AQ4020-01FTG.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30A 2.5pF AEC-Q101 Unidirection 3.3V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AQ4020-01FTG"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "576-AQ4020-01FTG"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Littelfuse/AQ4020-01FTG?qs=YCa%2FAAYMW015W3B84qpvIw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AQ4020-01FTG"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aq4020-01ftg/littelfuse?region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/AQ4020-01FTG/7902197"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "F10394CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 90)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "FILAMENT_SW")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.15 0 90)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "AQ4020-01FTG.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 31.8 28.6 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -2.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R5.1kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(P1-CC1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 48.8 28.8 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R1kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "FAN0_TACH")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 48.8 38.6 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "FAN1_TACH")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED-APA102-2020"
		(layer "F.Cu")
		(at 10.4 3.6)
		(descr "http://www.led-color.com/upload/201604/APA102-2020%20SMD%20LED.pdf")
		(tags "LED RGB SPI")
		(property "Reference" "D16"
			(at 0 2.11 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DotStar Micro LED"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED-APA102-2020"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/3341/3341_APA102-2020+SMD+LED.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "APA102-2020"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Adafruit"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.adafruit.com/product/3341"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Adafruit"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "APA102-2020"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "APA102-2020"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*APA102*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -1.6 -0.9 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.85 -0.9)
			(size 0.8 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "1" smd rect
			(at 0 -0.83 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -0.85 0)
			(size 0.8 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "unconnected-(D16-CKO-Pad2)")
			(pinfunction "CKO")
			(pintype "output+no_connect")
		)
		(pad "3" smd rect
			(at -0.85 0.9)
			(size 0.8 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "unconnected-(D16-SDO-Pad3)")
			(pinfunction "SDO")
			(pintype "output+no_connect")
		)
		(pad "4" smd rect
			(at 0.85 0.9)
			(size 0.8 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "/RGB_INDICATOR_SDO")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 0.85 0)
			(size 0.8 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "/RGB_INDICATOR_CLK")
			(pinfunction "CKI")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 0 0.59 90)
			(size 1.48 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at 0.85 -0.9)
			(size 0.8 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED-APA102-2020.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
		(layer "F.Cu")
		(at 48.8 20.3)
		(descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 3.3x3.3x1 mm Body [VSON] http://www.ti.com/lit/ds/symlink/csd87334q3d.pdf")
		(tags "VSON 0.65")
		(property "Reference" "Q1"
			(at 3.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "CSD17581Q3A"
			(at 0 2.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd17581q3a.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "60A Id, 30V Vds, NexFET N-Channel Power MOSFET, 3.2mOhm Ron, Qg Typ 20nC, VSON-8 3.3x3.3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/texas-instruments/CSD17581Q3A/6235429"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "296-47754-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "CSD17581Q3A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.9mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "October 2016"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VSON*3.3x3.3mm*P0.65mm*NexFET*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.526 0.242 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -0.09 -0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd rect
			(at -0.09 0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd rect
			(at 0.86 -0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd rect
			(at 0.86 0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 -0.9725)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 -0.33)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 0.33)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 0.9725)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.44 -0.97)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.44 -0.33)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.44 0.33)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.44 0.97)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd custom
			(at 0.385 0)
			(size 1.9 2.45)
			(layers "F.Cu" "F.Mask")
			(net 29 "/FAN0_MOSFET_GND")
			(pinfunction "D")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1.371 -0.72) (xy 0.95 -0.72) (xy 0.95 -0.58) (xy 1.37 -0.58) (xy 1.37 -0.08) (xy 0.95 -0.08)
						(xy 0.95 0.08) (xy 1.37 0.08) (xy 1.37 0.58) (xy 0.95 0.58) (xy 0.95 0.72) (xy 1.37 0.72) (xy 1.37 1.225)
						(xy -0.95 1.225) (xy -0.95 -1.225) (xy 1.371 -1.225)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 40.1 34.1 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "R5.1kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(P1-CC2)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 39.4 19.8 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 1.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "R45.3kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "R-FBT / 50mW / 0.1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "+5V5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(VR1-FB)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 33.73 36.2 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "R1.5kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "USB_PULL_UP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "USB_D+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0270_1x02-1MP_P1.50mm_Vertical"
		(layer "F.Cu")
		(at 55.2 46.8 -90)
		(descr "Molex CLIK-Mate series connector, 505405-0270 (http://www.molex.com/pdm_docs/sd/5054050270_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex CLIK-Mate side entry")
		(property "Reference" "J7"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 5.15 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0270_1x02-1MP_P1.50mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "PT100"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey "
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132250230/14122139"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132250230"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132250230CT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.75 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "/HOTEND_TH_VREF")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.75 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "/HOTEND_TH_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at -3.35 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at 3.35 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_505405-0270_1x02-1MP_P1.50mm_Vertical.stp"
			(offset
				(xyz 0 -2 9.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(locked yes)
		(layer "F.Cu")
		(at 4 56)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 45.4 24 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "R10kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "/FAN0_PWM_+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 50.4 10.2 180)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L10"
			(at 2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 180)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/HEATBREAK_TH_VREF")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 180)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "HEATBREAK_THERMISTOR")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 30.8 56.3)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.23 0)
			(layer "F.SilkS")
		)
		(property "Value" "25pF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "C0G / 25V / 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/OSC_IN")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 34.2 10.2 180)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D1"
			(at 2.9 -1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "SMAJ24A"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smaj_datasheet.pdf.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TVS DIODE 6VWM 10.3VC DO214AC 400W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/SMAJ6-0A/762252"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SMAJ6A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LITTELFUSE"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "SMAJ6.0ALFCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 71 "/+24V_INPUT")
			(pinfunction "A1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 29.2 8.2 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "NRST")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "GCT_USB4145-03-0170-C:USB4145030170C"
		(layer "F.Cu")
		(at 34 32.2)
		(descr "USB4145-03-0170-C-4")
		(tags "Connector")
		(property "Reference" "P1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "USB_C_Plug_USB2.0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "GCT_USB4145-03-0170-C:USB4145030170C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/5561/USB4145%20-%20Product%20Drawing.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "GCT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "USB4145-03-0170-C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/gct/USB4145-03-0170-C/16649098"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "2073-USB4145-03-0170-CCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -4 0)
			(size 0.71 0.71)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 4 0)
			(size 0.71 0.71)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -2.75 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "A4" smd rect
			(at -1.25 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/+5V_USB")
			(pinfunction "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "A5" smd rect
			(at -0.75 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(P1-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "A6" smd rect
			(at -0.25 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "USB_D+")
			(pinfunction "D+")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "A7" smd rect
			(at 0.25 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "USB_D-")
			(pinfunction "D-")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "A8" smd rect
			(at 0.75 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "unconnected-(P1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "A9" smd rect
			(at 1.25 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/+5V_USB")
			(pinfunction "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "A12" smd rect
			(at 2.75 -1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B1" smd rect
			(at 2.75 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B4" smd rect
			(at 1.25 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/+5V_USB")
			(pinfunction "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B5" smd rect
			(at 0.75 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(P1-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B6" smd rect
			(at 0.25 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "USB_D+")
			(pinfunction "D+")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B7" smd rect
			(at -0.25 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "USB_D-")
			(pinfunction "D-")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B8" smd rect
			(at -0.75 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "unconnected-(P1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B9" smd rect
			(at -1.25 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/+5V_USB")
			(pinfunction "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B12" smd rect
			(at -2.75 1.485)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "S1" thru_hole circle
			(at -4 -1.43)
			(size 1.875 1.875)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(P1-SHIELD-PadS1)")
			(pinfunction "SHIELD")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "S1" thru_hole circle
			(at -4 1.43)
			(size 1.875 1.875)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(P1-SHIELD-PadS1)_3")
			(pinfunction "SHIELD")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "S1" thru_hole circle
			(at 4 -1.43)
			(size 1.875 1.875)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(P1-SHIELD-PadS1)_2")
			(pinfunction "SHIELD")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "S1" thru_hole circle
			(at 4 1.43)
			(size 1.875 1.875)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(P1-SHIELD-PadS1)_1")
			(pinfunction "SHIELD")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/LIB_USB4145-03-0170-C/USB4145-03-0170-C.stp"
			(offset
				(xyz 0 0 7.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "F.Cu")
		(at 42.8 27.8)
		(descr "SOT-363, SC-70-6, SC-88")
		(tags "SOT-363 SC-70-6 SC-88")
		(property "Reference" "U1"
			(at 0 2.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC2G17DSFR"
			(at 0 2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc2g17.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC BUFFER 2 CHANNEL NON-INVERT 5.5V 6SON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6076"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "771-LVC1G17GV125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nexperia/74LVC1G17GV125?qs=me8TqzrmIYX3DxU5Fpa8sQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Nexperia"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "74LVC1G17GV,125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/nexperia-usa-inc/74LVC1G17GV-125/1231446"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "1727-6070-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSF6_TEX")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "FAN0_PWM")
			(pinfunction "1A")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "FAN1_PWM")
			(pinfunction "2A")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at 0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "/FAN1_PWM_+5V")
			(pinfunction "2Y")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "/FAN0_PWM_+5V")
			(pinfunction "1Y")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 10.6 43.2 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L5"
			(at 2.4 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(L5-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/LOAD_CELL_IN-")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 30.782659 49.359939 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 45.4 35.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "R10kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "/FAN1_PWM_+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 16.7 55.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "+5VA")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm_ThermalVias"
		(layer "F.Cu")
		(at 23.4 15.4)
		(descr "VSON, 8 Pin (https://www.ti.com/lit/ds/symlink/tlv767-q1.pdf#page=31), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "VSON NoLead")
		(property "Reference" "LDO1"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TPS7A21-Q1 5V @ 500mA"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm_ThermalVias"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a21-q1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "500mA, low-noise ultra-low-IQ high-PSRR low-dropout (LDO) voltage regulator DRB (Wettable flank VSON, 8)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.mouser.com/ProductDetail/Texas-Instruments/TPS7A2150PQWDRBRQ1?qs=ZcfC38r4PotpxWDbDIZdAw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "595-TPS7A2150PQWDRQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TPS7A2150PQWDRBRQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(zone_connect 2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 0)
			(size 1.33 1.93)
			(layers "F.Paste")
			(roundrect_rratio 0.18797)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.45 -0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.45 -0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.45 0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.45 0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 1.45 0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "+5V5")
			(pinfunction "EN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 1.45 0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 1.45 -0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 1.45 -0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "+5V5")
			(pinfunction "VIN")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 -0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 0)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.65 2.4)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections no)
			)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.65 2.4)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 -0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 0)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 10 55.2)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 33 "+5VA")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "F.Cu")
		(at 11.6 29.2 180)
		(descr "SOT-363, SC-70-6, SC-88")
		(tags "SOT-363 SC-70-6 SC-88")
		(property "Reference" "U3"
			(at 1.9 1.1 -90)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC2G17DSFR"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc2g17.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC BUFFER 2 CHANNEL NON-INVERT 5.5V 6SON"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6076"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "771-LVC1G17GV125"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nexperia/74LVC1G17GV125?qs=me8TqzrmIYX3DxU5Fpa8sQ%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Nexperia"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "74LVC1G17GV,125"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/nexperia-usa-inc/74LVC1G17GV-125/1231446"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "1727-6070-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSF6_TEX")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "DOTSTAR_LED_DATA")
			(pinfunction "1A")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -0.95 0 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "DOTSTAR_LED_CLOCK")
			(pinfunction "2A")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "/LED_CLK")
			(pinfunction "2Y")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 0.95 0 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/LED_SDI")
			(pinfunction "1Y")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 27.9 46.6 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 1.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 14.9 36.4 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 54.8 18.2 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 2.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R20kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/FAN0_MOSFET_GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 11.4 16.8)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 -1.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "FILAMENT_SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 19.4 15.6 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 18.4 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L7"
			(at -0.9 1.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/FILAMENT_SW_V+")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_PTS810"
		(layer "F.Cu")
		(at 32.8 5 90)
		(descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
		(tags "SPST Button Switch")
		(property "Reference" "SW1"
			(at 0.075 0.175 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_SPST"
			(at 0 2.6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_PTS810"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/1476/pts810.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/c-k/PTS810SJS250SMTR-LFS/4142163"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "CKN10878CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "C&K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PTS810SJS250SMTR LFS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.075 -1.075 90)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "NRST")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd rect
			(at 2.075 -1.075 90)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "NRST")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -2.075 1.075 90)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 1.075 90)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/PTS810/PTS810SJS250SMTR LFS.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(locked yes)
		(layer "F.Cu")
		(at 4 4)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Earth_Protective")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical"
		(layer "F.Cu")
		(at 55.2 35.8 -90)
		(descr "Molex CLIK-Mate series connector, 505405-0370 (http://www.molex.com/pdm_docs/sd/5054050270_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex CLIK-Mate side entry")
		(property "Reference" "J11"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 0 5.15 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "Print Fan"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132250370/14122180"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132250370"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132250370-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/FAN1_MOSFET_GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "FAN1_TACH")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 1.5 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "/+FANV_INPUT")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at -4.1 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at 4.1 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical.stp"
			(offset
				(xyz 0 -2 9.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 48.8 55.4 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 1.7 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 37 38.4)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.23 0)
			(layer "F.SilkS")
		)
		(property "Value" "R47Ω"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(U2-PB13)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "SPI_2_SCLK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 40.2 24)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 16V / 10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "Net-(VR1-VCC)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 14.9 39.6 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "R10kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "BOOT0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 40.982659 41.559939 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 51.2 6.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 3 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "HEATBREAK_THERMISTOR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 25.6 3.6 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D14"
			(at 1.4 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RED LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS22-2005-077/LTST-C193KRKT-5A.PDF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/liteon/LTST-C193KRKT-5A/2356244"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On Inc."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C193KRKT-5A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LTST-C193KRKT-5A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "160-1830-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/FAN1_MOSFET_GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "Net-(D14-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 33.8 15.6 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 36V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 54 "+5V5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 27.4 22.8 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 3.3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 54 "+5V5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 35.1 50.1 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm_ThermalVias"
		(layer "F.Cu")
		(at 23.4 22.6)
		(descr "VSON, 8 Pin (https://www.ti.com/lit/ds/symlink/tlv767-q1.pdf#page=31), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "VSON NoLead")
		(property "Reference" "LDO2"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TPS7A21-Q1 3.3V @ 500mA"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm_ThermalVias"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a21-q1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "500mA, low-noise ultra-low-IQ high-PSRR low-dropout (LDO) voltage regulator DRB (Wettable flank VSON, 8)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.mouser.com/ProductDetail/Texas-Instruments/TPS7A2133PQWDRBRQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "595-S7A2133PQWDRBRQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TPS7A2133PQWDRBRQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(zone_connect 2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 0)
			(size 1.33 1.93)
			(layers "F.Paste")
			(roundrect_rratio 0.18797)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.45 -0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pinfunction "VOUT")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.45 -0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.45 0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.45 0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 1.45 0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "+5V5")
			(pinfunction "EN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 1.45 0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 1.45 -0.325)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 1.45 -0.975)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "+5V5")
			(pinfunction "VIN")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 -0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 0)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -0.575 0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.65 2.4)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.65 2.4)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 -0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 0)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0.575 0.95)
			(size 0.5 0.5)
			(drill 0.2032)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 9.6 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L6"
			(at 1.1 -1.3 -90)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/FILAMENT_SW_GND")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 15.5 48.7)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -1.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/AIN0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/AIN1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 15.5 50.9)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -1.45 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/AIN0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ECS-.327-6-34QCS-TR:XTAL_ECS-.327-6-34QCS-TR"
		(layer "F.Cu")
		(at 32.8 53.3 180)
		(property "Reference" "Y1"
			(at -2.7 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Crystal"
			(at 3.064702 1.80631 0)
			(layer "F.Fab")
		)
		(property "Footprint" "ECS-.327-6-34QCS-TR:XTAL_ECS-.327-6-34QCS-TR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://ecsxtal.com/store/pdf/ECX-34Q.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2 Pin Crystal"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ECS"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ECS-.327-6-34QCS-TR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/ecs-inc/ecs-327-6-34qcs-tr/6050743"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "XC2162CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.25 0 180)
			(size 1.1 1.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/OSC_OUT")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.25 0 180)
			(size 1.1 1.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/OSC_IN")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/ECS-.327-6-34QCS-TR/ECS-.327-6-34QCS-TR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0270_1x02-1MP_P1.50mm_Vertical"
		(layer "F.Cu")
		(at 55.2 13.2 -90)
		(descr "Molex CLIK-Mate series connector, 505405-0270 (http://www.molex.com/pdm_docs/sd/5054050270_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex CLIK-Mate side entry")
		(property "Reference" "J9"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 5.15 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0270_1x02-1MP_P1.50mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "Heatbreak NTC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey "
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132250230/14122139"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132250230"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132250230CT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.75 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/HEATBREAK_TH_VREF")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.75 2.75 270)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "/HEATBREAK_TH_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at -3.35 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at 3.35 -2.3 270)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_505405-0270_1x02-1MP_P1.50mm_Vertical.stp"
			(offset
				(xyz 0 -2 9.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 48.9 48.9 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "R4.7kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 0.1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "HOTEND_THERMISTOR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 50 13.2 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "R4.7kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "HEATBREAK_THERMISTOR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 19.2 3.6 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.4 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R1kΩ"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D6-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "USB_PULL_UP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AQ4020-01FTG:SOD2613X114N"
		(layer "F.Cu")
		(at 11.4 32)
		(descr "SOD323")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D12"
			(at 0 1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "AQW05-01FTG"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AQ4020-01FTG:SOD2613X114N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/littelfuse_tvs_diode_array_aq3530-01ftg_datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30A 230pF AEC-Q101 Unidirectional 5V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AQW05-01FTG"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/AQW05-01FTG/22320797"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "18-AQW05-01FTGCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 90)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "/LED_SDI")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.15 0 90)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "AQ4020-01FTG.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 15.5 53.1 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 1.45 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R240Ω"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/AIN0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "Net-(L4-Pad2)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 24 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L8"
			(at -0.4 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "/LED_POWER")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AQ4020-01FTG:SOD2613X114N"
		(layer "F.Cu")
		(at 48.8 24 180)
		(descr "SOD323")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D7"
			(at 0 -1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "AQ4020-01FTG"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AQ4020-01FTG:SOD2613X114N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/2/AQ4020-01FTG.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30A 2.5pF AEC-Q101 Unidirection 3.3V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.14"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AQ4020-01FTG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "576-AQ4020-01FTG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Littelfuse/AQ4020-01FTG?qs=YCa%2FAAYMW015W3B84qpvIw%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AQ4020-01FTG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aq4020-01ftg/littelfuse?region=nac"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/AQ4020-01FTG/7902197"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "F10394CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "FAN0_TACH")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "AQ4020-01FTG.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 51.6 43 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L12"
			(at 0 1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "HOTEND_THERMISTOR")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "/HOTEND_TH_VREF")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AQ4020-01FTG:SOD2613X114N"
		(layer "F.Cu")
		(at 48.8 35.8 180)
		(descr "SOD323")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D8"
			(at 0 -1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "AQ4020-01FTG"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AQ4020-01FTG:SOD2613X114N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/2/AQ4020-01FTG.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30A 2.5pF AEC-Q101 Unidirection 3.3V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.14"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AQ4020-01FTG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "576-AQ4020-01FTG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Littelfuse/AQ4020-01FTG?qs=YCa%2FAAYMW015W3B84qpvIw%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AQ4020-01FTG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aq4020-01ftg/littelfuse?region=nac"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/AQ4020-01FTG/7902197"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "F10394CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "FAN1_TACH")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "AQ4020-01FTG.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 27.4 15.6 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 3.3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 54 "+5V5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 48.8 40.6 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 2.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R1kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "FAN1_TACH")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 19.4 19.2 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 1.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R1kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D2-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 23.4 12)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TH1"
			(at 2.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Thermistor_NTC"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Shenzhen%20Sunlord/SDNT_Series.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NTC Termistor, \"3900K Generic\", R25℃=100KΩ±1%, B25℃/50℃=3950±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/shenzhen-sunlord-electronics-co-ltd/SDNT1608X104F3950FTF/14119906"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "3442-SDNT1608X104F3950FTFCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Shenzhen Sunlord Electronics Co., Ltd."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SDNT1608X104F3950FTF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*NTC* *Thermistor* PIN?ARRAY* bornier* *Terminal?Block* R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "AMBIENT_THERMISTOR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 27.1 54.4 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D3"
			(at 4.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SMAJ24A"
			(at 0 2.6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 24.0Vr, SMA(DO-214AC)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/SMAJ6-0A/762252"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SMAJ6A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "LITTELFUSE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "SMAJ6.0ALFCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 32 "Earth_Protective")
			(pinfunction "A1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 27.42 30.01 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 3.35 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 54 "+5V5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AQ4020-01FTG:SOD2613X114N"
		(layer "F.Cu")
		(at 45 13.6 180)
		(descr "SOD323")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D9"
			(at 0 -1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "AQ4020-01FTG-C"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AQ4020-01FTG:SOD2613X114N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/2/AQ4020-01FTG.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30A 2.5pF AEC-Q101 Bidirectional 3.3V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.14"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AQ4020-01FTG-C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/AQ4020-01FTG-C/7902198?s=N4IgTCBcDaIIIEUAsAGMKC0KCMAxAKgOIYDCIAugL5A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "F10395CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "USB_D+")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.15 0 270)
			(size 0.5 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "AQ4020-01FTG.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 34.9 56.3 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "25pF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "C0G / 25V / 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/OSC_OUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 19.42 30.01 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 3.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 33 "+5VA")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 48.9 44.7 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "HOTEND_THERMISTOR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 19 55.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 1.82 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 39.6 15.6 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at -2.681605 -0.004635 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "/+24V_INPUT")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "+24V")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 15.5 46.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 1.55 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/AIN1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 51.6 50.6 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L13"
			(at 0 1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "/HOTEND_TH_GND")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 11.4 11.2)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "R4.7kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50mW / 0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "FILAMENT_SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical"
		(layer "F.Cu")
		(at 4.8 14 90)
		(descr "Molex CLIK-Mate series connector, 505405-0370 (http://www.molex.com/pdm_docs/sd/5054050270_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex CLIK-Mate side entry")
		(property "Reference" "J12"
			(at 0 -0.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 0 5.15 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "Filament Runout"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132250370/14122180"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132250370"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132250370-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/FILAMENT_SW_V+")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "FILAMENT_SW")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 1.5 2.75 90)
			(size 0.8 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/FILAMENT_SW_GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at -4.1 -2.3 90)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd roundrect
			(at 4.1 -2.3 90)
			(size 1.8 3.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_505405-0370_1x03-1MP_P1.50mm_Vertical.stp"
			(offset
				(xyz 0 -2 9.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 45.1 52.6 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 30.6 15.6 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -3.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 36V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 54 "+5V5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 45.1 56.2 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 25V / 10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 19.4 22.8 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "X7R / 10V / 10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 36 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Molex CLIK-Mate:Molex_CLIK-Mate_213226-0610_1x06-1MP_P1.50mm_Horizontal"
		(layer "F.Cu")
		(at 42.4 4 180)
		(tags "2132260610 ")
		(property "Reference" "J2"
			(at -2 0.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x08"
			(at 0 -4.219501 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Molex CLIK-Mate:Molex_CLIK-Mate_213226-0610_1x06-1MP_P1.50mm_Horizontal"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Name" "MCU Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/molex/2132271210/13922739"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "2132271210"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "900-2132271210CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.219501 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.75 -4.219501 180)
			(size 0.8128 2.8956)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "USB_D+")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -2.250001 -4.219501 180)
			(size 0.8128 2.8956)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "USB_D-")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -0.750001 -4.219501 180)
			(size 0.8128 2.8956)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "/+FANV_INPUT")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 0.750001 -4.219501 180)
			(size 0.8128 2.8956)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at 2.250001 -4.219501 180)
			(size 0.8128 2.8956)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at 3.75 -4.219501 180)
			(size 0.8128 2.8956)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/+24V_INPUT")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd rect
			(at -6.35 0.480499 180)
			(size 1.8034 3.81)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP" smd rect
			(at 6.35 0.480499 180)
			(size 1.8034 3.81)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Earth_Protective")
			(pinfunction "MountPin")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KIPRJMOD}/libs/Molex CLIK-Mate/Molex CLIK-Mate.pretty/Molex_CLIK-Mate_213226-0610_1x06-1MP_P1.50mm_Horizontal.step"
			(offset
				(xyz 0 0 3.78)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 180)
			)
		)
	)
	(footprint "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
		(layer "F.Cu")
		(at 48.8 32.2)
		(descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 3.3x3.3x1 mm Body [VSON] http://www.ti.com/lit/ds/symlink/csd87334q3d.pdf")
		(tags "VSON 0.65")
		(property "Reference" "Q2"
			(at 3.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "CSD17581Q3A"
			(at 0 2.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd17581q3a.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "60A Id, 30V Vds, NexFET N-Channel Power MOSFET, 3.2mOhm Ron, Qg Typ 20nC, VSON-8 3.3x3.3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" "https://www.digikey.com/en/products/detail/texas-instruments/CSD17581Q3A/6235429"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" "296-47754-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "CSD17581Q3A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.9mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "October 2016"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VSON*3.3x3.3mm*P0.65mm*NexFET*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.526 0.242 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -0.09 -0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd rect
			(at -0.09 0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd rect
			(at 0.86 -0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd rect
			(at 0.86 0.61)
			(size 0.57 0.738)
			(layers "F.Paste")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 -0.9725)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 -0.33)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 0.33)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 1.44 0.9725)
			(size 0.63 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.44 -0.97)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.44 -0.33)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.44 0.33)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.44 0.97)
			(size 0.63 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(Q2-G)")
			(pinfunction "G")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd custom
			(at 0.385 0)
			(size 1.9 2.45)
			(layers "F.Cu" "F.Mask")
			(net 42 "/FAN1_MOSFET_GND")
			(pinfunction "D")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1.371 -0.72) (xy 0.95 -0.72) (xy 0.95 -0.58) (xy 1.37 -0.58) (xy 1.37 -0.08) (xy 0.95 -0.08)
						(xy 0.95 0.08) (xy 1.37 0.08) (xy 1.37 0.58) (xy 0.95 0.58) (xy 0.95 0.72) (xy 1.37 0.72) (xy 1.37 1.225)
						(xy -0.95 1.225) (xy -0.95 -1.225) (xy 1.371 -1.225)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 40.4 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L3"
			(at 0 1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100MHz/3A"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "High Temp Load Cell Toolhead Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/LOAD_CELL_REF-")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 4 0)
		(end 56 0)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 4 60)
		(mid 1.171573 58.828427)
		(end 0 56)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 56 0)
		(mid 58.828427 1.171573)
		(end 60 4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 56 60)
		(end 4 60)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 60 56)
		(mid 58.828427 58.828427)
		(end 56 60)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 0 4)
		(mid 1.171573 1.171573)
		(end 4 0)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 56)
		(end 0 4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 60 4)
		(end 60 56)
		(layer "Edge.Cuts")
	)
	(gr_text "High Temp Toolhead"
		(at 23.387787 47.001745 0)
		(layer "B.SilkS")
	)
	(gr_text "FILAMENT"
		(at 3.60815 10.273572 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "HOT END"
		(at 56.465685 46.725 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "V0.1"
		(at 23.387787 49.001745 0)
		(layer "B.SilkS")
	)
	(gr_text "HE FAN"
		(at 56.376537 24.134776 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "LOAD CELL"
		(at 3.60815 41.395001 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "DOTSTAR"
		(at 3.60815 25.516429 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "HEATBREAK\n"
		(at 56.4 13.275 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "garethky"
		(at 23.387787 51.001745 0)
		(layer "B.SilkS")
	)
	(gr_text "PART FAN"
		(at 56.376537 39.440224 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "USB"
		(at 18.2 6.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5V"
		(at 14.7 14.6 270)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3.3V\n"
		(at 14.7 21.8 270)
		(layer "F.SilkS" knockout)
	)
	(gr_text "PART\n"
		(at 28.4 6.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "RGB"
		(at 10.35 6.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 22.3 35.1 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "CLK"
		(at 19.9 41.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "B0"
		(at 17.3 41.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3.3V"
		(at 18.6 35.1 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "RESET"
		(at 30.7 7.4 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "IO"
		(at 22.5 41.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5VA"
		(at 14.7 29 270)
		(layer "F.SilkS" knockout)
	)
	(gr_text "HE"
		(at 22.4 6.6 0)
		(layer "F.SilkS" knockout)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 0 0) (xy 60 0)
		)
		(height -8.585)
		(orientation 0)
		(gr_text "60.0000 mm"
			(at 30 -9.735 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 55 0) (xy 55 60)
		)
		(height 10.855)
		(orientation 1)
		(gr_text "60.0000 mm"
			(at 64.705 30 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 24)
		(net_name "SWD_IO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30207)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.6643 39.696448) (xy 31.659799 39.569984) (xy 31.645464 39.480923) (xy 31.620046 39.405881)
				(xy 31.582298 39.321477) (xy 31.53097 39.204329) (xy 31.3 39.299) (xy 31.123223 39.476777) (xy 31.207577 39.533145)
				(xy 31.291553 39.557437) (xy 31.3646 39.575512) (xy 31.416166 39.613229) (xy 31.4357 39.696448)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30137)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 43.4175 52.85) (xy 43.566599 52.8552) (xy 43.672049 52.8676) (xy 43.762949 52.8824) (xy 43.8684 52.8948)
				(xy 44.0175 52.9) (xy 44.0185 52.6) (xy 44.0175 52.3) (xy 43.8684 52.3052) (xy 43.762949 52.3176)
				(xy 43.672049 52.3324) (xy 43.566599 52.3448) (xy 43.4175 52.35)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30146)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.8393 3.775) (xy 31.881439 3.68676) (xy 31.923579 3.610141) (xy 31.96572 3.545141) (xy 32.00786 3.49176)
				(xy 32.05 3.45) (xy 31.725 2.924) (xy 31.4 3.45) (xy 31.442139 3.49176) (xy 31.484279 3.545141)
				(xy 31.52642 3.610141) (xy 31.56856 3.68676) (xy 31.6107 3.775)
			)
		)
	)
	(zone
		(net 18)
		(net_name "BOOT0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.675 38.8893) (xy 15.844999 39.013868) (xy 16.014999 39.178304) (xy 16.185 39.382606) (xy 16.355 39.626776)
				(xy 16.525 39.910814) (xy 17.376 39.275) (xy 16.525 38.425) (xy 16.355 38.525064) (xy 16.185 38.598666)
				(xy 16.014999 38.645806) (xy 15.844999 38.666484) (xy 15.675 38.6607)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30132)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.8857 11.575) (xy 49.82856 11.696381) (xy 49.77142 11.801833) (xy 49.714279 11.891354) (xy 49.657139 11.964945)
				(xy 49.6 12.022606) (xy 50 12.376) (xy 50.4 12.022606) (xy 50.34286 11.964945) (xy 50.28572 11.891354)
				(xy 50.228579 11.801833) (xy 50.171439 11.696381) (xy 50.1143 11.575)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/FILAMENT_SW_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.919918 11.586135) (xy 8.055519 11.466408) (xy 8.19112 11.357931) (xy 8.32672 11.260704) (xy 8.462321 11.174727)
				(xy 8.597923 11.1) (xy 8.400707 10.661793) (xy 7.8 10.682303) (xy 7.753273 10.814858) (xy 7.706546 10.936164)
				(xy 7.659818 11.04622) (xy 7.613091 11.145026) (xy 7.566365 11.232582)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30206)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 43.7 27.65) (xy 43.597063 27.649153) (xy 43.523466 27.644222) (xy 43.460904 27.631616) (xy 43.391073 27.607748)
				(xy 43.295671 27.56903) (xy 43.199 27.8) (xy 43.295671 28.03097) (xy 43.391073 27.99225) (xy 43.460904 27.968382)
				(xy 43.523466 27.955777) (xy 43.597063 27.950846) (xy 43.7 27.95)
			)
		)
	)
	(zone
		(net 51)
		(net_name "AMBIENT_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30195)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.0857 10.1) (xy 20.078163 10.226029) (xy 20.056575 10.313247) (xy 20.022469 10.385971) (xy 19.977378 10.468515)
				(xy 19.922836 10.585195) (xy 20.2 10.701) (xy 20.477164 10.585195) (xy 20.422621 10.468515) (xy 20.37753 10.385971)
				(xy 20.343424 10.313247) (xy 20.321836 10.226029) (xy 20.3143 10.1)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30184)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 47.9 28.65) (xy 47.775479 28.645988) (xy 47.687599 28.632878) (xy 47.61346 28.609058) (xy 47.530162 28.572914)
				(xy 47.414805 28.522836) (xy 47.299 28.8) (xy 47.414805 29.077164) (xy 47.530162 29.027084) (xy 47.61346 28.990941)
				(xy 47.687599 28.967121) (xy 47.775479 28.954011) (xy 47.9 28.95)
			)
		)
	)
	(zone
		(net 103)
		(net_name "DOTSTAR_LED_DATA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30261)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.7064 43.6357) (xy 28.622499 43.634248) (xy 28.562781 43.628408) (xy 28.51215 43.61595) (xy 28.455508 43.594646)
				(xy 28.377761 43.562268) (xy 28.299 43.75) (xy 28.377761 43.937732) (xy 28.455508 43.905352) (xy 28.51215 43.884048)
				(xy 28.562781 43.871591) (xy 28.622499 43.865751) (xy 28.7064 43.8643)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/FILAMENT_SW_V+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30123)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.719255 16.093202) (xy 7.764556 16.036698) (xy 7.809858 15.989127) (xy 7.855161 15.950486)
				(xy 7.900463 15.920777) (xy 7.945765 15.9) (xy 7.549293 15.499293) (xy 7.145735 15.9) (xy 7.189728 15.991351)
				(xy 7.233721 16.091702) (xy 7.277715 16.201052) (xy 7.321708 16.319403) (xy 7.365702 16.446755)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30228)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.183677 41.335695) (xy 37.261453 41.269419) (xy 37.325364 41.232935) (xy 37.384652 41.206381)
				(xy 37.448562 41.169898) (xy 37.52634 41.103623) (xy 37.383363 40.959232) (xy 37.238972 40.816255)
				(xy 37.172696 40.894031) (xy 37.136212 40.957942) (xy 37.109658 41.01723) (xy 37.073175 41.08114)
				(xy 37.0069 41.158918)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30187)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.825 8.304973) (xy 29.823393 8.427409) (xy 29.816093 8.514742) (xy 29.79938 8.588879) (xy 29.769534 8.671727)
				(xy 29.722836 8.785195) (xy 30 8.901) (xy 30.277164 8.785195) (xy 30.224325 8.670073) (xy 30.181962 8.588169)
				(xy 30.150801 8.515802) (xy 30.131571 8.429296) (xy 30.125 8.304973)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.5107 27.925) (xy 49.456604 28.063976) (xy 49.402509 28.185811) (xy 49.348414 28.290503) (xy 49.294319 28.378054)
				(xy 49.240224 28.448463) (xy 49.625 28.801) (xy 50.009776 28.448463) (xy 49.95568 28.378054) (xy 49.901585 28.290503)
				(xy 49.84749 28.185811) (xy 49.793395 28.063976) (xy 49.7393 27.925)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30210)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.4 48.1143) (xy 37.504186 48.118703) (xy 37.577235 48.132177) (xy 37.638624 48.155116) (xy 37.70783 48.187915)
				(xy 37.804329 48.23097) (xy 37.901 48) (xy 37.804329 47.76903) (xy 37.70783 47.812083) (xy 37.638624 47.844882)
				(xy 37.577235 47.867822) (xy 37.504186 47.881296) (xy 37.4 47.8857)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/FAN1_MOSFET_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30159)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 26.099092 3.003) (xy 26.248912 3.013817) (xy 26.353674 3.039611) (xy 26.443417 3.070398) (xy 26.54818 3.096192)
				(xy 26.698 3.10701) (xy 26.699 2.80701) (xy 26.698 2.50701) (xy 26.547895 2.518968) (xy 26.443275 2.547486)
				(xy 26.353816 2.581523) (xy 26.249196 2.610041) (xy 26.099092 2.622)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.025 53.725) (xy 8.01 53.914) (xy 7.995 54.091) (xy 7.98 54.256) (xy 7.965 54.409) (xy 7.95 54.55)
				(xy 8.525 55.201) (xy 9.032706 54.382097) (xy 8.981164 54.274677) (xy 8.929623 54.155258) (xy 8.878082 54.023838)
				(xy 8.826541 53.880419) (xy 8.775 53.725)
			)
		)
	)
	(zone
		(net 8)
		(net_name "USB_PULL_UP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30158)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.475 2.9655) (xy 19.625227 2.976888) (xy 19.730113 3.004044) (xy 19.819886 3.036456) (xy 19.924772 3.063612)
				(xy 20.075 3.075) (xy 20.076 2.775) (xy 20.075 2.475) (xy 19.924772 2.486388) (xy 19.819886 2.513544)
				(xy 19.730113 2.545956) (xy 19.625227 2.573112) (xy 19.475 2.5845)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/AIN1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30238)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.75 50.6893) (xy 17.795802 50.692823) (xy 17.841605 50.699989) (xy 17.887409 50.710797) (xy 17.933212 50.725247)
				(xy 17.979015 50.743339) (xy 18.3385 50.575) (xy 17.979015 50.406661) (xy 17.933212 50.424752) (xy 17.887409 50.439202)
				(xy 17.841605 50.45001) (xy 17.795802 50.457176) (xy 17.75 50.4607)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30188)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.895027 13.875) (xy 49.770703 13.868428) (xy 49.684196 13.849198) (xy 49.61183 13.818037)
				(xy 49.529925 13.775674) (xy 49.414805 13.722836) (xy 49.299 14) (xy 49.414805 14.277164) (xy 49.528271 14.230464)
				(xy 49.61112 14.200618) (xy 49.685257 14.183906) (xy 49.77259 14.176606) (xy 49.895027 14.175)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/FILAMENT_SW_V+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.686365 16.767418) (xy 7.709091 16.841876) (xy 7.731818 16.927585) (xy 7.754546 17.024544)
				(xy 7.777273 17.132753) (xy 7.8 17.252212) (xy 8.400707 17.338207) (xy 8.624466 16.9) (xy 8.507556 16.825273)
				(xy 8.390646 16.739296) (xy 8.273737 16.642069) (xy 8.156827 16.533592) (xy 8.039918 16.413865)
			)
		)
	)
	(zone
		(net 103)
		(net_name "DOTSTAR_LED_DATA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30215)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 12.7 29.9643) (xy 12.804186 29.968703) (xy 12.877235 29.982177) (xy 12.938624 30.005116) (xy 13.00783 30.037915)
				(xy 13.104329 30.08097) (xy 13.201 29.85) (xy 13.104329 29.61903) (xy 13.00783 29.662083) (xy 12.938624 29.694882)
				(xy 12.877235 29.717822) (xy 12.804186 29.731296) (xy 12.7 29.7357)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/OSC_OUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.9357 51.8) (xy 33.84856 51.952099) (xy 33.76142 52.083149) (xy 33.674279 52.193149) (xy 33.587139 52.282099)
				(xy 33.5 52.35) (xy 34.05 53.301) (xy 34.6 52.35) (xy 34.51286 52.282099) (xy 34.42572 52.193149)
				(xy 34.338579 52.083149) (xy 34.251439 51.952099) (xy 34.1643 51.8)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 46.23001 10.073701) (xy 46.295288 9.961146) (xy 46.360566 9.864229) (xy 46.425843 9.782949)
				(xy 46.491121 9.717306) (xy 46.5564 9.667301) (xy 46.15 8.218501) (xy 45.7436 9.667301) (xy 45.808878 9.717306)
				(xy 45.874156 9.782949) (xy 45.939433 9.864229) (xy 46.004711 9.961146) (xy 46.06999 10.073701)
			)
		)
	)
	(zone
		(net 18)
		(net_name "BOOT0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.906863 40.645218) (xy 18.77049 40.389042) (xy 18.634117 40.088724) (xy 18.497745 39.744264)
				(xy 18.361372 39.355662) (xy 18.225 38.922918) (xy 17.374293 39.274293) (xy 17.022919 40.125) (xy 17.367378 40.173088)
				(xy 17.711838 40.265319) (xy 18.056298 40.401691) (xy 18.400758 40.582206) (xy 18.745218 40.806863)
			)
		)
	)
	(zone
		(net 5)
		(net_name "SPI_2_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30249)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.766713 38.720135) (xy 37.694013 38.78373) (xy 37.634309 38.817804) (xy 37.575536 38.836948)
				(xy 37.505628 38.85575) (xy 37.412519 38.888801) (xy 37.499293 39.100707) (xy 37.711199 39.187481)
				(xy 37.744249 39.094371) (xy 37.763051 39.024462) (xy 37.782194 38.965689) (xy 37.816268 38.905986)
				(xy 37.879865 38.833287)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.435 54.745) (xy 17.35522 54.860574) (xy 17.275441 54.959649) (xy 17.195662 55.042223) (xy 17.115883 55.108298)
				(xy 17.036104 55.157873) (xy 16.7 54.726) (xy 17.036104 54.292127) (xy 17.185883 54.349701) (xy 17.335662 54.423776)
				(xy 17.485441 54.51435) (xy 17.63522 54.621425) (xy 17.785 54.745)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.945 29.025) (xy 26.11 28.996999) (xy 26.275 28.991499) (xy 26.44 29.0085) (xy 26.605 29.048)
				(xy 26.77 29.11) (xy 27.421 28.535) (xy 26.537381 28.122617) (xy 26.418904 28.268093) (xy 26.300428 28.39107)
				(xy 26.181952 28.491546) (xy 26.063476 28.569523) (xy 25.945 28.625)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30196)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.1143 12.3) (xy 50.121836 12.17397) (xy 50.143424 12.086751) (xy 50.17753 12.014027) (xy 50.222621 11.931484)
				(xy 50.277164 11.814805) (xy 50 11.699) (xy 49.722836 11.814805) (xy 49.777378 11.931484) (xy 49.822469 12.014027)
				(xy 49.856575 12.086751) (xy 49.878163 12.17397) (xy 49.8857 12.3)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.215 36.985) (xy 18.575798 37.013572) (xy 18.82129 37.092128) (xy 19.023854 37.209928) (xy 19.255871 37.356231)
				(xy 19.589719 37.520298) (xy 19.916 36.735) (xy 19.589719 35.949702) (xy 19.255871 36.113768) (xy 19.023854 36.260071)
				(xy 18.82129 36.377871) (xy 18.575798 36.456427) (xy 18.215 36.485)
			)
		)
	)
	(zone
		(net 74)
		(net_name "Net-(U2-PB13)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 36.2893 39.275) (xy 36.343395 39.136023) (xy 36.39749 39.014188) (xy 36.451585 38.909496) (xy 36.50568 38.821945)
				(xy 36.559776 38.751537) (xy 36.175 38.399) (xy 35.790224 38.751537) (xy 35.844319 38.821945) (xy 35.898414 38.909496)
				(xy 35.952509 39.014188) (xy 36.006604 39.136023) (xy 36.0607 39.275)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.4607 37.675) (xy 49.396985 37.832951) (xy 49.33327 37.970816) (xy 49.269556 38.088595) (xy 49.205841 38.186288)
				(xy 49.142127 38.263896) (xy 49.575 38.601) (xy 50.007873 38.263896) (xy 49.944158 38.186288) (xy 49.880443 38.088595)
				(xy 49.816729 37.970816) (xy 49.753014 37.832951) (xy 49.6893 37.675)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30180)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.55 19.4) (xy 8.554011 19.275479) (xy 8.567121 19.187599) (xy 8.590941 19.11346) (xy 8.627084 19.030162)
				(xy 8.677164 18.914805) (xy 8.4 18.799) (xy 8.122836 18.914805) (xy 8.172914 19.030162) (xy 8.209058 19.11346)
				(xy 8.232878 19.187599) (xy 8.245988 19.275479) (xy 8.25 19.4)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30240)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.66999 32.96) (xy 33.655992 32.998398) (xy 33.641994 33.032597) (xy 33.627996 33.062597) (xy 33.613998 33.088398)
				(xy 33.6 33.11) (xy 33.75 33.686) (xy 33.9 33.11) (xy 33.886002 33.088398) (xy 33.872004 33.062597)
				(xy 33.858006 33.032597) (xy 33.844008 32.998398) (xy 33.83001 32.96)
			)
		)
	)
	(zone
		(net 64)
		(net_name "Net-(P1-CC1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.4 29.266444) (xy 33.325 29.131346) (xy 33.25 28.981248) (xy 33.175 28.81615) (xy 33.1 28.636052)
				(xy 33.025 28.440955) (xy 32.625 28.599) (xy 32.522736 29.075) (xy 32.638188 29.083288) (xy 32.753641 29.106577)
				(xy 32.869094 29.144866) (xy 32.984547 29.198155) (xy 33.1 29.266444)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/AIN1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.1607 47.775) (xy 16.096985 47.932951) (xy 16.03327 48.070816) (xy 15.969556 48.188595) (xy 15.905841 48.286288)
				(xy 15.842127 48.363896) (xy 16.275 48.701) (xy 16.707873 48.363896) (xy 16.644158 48.286288) (xy 16.580443 48.188595)
				(xy 16.516729 48.070816) (xy 16.453014 47.932951) (xy 16.3893 47.775)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30205)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.7393 24.468934) (xy 49.807514 24.408863) (xy 49.875729 24.356934) (xy 49.943944 24.313147)
				(xy 50.012159 24.277502) (xy 50.080374 24.25) (xy 49.95 23.999) (xy 49.47245 24.25) (xy 49.4801 24.280451)
				(xy 49.48775 24.317571) (xy 49.4954 24.361358) (xy 49.50305 24.411812) (xy 49.5107 24.468934)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30173)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.435 54.16) (xy 17.433482 54.283671) (xy 17.426361 54.371923) (xy 17.409782 54.446858) (xy 17.379892 54.530581)
				(xy 17.332836 54.645195) (xy 17.61 54.761) (xy 17.887164 54.645195) (xy 17.840107 54.530581) (xy 17.810216 54.446858)
				(xy 17.793638 54.371923) (xy 17.786517 54.283671) (xy 17.785 54.16)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.6 54.825) (xy 9.499999 54.808999) (xy 9.399999 54.780999) (xy 9.3 54.741) (xy 9.2 54.689)
				(xy 9.1 54.625) (xy 8.524 55.2) (xy 9.1 55.775) (xy 9.2 55.710999) (xy 9.3 55.658999) (xy 9.399999 55.619)
				(xy 9.499999 55.591) (xy 9.6 55.575)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(D6-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.325 4.6155) (xy 18.429692 4.629215) (xy 18.534385 4.6555) (xy 18.639077 4.694355) (xy 18.74377 4.74578)
				(xy 18.848463 4.809776) (xy 19.201 4.425) (xy 18.848463 4.040224) (xy 18.74377 4.104219) (xy 18.639077 4.155644)
				(xy 18.534385 4.194499) (xy 18.429692 4.220784) (xy 18.325 4.2345)
			)
		)
	)
	(zone
		(net 67)
		(net_name "/HOTEND_TH_VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.686335 45.44798) (xy 51.645931 45.505525) (xy 51.605527 45.5545) (xy 51.565123 45.594905)
				(xy 51.524719 45.626738) (xy 51.484315 45.650001) (xy 52.450707 46.050707) (xy 52.615686 45.65)
				(xy 52.462144 45.61155) (xy 52.308603 45.555959) (xy 52.155062 45.483227) (xy 52.001521 45.393352)
				(xy 51.84798 45.286335)
			)
		)
	)
	(zone
		(net 81)
		(net_name "/HOTEND_TH_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.84798 48.313665) (xy 52.001521 48.206647) (xy 52.155062 48.116772) (xy 52.308602 48.04404)
				(xy 52.462143 47.988449) (xy 52.615685 47.95) (xy 52.450707 47.549293) (xy 51.484315 47.95) (xy 51.524719 47.973262)
				(xy 51.565123 48.005095) (xy 51.605527 48.045499) (xy 51.645931 48.094474) (xy 51.686335 48.15202)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30223)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.45 16.225) (xy 25.3975 16.223) (xy 25.345 16.2195) (xy 25.2925 16.214499) (xy 25.24 16.207999)
				(xy 25.1875 16.2) (xy 24.849 16.375) (xy 25.1875 16.55) (xy 25.24 16.542) (xy 25.2925 16.5355) (xy 25.345 16.530499)
				(xy 25.3975 16.526999) (xy 25.45 16.525)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30201)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.75835 14.448224) (xy 10.763717 14.396577) (xy 10.769084 14.350931) (xy 10.774451 14.311286)
				(xy 10.779818 14.277642) (xy 10.785185 14.25) (xy 10.25 13.999) (xy 10.13387 14.25) (xy 10.205426 14.275647)
				(xy 10.276982 14.308293) (xy 10.348537 14.347937) (xy 10.420094 14.394581) (xy 10.49165 14.448224)
			)
		)
	)
	(zone
		(net 5)
		(net_name "SPI_2_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30250)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 41.466713 57.020135) (xy 41.394013 57.08373) (xy 41.334309 57.117804) (xy 41.275536 57.136948)
				(xy 41.205628 57.15575) (xy 41.112519 57.188801) (xy 41.199293 57.400707) (xy 41.411199 57.487481)
				(xy 41.444249 57.394371) (xy 41.463051 57.324462) (xy 41.482194 57.265689) (xy 41.516268 57.205986)
				(xy 41.579865 57.133287)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.730011 10.073701) (xy 44.795289 9.961146) (xy 44.860567 9.864229) (xy 44.925844 9.782949)
				(xy 44.991122 9.717306) (xy 45.056401 9.667301) (xy 44.650001 8.218501) (xy 44.243601 9.667301)
				(xy 44.308879 9.717306) (xy 44.374157 9.782949) (xy 44.439434 9.864229) (xy 44.504712 9.961146)
				(xy 44.569991 10.073701)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30164)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.2 9.66665) (xy 19.145478 9.636199) (xy 19.090957 9.594309) (xy 19.036435 9.540979) (xy 18.981914 9.476209)
				(xy 18.927393 9.4) (xy 18.574 9.8) (xy 18.927393 10.2) (xy 18.981914 10.12379) (xy 19.036435 10.05902)
				(xy 19.090957 10.00569) (xy 19.145478 9.9638) (xy 19.2 9.93335)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 24.2 2.6095) (xy 24.110307 2.590784) (xy 24.020614 2.559499) (xy 23.930922 2.515644) (xy 23.841229 2.459219)
				(xy 23.751537 2.390224) (xy 23.399 2.775) (xy 23.751537 3.159776) (xy 23.841229 3.10078) (xy 23.930922 3.054355)
				(xy 24.020614 3.0205) (xy 24.110307 2.999215) (xy 24.2 2.9905)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/OSC_IN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.4357 51.8) (xy 31.34856 51.952099) (xy 31.26142 52.083149) (xy 31.174279 52.193149) (xy 31.087139 52.282099)
				(xy 31 52.35) (xy 31.55 53.301) (xy 32.1 52.35) (xy 32.01286 52.282099) (xy 31.92572 52.193149)
				(xy 31.838579 52.083149) (xy 31.751439 51.952099) (xy 31.6643 51.8)
			)
		)
	)
	(zone
		(net 97)
		(net_name "Net-(D17-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.963372 27.474984) (xy 16.886714 27.629275) (xy 16.810056 27.764174) (xy 16.733397 27.879681)
				(xy 16.656739 27.975796) (xy 16.580082 28.05252) (xy 16.999293 28.413207) (xy 17.41093 28.03907)
				(xy 17.353747 27.988201) (xy 17.296564 27.922523) (xy 17.239381 27.842034) (xy 17.182198 27.746736)
				(xy 17.125016 27.636628)
			)
		)
	)
	(zone
		(net 51)
		(net_name "AMBIENT_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.3143 10.675) (xy 20.373395 10.536023) (xy 20.43249 10.414188) (xy 20.491585 10.309496) (xy 20.55068 10.221945)
				(xy 20.609776 10.151537) (xy 20.225 9.799) (xy 19.840224 10.151537) (xy 19.889319 10.221945) (xy 19.938414 10.309496)
				(xy 19.987509 10.414188) (xy 20.036604 10.536023) (xy 20.0857 10.675)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(D6-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.1125 4.2345) (xy 17.997992 4.21057) (xy 17.883484 4.17182) (xy 17.768977 4.11825) (xy 17.654469 4.04986)
				(xy 17.539962 3.966651) (xy 17.199 4.3875) (xy 17.539962 4.808349) (xy 17.654469 4.740139) (xy 17.768977 4.686749)
				(xy 17.883484 4.648179) (xy 17.997992 4.624429) (xy 18.1125 4.6155)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30253)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.5936 46.3643) (xy 37.677499 46.365751) (xy 37.737217 46.371591) (xy 37.787849 46.384048)
				(xy 37.844491 46.405352) (xy 37.922239 46.437732) (xy 38.001 46.25) (xy 37.922239 46.062268) (xy 37.844491 46.094646)
				(xy 37.787849 46.11595) (xy 37.737217 46.128408) (xy 37.677499 46.134248) (xy 37.5936 46.1357)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/AIN0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.160082 51.1107) (xy 17.070323 51.045059) (xy 16.980565 50.959276) (xy 16.890806 50.853351)
				(xy 16.801048 50.727284) (xy 16.71129 50.581076) (xy 16.274 50.9) (xy 16.5 51.375) (xy 16.632016 51.328197)
				(xy 16.764032 51.301226) (xy 16.896049 51.294086) (xy 17.028065 51.306777) (xy 17.160082 51.3393)
			)
		)
	)
	(zone
		(net 78)
		(net_name "Net-(Q2-G)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30190)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 46.795 33.3605) (xy 46.87 33.365259) (xy 46.945 33.373589) (xy 47.02 33.38549) (xy 47.095 33.40096)
				(xy 47.17 33.42) (xy 47.361 33.17) (xy 47.17 32.92) (xy 47.095 32.939039) (xy 47.02 32.954509) (xy 46.945 32.96641)
				(xy 46.87 32.97474) (xy 46.795 32.9795)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30136)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.734704 19.134703) (xy 38.784478 19.152557) (xy 38.834253 19.179656) (xy 38.884029 19.216)
				(xy 38.933804 19.261588) (xy 38.983579 19.316421) (xy 39.400707 18.974293) (xy 39.048463 18.590224)
				(xy 38.931829 18.670378) (xy 38.815196 18.737962) (xy 38.698563 18.792977) (xy 38.58193 18.835421)
				(xy 38.465297 18.865296)
			)
		)
	)
	(zone
		(net 62)
		(net_name "Net-(D14-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 26.5125 4.197) (xy 26.397992 4.18057) (xy 26.283484 4.14932) (xy 26.168977 4.10325) (xy 26.054469 4.04236)
				(xy 25.939962 3.966651) (xy 25.599 4.3875) (xy 25.939962 4.808349) (xy 26.054469 4.732639) (xy 26.168977 4.671749)
				(xy 26.283484 4.625679) (xy 26.397992 4.594429) (xy 26.5125 4.578)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.963372 20.274984) (xy 16.886714 20.429275) (xy 16.810056 20.564174) (xy 16.733397 20.679681)
				(xy 16.656739 20.775796) (xy 16.580082 20.85252) (xy 16.999293 21.213207) (xy 17.41093 20.83907)
				(xy 17.353747 20.788201) (xy 17.296564 20.722523) (xy 17.239381 20.642034) (xy 17.182198 20.546736)
				(xy 17.125016 20.436628)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 43.968414 57.098743) (xy 44.115069 57.143256) (xy 44.261725 57.192269) (xy 44.408381 57.245783)
				(xy 44.555037 57.303796) (xy 44.701693 57.36631) (xy 45.100707 56.975707) (xy 44.85 56.525) (xy 44.779748 56.542682)
				(xy 44.709497 56.555865) (xy 44.639245 56.564548) (xy 44.568994 56.568731) (xy 44.498743 56.568414)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/OSC_OUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.9 55.375) (xy 33.858425 55.528779) (xy 33.81685 55.664558) (xy 33.775276 55.782337) (xy 33.733701 55.882116)
				(xy 33.692127 55.963896) (xy 34.125 56.301) (xy 34.547969 55.949074) (xy 34.478375 55.870259) (xy 34.408781 55.773444)
				(xy 34.339187 55.658629) (xy 34.269593 55.525814) (xy 34.2 55.375)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30177)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 48.75 49.8) (xy 48.745988 49.92452) (xy 48.732878 50.0124) (xy 48.709058 50.086539) (xy 48.672914 50.169837)
				(xy 48.622836 50.285195) (xy 48.9 50.401) (xy 49.177164 50.285195) (xy 49.127084 50.169837) (xy 49.090941 50.086539)
				(xy 49.067121 50.0124) (xy 49.054011 49.92452) (xy 49.05 49.8)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30224)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.45 23.425) (xy 25.3975 23.423) (xy 25.345 23.4195) (xy 25.2925 23.414499) (xy 25.24 23.407999)
				(xy 25.1875 23.4) (xy 24.849 23.575) (xy 25.1875 23.75) (xy 25.24 23.742) (xy 25.2925 23.7355) (xy 25.345 23.730499)
				(xy 25.3975 23.726999) (xy 25.45 23.725)
			)
		)
	)
	(zone
		(net 7)
		(net_name "ADS1220_DRDY")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30197)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.8607 54.180995) (xy 19.852655 54.30702) (xy 19.829852 54.393948) (xy 19.794284 54.466284)
				(xy 19.747947 54.548531) (xy 19.692836 54.665195) (xy 19.97 54.781) (xy 20.247164 54.665195) (xy 20.193326 54.548944)
				(xy 20.149498 54.466461) (xy 20.116803 54.393684) (xy 20.096362 54.306549) (xy 20.0893 54.180995)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/LOAD_CELL_IN+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.5625 47.0508) (xy 9.677007 47.073325) (xy 9.791515 47.115243) (xy 9.906022 47.176553) (xy 10.02053 47.257255)
				(xy 10.135038 47.357349) (xy 10.601 46.9365) (xy 10.135038 46.515651) (xy 10.02053 46.615744) (xy 9.906022 46.696446)
				(xy 9.791515 46.757756) (xy 9.677007 46.799674) (xy 9.5625 46.8222)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D5-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.8857 13.1375) (xy 16.82106 13.283595) (xy 16.75642 13.410776) (xy 16.691779 13.519043) (xy 16.627139 13.608396)
				(xy 16.5625 13.678835) (xy 17 14.0135) (xy 17.4375 13.678835) (xy 17.37286 13.608396) (xy 17.30822 13.519043)
				(xy 17.243579 13.410776) (xy 17.178939 13.283595) (xy 17.1143 13.1375)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.5107 39.725) (xy 49.456604 39.863976) (xy 49.402509 39.985811) (xy 49.348414 40.090503) (xy 49.294319 40.178054)
				(xy 49.240224 40.248463) (xy 49.625 40.601) (xy 50.009776 40.248463) (xy 49.95568 40.178054) (xy 49.901585 40.090503)
				(xy 49.84749 39.985811) (xy 49.793395 39.863976) (xy 49.7393 39.725)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/LED_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30208)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.1357 31.5) (xy 10.10856 31.566283) (xy 10.08142 31.624425) (xy 10.054279 31.674426) (xy 10.027139 31.716284)
				(xy 10 31.75) (xy 10.25 32.001) (xy 10.5 31.75) (xy 10.47286 31.716284) (xy 10.44572 31.674426)
				(xy 10.418579 31.624425) (xy 10.391439 31.566283) (xy 10.3643 31.5)
			)
		)
	)
	(zone
		(net 4)
		(net_name "SPI_2_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30230)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 40.3572 55.6857) (xy 40.262315 55.682643) (xy 40.19535 55.672653) (xy 40.138856 55.654502) (xy 40.075383 55.62696)
				(xy 39.987481 55.588801) (xy 39.899 55.8) (xy 39.987481 56.011199) (xy 40.075383 55.973038) (xy 40.138856 55.945497)
				(xy 40.19535 55.927346) (xy 40.262315 55.917356) (xy 40.3572 55.9143)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30145)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.6107 6.225) (xy 31.56856 6.313239) (xy 31.52642 6.389858) (xy 31.484279 6.454858) (xy 31.442139 6.508239)
				(xy 31.4 6.55) (xy 31.725 7.076) (xy 32.05 6.55) (xy 32.00786 6.508239) (xy 31.96572 6.454858) (xy 31.923579 6.389858)
				(xy 31.881439 6.313239) (xy 31.8393 6.225)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30255)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.5936 45.3643) (xy 37.677499 45.365751) (xy 37.737217 45.371591) (xy 37.787849 45.384048)
				(xy 37.844491 45.405352) (xy 37.922239 45.437732) (xy 38.001 45.25) (xy 37.922239 45.062268) (xy 37.844491 45.094646)
				(xy 37.787849 45.11595) (xy 37.737217 45.128408) (xy 37.677499 45.134248) (xy 37.5936 45.1357)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/LED_CLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.95202 28.086335) (xy 8.871615 28.103287) (xy 8.791211 28.108129) (xy 8.710808 28.100863) (xy 8.630404 28.081486)
				(xy 8.55 28.05) (xy 7.549293 28.450707) (xy 8.75 28.628457) (xy 8.822733 28.520782) (xy 8.895466 28.428897)
				(xy 8.968198 28.352802) (xy 9.040931 28.292496) (xy 9.113665 28.24798)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.15 13.86665) (xy 9.045307 13.848362) (xy 8.940614 13.814076) (xy 8.835922 13.763791) (xy 8.731229 13.697507)
				(xy 8.626537 13.615224) (xy 7.549 14) (xy 8.626537 14.384776) (xy 8.731229 14.302492) (xy 8.835922 14.236208)
				(xy 8.940614 14.185923) (xy 9.045307 14.151637) (xy 9.15 14.13335)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30221)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 43.225 27.95) (xy 43.285 27.954) (xy 43.345 27.961) (xy 43.405 27.970999) (xy 43.465 27.983999)
				(xy 43.525 28) (xy 43.751 27.8) (xy 43.525 27.6) (xy 43.465 27.616) (xy 43.405 27.629) (xy 43.345 27.638999)
				(xy 43.285 27.645999) (xy 43.225 27.65)
			)
		)
	)
	(zone
		(net 104)
		(net_name "DOTSTAR_LED_CLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30233)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 12.025 28.6643) (xy 12.077346 28.669633) (xy 12.129692 28.680109) (xy 12.182039 28.695726) (xy 12.234385 28.716486)
				(xy 12.286732 28.742388) (xy 12.551 28.55) (xy 12.286732 28.357612) (xy 12.234385 28.383513) (xy 12.182039 28.404273)
				(xy 12.129692 28.41989) (xy 12.077346 28.430366) (xy 12.025 28.4357)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/LED_CLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30266)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.5357 28.15) (xy 10.518559 28.200284) (xy 10.501419 28.245426) (xy 10.48428 28.285425) (xy 10.46714 28.320283)
				(xy 10.45 28.35) (xy 10.65 28.551) (xy 10.85 28.35) (xy 10.832859 28.320283) (xy 10.815719 28.285425)
				(xy 10.79858 28.245426) (xy 10.78144 28.200284) (xy 10.7643 28.15)
			)
		)
	)
	(zone
		(net 104)
		(net_name "DOTSTAR_LED_CLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30260)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.4064 44.1357) (xy 29.322499 44.134248) (xy 29.262781 44.128408) (xy 29.21215 44.11595) (xy 29.155508 44.094646)
				(xy 29.077761 44.062268) (xy 28.999 44.25) (xy 29.077761 44.437732) (xy 29.155508 44.405352) (xy 29.21215 44.384048)
				(xy 29.262781 44.371591) (xy 29.322499 44.365751) (xy 29.4064 44.3643)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/LED_CLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30209)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.3643 26.9) (xy 10.391439 26.833716) (xy 10.418579 26.775574) (xy 10.44572 26.725573) (xy 10.47286 26.683715)
				(xy 10.5 26.65) (xy 10.25 26.399) (xy 10 26.65) (xy 10.027139 26.683715) (xy 10.054279 26.725573)
				(xy 10.08142 26.775574) (xy 10.10856 26.833716) (xy 10.1357 26.9)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/+5V_USB")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30176)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 35.36697 32.1) (xy 35.362958 32.22452) (xy 35.349848 32.3124) (xy 35.326028 32.386539) (xy 35.289884 32.469837)
				(xy 35.239806 32.585195) (xy 35.51697 32.701) (xy 35.794134 32.585195) (xy 35.744054 32.469837)
				(xy 35.707911 32.386539) (xy 35.684091 32.3124) (xy 35.670981 32.22452) (xy 35.66697 32.1)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/OSC_IN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.725 54.8) (xy 31.8 54.650059) (xy 31.875 54.520089) (xy 31.95 54.410089) (xy 32.025 54.320059)
				(xy 32.1 54.25) (xy 31.55 53.299) (xy 31.015763 54.25) (xy 31.09761 54.318867) (xy 31.179457 54.4083)
				(xy 31.261305 54.518301) (xy 31.343152 54.648867) (xy 31.425 54.8)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(hatch full 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 22.39 29.02) (xy 21.308609 29.02) (xy 20.789531 29.986782) (xy 18.321945 29.986782) (xy 18.325729 27.708628)
				(xy 20.548383 27.714344) (xy 22.39 28.463973)
			)
		)
	)
	(zone
		(net 69)
		(net_name "Net-(L5-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 11.6375 42.2232) (xy 11.541985 42.176843) (xy 11.446471 42.111343) (xy 11.350956 42.0267) (xy 11.255442 41.922914)
				(xy 11.159928 41.799986) (xy 10.599 42.1375) (xy 10.98125 42.575) (xy 11.1125 42.511575) (xy 11.24375 42.467543)
				(xy 11.375 42.442904) (xy 11.50625 42.437656) (xy 11.6375 42.4518)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30198)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.915288 32.049789) (xy 33.817231 32.132453) (xy 33.735135 32.172612) (xy 33.653818 32.191806)
				(xy 33.558098 32.211576) (xy 33.432795 32.253464) (xy 33.546893 32.531335) (xy 33.824764 32.645433)
				(xy 33.86665 32.520128) (xy 33.88642 32.424409) (xy 33.905615 32.343092) (xy 33.945774 32.260996)
				(xy 34.028439 32.16294)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.7393 27.725) (xy 49.793014 27.568386) (xy 49.846729 27.431189) (xy 49.900443 27.31341) (xy 49.954158 27.215048)
				(xy 50.007873 27.136104) (xy 49.575 26.799) (xy 49.142583 27.136787) (xy 49.216206 27.214145) (xy 49.289829 27.311646)
				(xy 49.363453 27.429288) (xy 49.437076 27.567073) (xy 49.5107 27.725)
			)
		)
	)
	(zone
		(net 4)
		(net_name "SPI_2_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30259)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 35.1643 39.4064) (xy 35.165751 39.322499) (xy 35.171591 39.262781) (xy 35.184048 39.21215) (xy 35.205352 39.155508)
				(xy 35.237732 39.077761) (xy 35.05 38.999) (xy 34.862268 39.077761) (xy 34.894646 39.155508) (xy 34.91595 39.21215)
				(xy 34.928408 39.262781) (xy 34.934248 39.322499) (xy 34.9357 39.4064)
			)
		)
	)
	(zone
		(net 5)
		(net_name "SPI_2_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30169)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.556576 39.156575) (xy 37.654819 39.065245) (xy 37.753063 38.990969) (xy 37.851306 38.933747)
				(xy 37.94955 38.893579) (xy 38.047794 38.870465) (xy 37.825707 38.399293) (xy 37.425 38.675) (xy 37.428685 38.726552)
				(xy 37.43237 38.78917) (xy 37.436054 38.862855) (xy 37.439739 38.947606) (xy 37.443425 39.043424)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30152)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.55 29) (xy 10.400008 28.9896) (xy 10.295004 28.9648) (xy 10.204995 28.9352) (xy 10.099991 28.9104)
				(xy 9.95 28.9) (xy 9.949 29.2) (xy 9.95 29.5) (xy 10.099991 29.4896) (xy 10.204995 29.4648) (xy 10.295004 29.4352)
				(xy 10.400008 29.4104) (xy 10.55 29.4)
			)
		)
	)
	(zone
		(net 68)
		(net_name "Net-(L4-Pad2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 13.926018 52.549163) (xy 13.995814 52.659513) (xy 14.06561 52.787005) (xy 14.135407 52.931638)
				(xy 14.205203 53.093414) (xy 14.275 53.272333) (xy 14.675707 53.100707) (xy 14.754782 52.625) (xy 14.621358 52.611787)
				(xy 14.487934 52.581433) (xy 14.35451 52.533936) (xy 14.221086 52.469298) (xy 14.087663 52.387518)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/AIN0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.1607 52.225) (xy 16.116604 52.363772) (xy 16.072509 52.485504) (xy 16.028414 52.590197) (xy 15.984319 52.677849)
				(xy 15.940224 52.748463) (xy 16.325 53.101) (xy 16.705132 52.741513) (xy 16.641965 52.672494) (xy 16.578799 52.586333)
				(xy 16.515632 52.483031) (xy 16.452466 52.362586) (xy 16.3893 52.225)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/LOAD_CELL_IN-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.981309 44.557046) (xy 8.910354 44.560669) (xy 8.8394 44.553298) (xy 8.768445 44.534933) (xy 8.697491 44.505575)
				(xy 8.626537 44.465224) (xy 7.549293 44.850707) (xy 8.74269 45.086749) (xy 8.822742 44.980511) (xy 8.902795 44.890587)
				(xy 8.982848 44.816975) (xy 9.062901 44.759677) (xy 9.142954 44.718691)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30124)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 30.713632 7.924724) (xy 30.628126 7.916097) (xy 30.54262 7.893525) (xy 30.457115 7.857005) (xy 30.371609 7.806539)
				(xy 30.286104 7.742127) (xy 29.974293 8.200707) (xy 30.388808 8.564636) (xy 30.486101 8.428698)
				(xy 30.583395 8.312902) (xy 30.680688 8.217249) (xy 30.777982 8.141737) (xy 30.875276 8.086368)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30242)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.16999 32.96) (xy 34.155992 32.998398) (xy 34.141994 33.032597) (xy 34.127996 33.062597) (xy 34.113998 33.088398)
				(xy 34.1 33.11) (xy 34.25 33.686) (xy 34.4 33.11) (xy 34.386002 33.088398) (xy 34.372004 33.062597)
				(xy 34.358006 33.032597) (xy 34.344008 32.998398) (xy 34.33001 32.96)
			)
		)
	)
	(zone
		(net 68)
		(net_name "Net-(L4-Pad2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 11.418349 49.718204) (xy 11.374679 49.621903) (xy 11.331009 49.50621) (xy 11.287339 49.371126)
				(xy 11.243669 49.216649) (xy 11.2 49.042781) (xy 10.599293 49.060793) (xy 10.418781 49.499) (xy 10.586365 49.536385)
				(xy 10.75395 49.593163) (xy 10.921534 49.669333) (xy 11.089119 49.764895) (xy 11.256704 49.879849)
			)
		)
	)
	(zone
		(net 103)
		(net_name "DOTSTAR_LED_DATA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30234)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 13.075 29.7357) (xy 13.022653 29.730366) (xy 12.970307 29.71989) (xy 12.91796 29.704273) (xy 12.865614 29.683513)
				(xy 12.813268 29.657612) (xy 12.549 29.85) (xy 12.813268 30.042388) (xy 12.865614 30.016486) (xy 12.91796 29.995726)
				(xy 12.970307 29.980109) (xy 13.022653 29.969633) (xy 13.075 29.9643)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/FAN1_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30268)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 43.8643 28.85) (xy 43.88144 28.799715) (xy 43.89858 28.754573) (xy 43.915719 28.714574) (xy 43.932859 28.679716)
				(xy 43.95 28.65) (xy 43.75 28.449) (xy 43.55 28.65) (xy 43.56714 28.679716) (xy 43.58428 28.714574)
				(xy 43.601419 28.754573) (xy 43.618559 28.799715) (xy 43.6357 28.85)
			)
		)
	)
	(zone
		(net 100)
		(net_name "RGB_LED_CLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30217)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.1643 39.5) (xy 34.168703 39.395813) (xy 34.182177 39.322763) (xy 34.205116 39.261374) (xy 34.237915 39.192169)
				(xy 34.28097 39.095671) (xy 34.05 38.999) (xy 33.81903 39.095671) (xy 33.862083 39.192169) (xy 33.894882 39.261374)
				(xy 33.917822 39.322763) (xy 33.931296 39.395813) (xy 33.9357 39.5)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.735139 14.753033) (xy 28.648111 14.653791) (xy 28.561083 14.55005) (xy 28.474055 14.44181)
				(xy 28.387027 14.329069) (xy 28.3 14.211828) (xy 27.399293 14.124293) (xy 27.161828 14.7) (xy 27.335069 14.843027)
				(xy 27.50831 14.990555) (xy 27.68155 15.142583) (xy 27.854792 15.299111) (xy 28.028033 15.460139)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.728769 48.682323) (xy 34.71144 48.769199) (xy 34.694112 48.845795) (xy 34.676783 48.91211)
				(xy 34.659455 48.968143) (xy 34.642127 49.013896) (xy 35.100707 49.325707) (xy 35.464636 48.911191)
				(xy 35.388173 48.818706) (xy 35.31171 48.714222) (xy 35.235248 48.597737) (xy 35.158785 48.469253)
				(xy 35.082323 48.328769)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.7393 39.525) (xy 49.793014 39.368386) (xy 49.846729 39.231189) (xy 49.900443 39.11341) (xy 49.954158 39.015048)
				(xy 50.007873 38.936104) (xy 49.575 38.599) (xy 49.142583 38.936787) (xy 49.216206 39.014145) (xy 49.289829 39.111646)
				(xy 49.363453 39.229288) (xy 49.437076 39.367073) (xy 49.5107 39.525)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/LOAD_CELL_REF-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.775 42.3375) (xy 8.787499 42.240262) (xy 8.799999 42.146774) (xy 8.8125 42.057036) (xy 8.825 41.971048)
				(xy 8.8375 41.888811) (xy 8.4 41.4615) (xy 7.9625 41.888811) (xy 7.974999 41.971048) (xy 7.987499 42.057036)
				(xy 8 42.146774) (xy 8.0125 42.240262) (xy 8.025 42.3375)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(hatch full 0.5)
		(priority 6)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 28.95 14.968124) (xy 29.841159 15.85) (xy 34.95 15.85) (xy 35.3 16.2) (xy 35.3 20.6) (xy 32.8 20.6)
				(xy 32.8 19.2) (xy 31.9 18.3) (xy 29.9 18.3) (xy 28.95 19.2)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30133)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 48.7857 47.275) (xy 48.72856 47.396381) (xy 48.67142 47.501833) (xy 48.614279 47.591354) (xy 48.557139 47.664945)
				(xy 48.5 47.722606) (xy 48.9 48.076) (xy 49.3 47.722606) (xy 49.24286 47.664945) (xy 49.18572 47.591354)
				(xy 49.128579 47.501833) (xy 49.071439 47.396381) (xy 49.0143 47.275)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30161)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 30.106065 8.793934) (xy 30.156671 8.738165) (xy 30.207278 8.691798) (xy 30.257885 8.654831)
				(xy 30.308492 8.627264) (xy 30.359099 8.609099) (xy 29.974293 8.199293) (xy 29.590901 8.609099)
				(xy 29.651507 8.658527) (xy 29.712114 8.722938) (xy 29.77272 8.802331) (xy 29.833327 8.896707) (xy 29.893934 9.006065)
			)
		)
	)
	(zone
		(net 5)
		(net_name "SPI_2_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30174)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 41.387122 57.326029) (xy 41.446879 57.296583) (xy 41.506636 57.276258) (xy 41.566393 57.265052)
				(xy 41.62615 57.262966) (xy 41.685908 57.27) (xy 41.800707 56.696793) (xy 41.525 56.599226) (xy 41.474794 56.745355)
				(xy 41.424588 56.879784) (xy 41.374382 57.002514) (xy 41.324176 57.113546) (xy 41.273971 57.212878)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/AIN1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30125)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.67402 49.412375) (xy 16.684215 49.291989) (xy 16.694411 49.185559) (xy 16.704608 49.093084)
				(xy 16.714804 49.014564) (xy 16.725 48.95) (xy 16.274293 48.699293) (xy 15.974391 49.15996) (xy 16.081987 49.202488)
				(xy 16.189584 49.265158) (xy 16.297181 49.34797) (xy 16.404778 49.450924) (xy 16.512375 49.57402)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30144)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.05 50.4) (xy 49.099999 50.31099) (xy 49.149999 50.234224) (xy 49.2 50.169703) (xy 49.25 50.117426)
				(xy 49.3 50.077393) (xy 48.9 49.724) (xy 48.5 50.077393) (xy 48.549999 50.117426) (xy 48.599999 50.169703)
				(xy 48.65 50.234224) (xy 48.7 50.31099) (xy 48.75 50.4)
			)
		)
	)
	(zone
		(net 69)
		(net_name "Net-(L5-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 13.939873 43.726518) (xy 14.006898 43.840067) (xy 14.073923 43.970758) (xy 14.140949 44.118592)
				(xy 14.207974 44.283567) (xy 14.275 44.465685) (xy 14.675707 44.300707) (xy 14.765685 43.825) (xy 14.632851 43.807258)
				(xy 14.500018 43.772375) (xy 14.367184 43.720349) (xy 14.234351 43.651182) (xy 14.101518 43.564873)
			)
		)
	)
	(zone
		(net 35)
		(net_name "FAN0_PWM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30232)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 41.325 27.2643) (xy 41.377346 27.269633) (xy 41.429692 27.280109) (xy 41.482039 27.295726) (xy 41.534385 27.316486)
				(xy 41.586732 27.342388) (xy 41.851 27.15) (xy 41.586732 26.957612) (xy 41.534385 26.983513) (xy 41.482039 27.004273)
				(xy 41.429692 27.01989) (xy 41.377346 27.030366) (xy 41.325 27.0357)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/FAN0_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30120)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.72298 20.038665) (xy 44.877321 19.991647) (xy 45.031662 19.961772) (xy 45.186004 19.94904)
				(xy 45.340345 19.953449) (xy 45.494687 19.975) (xy 45.400707 19.574293) (xy 44.926857 19.365662)
				(xy 44.853752 19.502217) (xy 44.780648 19.621631) (xy 44.707543 19.723902) (xy 44.634439 19.809032)
				(xy 44.561335 19.87702)
			)
		)
	)
	(zone
		(net 61)
		(net_name "Net-(D13-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.525 4.578) (xy 22.629692 4.599215) (xy 22.734385 4.633) (xy 22.839077 4.679355) (xy 22.94377 4.73828)
				(xy 23.048463 4.809776) (xy 23.401 4.425) (xy 23.048463 4.040224) (xy 22.94377 4.096719) (xy 22.839077 4.140644)
				(xy 22.734385 4.171999) (xy 22.629692 4.190784) (xy 22.525 4.197)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/FAN0_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30265)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 43.6357 26.75) (xy 43.618559 26.800284) (xy 43.601419 26.845426) (xy 43.58428 26.885425) (xy 43.56714 26.920283)
				(xy 43.55 26.95) (xy 43.75 27.151) (xy 43.95 26.95) (xy 43.932859 26.920283) (xy 43.915719 26.885425)
				(xy 43.89858 26.845426) (xy 43.88144 26.800284) (xy 43.8643 26.75)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 36.025 49.075) (xy 35.90722 49.062425) (xy 35.789441 49.03785) (xy 35.671662 49.001276) (xy 35.553883 48.952701)
				(xy 35.436104 48.892127) (xy 35.099 49.325) (xy 35.436104 49.757873) (xy 35.553883 49.697298) (xy 35.671662 49.648723)
				(xy 35.789441 49.612149) (xy 35.90722 49.587574) (xy 36.025 49.575)
			)
		)
	)
	(zone
		(net 8)
		(net_name "USB_PULL_UP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30162)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.9 36.3143) (xy 33.960521 36.34647) (xy 34.021042 36.391125) (xy 34.081564 36.448265) (xy 34.142085 36.51789)
				(xy 34.202607 36.6) (xy 34.556 36.2) (xy 34.202607 35.8) (xy 34.142085 35.882109) (xy 34.081564 35.951734)
				(xy 34.021042 36.008874) (xy 33.960521 36.053529) (xy 33.9 36.0857)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30199)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.83001 30.396355) (xy 33.848529 30.267162) (xy 33.896533 30.185825) (xy 33.962694 30.122097)
				(xy 34.03568 30.045729) (xy 34.104164 29.926476) (xy 33.827 29.810671) (xy 33.549836 29.926476)
				(xy 33.597967 30.038094) (xy 33.632219 30.118818) (xy 33.654422 30.190721) (xy 33.666402 30.275875)
				(xy 33.66999 30.396355)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "F.Cu")
		(name "Guard Ring Copper")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.25 37.1) (xy 51.405 36.945) (xy 53.655 36.945) (xy 53.81 37.1) (xy 53.81 38.57) (xy 53.58 38.8)
				(xy 51.48 38.8) (xy 51.25 38.57)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/FAN1_MOSFET_GND")
		(layer "F.Cu")
		(name "FAN0 MOSFET THERMAL PAD")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.25)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 48.2 29.9) (xy 50.580951 29.9) (xy 51.199999 29.4) (xy 54.8 29.4) (xy 54.8 34.7) (xy 48.2 34.7)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.775 52.7375) (xy 8.787499 52.640262) (xy 8.799999 52.546774) (xy 8.8125 52.457036) (xy 8.825 52.371048)
				(xy 8.8375 52.288811) (xy 8.4 51.8615) (xy 7.9625 52.288811) (xy 7.974999 52.371048) (xy 7.987499 52.457036)
				(xy 8 52.546774) (xy 8.0125 52.640262) (xy 8.025 52.7375)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.507659 40.334939) (xy 39.653524 40.357133) (xy 39.79939 40.398827) (xy 39.945256 40.460021)
				(xy 40.091122 40.540715) (xy 40.236988 40.640909) (xy 40.983659 40.084939) (xy 40.236988 39.528969)
				(xy 40.091122 39.629163) (xy 39.945256 39.709857) (xy 39.79939 39.77105) (xy 39.653524 39.812745)
				(xy 39.507659 39.834939)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30156)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 23.6 2.9905) (xy 23.750227 3.001888) (xy 23.855113 3.029044) (xy 23.944886 3.061456) (xy 24.049772 3.088612)
				(xy 24.2 3.1) (xy 24.201 2.8) (xy 24.2 2.5) (xy 24.049772 2.511388) (xy 23.944886 2.538544) (xy 23.855113 2.570956)
				(xy 23.750227 2.598112) (xy 23.6 2.6095)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.975 39.325) (xy 30.011574 39.18322) (xy 30.048149 39.053441) (xy 30.084723 38.935662) (xy 30.121298 38.829883)
				(xy 30.157873 38.736104) (xy 29.725 38.399) (xy 29.292127 38.736104) (xy 29.328701 38.829883) (xy 29.365276 38.935662)
				(xy 29.40185 39.053441) (xy 29.438425 39.18322) (xy 29.475 39.325)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/HEATBREAK_TH_VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.769585 11.84798) (xy 51.728957 11.905573) (xy 51.68833 11.954571) (xy 51.647703 11.994975)
				(xy 51.607076 12.026785) (xy 51.566449 12.05) (xy 52.450707 12.450707) (xy 52.631156 12.05) (xy 52.49117 12.01155)
				(xy 52.351185 11.955959) (xy 52.2112 11.883227) (xy 52.071215 11.793352) (xy 51.93123 11.686335)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/AIN0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30237)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.75 51.3393) (xy 17.795802 51.342823) (xy 17.841605 51.349989) (xy 17.887409 51.360797) (xy 17.933212 51.375247)
				(xy 17.979015 51.393339) (xy 18.3385 51.225) (xy 17.979015 51.056661) (xy 17.933212 51.074752) (xy 17.887409 51.089202)
				(xy 17.841605 51.10001) (xy 17.795802 51.107176) (xy 17.75 51.1107)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30165)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49 28.9143) (xy 49.054521 28.947746) (xy 49.109042 28.99304) (xy 49.163564 29.05018) (xy 49.218085 29.119166)
				(xy 49.272607 29.2) (xy 49.626 28.8) (xy 49.272607 28.4) (xy 49.218085 28.480833) (xy 49.163564 28.549819)
				(xy 49.109042 28.606959) (xy 49.054521 28.652253) (xy 49 28.6857)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30269)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.749023 34.43545) (xy 33.769807 34.391961) (xy 33.790591 34.352672) (xy 33.811376 34.317582)
				(xy 33.83216 34.286691) (xy 33.852945 34.26) (xy 33.750707 33.684293) (xy 33.6 34.26) (xy 33.607174 34.268146)
				(xy 33.614348 34.278449) (xy 33.621523 34.290909) (xy 33.628697 34.305526) (xy 33.635872 34.322299)
			)
		)
	)
	(zone
		(net 6)
		(net_name "SPI_2_SDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30264)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.6643 40.2064) (xy 34.665751 40.122499) (xy 34.671591 40.062781) (xy 34.684048 40.01215) (xy 34.705352 39.955508)
				(xy 34.737732 39.877761) (xy 34.55 39.799) (xy 34.362268 39.877761) (xy 34.394646 39.955508) (xy 34.41595 40.01215)
				(xy 34.428408 40.062781) (xy 34.434248 40.122499) (xy 34.4357 40.2064)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/+5V_USB")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30183)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 32.65 33.3) (xy 32.654011 33.175479) (xy 32.667121 33.087599) (xy 32.690941 33.01346) (xy 32.727084 32.930162)
				(xy 32.777164 32.814805) (xy 32.5 32.699) (xy 32.222836 32.814805) (xy 32.272914 32.930162) (xy 32.309058 33.01346)
				(xy 32.332878 33.087599) (xy 32.345988 33.175479) (xy 32.35 33.3)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30168)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.195027 18.7845) (xy 39.0466 18.775712) (xy 38.942305 18.754756) (xy 38.852721 18.729743)
				(xy 38.748426 18.708788) (xy 38.6 18.7) (xy 38.599 19) (xy 38.714805 19.277164) (xy 38.828538 19.229325)
				(xy 38.911234 19.197104) (xy 38.985085 19.177636) (xy 39.072285 19.168056) (xy 39.195027 19.1655)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30218)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.5 28.6857) (xy 49.395813 28.681296) (xy 49.322763 28.667822) (xy 49.261374 28.644882) (xy 49.192169 28.612083)
				(xy 49.095671 28.56903) (xy 48.999 28.8) (xy 49.095671 29.03097) (xy 49.192169 28.987915) (xy 49.261374 28.955116)
				(xy 49.322763 28.932177) (xy 49.395813 28.918703) (xy 49.5 28.9143)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/HEATBREAK_TH_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.92473 14.713665) (xy 52.065756 14.606647) (xy 52.206783 14.516772) (xy 52.34781 14.44404)
				(xy 52.488837 14.388449) (xy 52.629864 14.35) (xy 52.450707 13.949293) (xy 51.560121 14.35) (xy 51.600713 14.373222)
				(xy 51.641306 14.405035) (xy 51.681899 14.445439) (xy 51.722492 14.494434) (xy 51.763085 14.55202)
			)
		)
	)
	(zone
		(net 18)
		(net_name "BOOT0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30127)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.775 38.6607) (xy 15.670307 38.640888) (xy 15.565614 38.603935) (xy 15.460922 38.54984) (xy 15.356229 38.478603)
				(xy 15.251537 38.390224) (xy 14.899 38.775) (xy 15.251537 39.159776) (xy 15.356229 39.071396) (xy 15.460922 39.000159)
				(xy 15.565614 38.946064) (xy 15.670307 38.909111) (xy 15.775 38.8893)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.85 35.9143) (xy 50.954692 35.934111) (xy 51.059385 35.971064) (xy 51.164077 36.025159) (xy 51.26877 36.096396)
				(xy 51.373463 36.184776) (xy 52.451 35.8) (xy 51.373463 35.415224) (xy 51.26877 35.503603) (xy 51.164077 35.57484)
				(xy 51.059385 35.628935) (xy 50.954692 35.665888) (xy 50.85 35.6857)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30273)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.96999 40) (xy 31.961943 40.038114) (xy 31.953897 40.07353) (xy 31.94585 40.106247) (xy 31.937804 40.136264)
				(xy 31.929758 40.163582) (xy 32.05 40.5635) (xy 32.170242 40.163582) (xy 32.162195 40.136264) (xy 32.154149 40.106247)
				(xy 32.146102 40.07353) (xy 32.138056 40.038114) (xy 32.13001 40)
			)
		)
	)
	(zone
		(net 4)
		(net_name "SPI_2_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30172)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.9 55.9143) (xy 39.946 55.929605) (xy 39.992 55.953328) (xy 40.037999 55.985468) (xy 40.083999 56.026025)
				(xy 40.13 56.075) (xy 40.7035 55.8) (xy 40.13 55.525) (xy 40.083999 55.573974) (xy 40.037999 55.614531)
				(xy 39.992 55.646671) (xy 39.946 55.670394) (xy 39.9 55.6857)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30203)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 45.552401 14.103733) (xy 45.552401 14.226806) (xy 45.552401 14.314149) (xy 45.552401 14.389582)
				(xy 45.552401 14.476925) (xy 45.552401 14.6) (xy 45.852401 14.601) (xy 46.064533 14.387868) (xy 45.966486 14.318608)
				(xy 45.871483 14.2839) (xy 45.790293 14.255408) (xy 45.733683 14.204797) (xy 45.712421 14.103733)
			)
		)
	)
	(zone
		(net 51)
		(net_name "AMBIENT_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.725 9.9143) (xy 21.840422 9.941381) (xy 21.955845 9.988491) (xy 22.071267 10.055631) (xy 22.18669 10.142801)
				(xy 22.302113 10.25) (xy 22.626 9.8) (xy 22.302113 9.35) (xy 22.18669 9.457198) (xy 22.071267 9.544368)
				(xy 21.955845 9.611508) (xy 21.840422 9.658618) (xy 21.725 9.6857)
			)
		)
	)
	(zone
		(net 8)
		(net_name "USB_PULL_UP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.6693 37.075) (xy 34.723395 36.936023) (xy 34.77749 36.814188) (xy 34.831585 36.709496) (xy 34.88568 36.621945)
				(xy 34.939776 36.551537) (xy 34.555 36.199) (xy 34.170224 36.551537) (xy 34.224319 36.621945) (xy 34.278414 36.709496)
				(xy 34.332509 36.814188) (xy 34.386604 36.936023) (xy 34.4407 37.075)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/FILAMENT_SW_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.22 11.7) (xy 7.197591 11.797999) (xy 7.175183 11.886999) (xy 7.152776 11.967) (xy 7.130368 12.038)
				(xy 7.10796 12.1) (xy 7.55 12.501) (xy 7.91194 12.1) (xy 7.873552 12.038) (xy 7.835164 11.967) (xy 7.796776 11.886999)
				(xy 7.758388 11.797999) (xy 7.72 11.7)
			)
		)
	)
	(zone
		(net 6)
		(net_name "SPI_2_SDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30231)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.2572 56.4857) (xy 39.162315 56.482643) (xy 39.09535 56.472653) (xy 39.038856 56.454502) (xy 38.975383 56.42696)
				(xy 38.887481 56.388801) (xy 38.799 56.6) (xy 38.887481 56.811199) (xy 38.975383 56.773038) (xy 39.038856 56.745497)
				(xy 39.09535 56.727346) (xy 39.162315 56.717356) (xy 39.2572 56.7143)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30178)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 12.3 11.35) (xy 12.42452 11.354011) (xy 12.5124 11.367121) (xy 12.586539 11.390941) (xy 12.669837 11.427084)
				(xy 12.785195 11.477164) (xy 12.901 11.2) (xy 12.785195 10.922836) (xy 12.669837 10.972914) (xy 12.586539 11.009058)
				(xy 12.5124 11.032878) (xy 12.42452 11.045988) (xy 12.3 11.05)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30186)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.7375 23.8857) (xy 50.6875 23.874844) (xy 50.6375 23.855846) (xy 50.587499 23.828705) (xy 50.537499 23.793423)
				(xy 50.4875 23.75) (xy 49.949 24) (xy 50.4875 24.25) (xy 50.537499 24.206576) (xy 50.587499 24.171294)
				(xy 50.6375 24.144153) (xy 50.6875 24.125155) (xy 50.7375 24.1143)
			)
		)
	)
	(zone
		(net 77)
		(net_name "Net-(Q1-G)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30191)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 46.795 21.4605) (xy 46.87 21.465259) (xy 46.945 21.473589) (xy 47.02 21.48549) (xy 47.095 21.50096)
				(xy 47.17 21.52) (xy 47.361 21.27) (xy 47.17 21.02) (xy 47.095 21.039039) (xy 47.02 21.054509) (xy 46.945 21.06641)
				(xy 46.87 21.07474) (xy 46.795 21.0795)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(P1-CC2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30252)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.880814 34.304039) (xy 34.884651 34.292349) (xy 34.888488 34.2821) (xy 34.892325 34.273292)
				(xy 34.896162 34.265925) (xy 34.9 34.26) (xy 34.749293 33.684293) (xy 34.634083 34.26) (xy 34.648074 34.301162)
				(xy 34.662065 34.343825) (xy 34.676056 34.387988) (xy 34.690047 34.433651) (xy 34.704039 34.480814)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.816355 37.2893) (xy 16.206902 37.320052) (xy 16.479222 37.393386) (xy 16.712132 37.480913)
				(xy 16.984452 37.554247) (xy 17.375 37.585) (xy 17.376 36.735) (xy 16.773959 36.133959) (xy 16.557411 36.411261)
				(xy 16.425241 36.663708) (xy 16.305584 36.870178) (xy 16.126576 37.009549) (xy 15.816355 37.0607)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30147)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 47.3 40.75) (xy 47.364521 40.775511) (xy 47.429042 40.813267) (xy 47.493564 40.863267) (xy 47.558085 40.925511)
				(xy 47.622607 41) (xy 47.976 40.6) (xy 47.622607 40.2) (xy 47.558085 40.274488) (xy 47.493564 40.336732)
				(xy 47.429042 40.386732) (xy 47.364521 40.424488) (xy 47.3 40.45)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30160)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.97298 19.588665) (xy 18.038076 19.582897) (xy 18.103173 19.587125) (xy 18.168269 19.601347)
				(xy 18.233366 19.625564) (xy 18.298463 19.659776) (xy 18.575707 19.199293) (xy 18.175 18.941306)
				(xy 18.102266 19.072732) (xy 18.029533 19.187017) (xy 17.956801 19.28416) (xy 17.884068 19.364161)
				(xy 17.811335 19.42702)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/FAN1_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.72298 31.838665) (xy 44.877321 31.791647) (xy 45.031662 31.761772) (xy 45.186004 31.74904)
				(xy 45.340345 31.753449) (xy 45.494687 31.775) (xy 45.400707 31.374293) (xy 44.926857 31.165662)
				(xy 44.853752 31.302217) (xy 44.780648 31.421631) (xy 44.707543 31.523902) (xy 44.634439 31.609032)
				(xy 44.561335 31.67702)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30166)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49 40.7143) (xy 49.054521 40.747746) (xy 49.109042 40.79304) (xy 49.163564 40.85018) (xy 49.218085 40.919166)
				(xy 49.272607 41) (xy 49.626 40.6) (xy 49.272607 40.2) (xy 49.218085 40.280833) (xy 49.163564 40.349819)
				(xy 49.109042 40.406959) (xy 49.054521 40.452253) (xy 49 40.4857)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30244)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.425 47.803546) (xy 34.422067 47.90201) (xy 34.415073 47.971714) (xy 34.406726 48.031831)
				(xy 34.399732 48.101535) (xy 34.3968 48.2) (xy 34.6 48.201) (xy 34.787732 48.122239) (xy 34.751169 48.045357)
				(xy 34.720107 47.991277) (xy 34.696053 47.94377) (xy 34.680514 47.886603) (xy 34.675 47.803546)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30222)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.45 30.625) (xy 25.3975 30.623) (xy 25.345 30.6195) (xy 25.2925 30.614499) (xy 25.24 30.607999)
				(xy 25.1875 30.6) (xy 24.849 30.775) (xy 25.1875 30.95) (xy 25.24 30.942) (xy 25.2925 30.9355) (xy 25.345 30.930499)
				(xy 25.3975 30.926999) (xy 25.45 30.925)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30200)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 45.087581 14.091122) (xy 45.06659 14.194766) (xy 45.010524 14.248152) (xy 44.929743 14.27939)
				(xy 44.834605 14.316592) (xy 44.735469 14.387868) (xy 44.947601 14.601) (xy 45.247601 14.6) (xy 45.247601 14.473798)
				(xy 45.247601 14.384235) (xy 45.247601 14.306886) (xy 45.247601 14.217323) (xy 45.247601 14.091122)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/AIN1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30126)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.67402 49.412375) (xy 16.684215 49.291989) (xy 16.694411 49.185559) (xy 16.704608 49.093084)
				(xy 16.714804 49.014564) (xy 16.725 48.95) (xy 16.274293 48.699293) (xy 15.974391 49.15996) (xy 16.081987 49.202488)
				(xy 16.189584 49.265158) (xy 16.297181 49.34797) (xy 16.404778 49.450924) (xy 16.512375 49.57402)
			)
		)
	)
	(zone
		(net 61)
		(net_name "Net-(D13-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.3125 4.197) (xy 22.197992 4.18057) (xy 22.083484 4.14932) (xy 21.968977 4.10325) (xy 21.854469 4.04236)
				(xy 21.739962 3.966651) (xy 21.399 4.3875) (xy 21.739962 4.808349) (xy 21.854469 4.732639) (xy 21.968977 4.671749)
				(xy 22.083484 4.625679) (xy 22.197992 4.594429) (xy 22.3125 4.578)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30149)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 12.9 11.05) (xy 12.835478 11.024488) (xy 12.770957 10.986732) (xy 12.706435 10.936732) (xy 12.641914 10.874488)
				(xy 12.577393 10.8) (xy 12.224 11.2) (xy 12.577393 11.6) (xy 12.641914 11.525511) (xy 12.706435 11.463267)
				(xy 12.770957 11.413267) (xy 12.835478 11.375511) (xy 12.9 11.35)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(VR1-FB)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 40.725 20.8155) (xy 40.829692 20.829215) (xy 40.934385 20.8555) (xy 41.039077 20.894355) (xy 41.14377 20.94578)
				(xy 41.248463 21.009776) (xy 41.601 20.625) (xy 41.248463 20.240224) (xy 41.14377 20.304219) (xy 41.039077 20.355644)
				(xy 40.934385 20.394499) (xy 40.829692 20.420784) (xy 40.725 20.4345)
			)
		)
	)
	(zone
		(net 77)
		(net_name "Net-(Q1-G)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 46.275 21.0795) (xy 46.171072 21.057295) (xy 46.067144 21.022521) (xy 45.963215 20.975177) (xy 45.859287 20.915263)
				(xy 45.75536 20.842779) (xy 45.399 21.225) (xy 45.751537 21.609776) (xy 45.856229 21.55478) (xy 45.960922 21.512355)
				(xy 46.065614 21.4825) (xy 46.170307 21.465215) (xy 46.275 21.4605)
			)
		)
	)
	(zone
		(net 25)
		(net_name "SW_CLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.197904 40.396259) (xy 20.966568 40.105973) (xy 20.8734 39.856946) (xy 20.846139 39.608408)
				(xy 20.812525 39.319589) (xy 20.700298 38.949719) (xy 19.914293 39.274293) (xy 19.589719 40.060298)
				(xy 19.959589 40.172525) (xy 20.248408 40.206139) (xy 20.496946 40.2334) (xy 20.745973 40.326568)
				(xy 21.036259 40.557904)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30254)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.4436 46.8643) (xy 38.527499 46.865751) (xy 38.587217 46.871591) (xy 38.637849 46.884048)
				(xy 38.694491 46.905352) (xy 38.772239 46.937732) (xy 38.851 46.75) (xy 38.772239 46.562268) (xy 38.694491 46.594646)
				(xy 38.637849 46.61595) (xy 38.587217 46.628408) (xy 38.527499 46.634248) (xy 38.4436 46.6357)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/AIN0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.22402 49.412375) (xy 15.214216 49.288022) (xy 15.204412 49.143527) (xy 15.194608 48.978891)
				(xy 15.184804 48.794112) (xy 15.175 48.589192) (xy 14.724293 48.699293) (xy 14.46257 49.167554)
				(xy 14.582531 49.208563) (xy 14.702492 49.269714) (xy 14.822453 49.351007) (xy 14.942414 49.452442)
				(xy 15.062375 49.57402)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+24V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.15)
		)
		(polygon
			(pts
				(xy 36.6 20.2) (xy 35.600875 20.2) (xy 35.600875 16.97283) (xy 36.471602 16.095875) (xy 40.4 16.095875)
				(xy 40.4 17.3) (xy 38.300006 17.300002) (xy 36.6 18.999996)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.1143 10.968605) (xy 50.04644 10.820994) (xy 49.97858 10.653991) (xy 49.91072 10.467595) (xy 49.84286 10.261808)
				(xy 49.775 10.03663) (xy 49.3375 10.199) (xy 49.277586 10.8) (xy 49.399208 10.795858) (xy 49.520831 10.810647)
				(xy 49.642454 10.844368) (xy 49.764077 10.897021) (xy 49.8857 10.968605)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30157)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28 2.9905) (xy 28.150227 3.001888) (xy 28.255113 3.029044) (xy 28.344886 3.061456) (xy 28.449772 3.088612)
				(xy 28.6 3.1) (xy 28.601 2.8) (xy 28.6 2.5) (xy 28.449772 2.511388) (xy 28.344886 2.538544) (xy 28.255113 2.570956)
				(xy 28.150227 2.598112) (xy 28 2.6095)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30175)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.4625 14.13335) (xy 9.512499 14.142682) (xy 9.562499 14.159013) (xy 9.6125 14.182343) (xy 9.6625 14.212672)
				(xy 9.7125 14.25) (xy 10.251 14) (xy 9.7125 13.75) (xy 9.6625 13.787327) (xy 9.6125 13.817656) (xy 9.562499 13.840986)
				(xy 9.512499 13.857317) (xy 9.4625 13.86665)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30130)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.612375 45.07598) (xy 49.5199 45.093694) (xy 49.427425 45.097453) (xy 49.33495 45.087257)
				(xy 49.242475 45.063106) (xy 49.15 45.025) (xy 48.899293 45.475707) (xy 49.35996 45.775609) (xy 49.442772 45.627728)
				(xy 49.525584 45.499989) (xy 49.608396 45.392392) (xy 49.691208 45.304937) (xy 49.77402 45.237625)
			)
		)
	)
	(zone
		(net 48)
		(net_name "SPI_1_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30229)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 26.5572 43.7) (xy 26.462694 43.698008) (xy 26.395563 43.690577) (xy 26.338713 43.675523) (xy 26.27505 43.650659)
				(xy 26.187481 43.613801) (xy 26.099 43.825) (xy 26.187481 44.036199) (xy 26.27505 43.99934) (xy 26.338713 43.974476)
				(xy 26.395563 43.959421) (xy 26.462694 43.951991) (xy 26.5572 43.95)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/+5V_USB")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30182)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 35.66697 33.3) (xy 35.670981 33.175479) (xy 35.684091 33.087599) (xy 35.707911 33.01346) (xy 35.744054 32.930162)
				(xy 35.794134 32.814805) (xy 35.51697 32.699) (xy 35.239806 32.814805) (xy 35.289884 32.930162)
				(xy 35.326028 33.01346) (xy 35.349848 33.087599) (xy 35.362958 33.175479) (xy 35.36697 33.3)
			)
		)
	)
	(zone
		(net 51)
		(net_name "AMBIENT_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.5107 11.125) (xy 22.447533 11.262586) (xy 22.384366 11.383031) (xy 22.3212 11.486333) (xy 22.258033 11.572494)
				(xy 22.194867 11.641513) (xy 22.575 12.001) (xy 22.959776 11.648463) (xy 22.91568 11.577849) (xy 22.871585 11.490197)
				(xy 22.82749 11.385504) (xy 22.783395 11.263772) (xy 22.7393 11.125)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30154)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.5375 49.797514) (xy 18.5466 49.648412) (xy 18.5683 49.543709) (xy 18.594199 49.453804) (xy 18.6159 49.349101)
				(xy 18.625 49.2) (xy 18.325 49.199) (xy 18.025 49.2) (xy 18.0367 49.349695) (xy 18.0646 49.454101)
				(xy 18.0979 49.543412) (xy 18.1258 49.647818) (xy 18.1375 49.797514)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.70835 12.075) (xy 10.758635 11.938309) (xy 10.80892 11.817618) (xy 10.859205 11.712925) (xy 10.90949 11.624231)
				(xy 10.959776 11.551537) (xy 10.575 11.199) (xy 10.190224 11.551537) (xy 10.240509 11.624231) (xy 10.290794 11.712925)
				(xy 10.341079 11.817618) (xy 10.391364 11.938309) (xy 10.44165 12.075)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30270)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.31242 32.804909) (xy 34.320146 32.780257) (xy 34.341198 32.78322) (xy 34.372385 32.80108)
				(xy 34.410515 32.821121) (xy 34.4524 32.830628) (xy 34.4524 32.529628) (xy 34.1524 32.530628) (xy 34.1524 32.598649)
				(xy 34.1524 32.646922) (xy 34.1524 32.688613) (xy 34.1524 32.736887) (xy 34.1524 32.804909)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.60948 22.412652) (xy 27.695391 22.269992) (xy 27.781302 22.147397) (xy 27.867213 22.044866)
				(xy 27.953124 21.9624) (xy 28.039036 21.9) (xy 27.400707 21.324293) (xy 26.882768 21.9) (xy 26.985684 21.924349)
				(xy 27.0886 21.966576) (xy 27.191515 22.02668) (xy 27.294431 22.104661) (xy 27.397348 22.20052)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/HEATBREAK_TH_VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.5768 11.2375) (xy 51.638109 11.084208) (xy 51.699419 10.950308) (xy 51.760729 10.835801)
				(xy 51.822039 10.740685) (xy 51.883349 10.664962) (xy 51.4625 10.199) (xy 51.041651 10.664962) (xy 51.10296 10.740685)
				(xy 51.16427 10.835801) (xy 51.22558 10.950308) (xy 51.28689 11.084208) (xy 51.3482 11.2375)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(P1-CC2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30121)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.225 35.05) (xy 39.329692 35.068955) (xy 39.434385 35.10441) (xy 39.539077 35.156365) (xy 39.64377 35.22482)
				(xy 39.748463 35.309776) (xy 40.101 34.925) (xy 39.748463 34.540224) (xy 39.64377 34.625179) (xy 39.539077 34.693634)
				(xy 39.434385 34.745589) (xy 39.329692 34.781044) (xy 39.225 34.8)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30135)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.178763 55.221224) (xy 19.22483 55.183428) (xy 19.270897 55.153318) (xy 19.316964 55.130893)
				(xy 19.363031 55.116153) (xy 19.409099 55.109099) (xy 18.999293 54.724293) (xy 18.550587 55.048765)
				(xy 18.605511 55.129967) (xy 18.660436 55.223169) (xy 18.715361 55.328371) (xy 18.770286 55.445573)
				(xy 18.825211 55.574776)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/AIN0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.67598 50.187625) (xy 15.705783 50.316544) (xy 15.735587 50.465606) (xy 15.765392 50.634809)
				(xy 15.795196 50.824155) (xy 15.825 51.033643) (xy 16.275707 50.900707) (xy 16.50273 50.425543)
				(xy 16.369708 50.385914) (xy 16.236687 50.326143) (xy 16.103667 50.246231) (xy 15.970646 50.146176)
				(xy 15.837625 50.02598)
			)
		)
	)
	(zone
		(net 100)
		(net_name "RGB_LED_CLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30214)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.3 4.3643) (xy 15.404186 4.368703) (xy 15.477235 4.382177) (xy 15.538624 4.405116) (xy 15.60783 4.437915)
				(xy 15.704329 4.48097) (xy 15.801 4.25) (xy 15.704329 4.01903) (xy 15.60783 4.062083) (xy 15.538624 4.094882)
				(xy 15.477235 4.117822) (xy 15.404186 4.131296) (xy 15.3 4.1357)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/+5V_USB")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30179)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 32.35 32.1) (xy 32.345988 32.22452) (xy 32.332878 32.3124) (xy 32.309058 32.386539) (xy 32.272914 32.469837)
				(xy 32.222836 32.585195) (xy 32.5 32.701) (xy 32.777164 32.585195) (xy 32.727084 32.469837) (xy 32.690941 32.386539)
				(xy 32.667121 32.3124) (xy 32.654011 32.22452) (xy 32.65 32.1)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30274)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.0143 46.8) (xy 48.97181 46.725271) (xy 48.873021 46.708622) (xy 48.760949 46.738904) (xy 48.678613 46.80497)
				(xy 48.66903 46.895671) (xy 48.9 46.799) (xy 48.66903 46.895671) (xy 48.692249 46.905242) (xy 48.722569 46.870377)
				(xy 48.752946 46.821158) (xy 48.776337 46.787671) (xy 48.7857 46.8)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch full 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 22.38 14.6) (xy 21.298609 14.6) (xy 20.3 15.666782) (xy 18.320743 15.666782) (xy 18.324693 13.288652)
				(xy 20.538383 13.294344) (xy 22.38 14.043973)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.571967 52.575863) (xy 44.702862 52.50669) (xy 44.833757 52.442017) (xy 44.964653 52.381845)
				(xy 45.095548 52.326172) (xy 45.226444 52.275) (xy 45.100707 51.824293) (xy 44.627717 51.586338)
				(xy 44.510501 51.687177) (xy 44.393285 51.783516) (xy 44.276069 51.875355) (xy 44.158853 51.962694)
				(xy 44.041637 52.045533)
			)
		)
	)
	(zone
		(net 104)
		(net_name "DOTSTAR_LED_CLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30219)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 12.4 28.4357) (xy 12.295813 28.431296) (xy 12.222763 28.417822) (xy 12.161374 28.394882) (xy 12.092169 28.362083)
				(xy 11.995671 28.31903) (xy 11.899 28.55) (xy 11.995671 28.78097) (xy 12.092169 28.737915) (xy 12.161374 28.705116)
				(xy 12.222763 28.682177) (xy 12.295813 28.668703) (xy 12.4 28.6643)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.894271 48.294774) (xy 29.831557 48.462814) (xy 29.768843 48.618855) (xy 29.70613 48.762896)
				(xy 29.643416 48.894937) (xy 29.580703 49.014978) (xy 30.006952 49.360646) (xy 30.440532 49.023835)
				(xy 30.40199 48.972733) (xy 30.363448 48.909631) (xy 30.324907 48.83453) (xy 30.286365 48.747428)
				(xy 30.247824 48.648327)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.475 2.6095) (xy 28.370307 2.590784) (xy 28.265614 2.559499) (xy 28.160922 2.515644) (xy 28.056229 2.459219)
				(xy 27.951537 2.390224) (xy 27.599 2.775) (xy 27.951537 3.159776) (xy 28.056229 3.10078) (xy 28.160922 3.054355)
				(xy 28.265614 3.0205) (xy 28.370307 2.999215) (xy 28.475 2.9905)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.0143 46.375) (xy 49.08144 46.219518) (xy 49.14858 46.084066) (xy 49.21572 45.968643) (xy 49.28286 45.873249)
				(xy 49.35 45.797886) (xy 48.9 45.474) (xy 48.45 45.797886) (xy 48.51714 45.873249) (xy 48.58428 45.968643)
				(xy 48.65142 46.084066) (xy 48.71856 46.219518) (xy 48.7857 46.375)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 46.025 56.6) (xy 45.89 56.594) (xy 45.755 56.5835) (xy 45.62 56.5685) (xy 45.485 56.549) (xy 45.35 56.525)
				(xy 45.099 56.975) (xy 45.35 57.425) (xy 45.485 57.401) (xy 45.62 57.3815) (xy 45.755 57.3665) (xy 45.89 57.356)
				(xy 46.025 57.35)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.5107 25.875) (xy 49.437076 26.032926) (xy 49.363453 26.17071) (xy 49.289829 26.288353) (xy 49.216206 26.385853)
				(xy 49.142583 26.463212) (xy 49.575 26.801) (xy 50.007873 26.463896) (xy 49.954158 26.384951) (xy 49.900443 26.286589)
				(xy 49.846729 26.16881) (xy 49.793014 26.031613) (xy 49.7393 25.875)
			)
		)
	)
	(zone
		(net 6)
		(net_name "SPI_2_SDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30171)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.855 56.7143) (xy 39.91 56.727329) (xy 39.965 56.749914) (xy 40.019999 56.782054) (xy 40.074999 56.823749)
				(xy 40.13 56.875) (xy 40.7035 56.6) (xy 40.13 56.325) (xy 40.074999 56.37625) (xy 40.019999 56.417945)
				(xy 39.965 56.450085) (xy 39.91 56.47267) (xy 39.855 56.4857)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 36.175 49.575) (xy 36.292779 49.587574) (xy 36.410558 49.612149) (xy 36.528337 49.648723) (xy 36.646116 49.697298)
				(xy 36.763896 49.757873) (xy 37.101 49.325) (xy 36.763896 48.892127) (xy 36.646116 48.952701) (xy 36.528337 49.001276)
				(xy 36.410558 49.03785) (xy 36.292779 49.062425) (xy 36.175 49.075)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.3393 27.475) (xy 20.393395 27.336023) (xy 20.44749 27.214188) (xy 20.501585 27.109496) (xy 20.55568 27.021945)
				(xy 20.609776 26.951537) (xy 20.225 26.599) (xy 19.840224 26.951537) (xy 19.894319 27.021945) (xy 19.948414 27.109496)
				(xy 20.002509 27.214188) (xy 20.056604 27.336023) (xy 20.1107 27.475)
			)
		)
	)
	(zone
		(net 49)
		(net_name "SPI_1_SDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30192)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.6857 54.18) (xy 21.678163 54.306029) (xy 21.656575 54.393247) (xy 21.622469 54.465971) (xy 21.577378 54.548515)
				(xy 21.522836 54.665195) (xy 21.8 54.781) (xy 22.077164 54.665195) (xy 22.022621 54.548515) (xy 21.97753 54.465971)
				(xy 21.943424 54.393247) (xy 21.921836 54.306029) (xy 21.9143 54.18)
			)
		)
	)
	(zone
		(net 57)
		(net_name "Net-(VR1-VCC)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30226)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.63 22.275) (xy 37.583 22.2682) (xy 37.536 22.2563) (xy 37.488999 22.239299) (xy 37.441999 22.217199)
				(xy 37.395 22.19) (xy 37.159 22.425) (xy 37.395 22.66) (xy 37.441999 22.6328) (xy 37.488999 22.6107)
				(xy 37.536 22.593699) (xy 37.583 22.581799) (xy 37.63 22.575)
			)
		)
	)
	(zone
		(net 67)
		(net_name "/HOTEND_TH_VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.7143 44.9375) (xy 51.778939 44.814584) (xy 51.843579 44.708257) (xy 51.90822 44.618519) (xy 51.97286 44.54537)
				(xy 52.0375 44.488811) (xy 51.6 44.0615) (xy 51.1625 44.488811) (xy 51.227139 44.54537) (xy 51.291779 44.618519)
				(xy 51.35642 44.708257) (xy 51.42106 44.814584) (xy 51.4857 44.9375)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30216)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.5 40.4857) (xy 49.395813 40.481296) (xy 49.322763 40.467822) (xy 49.261374 40.444882) (xy 49.192169 40.412083)
				(xy 49.095671 40.36903) (xy 48.999 40.6) (xy 49.095671 40.83097) (xy 49.192169 40.787915) (xy 49.261374 40.755116)
				(xy 49.322763 40.732177) (xy 49.395813 40.718703) (xy 49.5 40.7143)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30271)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.8476 32.804909) (xy 33.8476 32.736887) (xy 33.8476 32.688613) (xy 33.8476 32.646922) (xy 33.8476 32.598649)
				(xy 33.8476 32.530628) (xy 33.5476 32.529628) (xy 33.5476 32.830628) (xy 33.589483 32.821121) (xy 33.627614 32.80108)
				(xy 33.658801 32.78322) (xy 33.679853 32.780257) (xy 33.68758 32.804909)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.925 21.825) (xy 26.09 21.795) (xy 26.255 21.7875) (xy 26.42 21.8025) (xy 26.585 21.84) (xy 26.75 21.9)
				(xy 27.401 21.325) (xy 26.516298 20.91806) (xy 26.398038 21.064448) (xy 26.279778 21.188336) (xy 26.161519 21.289724)
				(xy 26.043259 21.368612) (xy 25.925 21.425)
			)
		)
	)
	(zone
		(net 49)
		(net_name "SPI_1_SDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30227)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.577491 53.315847) (xy 21.551992 53.225674) (xy 21.526494 53.131859) (xy 21.500996 53.034402)
				(xy 21.475498 52.933303) (xy 21.45 52.828563) (xy 21.274293 52.861793) (xy 21.256563 53.275) (xy 21.288419 53.308214)
				(xy 21.320276 53.34507) (xy 21.352133 53.385568) (xy 21.38399 53.429708) (xy 21.415847 53.477491)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30248)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.547958 46.625) (xy 29.444573 46.633573) (xy 29.37448 46.657008) (xy 29.316774 46.691877)
				(xy 29.250548 46.734753) (xy 29.154898 46.782207) (xy 29.231659 46.969939) (xy 29.376343 47.113623)
				(xy 29.419987 47.048901) (xy 29.439318 46.984734) (xy 29.453989 46.929066) (xy 29.483652 46.88984)
				(xy 29.547958 46.875)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/FAN0_MOSFET_GND")
		(layer "F.Cu")
		(name "FAN0 MOSFET THERMAL PAD")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.25)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 48.2 17.9) (xy 50.6 17.9) (xy 51 17.6) (xy 54.8 17.6) (xy 54.8 22.9) (xy 48.2 22.9)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30181)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 47.9 40.45) (xy 47.775479 40.445988) (xy 47.687599 40.432878) (xy 47.61346 40.409058) (xy 47.530162 40.372914)
				(xy 47.414805 40.322836) (xy 47.299 40.6) (xy 47.414805 40.877164) (xy 47.530162 40.827084) (xy 47.61346 40.790941)
				(xy 47.687599 40.767121) (xy 47.775479 40.754011) (xy 47.9 40.75)
			)
		)
	)
	(zone
		(net 49)
		(net_name "SPI_1_SDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30257)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.4064 43.1357) (xy 29.322499 43.134248) (xy 29.262781 43.128408) (xy 29.21215 43.11595) (xy 29.155508 43.094646)
				(xy 29.077761 43.062268) (xy 28.999 43.25) (xy 29.077761 43.437732) (xy 29.155508 43.405352) (xy 29.21215 43.384048)
				(xy 29.262781 43.371591) (xy 29.322499 43.365751) (xy 29.4064 43.3643)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30155)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.251013 7.710632) (xy 31.332734 7.663221) (xy 31.414455 7.628453) (xy 31.496177 7.606326)
				(xy 31.577898 7.596842) (xy 31.65962 7.6) (xy 31.725707 7.074293) (xy 31.4 6.94038) (xy 31.337873 7.087385)
				(xy 31.275747 7.221748) (xy 31.21362 7.34347) (xy 31.151494 7.452549) (xy 31.089368 7.548987)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30141)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.25 18.8) (xy 8.1925 18.869561) (xy 8.135 18.927961) (xy 8.077499 18.975199) (xy 8.019999 19.011274)
				(xy 7.9625 19.036188) (xy 8.4 19.4635) (xy 8.8375 19.036188) (xy 8.78 19.011274) (xy 8.7225 18.975199)
				(xy 8.664999 18.927961) (xy 8.607499 18.869561) (xy 8.55 18.8)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.075 36.485) (xy 18.714201 36.456427) (xy 18.468709 36.377871) (xy 18.266144 36.260071) (xy 18.034128 36.113768)
				(xy 17.700281 35.949702) (xy 17.374 36.735) (xy 17.700281 37.520298) (xy 18.034128 37.356231) (xy 18.266144 37.209928)
				(xy 18.468709 37.092128) (xy 18.714201 37.013572) (xy 19.075 36.985)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.15 53.839918) (xy 19.056215 53.962676) (xy 18.96243 54.068934) (xy 18.868645 54.158692) (xy 18.77486 54.23195)
				(xy 18.681076 54.288709) (xy 19 54.726) (xy 19.475 54.737761) (xy 19.479999 54.525192) (xy 19.484999 54.329123)
				(xy 19.49 54.149555) (xy 19.495 53.986486) (xy 19.5 53.839918)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/OSC_OUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.2 54.8) (xy 34.279999 54.649195) (xy 34.359999 54.518793) (xy 34.44 54.408793) (xy 34.52 54.319195)
				(xy 34.6 54.25) (xy 34.05 53.299) (xy 33.5 54.25) (xy 33.579999 54.319195) (xy 33.659999 54.408793)
				(xy 33.74 54.518793) (xy 33.82 54.649195) (xy 33.9 54.8)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/FAN0_MOSFET_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30167)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.802486 3.003) (xy 21.951795 3.013088) (xy 22.056395 3.037144) (xy 22.14609 3.065856) (xy 22.25069 3.089912)
				(xy 22.4 3.1) (xy 22.401 2.8) (xy 22.285195 2.522836) (xy 22.171233 2.569356) (xy 22.087902 2.598475)
				(xy 22.013281 2.61425) (xy 21.925449 2.620738) (xy 21.802486 2.622)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.943296 42.755849) (xy 51.11088 42.640895) (xy 51.278465 42.545333) (xy 51.446049 42.469163)
				(xy 51.613634 42.412385) (xy 51.781219 42.375) (xy 51.600707 41.936793) (xy 51 41.918782) (xy 50.95633 42.09265)
				(xy 50.91266 42.247126) (xy 50.86899 42.382211) (xy 50.82532 42.497903) (xy 50.781651 42.594204)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/FAN1_MOSFET_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 26.5125 2.622) (xy 26.397992 2.60557) (xy 26.283484 2.57432) (xy 26.168977 2.52825) (xy 26.054469 2.46736)
				(xy 25.939962 2.391651) (xy 25.599 2.8125) (xy 25.939962 3.233349) (xy 26.054469 3.157639) (xy 26.168977 3.096749)
				(xy 26.283484 3.050679) (xy 26.397992 3.019429) (xy 26.5125 3.003)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.49165 15.875) (xy 10.431745 16.030777) (xy 10.37184 16.167555) (xy 10.311936 16.285334) (xy 10.252031 16.384114)
				(xy 10.192127 16.463896) (xy 10.625 16.801) (xy 11.057873 16.463896) (xy 10.997968 16.384114) (xy 10.938063 16.285334)
				(xy 10.878159 16.167555) (xy 10.818254 16.030777) (xy 10.75835 15.875)
			)
		)
	)
	(zone
		(net 8)
		(net_name "USB_PULL_UP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30220)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.4 36.0857) (xy 34.295813 36.081296) (xy 34.222763 36.067822) (xy 34.161374 36.044882) (xy 34.092169 36.012083)
				(xy 33.995671 35.96903) (xy 33.899 36.2) (xy 33.995671 36.43097) (xy 34.092169 36.387915) (xy 34.161374 36.355116)
				(xy 34.222763 36.332177) (xy 34.295813 36.318703) (xy 34.4 36.3143)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/FAN1_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.561335 34.62298) (xy 44.634068 34.697008) (xy 44.706801 34.788178) (xy 44.779533 34.89649)
				(xy 44.852266 35.021944) (xy 44.925 35.164541) (xy 45.400707 34.975707) (xy 45.505715 34.575) (xy 45.349167 34.586551)
				(xy 45.19262 34.58096) (xy 45.036074 34.558226) (xy 44.879527 34.518351) (xy 44.72298 34.461335)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30139)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.01 55.01) (xy 17.159099 55.0152) (xy 17.264549 55.0276) (xy 17.355449 55.0424) (xy 17.4609 55.0548)
				(xy 17.61 55.06) (xy 17.611 54.76) (xy 17.61 54.46) (xy 17.4609 54.4652) (xy 17.355449 54.4776)
				(xy 17.264549 54.4924) (xy 17.159099 54.5048) (xy 17.01 54.51)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/AIN1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.3893 45.175) (xy 16.452466 45.037413) (xy 16.515632 44.916968) (xy 16.578799 44.813665) (xy 16.641965 44.727504)
				(xy 16.705132 44.658486) (xy 16.325 44.299) (xy 15.940224 44.651537) (xy 15.984319 44.72215) (xy 16.028414 44.809802)
				(xy 16.072509 44.914495) (xy 16.116604 45.036227) (xy 16.1607 45.175)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.048033 27.199861) (xy 27.874792 27.360888) (xy 27.701551 27.517416) (xy 27.528309 27.669444)
				(xy 27.355069 27.816972) (xy 27.181828 27.96) (xy 27.419293 28.535707) (xy 28.32 28.448172) (xy 28.407027 28.33093)
				(xy 28.494055 28.218189) (xy 28.581083 28.109949) (xy 28.668111 28.006208) (xy 28.755139 27.906967)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/LED_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.113665 30.15202) (xy 9.040931 30.107503) (xy 8.968198 30.047197) (xy 8.895466 29.971102) (xy 8.822733 29.879217)
				(xy 8.75 29.771543) (xy 7.549293 29.949293) (xy 8.55 30.35) (xy 8.630404 30.318513) (xy 8.710808 30.299136)
				(xy 8.791211 30.29187) (xy 8.871615 30.296712) (xy 8.95202 30.313665)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/FAN0_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30129)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.561335 22.92298) (xy 44.63531 22.985344) (xy 44.709285 23.064851) (xy 44.783259 23.161499)
				(xy 44.857234 23.27529) (xy 44.93121 23.406223) (xy 45.400707 23.175707) (xy 45.483159 22.775) (xy 45.331123 22.806551)
				(xy 45.179087 22.82096) (xy 45.027051 22.818227) (xy 44.875015 22.798352) (xy 44.72298 22.761335)
			)
		)
	)
	(zone
		(net 51)
		(net_name "AMBIENT_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30134)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.025 9.6857) (xy 20.935478 9.66042) (xy 20.845957 9.61921) (xy 20.756435 9.56207) (xy 20.666914 9.489)
				(xy 20.577393 9.4) (xy 20.224 9.8) (xy 20.577393 10.2) (xy 20.666914 10.110999) (xy 20.756435 10.037929)
				(xy 20.845957 9.980789) (xy 20.935478 9.939579) (xy 21.025 9.9143)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30243)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.33001 31.44) (xy 34.344008 31.401601) (xy 34.358006 31.367402) (xy 34.372004 31.337402) (xy 34.386002 31.311601)
				(xy 34.4 31.29) (xy 34.25 30.714) (xy 34.1 31.29) (xy 34.113998 31.311601) (xy 34.127996 31.337402)
				(xy 34.141994 31.367402) (xy 34.155992 31.401601) (xy 34.16999 31.44)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30241)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.66999 29.99) (xy 33.655992 30.028398) (xy 33.641994 30.062597) (xy 33.627996 30.092597) (xy 33.613998 30.118398)
				(xy 33.6 30.14) (xy 33.75 30.716) (xy 33.9 30.14) (xy 33.886002 30.118398) (xy 33.872004 30.092597)
				(xy 33.858006 30.062597) (xy 33.844008 30.028398) (xy 33.83001 29.99)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SPI_1_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30262)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.7064 42.6357) (xy 28.622499 42.634248) (xy 28.562781 42.628408) (xy 28.51215 42.61595) (xy 28.455508 42.594646)
				(xy 28.377761 42.562268) (xy 28.299 42.75) (xy 28.377761 42.937732) (xy 28.455508 42.905352) (xy 28.51215 42.884048)
				(xy 28.562781 42.871591) (xy 28.622499 42.865751) (xy 28.7064 42.8643)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D5-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30143)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.921724 12.239921) (xy 17.997071 12.25772) (xy 18.072419 12.288605) (xy 18.147767 12.332576)
				(xy 18.223115 12.389633) (xy 18.298463 12.459776) (xy 18.575707 11.999293) (xy 18.18496 11.674922)
				(xy 18.099983 11.789876) (xy 18.015007 11.887689) (xy 17.930031 11.96836) (xy 17.845055 12.031889)
				(xy 17.760079 12.078276)
			)
		)
	)
	(zone
		(net 51)
		(net_name "AMBIENT_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.7393 10.725) (xy 22.803014 10.567048) (xy 22.866729 10.429183) (xy 22.930443 10.311404) (xy 22.994158 10.213711)
				(xy 23.057873 10.136104) (xy 22.625 9.799) (xy 22.192127 10.136104) (xy 22.255841 10.213711) (xy 22.319556 10.311404)
				(xy 22.38327 10.429183) (xy 22.446985 10.567048) (xy 22.5107 10.725)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/+5V_USB")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 35.4 27.172183) (xy 35.738705 26.947746) (xy 36.07741 26.768309) (xy 36.416115 26.633873) (xy 36.75482 26.544436)
				(xy 37.093526 26.5) (xy 36.7 25.599) (xy 35.45 25.627234) (xy 35.379999 26.026223) (xy 35.309999 26.380213)
				(xy 35.24 26.689203) (xy 35.17 26.953193) (xy 35.1 27.172183)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30204)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.6893 36.248224) (xy 49.764666 36.192295) (xy 49.840032 36.144508) (xy 49.915398 36.104863)
				(xy 49.990764 36.07336) (xy 50.06613 36.05) (xy 49.95 35.799) (xy 49.414815 36.05) (xy 49.423992 36.077437)
				(xy 49.433169 36.110977) (xy 49.442346 36.150622) (xy 49.451523 36.196371) (xy 49.4607 36.248224)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/FAN0_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.72298 23.738665) (xy 44.881633 23.671648) (xy 45.040287 23.621773) (xy 45.19894 23.58904)
				(xy 45.357594 23.573449) (xy 45.516248 23.575) (xy 45.400707 23.174293) (xy 44.925 23.003179) (xy 44.852266 23.152231)
				(xy 44.779533 23.284141) (xy 44.706801 23.398909) (xy 44.634068 23.496535) (xy 44.561335 23.57702)
			)
		)
	)
	(zone
		(net 32)
		(net_name "Earth_Protective")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 28.45 54.95) (xy 28.1 54.6) (xy 26.05 54.6) (xy 25.7 54.95) (xy 25.7 58.3) (xy 25.75 58.35)
				(xy 28.375 58.35) (xy 28.45 58.275)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30246)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.31242 34.41) (xy 34.327153 34.371601) (xy 34.341887 34.337402) (xy 34.35662 34.307402) (xy 34.371354 34.281601)
				(xy 34.386088 34.26) (xy 34.25 33.684) (xy 34.1 34.26) (xy 34.11048 34.281601) (xy 34.12096 34.307402)
				(xy 34.131439 34.337402) (xy 34.141919 34.371601) (xy 34.1524 34.41)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.3393 20.075) (xy 20.393395 19.936023) (xy 20.44749 19.814188) (xy 20.501585 19.709496) (xy 20.55568 19.621945)
				(xy 20.609776 19.551537) (xy 20.225 19.199) (xy 19.840224 19.551537) (xy 19.894319 19.621945) (xy 19.948414 19.709496)
				(xy 20.002509 19.814188) (xy 20.056604 19.936023) (xy 20.1107 20.075)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+24V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30153)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 32.9 24.934486) (xy 32.9104 24.784494) (xy 32.9352 24.67949) (xy 32.9648 24.589481) (xy 32.9896 24.484477)
				(xy 33 24.334486) (xy 32.7 24.333486) (xy 32.4 24.334486) (xy 32.4104 24.484477) (xy 32.4352 24.589481)
				(xy 32.4648 24.67949) (xy 32.4896 24.784494) (xy 32.5 24.934486)
			)
		)
	)
	(zone
		(net 48)
		(net_name "SPI_1_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30239)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.85 51.7607) (xy 22.804197 51.757176) (xy 22.758394 51.75001) (xy 22.71259 51.739202) (xy 22.666787 51.724752)
				(xy 22.620985 51.706661) (xy 22.2615 51.875) (xy 22.620985 52.043339) (xy 22.666787 52.025247) (xy 22.71259 52.010797)
				(xy 22.758394 51.999989) (xy 22.804197 51.992823) (xy 22.85 51.9893)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.739579 46.719939) (xy 28.550909 46.784951) (xy 28.36224 46.837963) (xy 28.17357 46.878975)
				(xy 27.984901 46.907987) (xy 27.796232 46.925) (xy 27.899 47.375) (xy 28.365067 47.649932) (xy 28.439969 47.539933)
				(xy 28.514871 47.441934) (xy 28.589774 47.355936) (xy 28.664676 47.281937) (xy 28.739579 47.219939)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.0143 46.375) (xy 49.08144 46.219518) (xy 49.14858 46.084066) (xy 49.21572 45.968643) (xy 49.28286 45.873249)
				(xy 49.35 45.797886) (xy 48.9 45.474) (xy 48.45 45.797886) (xy 48.51714 45.873249) (xy 48.58428 45.968643)
				(xy 48.65142 46.084066) (xy 48.71856 46.219518) (xy 48.7857 46.375)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/LED_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30267)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.7643 30.25) (xy 10.78144 30.199715) (xy 10.79858 30.154573) (xy 10.815719 30.114574) (xy 10.832859 30.079716)
				(xy 10.85 30.05) (xy 10.65 29.849) (xy 10.45 30.05) (xy 10.46714 30.079716) (xy 10.48428 30.114574)
				(xy 10.501419 30.154573) (xy 10.518559 30.199715) (xy 10.5357 30.25)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.298926 20.091694) (xy 28.08284 20.232355) (xy 27.866755 20.368516) (xy 27.65067 20.500177)
				(xy 27.434585 20.627338) (xy 27.2185 20.75) (xy 27.399293 21.325707) (xy 28.3 21.395618) (xy 28.441206 21.267254)
				(xy 28.582412 21.14339) (xy 28.723619 21.024027) (xy 28.864825 20.909163) (xy 29.006032 20.7988)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30202)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.44165 13.531066) (xy 10.377245 13.58885) (xy 10.31284 13.639636) (xy 10.248435 13.683423)
				(xy 10.18403 13.72021) (xy 10.119626 13.75) (xy 10.25 14.001) (xy 10.72755 13.75) (xy 10.72371 13.719399)
				(xy 10.71987 13.682205) (xy 10.71603 13.638418) (xy 10.71219 13.588038) (xy 10.70835 13.531066)
			)
		)
	)
	(zone
		(net 81)
		(net_name "/HOTEND_TH_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.4857 48.6625) (xy 51.42106 48.785415) (xy 51.35642 48.891742) (xy 51.291779 48.981479) (xy 51.227139 49.054628)
				(xy 51.1625 49.111188) (xy 51.6 49.5385) (xy 52.0375 49.111188) (xy 51.97286 49.054628) (xy 51.90822 48.981479)
				(xy 51.843579 48.891742) (xy 51.778939 48.785415) (xy 51.7143 48.6625)
			)
		)
	)
	(zone
		(net 97)
		(net_name "Net-(D17-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30142)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.921724 26.839921) (xy 17.997071 26.85772) (xy 18.072419 26.888605) (xy 18.147767 26.932576)
				(xy 18.223115 26.989633) (xy 18.298463 27.059776) (xy 18.575707 26.599293) (xy 18.18496 26.274922)
				(xy 18.099983 26.389876) (xy 18.015007 26.487689) (xy 17.930031 26.56836) (xy 17.845055 26.631889)
				(xy 17.760079 26.678276)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 47.8 56.1) (xy 48.1 55.8) (xy 49.5 55.8) (xy 49.8 56.1) (xy 49.8 57.3) (xy 49.5 57.6) (xy 48.1 57.6)
				(xy 47.8 57.3)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.628536 9.209819) (xy 49.524667 9.327019) (xy 49.420798 9.424827) (xy 49.316929 9.503244)
				(xy 49.21306 9.562268) (xy 49.109192 9.601901) (xy 49.336793 10.200707) (xy 49.775 10.285064) (xy 49.778036 10.06356)
				(xy 49.781072 9.861448) (xy 49.784108 9.678727) (xy 49.787144 9.515399) (xy 49.790181 9.371464)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30247)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 30.675 40.309416) (xy 30.667465 40.205563) (xy 30.646504 40.134467) (xy 30.614584 40.075579)
				(xy 30.574171 40.008352) (xy 30.527732 39.912239) (xy 30.34 39.989) (xy 30.196316 40.133684) (xy 30.259254 40.177271)
				(xy 30.320862 40.19806) (xy 30.373869 40.214628) (xy 30.411005 40.245554) (xy 30.425 40.309416)
			)
		)
	)
	(zone
		(net 7)
		(net_name "ADS1220_DRDY")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30236)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.0893 53.45) (xy 20.100107 53.396913) (xy 20.110915 53.347468) (xy 20.121723 53.301664) (xy 20.132531 53.259503)
				(xy 20.143339 53.220985) (xy 19.975 52.8615) (xy 19.806661 53.220985) (xy 19.817468 53.259503) (xy 19.828276 53.301664)
				(xy 19.839084 53.347468) (xy 19.849892 53.396913) (xy 19.8607 53.45)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30148)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 47.3 28.95) (xy 47.364521 28.975511) (xy 47.429042 29.013267) (xy 47.493564 29.063267) (xy 47.558085 29.125511)
				(xy 47.622607 29.2) (xy 47.976 28.8) (xy 47.622607 28.4) (xy 47.558085 28.474488) (xy 47.493564 28.536732)
				(xy 47.429042 28.586732) (xy 47.364521 28.624488) (xy 47.3 28.65)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.3393 12.875) (xy 20.393395 12.736023) (xy 20.44749 12.614188) (xy 20.501585 12.509496) (xy 20.55568 12.421945)
				(xy 20.609776 12.351537) (xy 20.225 11.999) (xy 19.840224 12.351537) (xy 19.894319 12.421945) (xy 19.948414 12.509496)
				(xy 20.002509 12.614188) (xy 20.056604 12.736023) (xy 20.1107 12.875)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/LED_GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 14)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 6.23 31.23) (xy 6.38 31.08) (xy 8.58 31.08) (xy 9.23 31.73) (xy 9.23 33.63) (xy 9.03 33.83)
				(xy 7.63 33.83) (xy 6.23 32.43)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/LED_POWER")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 7.53 24.58) (xy 8.98 24.58) (xy 9.23 24.83) (xy 9.23 26.73) (xy 8.58 27.38) (xy 6.33 27.38)
				(xy 6.23 27.28) (xy 6.23 25.88)
			)
		)
	)
	(zone
		(net 62)
		(net_name "Net-(D14-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 26.725 4.578) (xy 26.829692 4.599215) (xy 26.934385 4.633) (xy 27.039077 4.679355) (xy 27.14377 4.73828)
				(xy 27.248463 4.809776) (xy 27.601 4.425) (xy 27.248463 4.040224) (xy 27.14377 4.096719) (xy 27.039077 4.140644)
				(xy 26.934385 4.171999) (xy 26.829692 4.190784) (xy 26.725 4.197)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.8 17.6) (xy 10.851574 17.47722) (xy 10.903149 17.369441) (xy 10.954723 17.276662) (xy 11.006298 17.198883)
				(xy 11.057873 17.136104) (xy 10.625 16.799) (xy 10.192127 17.136104) (xy 10.233701 17.198883) (xy 10.275276 17.276662)
				(xy 10.31685 17.369441) (xy 10.358425 17.47722) (xy 10.4 17.6)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/LOAD_CELL_IN-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.5625 44.3768) (xy 9.677007 44.399325) (xy 9.791515 44.441243) (xy 9.906022 44.502553) (xy 10.02053 44.583255)
				(xy 10.135038 44.683349) (xy 10.601 44.2625) (xy 10.135038 43.841651) (xy 10.02053 43.941744) (xy 9.906022 44.022446)
				(xy 9.791515 44.083756) (xy 9.677007 44.125674) (xy 9.5625 44.1482)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(VR1-FB)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30225)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.885 21.375) (xy 37.829 21.370999) (xy 37.773 21.363999) (xy 37.716999 21.354) (xy 37.660999 21.341)
				(xy 37.605 21.325) (xy 37.259 21.5) (xy 37.605 21.675) (xy 37.660999 21.658999) (xy 37.716999 21.645999)
				(xy 37.773 21.636) (xy 37.829 21.629) (xy 37.885 21.625)
			)
		)
	)
	(zone
		(net 57)
		(net_name "Net-(VR1-VCC)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.294529 23.256661) (xy 38.385623 23.40475) (xy 38.476717 23.573839) (xy 38.567811 23.763927)
				(xy 38.658905 23.975017) (xy 38.75 24.207106) (xy 39.250707 24.000707) (xy 39.232107 23.275) (xy 39.087017 23.270905)
				(xy 38.941928 23.245811) (xy 38.796839 23.199717) (xy 38.65175 23.132623) (xy 38.506661 23.044529)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/FAN1_PWM_+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30128)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 44.561335 31.12298) (xy 44.63531 31.185344) (xy 44.709285 31.264851) (xy 44.783259 31.361499)
				(xy 44.857234 31.47529) (xy 44.93121 31.606223) (xy 45.400707 31.375707) (xy 45.483159 30.975) (xy 45.331123 31.006551)
				(xy 45.179087 31.02096) (xy 45.027051 31.018226) (xy 44.875015 30.998352) (xy 44.72298 30.961335)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30163)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.193935 14.106066) (xy 49.28484 14.136808) (xy 49.375746 14.18255) (xy 49.466651 14.243291)
				(xy 49.557557 14.319033) (xy 49.648463 14.409776) (xy 50.000707 14.025707) (xy 49.583579 13.683579)
				(xy 49.548076 13.742164) (xy 49.512573 13.792493) (xy 49.477071 13.834564) (xy 49.441568 13.868378)
				(xy 49.406066 13.893935)
			)
		)
	)
	(zone
		(net 34)
		(net_name "Net-(U2-PB3)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30131)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.675 42.1357) (xy 27.57494 42.103984) (xy 27.47488 42.055126) (xy 27.374821 41.989127) (xy 27.274761 41.905985)
				(xy 27.174702 41.805702) (xy 26.799 42.175) (xy 27.151537 42.559776) (xy 27.256229 42.487154) (xy 27.360922 42.431296)
				(xy 27.465614 42.392201) (xy 27.570307 42.369869) (xy 27.675 42.3643)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30185)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.7375 35.6857) (xy 50.6875 35.674844) (xy 50.6375 35.655846) (xy 50.587499 35.628705) (xy 50.537499 35.593423)
				(xy 50.4875 35.55) (xy 49.949 35.8) (xy 50.4875 36.05) (xy 50.537499 36.006576) (xy 50.587499 35.971294)
				(xy 50.6375 35.944153) (xy 50.6875 35.925155) (xy 50.7375 35.9143)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/LOAD_CELL_REF+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.025 48.8625) (xy 8.0125 48.959737) (xy 8 49.053225) (xy 7.987499 49.142962) (xy 7.974999 49.22895)
				(xy 7.9625 49.311188) (xy 8.4 49.7385) (xy 8.8375 49.311188) (xy 8.825 49.22895) (xy 8.8125 49.142962)
				(xy 8.799999 49.053225) (xy 8.787499 48.959737) (xy 8.775 48.8625)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SPI_1_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30194)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.5107 53.201) (xy 20.503163 53.327029) (xy 20.481575 53.414247) (xy 20.447469 53.486971) (xy 20.402378 53.569515)
				(xy 20.347836 53.686195) (xy 20.625 53.802) (xy 20.902164 53.686195) (xy 20.847621 53.569515) (xy 20.80253 53.486971)
				(xy 20.768424 53.414247) (xy 20.746836 53.327029) (xy 20.7393 53.201)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.925 14.625) (xy 26.09 14.595) (xy 26.255 14.5875) (xy 26.42 14.6025) (xy 26.585 14.64) (xy 26.75 14.7)
				(xy 27.401 14.125) (xy 26.516298 13.71806) (xy 26.398038 13.864448) (xy 26.279778 13.988336) (xy 26.161519 14.089724)
				(xy 26.043259 14.168612) (xy 25.925 14.225)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30212)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 48.7857 46.3) (xy 48.781296 46.404186) (xy 48.767822 46.477235) (xy 48.744882 46.538624) (xy 48.712083 46.60783)
				(xy 48.66903 46.704329) (xy 48.9 46.801) (xy 49.13097 46.704329) (xy 49.087915 46.60783) (xy 49.055116 46.538624)
				(xy 49.032177 46.477235) (xy 49.018703 46.404186) (xy 49.0143 46.3)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30140)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.75 54.798395) (xy 18.745006 54.947373) (xy 18.733099 55.052765) (xy 18.718887 55.143629)
				(xy 18.70698 55.249021) (xy 18.701987 55.398) (xy 19.001987 55.399) (xy 19.301987 55.398) (xy 19.29658 55.248974)
				(xy 19.283687 55.143605) (xy 19.268299 55.052789) (xy 19.255406 54.94742) (xy 19.25 54.798395)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "F.Cu")
		(name "Guard Ring Copper")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.25 25.41) (xy 51.405 25.255) (xy 53.655 25.255) (xy 53.81 25.41) (xy 53.81 26.88) (xy 53.58 27.11)
				(xy 51.48 27.11) (xy 51.25 26.88)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/+24V_INPUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 38.9 15) (xy 38.9 12.7) (xy 37.3 11.1) (xy 35 11.1) (xy 35 9.4) (xy 35.1 9.3) (xy 37.5 9.3)
				(xy 38.4 8.4) (xy 39.1 8.4) (xy 39.1 10.2) (xy 40.3 11.4) (xy 40.3 15)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30272)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 32.46999 40) (xy 32.461943 40.038114) (xy 32.453897 40.07353) (xy 32.44585 40.106247) (xy 32.437804 40.136264)
				(xy 32.429758 40.163582) (xy 32.55 40.5635) (xy 32.670242 40.163582) (xy 32.662195 40.136264) (xy 32.654149 40.106247)
				(xy 32.646102 40.07353) (xy 32.638056 40.038114) (xy 32.63001 40)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30150)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.125 48.6) (xy 18.1146 48.749991) (xy 18.0898 48.854995) (xy 18.060199 48.945004) (xy 18.0354 49.050008)
				(xy 18.025 49.2) (xy 18.325 49.201) (xy 18.625 49.2) (xy 18.6146 49.050008) (xy 18.5898 48.945004)
				(xy 18.560199 48.854995) (xy 18.5354 48.749991) (xy 18.525 48.6)
			)
		)
	)
	(zone
		(net 78)
		(net_name "Net-(Q2-G)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 46.275 32.9795) (xy 46.184046 32.946596) (xy 46.093092 32.901122) (xy 46.002138 32.843079) (xy 45.911184 32.772465)
				(xy 45.820231 32.689282) (xy 45.399 33.025) (xy 45.675 33.425) (xy 45.795 33.38696) (xy 45.915 33.36149)
				(xy 46.035 33.34859) (xy 46.155 33.34826) (xy 46.275 33.3605)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.735139 21.953033) (xy 28.648111 21.853791) (xy 28.561083 21.75005) (xy 28.474055 21.64181)
				(xy 28.387027 21.529069) (xy 28.3 21.411828) (xy 27.399293 21.324293) (xy 27.161828 21.9) (xy 27.335069 22.043027)
				(xy 27.50831 22.190555) (xy 27.68155 22.342583) (xy 27.854792 22.499111) (xy 28.028033 22.660139)
			)
		)
	)
	(zone
		(net 99)
		(net_name "RGB_LED_DATA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30211)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.299293 3.0643) (xy 15.403479 3.068703) (xy 15.476528 3.082177) (xy 15.537917 3.105116) (xy 15.607123 3.137915)
				(xy 15.703622 3.18097) (xy 15.800293 2.95) (xy 15.703622 2.71903) (xy 15.607123 2.762083) (xy 15.537917 2.794882)
				(xy 15.476528 2.817822) (xy 15.403479 2.831296) (xy 15.299293 2.8357)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/HEATBREAK_TH_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.418271 14.896835) (xy 51.342947 15.063259) (xy 51.267623 15.210292) (xy 51.192298 15.337932)
				(xy 51.116975 15.446181) (xy 51.041651 15.535038) (xy 51.461793 16.000707) (xy 51.883349 15.535038)
				(xy 51.822662 15.473623) (xy 51.761975 15.39526) (xy 51.701288 15.299949) (xy 51.640601 15.187688)
				(xy 51.579915 15.058479)
			)
		)
	)
	(zone
		(net 48)
		(net_name "SPI_1_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30170)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 26.1 43.95) (xy 26.156715 43.97188) (xy 26.213431 44.004462) (xy 26.270147 44.047747) (xy 26.326863 44.101733)
				(xy 26.383579 44.166421) (xy 26.801 43.825) (xy 26.383579 43.483579) (xy 26.326863 43.548266) (xy 26.270147 43.602252)
				(xy 26.213431 43.645537) (xy 26.156715 43.678119) (xy 26.1 43.7)
			)
		)
	)
	(zone
		(net 8)
		(net_name "USB_PULL_UP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.075 2.5845) (xy 19.970307 2.570784) (xy 19.865614 2.544499) (xy 19.760922 2.505644) (xy 19.656229 2.454219)
				(xy 19.551537 2.390224) (xy 19.199 2.775) (xy 19.551537 3.159776) (xy 19.656229 3.09578) (xy 19.760922 3.044355)
				(xy 19.865614 3.0055) (xy 19.970307 2.979215) (xy 20.075 2.9655)
			)
		)
	)
	(zone
		(net 48)
		(net_name "SPI_1_SCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30213)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.51 51.9893) (xy 22.614186 51.993703) (xy 22.687235 52.007177) (xy 22.748624 52.030116) (xy 22.81783 52.062915)
				(xy 22.914329 52.10597) (xy 23.011 51.875) (xy 22.914329 51.64403) (xy 22.81783 51.687083) (xy 22.748624 51.719882)
				(xy 22.687235 51.742822) (xy 22.614186 51.756296) (xy 22.51 51.7607)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30256)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.4357 47.7936) (xy 33.434248 47.877499) (xy 33.428408 47.937217) (xy 33.41595 47.987849) (xy 33.394646 48.044491)
				(xy 33.362268 48.122239) (xy 33.55 48.201) (xy 33.737732 48.122239) (xy 33.705352 48.044491) (xy 33.684048 47.987849)
				(xy 33.671591 47.937217) (xy 33.665751 47.877499) (xy 33.6643 47.7936)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30151)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.4 17) (xy 10.3896 17.149991) (xy 10.3648 17.254995) (xy 10.3352 17.345004) (xy 10.3104 17.450008)
				(xy 10.3 17.6) (xy 10.6 17.601) (xy 10.9 17.6) (xy 10.8896 17.450008) (xy 10.8648 17.345004) (xy 10.8352 17.254995)
				(xy 10.8104 17.149991) (xy 10.8 17)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.85 24.1143) (xy 50.954692 24.134111) (xy 51.059385 24.171064) (xy 51.164077 24.225159) (xy 51.26877 24.296396)
				(xy 51.373463 24.384776) (xy 52.451 24) (xy 51.373463 23.615224) (xy 51.26877 23.703603) (xy 51.164077 23.77484)
				(xy 51.059385 23.828935) (xy 50.954692 23.865888) (xy 50.85 23.8857)
			)
		)
	)
	(zone
		(net 17)
		(net_name "FAN1_PWM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30245)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 42.448499 28.386856) (xy 42.381742 28.371485) (xy 42.314986 28.350972) (xy 42.24823 28.325316)
				(xy 42.181474 28.294519) (xy 42.114718 28.258581) (xy 41.849293 28.449293) (xy 42.113268 28.642388)
				(xy 42.147985 28.613326) (xy 42.182703 28.589406) (xy 42.21742 28.570628) (xy 42.252138 28.556992)
				(xy 42.286856 28.548499)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/OSC_IN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 31.425 55.375) (xy 31.368425 55.528779) (xy 31.31185 55.664558) (xy 31.255276 55.782337) (xy 31.198701 55.882116)
				(xy 31.142127 55.963896) (xy 31.575 56.301) (xy 32.007873 55.963896) (xy 31.951298 55.882116) (xy 31.894723 55.782337)
				(xy 31.838149 55.664558) (xy 31.781574 55.528779) (xy 31.725 55.375)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/FAN0_MOSFET_GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.3125 2.622) (xy 22.197992 2.60557) (xy 22.083484 2.57432) (xy 21.968977 2.52825) (xy 21.854469 2.46736)
				(xy 21.739962 2.391651) (xy 21.399 2.8125) (xy 21.739962 3.233349) (xy 21.854469 3.157639) (xy 21.968977 3.096749)
				(xy 22.083484 3.050679) (xy 22.197992 3.019429) (xy 22.3125 3.003)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SPI_1_SDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30235)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.7393 53.45) (xy 20.750107 53.396913) (xy 20.760915 53.347468) (xy 20.771723 53.301664) (xy 20.782531 53.259503)
				(xy 20.793339 53.220985) (xy 20.625 52.8615) (xy 20.456661 53.220985) (xy 20.467468 53.259503) (xy 20.478276 53.301664)
				(xy 20.489084 53.347468) (xy 20.499892 53.396913) (xy 20.5107 53.45)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30193)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.8857 11.1) (xy 49.878163 11.226029) (xy 49.856575 11.313247) (xy 49.822469 11.385971) (xy 49.777378 11.468515)
				(xy 49.722836 11.585195) (xy 50 11.701) (xy 50.277164 11.585195) (xy 50.222621 11.468515) (xy 50.17753 11.385971)
				(xy 50.143424 11.313247) (xy 50.121836 11.226029) (xy 50.1143 11.1)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/LOAD_CELL_IN+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.172243 46.410599) (xy 9.082384 46.373916) (xy 8.992526 46.320091) (xy 8.902667 46.249125)
				(xy 8.812809 46.161016) (xy 8.722951 46.055766) (xy 7.549293 46.349293) (xy 8.626537 46.734776)
				(xy 8.703349 46.677247) (xy 8.780161 46.632229) (xy 8.856974 46.599723) (xy 8.933786 46.579727)
				(xy 9.010599 46.572243)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+24V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 32.5 24.334486) (xy 32.36 24.454969) (xy 32.22 24.551762) (xy 32.079999 24.624865) (xy 31.939999 24.674278)
				(xy 31.8 24.7) (xy 32.7 25.601) (xy 33.6 24.7) (xy 33.46 24.674278) (xy 33.32 24.624865) (xy 33.179999 24.551762)
				(xy 33.039999 24.454969) (xy 32.9 24.334486)
			)
		)
	)
	(zone
		(net 99)
		(net_name "RGB_LED_DATA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30263)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.6643 40.2064) (xy 33.665751 40.122499) (xy 33.671591 40.062781) (xy 33.684048 40.01215) (xy 33.705352 39.955508)
				(xy 33.737732 39.877761) (xy 33.55 39.799) (xy 33.362268 39.877761) (xy 33.394646 39.955508) (xy 33.41595 40.01215)
				(xy 33.428408 40.062781) (xy 33.434248 40.122499) (xy 33.4357 40.2064)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.825 37.0607) (xy 15.70722 37.037157) (xy 15.589441 36.993529) (xy 15.471662 36.929814) (xy 15.353883 36.846013)
				(xy 15.236104 36.742127) (xy 14.899 37.175) (xy 15.236104 37.607873) (xy 15.353883 37.503986) (xy 15.471662 37.420185)
				(xy 15.589441 37.35647) (xy 15.70722 37.312842) (xy 15.825 37.2893)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/AIN0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 16.3893 51.825) (xy 16.453014 51.667048) (xy 16.516729 51.529183) (xy 16.580443 51.411404) (xy 16.644158 51.313711)
				(xy 16.707873 51.236104) (xy 16.275 50.899) (xy 15.842127 51.236104) (xy 15.905841 51.313711) (xy 15.969556 51.411404)
				(xy 16.03327 51.529183) (xy 16.096985 51.667048) (xy 16.1607 51.825)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30122)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.937625 8.22402) (xy 51.049337 8.102094) (xy 51.16105 8.00031) (xy 51.272764 7.918669) (xy 51.384477 7.857169)
				(xy 51.49619 7.815812) (xy 51.200707 7.374293) (xy 50.725 7.6) (xy 50.735195 7.664564) (xy 50.745391 7.743084)
				(xy 50.755588 7.835559) (xy 50.765784 7.941989) (xy 50.77598 8.062375)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30138)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 43.4 56.85) (xy 43.549099 56.8552) (xy 43.654549 56.8676) (xy 43.745449 56.8824) (xy 43.8509 56.8948)
				(xy 44 56.9) (xy 44.001 56.6) (xy 44 56.3) (xy 43.8509 56.3052) (xy 43.745449 56.3176) (xy 43.654549 56.3324)
				(xy 43.549099 56.3448) (xy 43.4 56.35)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch full 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 22.38 21.8) (xy 21.298609 21.8) (xy 20.779531 22.766782) (xy 18.311945 22.766782) (xy 18.315729 20.488628)
				(xy 20.538383 20.494344) (xy 22.38 21.243973)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.525 48.375) (xy 18.571574 48.22722) (xy 18.618149 48.094441) (xy 18.664723 47.976662) (xy 18.711298 47.873883)
				(xy 18.757873 47.786104) (xy 18.3 47.474) (xy 17.859195 47.811648) (xy 17.912356 47.894318) (xy 17.965517 47.991988)
				(xy 18.018677 48.104659) (xy 18.071838 48.232329) (xy 18.125 48.375)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30251)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 30.425 47.745453) (xy 30.412491 47.825264) (xy 30.380272 47.874469) (xy 30.336299 47.912439)
				(xy 30.288531 47.958551) (xy 30.244927 48.032178) (xy 30.432659 48.110939) (xy 30.635859 48.109939)
				(xy 30.639929 48.019244) (xy 30.649636 47.955245) (xy 30.661222 47.900145) (xy 30.670929 47.836146)
				(xy 30.675 47.745453)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30189)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.6 9.93335) (xy 18.725181 9.93901) (xy 18.812771 9.956085) (xy 18.88629 9.98471) (xy 18.969258 10.025024)
				(xy 19.085195 10.077164) (xy 19.201 9.8) (xy 19.085195 9.522836) (xy 18.969258 9.574975) (xy 18.88629 9.615289)
				(xy 18.812771 9.643914) (xy 18.725181 9.660989) (xy 18.6 9.66665)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.08948 29.622652) (xy 27.230348 29.469121) (xy 27.371216 29.341091) (xy 27.512083 29.23856)
				(xy 27.652952 29.16153) (xy 27.79382 29.11) (xy 27.420707 28.534293) (xy 26.593223 29.036777) (xy 26.650047 29.083357)
				(xy 26.706872 29.144021) (xy 26.763698 29.21877) (xy 26.820523 29.307603) (xy 26.877348 29.41052)
			)
		)
	)
	(zone
		(net 7)
		(net_name "ADS1220_DRDY")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30258)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.4064 45.1357) (xy 29.322499 45.134248) (xy 29.262781 45.128408) (xy 29.21215 45.11595) (xy 29.155508 45.094646)
				(xy 29.077761 45.062268) (xy 28.999 45.25) (xy 29.077761 45.437732) (xy 29.155508 45.405352) (xy 29.21215 45.384048)
				(xy 29.262781 45.371591) (xy 29.322499 45.365751) (xy 29.4064 45.3643)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.25)
		)
		(polygon
			(pts
				(xy 5.5 20.3) (xy 6.7 20.3) (xy 9 22.6) (xy 9 23.4) (xy 7.9 23.4) (xy 6.6 22.1) (xy 5.5 22.1)
			)
		)
	)
	(zone
		(net 32)
		(net_name "Earth_Protective")
		(locked yes)
		(layers "F.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "B.Cu")
		(name "Guard Ring Copper")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 0 0) (xy 60 0) (xy 60 60) (xy 0 60)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "In1.Cu" "In2.Cu" "In4.Cu" "B.Cu")
		(name "Ground Fill")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 2 2) (xy 58 2) (xy 58 58) (xy 2 58)
			)
		)
	)
	(zone
		(net 6)
		(net_name "SPI_2_SDO")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.71999 56.1428) (xy 38.713552 56.239175) (xy 38.695429 56.305487) (xy 38.667406 56.360582)
				(xy 38.631268 56.423309) (xy 38.588801 56.512519) (xy 38.8 56.601) (xy 39.011199 56.512519) (xy 38.96873 56.423309)
				(xy 38.932592 56.360582) (xy 38.90457 56.305487) (xy 38.886447 56.239175) (xy 38.88001 56.1428)
			)
		)
	)
	(zone
		(net 48)
		(net_name "SPI_1_SCLK")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 23.331535 51.501624) (xy 23.247844 51.568186) (xy 23.175995 51.594789) (xy 23.10427 51.60235)
				(xy 23.020953 51.611791) (xy 22.914329 51.64403) (xy 23.009293 51.875707) (xy 23.24097 51.970671)
				(xy 23.278368 51.874834) (xy 23.304819 51.805316) (xy 23.332942 51.748126) (xy 23.375358 51.689276)
				(xy 23.444686 51.614775)
			)
		)
	)
	(zone
		(net 5)
		(net_name "SPI_2_SCLK")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 41.11999 56.9428) (xy 41.113552 57.039175) (xy 41.095429 57.105487) (xy 41.067406 57.160582)
				(xy 41.031268 57.223309) (xy 40.988801 57.312519) (xy 41.2 57.401) (xy 41.411199 57.312519) (xy 41.36873 57.223309)
				(xy 41.332592 57.160582) (xy 41.30457 57.105487) (xy 41.286447 57.039175) (xy 41.28001 56.9428)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.06967 18.681802) (xy 38.154882 18.772688) (xy 38.207753 18.844098) (xy 38.243333 18.913365)
				(xy 38.276676 18.997823) (xy 38.322836 19.114805) (xy 38.600707 19.000707) (xy 38.714805 18.722836)
				(xy 38.597823 18.676676) (xy 38.513365 18.643333) (xy 38.444098 18.607753) (xy 38.372688 18.554882)
				(xy 38.281802 18.46967)
			)
		)
	)
	(zone
		(net 49)
		(net_name "SPI_1_SDO")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.167688 54.299161) (xy 22.069631 54.381825) (xy 21.987535 54.421984) (xy 21.906218 54.441178)
				(xy 21.810498 54.460948) (xy 21.685195 54.502836) (xy 21.799293 54.780707) (xy 22.077164 54.894805)
				(xy 22.11905 54.7695) (xy 22.13882 54.673781) (xy 22.158015 54.592464) (xy 22.198174 54.510368)
				(xy 22.280839 54.412312)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 45.702262 15.106774) (xy 45.724088 15.002323) (xy 45.782233 14.949743) (xy 45.865692 14.919924)
				(xy 45.963459 14.883757) (xy 46.064533 14.812132) (xy 45.852401 14.599) (xy 45.552401 14.6) (xy 45.552401 14.725679)
				(xy 45.552401 14.814872) (xy 45.552401 14.891901) (xy 45.552401 14.981094) (xy 45.552402 15.106774)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 48.703022 29.210129) (xy 48.783312 29.140829) (xy 48.849734 29.104929) (xy 48.915276 29.085762)
				(xy 48.992926 29.066664) (xy 49.095671 29.03097) (xy 49.000707 28.799293) (xy 48.76903 28.704329)
				(xy 48.733334 28.807073) (xy 48.714236 28.884722) (xy 48.69507 28.950264) (xy 48.65917 29.016686)
				(xy 48.589871 29.096978)
			)
		)
	)
	(zone
		(net 48)
		(net_name "SPI_1_SCLK")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.6428 43.90501) (xy 25.739175 43.911447) (xy 25.805487 43.92957) (xy 25.860582 43.957592)
				(xy 25.923309 43.99373) (xy 26.012519 44.036199) (xy 26.101 43.825) (xy 26.012519 43.613801) (xy 25.923309 43.656268)
				(xy 25.860582 43.692406) (xy 25.805487 43.720429) (xy 25.739175 43.738552) (xy 25.6428 43.74499)
			)
		)
	)
	(zone
		(net 4)
		(net_name "SPI_2_SDI")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 35.393943 39.230792) (xy 35.337096 39.167085) (xy 35.305192 39.115368) (xy 35.28609 39.064649)
				(xy 35.26765 39.003936) (xy 35.237732 38.922239) (xy 35.049293 38.999293) (xy 34.972239 39.187732)
				(xy 35.053936 39.21765) (xy 35.114649 39.23609) (xy 35.165368 39.255192) (xy 35.217085 39.287096)
				(xy 35.280792 39.343943)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.152401 32.023854) (xy 34.1524 32.149533) (xy 34.1524 32.238726) (xy 34.1524 32.315755) (xy 34.1524 32.404948)
				(xy 34.1524 32.530628) (xy 34.4524 32.531628) (xy 34.664532 32.318496) (xy 34.563458 32.24687) (xy 34.465691 32.210703)
				(xy 34.382232 32.180884) (xy 34.324087 32.128304) (xy 34.302261 32.023854)
			)
		)
	)
	(zone
		(net 6)
		(net_name "SPI_2_SDO")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.63001 40.2064) (xy 34.63486 40.121156) (xy 34.64887 40.062027) (xy 34.671226 40.012655) (xy 34.701118 39.956686)
				(xy 34.737732 39.877761) (xy 34.55 39.799) (xy 34.362268 39.877761) (xy 34.398881 39.956686) (xy 34.428772 40.012655)
				(xy 34.451129 40.062027) (xy 34.465139 40.121156) (xy 34.46999 40.2064)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.08001 41.1) (xy 49.087781 40.994223) (xy 49.109364 40.92187) (xy 49.142156 40.861972) (xy 49.183558 40.793562)
				(xy 49.23097 40.695671) (xy 49 40.599) (xy 48.76903 40.695671) (xy 48.81644 40.793562) (xy 48.857842 40.861972)
				(xy 48.890635 40.92187) (xy 48.912217 40.994223) (xy 48.91999 41.1)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/+5V_USB")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 32.694454 33.146967) (xy 32.650295 33.081129) (xy 32.652422 33.023303) (xy 32.6849 32.96518)
				(xy 32.731792 32.89845) (xy 32.777164 32.814805) (xy 32.499293 32.699293) (xy 32.222836 32.814805)
				(xy 32.270714 32.964234) (xy 32.28982 33.07958) (xy 32.307399 33.178176) (xy 32.350699 33.277356)
				(xy 32.446967 33.394454)
			)
		)
	)
	(zone
		(net 24)
		(net_name "SWD_IO")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 24.150027 39.21999) (xy 23.778375 39.172553) (xy 23.539098 39.048468) (xy 23.348672 38.875072)
				(xy 23.123573 38.679704) (xy 22.780281 38.489702) (xy 22.454 39.275) (xy 22.780281 40.060298) (xy 23.120612 39.877176)
				(xy 23.3474 39.694418) (xy 23.540997 39.535192) (xy 23.781754 39.422667) (xy 24.150027 39.38001)
			)
		)
	)
	(zone
		(net 5)
		(net_name "SPI_2_SCLK")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 37.233287 39.479865) (xy 37.305986 39.416268) (xy 37.365689 39.382194) (xy 37.424462 39.363051)
				(xy 37.494371 39.344249) (xy 37.587481 39.311199) (xy 37.500707 39.099293) (xy 37.288801 39.012519)
				(xy 37.25575 39.105628) (xy 37.236948 39.175536) (xy 37.217804 39.234309) (xy 37.18373 39.294013)
				(xy 37.120135 39.366713)
			)
		)
	)
	(zone
		(net 13)
		(net_name "FAN0_TACH")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.4064 46.16999) (xy 38.321156 46.165139) (xy 38.262027 46.151129) (xy 38.212655 46.128772)
				(xy 38.156686 46.098881) (xy 38.077761 46.062268) (xy 37.999 46.25) (xy 38.077761 46.437732) (xy 38.156686 46.401118)
				(xy 38.212655 46.371226) (xy 38.262027 46.34887) (xy 38.321156 46.33486) (xy 38.4064 46.33001)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.90193 30.411671) (xy 33.913306 30.283595) (xy 33.944149 30.197273) (xy 33.989527 30.126468)
				(xy 34.044508 30.044947) (xy 34.104164 29.926476) (xy 33.827 29.810671) (xy 33.549836 29.926476)
				(xy 33.60949 30.044947) (xy 33.664472 30.126468) (xy 33.70985 30.197273) (xy 33.740693 30.283595)
				(xy 33.75207 30.411671)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SPI_1_SDI")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.8936 42.83001) (xy 27.978843 42.83486) (xy 28.037972 42.84887) (xy 28.087343 42.871226) (xy 28.143313 42.901118)
				(xy 28.222239 42.937732) (xy 28.301 42.75) (xy 28.222239 42.562268) (xy 28.143313 42.598881) (xy 28.087343 42.628772)
				(xy 28.037972 42.651129) (xy 27.978843 42.665139) (xy 27.8936 42.66999)
			)
		)
	)
	(zone
		(net 16)
		(net_name "FAN1_TACH")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.193943 46.980792) (xy 39.137096 46.917085) (xy 39.105192 46.865368) (xy 39.08609 46.814649)
				(xy 39.06765 46.753936) (xy 39.037732 46.672239) (xy 38.849293 46.749293) (xy 38.772239 46.937732)
				(xy 38.853936 46.96765) (xy 38.914649 46.98609) (xy 38.965368 47.005192) (xy 39.017085 47.037096)
				(xy 39.080792 47.093943)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "In2.Cu")
		(name "3.3V Power Plane")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 2 2) (xy 58 2) (xy 58 58) (xy 2 58)
			)
		)
	)
	(zone
		(net 7)
		(net_name "ADS1220_DRDY")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.769208 45.593943) (xy 28.832913 45.537096) (xy 28.88463 45.505192) (xy 28.935349 45.48609)
				(xy 28.996062 45.46765) (xy 29.077761 45.437732) (xy 29.000707 45.249293) (xy 28.812268 45.172239)
				(xy 28.782349 45.253936) (xy 28.763909 45.314649) (xy 28.744807 45.365368) (xy 28.712903 45.417085)
				(xy 28.656057 45.480792)
			)
		)
	)
	(zone
		(net 49)
		(net_name "SPI_1_SDO")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.5936 43.33001) (xy 28.678843 43.33486) (xy 28.737972 43.34887) (xy 28.787343 43.371226) (xy 28.843313 43.401118)
				(xy 28.922239 43.437732) (xy 29.001 43.25) (xy 28.922239 43.062268) (xy 28.843313 43.098881) (xy 28.787343 43.128772)
				(xy 28.737972 43.151129) (xy 28.678843 43.165139) (xy 28.5936 43.16999)
			)
		)
	)
	(zone
		(net 99)
		(net_name "RGB_LED_DATA")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.299293 3.03001) (xy 15.405068 3.037781) (xy 15.477421 3.059364) (xy 15.537319 3.092156) (xy 15.60573 3.133558)
				(xy 15.703622 3.18097) (xy 15.800293 2.95) (xy 15.703622 2.71903) (xy 15.60573 2.76644) (xy 15.537319 2.807842)
				(xy 15.477421 2.840635) (xy 15.405068 2.862217) (xy 15.299293 2.86999)
			)
		)
	)
	(zone
		(net 99)
		(net_name "RGB_LED_DATA")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.206057 39.569208) (xy 33.262903 39.632913) (xy 33.294807 39.68463) (xy 33.313909 39.735349)
				(xy 33.332349 39.796062) (xy 33.362268 39.877761) (xy 33.550707 39.800707) (xy 33.627761 39.612268)
				(xy 33.546062 39.582349) (xy 33.485349 39.563909) (xy 33.43463 39.544807) (xy 33.382913 39.512903)
				(xy 33.319208 39.456057)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.08001 12.3) (xy 50.090893 12.17221) (xy 50.120547 12.085762) (xy 50.164475 12.01469) (xy 50.218179 11.933026)
				(xy 50.277164 11.814805) (xy 50 11.699) (xy 49.722836 11.814805) (xy 49.78182 11.933026) (xy 49.835524 12.01469)
				(xy 49.879451 12.085762) (xy 49.909106 12.17221) (xy 49.91999 12.3)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/+5V_USB")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 35.487293 33.360194) (xy 35.592668 33.246265) (xy 35.656394 33.155891) (xy 35.698118 33.067941)
				(xy 35.737482 32.961289) (xy 35.794134 32.814805) (xy 35.517677 32.699293) (xy 35.21697 32.7) (xy 35.233374 32.808253)
				(xy 35.267095 32.892466) (xy 35.294898 32.963823) (xy 35.293547 33.033508) (xy 35.239806 33.112707)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 45.2476 15.106774) (xy 45.2476 14.981094) (xy 45.2476 14.891901) (xy 45.2476 14.814872) (xy 45.2476 14.725679)
				(xy 45.247601 14.6) (xy 44.947601 14.599) (xy 44.735469 14.812132) (xy 44.836541 14.883757) (xy 44.934309 14.919924)
				(xy 45.017767 14.949743) (xy 45.075912 15.002323) (xy 45.09774 15.106774)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SPI_1_SDI")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.54499 53.201) (xy 20.534106 53.328789) (xy 20.504451 53.415236) (xy 20.460524 53.486309)
				(xy 20.40682 53.567972) (xy 20.347836 53.686195) (xy 20.625 53.802) (xy 20.902164 53.686195) (xy 20.843179 53.567972)
				(xy 20.789475 53.486309) (xy 20.745547 53.415236) (xy 20.715893 53.328789) (xy 20.70501 53.201)
			)
		)
	)
	(zone
		(net 100)
		(net_name "RGB_LED_CLOCK")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.639871 38.703022) (xy 33.70917 38.783312) (xy 33.74507 38.849734) (xy 33.764236 38.915276)
				(xy 33.783334 38.992926) (xy 33.81903 39.095671) (xy 34.050707 39.000707) (xy 34.145671 38.76903)
				(xy 34.042926 38.733334) (xy 33.965276 38.714236) (xy 33.899734 38.69507) (xy 33.833312 38.65917)
				(xy 33.753022 38.589871)
			)
		)
	)
	(zone
		(net 30)
		(net_name "USB_D+")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.010679 32.883353) (xy 34.09566 32.817473) (xy 34.17005 32.796848) (xy 34.246121 32.80389)
				(xy 34.336147 32.821012) (xy 34.4524 32.830628) (xy 34.453107 32.529921) (xy 34.240268 32.318496)
				(xy 34.147484 32.424105) (xy 34.093209 32.508967) (xy 34.051769 32.586913) (xy 33.997494 32.671775)
				(xy 33.904712 32.777386)
			)
		)
	)
	(zone
		(net 24)
		(net_name "SWD_IO")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 30.8 39.38001) (xy 30.905775 39.387781) (xy 30.978128 39.409364) (xy 31.038026 39.442156) (xy 31.106437 39.483558)
				(xy 31.204329 39.53097) (xy 31.301 39.3) (xy 31.204329 39.06903) (xy 31.106437 39.11644) (xy 31.038026 39.157842)
				(xy 30.978128 39.190635) (xy 30.905775 39.212217) (xy 30.8 39.21999)
			)
		)
	)
	(zone
		(net 4)
		(net_name "SPI_2_SDI")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 39.71999 55.368566) (xy 39.714936 55.475954) (xy 39.702886 55.55169) (xy 39.688503 55.616875)
				(xy 39.676453 55.692611) (xy 39.6714 55.8) (xy 39.9 55.801) (xy 40.061645 55.638355) (xy 39.998599 55.581752)
				(xy 39.948034 55.540548) (xy 39.910828 55.500665) (xy 39.887861 55.44803) (xy 39.88001 55.368566)
			)
		)
	)
	(zone
		(net 31)
		(net_name "USB_D-")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.697739 32.023854) (xy 33.675911 32.128304) (xy 33.617766 32.180884) (xy 33.534308 32.210703)
				(xy 33.43654 32.24687) (xy 33.335468 32.318496) (xy 33.5476 32.531628) (xy 33.8476 32.530628) (xy 33.847599 32.404948)
				(xy 33.847599 32.315755) (xy 33.847599 32.238726) (xy 33.847599 32.149533) (xy 33.847599 32.023854)
			)
		)
	)
	(zone
		(net 51)
		(net_name "AMBIENT_THERMISTOR")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.680839 11.067688) (xy 20.598174 10.969631) (xy 20.558015 10.887535) (xy 20.53882 10.806218)
				(xy 20.51905 10.710498) (xy 20.477164 10.585195) (xy 20.199293 10.699293) (xy 20.085195 10.977164)
				(xy 20.210498 11.01905) (xy 20.306218 11.03882) (xy 20.387535 11.058015) (xy 20.469631 11.098174)
				(xy 20.567688 11.180839)
			)
		)
	)
	(zone
		(net 50)
		(net_name "HEATBREAK_THERMISTOR")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.4064 45.16999) (xy 38.321156 45.165139) (xy 38.262027 45.151129) (xy 38.212655 45.128772)
				(xy 38.156686 45.098881) (xy 38.077761 45.062268) (xy 37.999 45.25) (xy 38.077761 45.437732) (xy 38.156686 45.401118)
				(xy 38.212655 45.371226) (xy 38.262027 45.34887) (xy 38.321156 45.33486) (xy 38.4064 45.33001)
			)
		)
	)
	(zone
		(net 54)
		(net_name "+5V5")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 34.826776 18.881092) (xy 34.752636 18.947876) (xy 34.694246 18.98873) (xy 34.641106 19.02094)
				(xy 34.582717 19.061794) (xy 34.508579 19.128579) (xy 34.649293 19.270707) (xy 34.791421 19.411421)
				(xy 34.858205 19.337282) (xy 34.899058 19.278892) (xy 34.931268 19.225752) (xy 34.972122 19.167362)
				(xy 35.038908 19.093224)
			)
		)
	)
	(zone
		(net 100)
		(net_name "RGB_LED_CLOCK")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 15.88001 4.75) (xy 15.887781 4.644223) (xy 15.909364 4.57187) (xy 15.942156 4.511972) (xy 15.983558 4.443562)
				(xy 16.03097 4.345671) (xy 15.8 4.249) (xy 15.56903 4.345671) (xy 15.61644 4.443562) (xy 15.657842 4.511972)
				(xy 15.690635 4.57187) (xy 15.712217 4.644223) (xy 15.71999 4.75)
			)
		)
	)
	(zone
		(net 7)
		(net_name "ADS1220_DRDY")
		(layer "In2.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.450839 55.147688) (xy 20.368174 55.049631) (xy 20.328015 54.967535) (xy 20.30882 54.886218)
				(xy 20.28905 54.790498) (xy 20.247164 54.665195) (xy 19.969293 54.779293) (xy 19.855195 55.057164)
				(xy 19.980498 55.09905) (xy 20.076218 55.11882) (xy 20.157535 55.138015) (xy 20.239631 55.178174)
				(xy 20.337688 55.260839)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 17.46 54.16) (xy 17.455988 54.28452) (xy 17.442878 54.3724) (xy 17.419058 54.446539) (xy 17.382914 54.529837)
				(xy 17.332836 54.645195) (xy 17.61 54.761) (xy 17.887164 54.645195) (xy 17.837084 54.529837) (xy 17.800941 54.446539)
				(xy 17.777121 54.3724) (xy 17.764011 54.28452) (xy 17.76 54.16)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.76 29.87) (xy 18.784718 29.842264) (xy 18.712054 29.781384) (xy 18.599313 29.720853) (xy 18.503804 29.694163)
				(xy 18.482836 29.734805) (xy 18.761 29.62) (xy 18.482836 29.734805) (xy 18.567314 29.778134) (xy 18.684241 29.697821)
				(xy 18.786645 29.559363) (xy 18.827555 29.428256) (xy 18.76 29.37)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+24V")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 36.3 19.75) (xy 36.188299 19.7474) (xy 36.109149 19.7412) (xy 36.040849 19.7338) (xy 35.961699 19.7276)
				(xy 35.85 19.725) (xy 35.849 19.95) (xy 35.85 20.175) (xy 35.961699 20.1724) (xy 36.040849 20.1662)
				(xy 36.109149 20.1588) (xy 36.188299 20.1526) (xy 36.3 20.15)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 24.680839 3.167688) (xy 24.598174 3.069631) (xy 24.558015 2.987535) (xy 24.53882 2.906218) (xy 24.51905 2.810498)
				(xy 24.477164 2.685195) (xy 24.199293 2.799293) (xy 24.085195 3.077164) (xy 24.210498 3.11905) (xy 24.306218 3.13882)
				(xy 24.387535 3.158015) (xy 24.469631 3.198174) (xy 24.567688 3.280839)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.46 29.87) (xy 19.609099 29.8752) (xy 19.714549 29.8876) (xy 19.805449 29.9024) (xy 19.9109 29.9148)
				(xy 20.06 29.92) (xy 20.061 29.62) (xy 20.06 29.32) (xy 19.9109 29.3252) (xy 19.805449 29.3376)
				(xy 19.714549 29.3524) (xy 19.609099 29.3648) (xy 19.46 29.37)
			)
		)
	)
	(zone
		(net 36)
		(net_name "+3V3")
		(layer "In3.Cu")
		(name "3.3V Fill")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 1.9 2.1) (xy 57.9 2.1) (xy 57.9 58.1) (xy 1.9 58.1)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 42.7 27.95) (xy 42.802936 27.950846) (xy 42.876533 27.955777) (xy 42.939095 27.968382) (xy 43.008926 27.99225)
				(xy 43.104329 28.03097) (xy 43.201 27.8) (xy 43.104329 27.56903) (xy 43.008926 27.607748) (xy 42.939095 27.631616)
				(xy 42.876533 27.644222) (xy 42.802936 27.649153) (xy 42.7 27.65)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.232312 3.280839) (xy 28.330368 3.198174) (xy 28.412464 3.158015) (xy 28.493781 3.13882) (xy 28.5895 3.11905)
				(xy 28.714805 3.077164) (xy 28.600707 2.799293) (xy 28.322836 2.685195) (xy 28.280948 2.810498)
				(xy 28.261178 2.906218) (xy 28.241984 2.987535) (xy 28.201825 3.069631) (xy 28.119161 3.167688)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 18.175 48.6) (xy 18.170988 48.72452) (xy 18.157878 48.8124) (xy 18.134058 48.886539) (xy 18.097914 48.969837)
				(xy 18.047836 49.085195) (xy 18.325 49.201) (xy 18.602164 49.085195) (xy 18.552084 48.969837) (xy 18.515941 48.886539)
				(xy 18.492121 48.8124) (xy 18.479011 48.72452) (xy 18.475 48.6)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.847487 54.59896) (xy 9.73838 54.700711) (xy 9.655047 54.766508) (xy 9.580306 54.820319) (xy 9.496973 54.886115)
				(xy 9.387868 54.987868) (xy 9.599293 55.200707) (xy 9.812132 55.412132) (xy 9.913883 55.303025)
				(xy 9.97968 55.219692) (xy 10.033491 55.144951) (xy 10.099287 55.061618) (xy 10.20104 54.952513)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.15 21.678077) (xy 7.15 21.559513) (xy 7.15 21.475371) (xy 7.15 21.402704) (xy 7.15 21.318562)
				(xy 7.15 21.2) (xy 6.9 21.199) (xy 6.66903 21.295671) (xy 6.718935 21.390179) (xy 6.767701 21.453782)
				(xy 6.809612 21.508371) (xy 6.83895 21.575839) (xy 6.85 21.678077)
			)
		)
	)
	(zone
		(net 33)
		(net_name "+5VA")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.41 29.87) (xy 19.434718 29.842264) (xy 19.362054 29.781384) (xy 19.249313 29.720853) (xy 19.153804 29.694163)
				(xy 19.132836 29.734805) (xy 19.411 29.62) (xy 19.132836 29.734805) (xy 19.217314 29.778134) (xy 19.334241 29.697821)
				(xy 19.436645 29.559363) (xy 19.477555 29.428256) (xy 19.41 29.37)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+24V")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.3 24.134486) (xy 33.150008 24.124086) (xy 33.045004 24.099286) (xy 32.954995 24.069686) (xy 32.849991 24.044886)
				(xy 32.7 24.034486) (xy 32.699 24.334486) (xy 32.7 24.634486) (xy 32.849991 24.624086) (xy 32.954995 24.599286)
				(xy 33.045004 24.569686) (xy 33.150008 24.544886) (xy 33.3 24.534486)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.41967 28.881802) (xy 9.504882 28.972688) (xy 9.557753 29.044098) (xy 9.593333 29.113365) (xy 9.626676 29.197823)
				(xy 9.672836 29.314805) (xy 9.950707 29.200707) (xy 10.064805 28.922836) (xy 9.947823 28.876676)
				(xy 9.863365 28.843333) (xy 9.794098 28.807753) (xy 9.722688 28.754882) (xy 9.631802 28.66967)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "In3.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.712132 15.2) (xy 20.599124 15.099151) (xy 20.507388 15.042542) (xy 20.417424 15.00864) (xy 20.309729 14.975914)
				(xy 20.164805 14.922836) (xy 20.049293 15.199293) (xy 20.05 15.5) (xy 20.169269 15.475299) (xy 20.260749 15.422384)
				(xy 20.337594 15.373032) (xy 20.412959 15.359022) (xy 20.5 15.412132)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 42.669162 4.832312) (xy 42.751826 4.930368) (xy 42.791985 5.012464) (xy 42.811179 5.093781)
				(xy 42.830949 5.1895) (xy 42.872837 5.314805) (xy 43.150708 5.200707) (xy 43.264806 4.922836) (xy 43.139501 4.880948)
				(xy 43.043782 4.861178) (xy 42.962465 4.841984) (xy 42.880369 4.801825) (xy 42.782313 4.719161)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/FAN0_MOSFET_GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.519161 18.732312) (xy 50.601825 18.830368) (xy 50.641984 18.912464) (xy 50.661178 18.993781)
				(xy 50.680948 19.0895) (xy 50.722836 19.214805) (xy 51.000707 19.100707) (xy 51.114805 18.822836)
				(xy 50.9895 18.780948) (xy 50.893781 18.761178) (xy 50.812464 18.741984) (xy 50.730368 18.701825)
				(xy 50.632312 18.619161)
			)
		)
	)
	(zone
		(net 8)
		(net_name "USB_PULL_UP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.607383 3.077589) (xy 20.523405 2.989454) (xy 20.469781 2.921029) (xy 20.432625 2.854932)
				(xy 20.398048 2.773781) (xy 20.352164 2.660195) (xy 20.074293 2.774293) (xy 19.960195 3.052164)
				(xy 20.085329 3.092189) (xy 20.18196 3.10804) (xy 20.264577 3.122585) (xy 20.347673 3.158693) (xy 20.445738 3.239234)
			)
		)
	)
	(zone
		(net 103)
		(net_name "DOTSTAR_LED_DATA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.956057 43.519208) (xy 28.012903 43.582913) (xy 28.044807 43.63463) (xy 28.063909 43.685349)
				(xy 28.082349 43.746062) (xy 28.112268 43.827761) (xy 28.300707 43.750707) (xy 28.377761 43.562268)
				(xy 28.296062 43.532349) (xy 28.235349 43.513909) (xy 28.18463 43.494807) (xy 28.132913 43.462903)
				(xy 28.069208 43.406057)
			)
		)
	)
	(zone
		(net 103)
		(net_name "DOTSTAR_LED_DATA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 13.28001 30.35) (xy 13.287781 30.244223) (xy 13.309364 30.17187) (xy 13.342156 30.111972) (xy 13.383558 30.043562)
				(xy 13.43097 29.945671) (xy 13.2 29.849) (xy 12.96903 29.945671) (xy 13.01644 30.043562) (xy 13.057842 30.111972)
				(xy 13.090635 30.17187) (xy 13.112217 30.244223) (xy 13.11999 30.35)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/FAN0_MOSFET_GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22.880839 3.167688) (xy 22.798174 3.069631) (xy 22.758015 2.987535) (xy 22.73882 2.906218) (xy 22.71905 2.810498)
				(xy 22.677164 2.685195) (xy 22.399293 2.799293) (xy 22.285195 3.077164) (xy 22.410498 3.11905) (xy 22.506218 3.13882)
				(xy 22.587535 3.158015) (xy 22.669631 3.198174) (xy 22.767688 3.280839)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.4357 47.7936) (xy 33.434248 47.877499) (xy 33.428408 47.937217) (xy 33.41595 47.987849) (xy 33.394646 48.044491)
				(xy 33.362268 48.122239) (xy 33.55 48.201) (xy 33.737732 48.122239) (xy 33.705352 48.044491) (xy 33.684048 47.987849)
				(xy 33.671591 47.937217) (xy 33.665751 47.877499) (xy 33.6643 47.7936)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/FAN1_MOSFET_GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 50.51999 30.565685) (xy 50.530333 30.709228) (xy 50.559132 30.807539) (xy 50.603045 30.888991)
				(xy 50.658728 30.981955) (xy 50.722836 31.114805) (xy 51 31.001) (xy 51.114805 30.722836) (xy 50.987576 30.694714)
				(xy 50.869496 30.695877) (xy 50.77155 30.695386) (xy 50.704726 30.662302) (xy 50.68001 30.565685)
			)
		)
	)
	(zone
		(net 104)
		(net_name "DOTSTAR_LED_CLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 11.98001 29.05) (xy 11.987781 28.944223) (xy 12.009364 28.87187) (xy 12.042156 28.811972) (xy 12.083558 28.743562)
				(xy 12.13097 28.645671) (xy 11.9 28.549) (xy 11.66903 28.645671) (xy 11.71644 28.743562) (xy 11.757842 28.811972)
				(xy 11.790635 28.87187) (xy 11.812217 28.944223) (xy 11.81999 29.05)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 38.4 47.8857) (xy 38.295813 47.881296) (xy 38.222763 47.867822) (xy 38.161374 47.844882) (xy 38.092169 47.812083)
				(xy 37.995671 47.76903) (xy 37.899 48) (xy 37.995671 48.23097) (xy 38.092169 48.187915) (xy 38.161374 48.155116)
				(xy 38.222763 48.132177) (xy 38.295813 48.118703) (xy 38.4 48.1143)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/+FANV_INPUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.080839 3.167688) (xy 28.998174 3.069631) (xy 28.958015 2.987535) (xy 28.93882 2.906218) (xy 28.91905 2.810498)
				(xy 28.877164 2.685195) (xy 28.599293 2.799293) (xy 28.485195 3.077164) (xy 28.610498 3.11905) (xy 28.706218 3.13882)
				(xy 28.787535 3.158015) (xy 28.869631 3.198174) (xy 28.967688 3.280839)
			)
		)
	)
	(zone
		(net 14)
		(net_name "NRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 30.1143 9.5) (xy 30.121836 9.37397) (xy 30.143424 9.286751) (xy 30.17753 9.214027) (xy 30.222621 9.131484)
				(xy 30.277164 9.014805) (xy 30 8.899) (xy 29.722836 9.014805) (xy 29.777378 9.131484) (xy 29.822469 9.214027)
				(xy 29.856575 9.286751) (xy 29.878163 9.37397) (xy 29.8857 9.5)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/FAN1_MOSFET_GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.178839 3.174698) (xy 27.096174 3.076641) (xy 27.056015 2.994545) (xy 27.03682 2.913228) (xy 27.01705 2.817508)
				(xy 26.975164 2.692205) (xy 26.697293 2.806303) (xy 26.583195 3.084174) (xy 26.708498 3.12606) (xy 26.804218 3.14583)
				(xy 26.885535 3.165025) (xy 26.967631 3.205184) (xy 27.065688 3.287849)
			)
		)
	)
	(zone
		(net 8)
		(net_name "USB_PULL_UP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 33.465624 35.927269) (xy 33.536181 36.004053) (xy 33.578307 36.065235) (xy 33.605495 36.124864)
				(xy 33.631238 36.196992) (xy 33.66903 36.295671) (xy 33.900707 36.200707) (xy 33.995671 35.96903)
				(xy 33.896992 35.931238) (xy 33.824864 35.905495) (xy 33.765235 35.878307) (xy 33.704053 35.836181)
				(xy 33.627269 35.765624)
			)
		)
	)
	(zone
		(net 2)
		(net_name "FILAMENT_SW")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.7143 18.2) (xy 10.721836 18.07397) (xy 10.743424 17.986751) (xy 10.77753 17.914027) (xy 10.822621 17.831484)
				(xy 10.877164 17.714805) (xy 10.6 17.599) (xy 10.322836 17.714805) (xy 10.377378 17.831484) (xy 10.422469 17.914027)
				(xy 10.456575 17.986751) (xy 10.478163 18.07397) (xy 10.4857 18.2)
			)
		)
	)
	(zone
		(net 104)
		(net_name "DOTSTAR_LED_CLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.769208 44.593943) (xy 28.832913 44.537096) (xy 28.88463 44.505192) (xy 28.935349 44.48609)
				(xy 28.996062 44.46765) (xy 29.077761 44.437732) (xy 29.000707 44.249293) (xy 28.812268 44.172239)
				(xy 28.782349 44.253936) (xy 28.763909 44.314649) (xy 28.744807 44.365368) (xy 28.712903 44.417085)
				(xy 28.656057 44.480792)
			)
		)
	)
	(zone
		(net 66)
		(net_name "HOTEND_THERMISTOR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 48.627269 47.234376) (xy 48.704053 47.163818) (xy 48.765235 47.121692) (xy 48.824864 47.094503)
				(xy 48.896992 47.06876) (xy 48.995671 47.03097) (xy 48.900707 46.799293) (xy 48.66903 46.704329)
				(xy 48.631238 46.803007) (xy 48.605495 46.875135) (xy 48.578307 46.934764) (xy 48.536181 46.995945)
				(xy 48.465624 47.072731)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(name "Guard Ring Keep Out")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
			(hatch_thickness 1)
			(hatch_gap 1.5)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 2 2) (xy 58 2) (xy 58 58) (xy 2 58)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(locked yes)
		(layers "*.Mask")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 0 20.1) (xy 0 19.4) (xy 0 15.9) (xy 0 15.1) (xy 0 0) (xy 60 0) (xy 60 60) (xy 0 60)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(name "Guard Ring Keep Out Top Layer")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
			(hatch_thickness 1)
			(hatch_gap 1.5)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 1.892003 19.500239) (xy 0.1 19.500318) (xy 0.1 8.501048) (xy 1.909593 8.500993) (xy 1.92 1.991934)
				(xy 34.6 2.001527) (xy 34.6 0) (xy 50.2 0) (xy 50.2 2) (xy 58 2) (xy 57.995729 8.4) (xy 59.9 8.4)
				(xy 59.9 51.55) (xy 58 51.55) (xy 58 58.1) (xy 1.9 58.1) (xy 1.9 51.9) (xy 0.1 51.9) (xy 0.1 39.35)
				(xy 1.9 39.35) (xy 1.9 35.45) (xy 0.1 35.45) (xy 0.1 22.9) (xy 1.886569 22.9)
			)
		)
	)
)
