(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 72)
    (no_connects 0)
    (area 162.149999 43.549999 208.050001 89.350001)
    (thickness 1.6)
    (drawings 8)
    (tracks 558)
    (zones 0)
    (modules 32)
    (nets 45)
  )
  (page A4)
  (title_block
    (title "Water Leak Detector")
    (date 2018-03-29)
    (rev 0)
    (company "Author: Thong Huynh")
    (comment 1 "Team Naura - WSU")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00c3f_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/Users/Thong_Huynh/Desktop/EE 416/pics/"))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 RST)
  (net 3 AVCC)
  (net 4 GND)
  (net 5 "Net-(C2-Pad1)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 XTAL1)
  (net 8 XTAL2)
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 PB6)
  (net 12 PB7)
  (net 13 PB5)
  (net 14 PD1)
  (net 15 PD0)
  (net 16 PA0)
  (net 17 PA1)
  (net 18 PA2)
  (net 19 PA3)
  (net 20 PA4)
  (net 21 PA5)
  (net 22 PA6)
  (net 23 PB0)
  (net 24 PB1)
  (net 25 PB2)
  (net 26 PB3)
  (net 27 PB4)
  (net 28 PC0)
  (net 29 PC1)
  (net 30 PC2)
  (net 31 PC3)
  (net 32 PC4)
  (net 33 PC5)
  (net 34 PC6)
  (net 35 PC7)
  (net 36 PD2)
  (net 37 PD3)
  (net 38 PD4)
  (net 39 PD5)
  (net 40 /SIGNAL)
  (net 41 PD7)
  (net 42 PROBE)
  (net 43 "Net-(Q1-Pad2)")
  (net 44 /ANALOG_SIGNAL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ANALOG_SIGNAL)
    (add_net /SIGNAL)
    (add_net AVCC)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net PA0)
    (add_net PA1)
    (add_net PA2)
    (add_net PA3)
    (add_net PA4)
    (add_net PA5)
    (add_net PA6)
    (add_net PB0)
    (add_net PB1)
    (add_net PB2)
    (add_net PB3)
    (add_net PB4)
    (add_net PB5)
    (add_net PB6)
    (add_net PB7)
    (add_net PC0)
    (add_net PC1)
    (add_net PC2)
    (add_net PC3)
    (add_net PC4)
    (add_net PC5)
    (add_net PC6)
    (add_net PC7)
    (add_net PD0)
    (add_net PD1)
    (add_net PD2)
    (add_net PD3)
    (add_net PD4)
    (add_net PD5)
    (add_net PD7)
    (add_net PROBE)
    (add_net RST)
    (add_net VCC)
    (add_net XTAL1)
    (add_net XTAL2)
  )
  (module robosub_footprints:robosub_logo-medium (layer F.Cu) (tedit 5ABDB71C)
    (at 202 66.1 90)
    (fp_text reference "" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Diodes_SMD:D_MELF-RM10_Universal_Handsoldering (layer F.Cu) (tedit 5905D8D3)
    (at 195.07 77.84)
    (descr "Diode, Universal, MELF, RM10, Handsoldering, SMD, Thruhole,")
    (tags "Diode Universal MELF RM10 Handsoldering SMD Thruhole ")
    (fp_text reference 1N4148 (at 0 -2.5) (layer F.SilkS))
    (fp_text value D1 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at -5 0) (size 4.5 2.7) (drill 1.19888 (offset 1.1 0)) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole rect (at 5 0 180) (size 4.5 2.7) (drill 1.19888 (offset 1.1 0)) (layers *.Cu *.Mask)
      (net 2 RST))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ABDAF87)
    (at 197.7 67.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.11 -1.4 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at -0.12 0.03 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 AVCC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ABDB05A)
    (at 192.1 63.75 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.05 1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0.07 -0.04 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ABD8740)
    (at 172 52.85)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.1 -3.05) (layer F.SilkS))
    (fp_text value 10uF (at -1.5 1.2) (layer F.Fab))
    (fp_text user %R (at -0.05 -1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ABD8725)
    (at 172 51 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0.1 -2.95 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.05 -0.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ABDAFA4)
    (at 181.3 57.85)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -0.17 -1.36) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at -0.04 0.02) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 XTAL1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ABDAC5C)
    (at 186.25 57.35)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.07 -1.04) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 XTAL2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 180.63 50.19)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED_Small (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 5ABDB054)
    (at 195.65 63.1 90)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D2 (at -0.04 1.83 90) (layer F.SilkS))
    (fp_text value LED_Small (at 0 1.55 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 595FCA25)
    (at 169.55 77.15 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D3 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /ANALOG_SIGNAL))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch1.27mm (layer F.Cu) (tedit 5ABDB04B)
    (at 195.05 56.2)
    (descr "Through hole straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 1.27mm double row")
    (fp_text reference J1 (at 0.87 4.21) (layer F.SilkS))
    (fp_text value AVR_ISP (at 0.635 4.235) (layer F.Fab))
    (fp_text user %R (at 0.635 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 PB6))
    (pad 2 thru_hole oval (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 PB7))
    (pad 4 thru_hole oval (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 PB5))
    (pad 5 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 RST))
    (pad 6 thru_hole oval (at 1.27 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.00mm (layer F.Cu) (tedit 5ABDC99E)
    (at 205.75 73.01)
    (descr "Through hole straight pin header, 1x08, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.00mm single row")
    (fp_text reference J3 (at 0.1 -2.6) (layer F.SilkS))
    (fp_text value PortA (at 0.15 8.59 90) (layer F.Fab))
    (fp_text user %R (at 0 7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /ANALOG_SIGNAL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.00mm (layer F.Cu) (tedit 5ABDB0C4)
    (at 205.7 45.83)
    (descr "Through hole straight pin header, 1x08, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.00mm single row")
    (fp_text reference J4 (at 0 16.61) (layer F.SilkS))
    (fp_text value PortB (at 0.27 3.9 90) (layer F.Fab))
    (fp_text user %R (at 0 7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 PB0))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 PB4))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 PB5))
    (pad 7 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 PB6))
    (pad 8 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 PB7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.00mm (layer F.Cu) (tedit 5ABDB0C8)
    (at 164.32 45.71)
    (descr "Through hole straight pin header, 1x08, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.00mm single row")
    (fp_text reference J5 (at 0.11 16.71) (layer F.SilkS))
    (fp_text value PortC (at 0.06 3.1 90) (layer F.Fab))
    (fp_text user %R (at 0 7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.00mm (layer F.Cu) (tedit 5ABDB0CC)
    (at 164.37 72.9)
    (descr "Through hole straight pin header, 1x08, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.00mm single row")
    (fp_text reference J6 (at 0 -2.06) (layer F.SilkS))
    (fp_text value PortD (at -0.08 10.14 90) (layer F.Fab))
    (fp_text user %R (at 0 7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 PD0))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 PD1))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /SIGNAL))
    (pad 8 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm (layer F.Cu) (tedit 5ABDAAA9)
    (at 197.9 45.79 90)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J8 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Power (at -2.27 0.61 180) (layer F.Fab))
    (fp_text user %R (at 0 1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer F.Cu) (tedit 5ABDAF8C)
    (at 195.65 67.45 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at -0.02 1.55 270) (layer F.SilkS))
    (fp_text value 10uH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 AVCC))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_GH_SM02B-GHS-TB_02x1.25mm_Angled (layer F.Cu) (tedit 5ABDB0D4)
    (at 180.7 84.95)
    (descr "JST GH series connector, SM02B-GHS-TB, side entry type")
    (tags "connector jst GH SMT side horizontal entry 1.25mm pitch")
    (attr smd)
    (fp_text reference P1 (at 0 -3.8) (layer F.SilkS))
    (fp_text value Probe_Port (at 0.52 1.16) (layer F.Fab))
    (fp_text user %R (at 0 0.45) (layer F.Fab))
    (pad 1 smd rect (at -0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 42 PROBE))
    (pad "" smd rect (at 2.35 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.35 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_JST:JST_GH_SM02B-GHS-TB_02x1.25mm_Angled (layer F.Cu) (tedit 5ABDB0D2)
    (at 172.6 85)
    (descr "JST GH series connector, SM02B-GHS-TB, side entry type")
    (tags "connector jst GH SMT side horizontal entry 1.25mm pitch")
    (attr smd)
    (fp_text reference P2 (at 0 -3.8) (layer F.SilkS))
    (fp_text value Probe_Port (at 0.32 0.94) (layer F.Fab))
    (fp_text user %R (at 0 0.45) (layer F.Fab))
    (pad 1 smd rect (at -0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 42 PROBE))
    (pad "" smd rect (at 2.35 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.35 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 178 77.1)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 40 /SIGNAL))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5ABDAC6A)
    (at 186.4 54.95)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.02 -1.17) (layer F.SilkS))
    (fp_text value 330R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 PB0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 188.9 75.15)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 220 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5ABDA1F6)
    (at 188.75 80.55)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.01 1.54 180) (layer F.SilkS))
    (fp_text value 10K (at -3.59 0.48) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5ABDB06C)
    (at 183 76.35 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.07 1.54 90) (layer F.SilkS))
    (fp_text value 1k (at -0.01 -1.47 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /SIGNAL))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 175.4 76.55 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /SIGNAL))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 /ANALOG_SIGNAL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 174.1 72.75)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 27k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 172.65 77 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 PROBE))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 5ABDC6E3)
    (at 189.96 47.69)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference S1 (at -0.06 4.01) (layer F.SilkS))
    (fp_text value SW_Push (at 0.14 1.4) (layer F.Fab))
    (fp_text user %R (at -0.11 -0.3) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad 1 smd rect (at -3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ATMEGA1284P-AU:QFP80P1200X1200X120-44N (layer F.Cu) (tedit 5ABDC7D3)
    (at 184.45 65.5)
    (attr smd)
    (fp_text reference U1 (at 0.00001 9.05685) (layer F.SilkS))
    (fp_text value ATMEGA1284P-AU (at 2.55 -12.1) (layer F.SilkS))
    (pad 1 smd rect (at -5.7404 -3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 13 PB5))
    (pad 2 smd rect (at -5.7404 -3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 11 PB6))
    (pad 3 smd rect (at -5.7404 -2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 12 PB7))
    (pad 4 smd rect (at -5.7404 -1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad 5 smd rect (at -5.7404 -0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 6 smd rect (at -5.7404 0 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at -5.7404 0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 8 XTAL2))
    (pad 8 smd rect (at -5.7404 1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 7 XTAL1))
    (pad 9 smd rect (at -5.7404 2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 15 PD0))
    (pad 10 smd rect (at -5.7404 3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 14 PD1))
    (pad 11 smd rect (at -5.7404 3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 36 PD2))
    (pad 12 smd rect (at -3.9878 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 37 PD3))
    (pad 13 smd rect (at -3.2004 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 38 PD4))
    (pad 14 smd rect (at -2.3876 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 39 PD5))
    (pad 15 smd rect (at -1.6002 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 40 /SIGNAL))
    (pad 16 smd rect (at -0.7874 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 41 PD7))
    (pad 17 smd rect (at 0 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 18 smd rect (at 0.7874 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 19 smd rect (at 1.6002 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 28 PC0))
    (pad 20 smd rect (at 2.3876 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 29 PC1))
    (pad 21 smd rect (at 3.2004 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 30 PC2))
    (pad 22 smd rect (at 3.9878 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 31 PC3))
    (pad 23 smd rect (at 5.7404 3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 32 PC4))
    (pad 24 smd rect (at 5.7404 3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 33 PC5))
    (pad 25 smd rect (at 5.7404 2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 34 PC6))
    (pad 26 smd rect (at 5.7404 1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 35 PC7))
    (pad 27 smd rect (at 5.7404 0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 AVCC))
    (pad 28 smd rect (at 5.7404 0 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 29 smd rect (at 5.7404 -0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad1)"))
    (pad 30 smd rect (at 5.7404 -1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 44 /ANALOG_SIGNAL))
    (pad 31 smd rect (at 5.7404 -2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 22 PA6))
    (pad 32 smd rect (at 5.7404 -3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 21 PA5))
    (pad 33 smd rect (at 5.7404 -3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 20 PA4))
    (pad 34 smd rect (at 3.9878 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 19 PA3))
    (pad 35 smd rect (at 3.2004 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 18 PA2))
    (pad 36 smd rect (at 2.3876 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 17 PA1))
    (pad 37 smd rect (at 1.6002 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 16 PA0))
    (pad 38 smd rect (at 0.7874 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 39 smd rect (at 0 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 40 smd rect (at -0.7874 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 23 PB0))
    (pad 41 smd rect (at -1.6002 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 24 PB1))
    (pad 42 smd rect (at -2.3876 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 25 PB2))
    (pad 43 smd rect (at -3.2004 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 26 PB3))
    (pad 44 smd rect (at -3.9878 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 27 PB4))
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 169.7 66.85 90)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.44 -3.525 90) (layer F.SilkS))
    (fp_text value 16MHz (at 2.44 3.525 90) (layer F.Fab))
    (fp_text user %R (at 2.44 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 XTAL1))
    (pad 2 thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 XTAL2))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5ABDA133)
    (at 168.9 46.1 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0.22 -2.43 90) (layer F.SilkS))
    (fp_text value FTDI (at 0.15 15.24 90) (layer F.Fab))
    (fp_text user J2 (at 0.1 6.2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 PD1))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 PD0))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text "EE 416 - Spring 2018\nMentors:\nAaron Darnton\nAlex Read\n\nCo-mentor:\nDaniel Hubert\n\nFaculty Volunteer:\nAndy O’fallon\n\nProfessor:\nPatrick Pedrow\n" (at 184.3 64.4) (layer B.SilkS))
  (gr_text "Team Naura - WSU:\nThong Huynh\nNicholas Heitman\nHenderson Reaves\nLuke Riske" (at 196.2 85.7) (layer F.SilkS))
  (gr_line (start 162.2 89.3) (end 162.2 43.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 208 89.3) (end 162.2 89.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 208 43.6) (end 208 89.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.2 43.6) (end 208 43.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 45.700438 (width 0.3) (layer F.SilkS)
    (gr_text "45.700 mm" (at 225.84995 66.435777 270.2507458) (layer F.SilkS))
    (feature1 (pts (xy 222.7 89.3) (xy 227.299937 89.279869)))
    (feature2 (pts (xy 222.5 43.6) (xy 227.099937 43.579869)))
    (crossbar (pts (xy 224.399963 43.591685) (xy 224.599963 89.291685)))
    (arrow1a (pts (xy 224.599963 89.291685) (xy 224.008618 88.167758)))
    (arrow1b (pts (xy 224.599963 89.291685) (xy 225.181448 88.162626)))
    (arrow2a (pts (xy 224.399963 43.591685) (xy 223.818478 44.720744)))
    (arrow2b (pts (xy 224.399963 43.591685) (xy 224.991308 44.715612)))
  )
  (dimension 46.000435 (width 0.3) (layer F.SilkS)
    (gr_text "46.000 mm" (at 185.122825 100.849913 0.2491105152) (layer F.SilkS))
    (feature1 (pts (xy 208.1 95.5) (xy 208.128695 102.0999)))
    (feature2 (pts (xy 162.1 95.7) (xy 162.128695 102.2999)))
    (crossbar (pts (xy 162.116956 99.599926) (xy 208.116956 99.399926)))
    (arrow1a (pts (xy 208.116956 99.399926) (xy 206.993013 99.991239)))
    (arrow1b (pts (xy 208.116956 99.399926) (xy 206.987913 98.818409)))
    (arrow2a (pts (xy 162.116956 99.599926) (xy 163.245999 100.181443)))
    (arrow2b (pts (xy 162.116956 99.599926) (xy 163.240899 99.008613)))
  )
)
