(kicad_pcb (version 20171130) (host pcbnew 5.1.7+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 1588)
    (zones 0)
    (modules 64)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.5)
    (user_trace_width 0.762)
    (user_trace_width 1)
    (trace_clearance 0.127)
    (zone_clearance 0.1)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3048)
    (uvia_drill 0.1016)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2.75)
    (pad_drill 0)
    (pad_to_mask_clearance -0.0254)
    (pad_to_paste_clearance -0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 VCC)
  (net 5 Vtrans)
  (net 6 /Transformer/out+)
  (net 7 "Net-(Q1-Pad3)")
  (net 8 /Transformer/in-)
  (net 9 "Net-(Q1-Pad1)")
  (net 10 "Net-(R15-Pad2)")
  (net 11 ~FAULT~)
  (net 12 "Net-(C15-Pad1)")
  (net 13 "Net-(C16-Pad1)")
  (net 14 "Net-(D2-Pad2)")
  (net 15 FIRE)
  (net 16 CHARGE)
  (net 17 CHARGE_IGN)
  (net 18 ~FAULT_5V~)
  (net 19 ~FAULT_IGN_5V~)
  (net 20 Charged)
  (net 21 +5V)
  (net 22 "Net-(Q2-Pad3)")
  (net 23 "Net-(Q2-Pad2)")
  (net 24 "Net-(Q2-Pad1)")
  (net 25 "Net-(Q3-Pad1)")
  (net 26 "Net-(R7-Pad2)")
  (net 27 "Net-(R13-Pad2)")
  (net 28 "Net-(R14-Pad2)")
  (net 29 "Net-(R16-Pad2)")
  (net 30 "Net-(R17-Pad1)")
  (net 31 "Net-(R18-Pad1)")
  (net 32 "Net-(R19-Pad1)")
  (net 33 "Net-(R20-Pad1)")
  (net 34 "Net-(R21-Pad1)")
  (net 35 "Net-(R22-Pad1)")
  (net 36 "Net-(R23-Pad1)")
  (net 37 "Net-(R24-Pad1)")
  (net 38 "Net-(R25-Pad1)")
  (net 39 "Net-(R27-Pad1)")
  (net 40 ~FAULT_IGN~)
  (net 41 "Net-(U3-Pad15)")
  (net 42 "Net-(U3-Pad12)")
  (net 43 "Net-(U3-Pad10)")
  (net 44 CHARGE_IGN_5V)
  (net 45 CHARGE_5V)
  (net 46 FIRE_5V)
  (net 47 "Net-(U4-Pad15)")
  (net 48 "Net-(U4-Pad12)")
  (net 49 "Net-(U4-Pad10)")
  (net 50 "Net-(U4-Pad6)")
  (net 51 "Net-(J3-Pad1)")
  (net 52 "Net-(C17-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net +5V)
    (add_net CHARGE)
    (add_net CHARGE_5V)
    (add_net CHARGE_IGN)
    (add_net CHARGE_IGN_5V)
    (add_net Charged)
    (add_net FIRE)
    (add_net FIRE_5V)
    (add_net GND)
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R27-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad6)")
    (add_net VCC)
    (add_net ~FAULT_5V~)
    (add_net ~FAULT_IGN_5V~)
    (add_net ~FAULT_IGN~)
    (add_net ~FAULT~)
  )
  (net_class "High Current" ""
    (clearance 0.15)
    (trace_width 0.381)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net "Net-(Q1-Pad1)")
  )
  (net_class "High Voltage" ""
    (clearance 5.588)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
  )
  (net_class "High Voltage Low Clearence" ""
    (clearance 1.27)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net /Transformer/out+)
    (add_net "Net-(C1-Pad1)")
  )
  (net_class "Mid Voltage" ""
    (clearance 1.27)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
  )
  (net_class "Mid Voltage Low Clearence" ""
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net /Transformer/in-)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net Vtrans)
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69 140.975 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0.025 -2 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.9 136.775 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 3 0 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 69.5 106)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C9 (at 0 4) (layer F.SilkS))
    (fp_text value 1000uF (at 3.75 10.25) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L31.5mm_W20.0mm_P27.50mm_MKS4 (layer F.Cu) (tedit 5AE50EF0)
    (at 179.5 117.5 270)
    (descr "C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 27.50mm  length 31.5mm width 20mm Capacitor")
    (fp_text reference C2 (at 13.5 0 90) (layer F.SilkS))
    (fp_text value 5uF (at 13.75 11.25 90) (layer F.Fab))
    (fp_text user %R (at 13.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 27.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L31.5mm_W20.0mm_P27.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.025 143.5)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.475 0) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.475 0) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 92.5 142 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C14 (at 6 -4.5 180) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 5.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 103.5 133.225 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 3.275 0 90) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-247-2_Vertical (layer F.Cu) (tedit 5AC86DC3)
    (at 166 118.5 180)
    (descr "TO-247-2, Vertical, RM 10.9mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-2 Vertical RM 10.9mm")
    (fp_text reference D2 (at 5.5 0) (layer F.SilkS))
    (fp_text value NDSH25170A (at 5.45 3.95) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.45) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.9 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:Banana_Jack_2Pin (layer F.Cu) (tedit 5A1AB217)
    (at 212 142.97 90)
    (descr "Dual banana socket, footprint - 2 x 6mm drills")
    (tags "banana socket")
    (fp_text reference J3 (at 14.97 0 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 14.985 6.29 90) (layer F.Fab))
    (fp_text user %R (at 14.985 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 29.97 0 90) (size 10.16 10.16) (drill 6.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 10.16 10.16) (drill 6.1) (layers *.Cu *.Mask)
      (net 51 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector.3dshapes/Banana_Jack_2Pin.wrl
      (offset (xyz 14.98599977493286 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 53 150 180)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J4 (at 2 0) (layer F.SilkS))
    (fp_text value Conn_01x12_Female (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 FIRE_5V))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 CHARGE_5V))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 CHARGE_IGN_5V))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 ~FAULT_5V~))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 ~FAULT_IGN_5V~))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 Charged))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 +5V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-264-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 123 136 270)
    (descr "TO-264-3, Vertical, RM 5.45mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf")
    (tags "TO-264-3 Vertical RM 5.45mm")
    (fp_text reference Q2 (at 5.5 4.5 90) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 5.45 4.35 90) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.02 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.9 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 22 "Net-(Q2-Pad3)"))
    (pad 2 thru_hole oval (at 5.45 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 23 "Net-(Q2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-264-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-247-3_Vertical (layer F.Cu) (tedit 5AC86DC3)
    (at 198.5 148.4 90)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (fp_text reference Q3 (at 5.45 -3.45 90) (layer F.SilkS))
    (fp_text value Q_NIGBT_GCE (at 5.45 3.95 90) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.45 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.9 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.45 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 51 "Net-(J3-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 25 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 113 147.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 4m (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9625 0 90) (size 1.225 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.204082)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9625 0 90) (size 1.225 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.204082)
      (net 22 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 108 147.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 0 90) (layer F.SilkS))
    (fp_text value 4m (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9625 0 90) (size 1.225 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.204082)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9625 0 90) (size 1.225 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.204082)
      (net 22 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 165.5 124.4625 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 2M (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 13 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 112.5 89.2875 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 2.43k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 52 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 106 133.9625 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 4.0375 0 90) (layer B.SilkS))
    (fp_text value 4.87k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 13 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 126.5 139.825 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 36.5k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R14-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 99.5 123.325 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 80.6k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R16-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97 123.4125 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 3.4125 0 90) (layer F.SilkS))
    (fp_text value 453k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 5 Vtrans))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 32 "Net-(R19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.5875 131.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -3.5 0) (layer F.SilkS))
    (fp_text value 453k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 33 "Net-(R20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 94.5 123.4125 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 3.4125 0 90) (layer F.SilkS))
    (fp_text value 1.3M (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 5 Vtrans))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 35 "Net-(R22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.5875 129 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at -3.5875 0) (layer F.SilkS))
    (fp_text value 169k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 37 "Net-(R24-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.575 135.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at -2.93 0.14) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R27-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.57 133.63 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at -2.93 0.13) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 ~FAULT_IGN~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module High_Voltage_Power_Supply:Transformer_Coilcraft_GA3460-BL (layer F.Cu) (tedit 5F9A7045)
    (at 139.5 136)
    (fp_text reference TR3 (at 0 0) (layer F.SilkS))
    (fp_text value GA3460-BL (at 0 2) (layer F.Fab))
    (pad 12 smd rect (at -10 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 11 smd rect (at -6 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 10 smd rect (at -2 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 9 smd rect (at 2 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 8 smd rect (at 6 -14.7) (size 2 2.75) (layers Dwgs.User))
    (pad 7 smd rect (at 10 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (pad 6 smd rect (at 10 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 6 13.5) (size 2 2.75) (layers Dwgs.User))
    (pad 4 smd rect (at 2 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at -2 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at -6 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -10 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q2-Pad2)"))
  )
  (module Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias (layer F.Cu) (tedit 5A6719D8)
    (at 96.67 135.45 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [HTSSOP], with thermal pad with vias")
    (tags "HTSSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 -4.3 90) (layer F.SilkS))
    (fp_text value LT3751-TSSOP (at 0 4.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 21 thru_hole circle (at -1.3 2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 -1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 -1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 -1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 -2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 -2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad "" smd rect (at -0.85 2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at -0.85 0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at -0.85 -0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 -0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 -2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at -0.85 -2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad 21 smd rect (at 0 0 270) (size 3.4 6.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 -2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 20 smd rect (at 2.95 -2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R14-Pad2)"))
    (pad 19 smd rect (at 2.95 -2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.95 -1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 2.95 -0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.95 -0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.95 0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(Q2-Pad1)"))
    (pad 14 smd rect (at 2.95 0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 13 smd rect (at 2.95 1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 12 smd rect (at 2.95 2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q2-Pad3)"))
    (pad 11 smd rect (at 2.95 2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -2.95 2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C16-Pad1)"))
    (pad 9 smd rect (at -2.95 2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -2.95 1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 CHARGE_IGN))
    (pad 7 smd rect (at -2.95 0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R27-Pad1)"))
    (pad 6 smd rect (at -2.95 0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 ~FAULT_IGN~))
    (pad 5 smd rect (at -2.95 -0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R20-Pad1)"))
    (pad 4 smd rect (at -2.95 -0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R24-Pad1)"))
    (pad 3 smd rect (at -2.95 -1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at -2.95 -2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R19-Pad1)"))
    (pad 1 smd rect (at -2.95 -2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R16-Pad2)"))
    (pad 21 smd rect (at 0 0 270) (size 3.4 6.5) (layers B.Cu)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 63.5 130.905)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0 -5.9) (layer F.SilkS))
    (fp_text value MC14504B (at 0 5.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 15 smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(U3-Pad15)"))
    (pad 14 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(U3-Pad12)"))
    (pad 11 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(U3-Pad10)"))
    (pad 9 smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 CHARGE_IGN_5V))
    (pad 6 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 CHARGE_IGN))
    (pad 5 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CHARGE_5V))
    (pad 4 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 CHARGE))
    (pad 3 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 FIRE_5V))
    (pad 2 smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 FIRE))
    (pad 1 smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 63.525 145.055)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U4 (at 0 -5.9) (layer F.SilkS))
    (fp_text value MC14504B (at 0 5.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +5V))
    (pad 15 smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(U4-Pad15)"))
    (pad 14 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(U4-Pad12)"))
    (pad 11 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(U4-Pad10)"))
    (pad 9 smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(U4-Pad6)"))
    (pad 5 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 ~FAULT_IGN~))
    (pad 4 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 ~FAULT_5V~))
    (pad 3 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 ~FAULT~))
    (pad 2 smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 ~FAULT_IGN_5V~))
    (pad 1 smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:Analog_KS-4 (layer F.Cu) (tedit 5A02FF57)
    (at 69.5 136.85 180)
    (descr "Analog Devices KS-4, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sc70ks/ks_4.pdf")
    (tags "Analog Devices KS-4 (like EIAJ SC-82)")
    (attr smd)
    (fp_text reference U5 (at 0 1.85) (layer F.SilkS))
    (fp_text value ADCMP356 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at 0.825 -0.65 180) (size 0.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 3 smd rect (at 0.825 0.65 180) (size 0.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 Charged))
    (pad 2 smd rect (at -0.825 0.5 180) (size 0.75 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.825 -0.65 180) (size 0.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/Analog_KS-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer B.Cu) (tedit 5A02FF57)
    (at 192.9 149)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U6 (at 0 2.9) (layer B.SilkS))
    (fp_text value ZXGD3004E6 (at 0 -2.9) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 15 FIRE))
    (pad 6 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(Q3-Pad1)"))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(Q3-Pad1)"))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 15 FIRE))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 111 118.5 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C10 (at 0 -4 90) (layer F.SilkS))
    (fp_text value 1000uF (at 3.75 10.25 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 122 123.975 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.3 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 2.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 2.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 118.5 123.975 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.3 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 2.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 2.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 94.0625 81 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 3.0625 0) (layer F.SilkS))
    (fp_text value 169k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(R23-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module High_Voltage_Power_Supply:Transformer_Coilcraft_GA3460-BL (layer F.Cu) (tedit 5F7656F7)
    (at 177 79.7)
    (fp_text reference TR2 (at 0 0) (layer F.SilkS))
    (fp_text value GA3460-BL (at 0 17) (layer F.Fab))
    (pad 12 smd rect (at -10 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 11 smd rect (at -6 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 10 smd rect (at -2 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 9 smd rect (at 2 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 8 smd rect (at 6 -14.7) (size 2 2.75) (layers Dwgs.User))
    (pad 7 smd rect (at 10 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /Transformer/out+))
    (pad 6 smd rect (at 10 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 6 13.5) (size 2 2.75) (layers Dwgs.User))
    (pad 4 smd rect (at 2 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
    (pad 3 smd rect (at -2 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
    (pad 2 smd rect (at -6 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
    (pad 1 smd rect (at -10 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
  )
  (module Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias (layer F.Cu) (tedit 5A6719D8)
    (at 104 86 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [HTSSOP], with thermal pad with vias")
    (tags "HTSSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -4.3 270) (layer F.SilkS))
    (fp_text value LT3751-TSSOP (at 0 4.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 21 thru_hole circle (at -1.3 2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 -1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 -1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 -1.475 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.3 -2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 -2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad "" smd rect (at -0.85 2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at -0.85 0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at -0.85 -0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 -0.7375 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at 0.85 -2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad "" smd rect (at -0.85 -2.2125 270) (size 1.4 1.075) (layers F.Paste))
    (pad 21 smd rect (at 0 0 270) (size 3.4 6.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at -1.3 -2.95 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 20 smd rect (at 2.95 -2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R13-Pad2)"))
    (pad 19 smd rect (at 2.95 -2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.95 -1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 2.95 -0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.95 -0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.95 0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (pad 14 smd rect (at 2.95 0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 13 smd rect (at 2.95 1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 12 smd rect (at 2.95 2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (pad 11 smd rect (at 2.95 2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -2.95 2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C15-Pad1)"))
    (pad 9 smd rect (at -2.95 2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -2.95 1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 CHARGE))
    (pad 7 smd rect (at -2.95 0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R25-Pad1)"))
    (pad 6 smd rect (at -2.95 0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 ~FAULT~))
    (pad 5 smd rect (at -2.95 -0.33 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R18-Pad1)"))
    (pad 4 smd rect (at -2.95 -0.97 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R23-Pad1)"))
    (pad 3 smd rect (at -2.95 -1.62 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at -2.95 -2.27 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R17-Pad1)"))
    (pad 1 smd rect (at -2.95 -2.92 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R15-Pad2)"))
    (pad 21 smd rect (at 0 0 270) (size 3.4 6.5) (layers B.Cu)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module High_Voltage_Power_Supply:Transformer_Coilcraft_GA3460-BL (layer F.Cu) (tedit 5F76571F)
    (at 145 79.7)
    (fp_text reference TR1 (at 0 0) (layer F.SilkS))
    (fp_text value GA3460-BL (at 0 17) (layer F.Fab))
    (pad 12 smd rect (at -10 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 11 smd rect (at -6 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 10 smd rect (at -2 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 9 smd rect (at 2 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 5 Vtrans))
    (pad 8 smd rect (at 6 -14.7) (size 2 2.75) (layers Dwgs.User))
    (pad 7 smd rect (at 10 -14.7) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /Transformer/out+))
    (pad 6 smd rect (at 10 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 6 13.5) (size 2 2.75) (layers Dwgs.User))
    (pad 4 smd rect (at 2 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
    (pad 3 smd rect (at -2 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
    (pad 2 smd rect (at -6 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
    (pad 1 smd rect (at -10 13.5) (size 2 2.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Transformer/in-))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 112.5 83.4 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -3.9 0 270) (layer B.SilkS))
    (fp_text value 2.43k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 52 "Net-(C17-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202 79.4 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 2M (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C15-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202 74.1 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 2M (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 108 67.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 3.5 0 270) (layer B.SilkS))
    (fp_text value 1.3M (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 Vtrans))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R21-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 94.0625 83 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 3.0625 0) (layer F.SilkS))
    (fp_text value 453k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 111.5 67.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 3.4375 0 270) (layer B.SilkS))
    (fp_text value 453k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 Vtrans))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.2125 85 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 3.2125 0) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 ~FAULT~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.2125 87 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 3.2125 0) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R25-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer F.Cu) (tedit 5B301BBD)
    (at 100 105 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 4m (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 7 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer F.Cu) (tedit 5B301BBD)
    (at 105 105 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 4m (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 7 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer F.Cu) (tedit 5B301BBD)
    (at 110 105 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 4m (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 7 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer F.Cu) (tedit 5B301BBD)
    (at 115 105 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 0 90) (layer F.SilkS))
    (fp_text value 4m (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 7 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130 90.7875 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 36.5k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /Transformer/in-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.5 67.2875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -2.7125 0 270) (layer B.SilkS))
    (fp_text value 80.6k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R15-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-264-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 125 94.55 270)
    (descr "TO-264-3, Vertical, RM 5.45mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf")
    (tags "TO-264-3 Vertical RM 5.45mm")
    (fp_text reference Q1 (at 5.45 -3.02 90) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 5.45 4.35 90) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.02 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.9 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 5.45 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 /Transformer/in-))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-264-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:Banana_Jack_2Pin (layer F.Cu) (tedit 5A1AB217)
    (at 212 89.97 90)
    (descr "Dual banana socket, footprint - 2 x 6mm drills")
    (tags "banana socket")
    (fp_text reference J2 (at 14.985 -6.24 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 14.985 6.29 90) (layer F.Fab))
    (fp_text user %R (at 14.985 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 29.97 0 90) (size 10.16 10.16) (drill 6.1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 10.16 10.16) (drill 6.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector.3dshapes/Banana_Jack_2Pin.wrl
      (offset (xyz 14.98599977493286 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:Banana_Jack_2Pin (layer F.Cu) (tedit 5A1AB217)
    (at 80 89.97 90)
    (descr "Dual banana socket, footprint - 2 x 6mm drills")
    (tags "banana socket")
    (fp_text reference J1 (at 14.97 0 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 14.985 6.29 90) (layer F.Fab))
    (fp_text user %R (at 14.985 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 29.97 0 90) (size 10.16 10.16) (drill 6.1) (layers *.Cu *.Mask)
      (net 5 Vtrans))
    (pad 1 thru_hole circle (at 0 0 90) (size 10.16 10.16) (drill 6.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector.3dshapes/Banana_Jack_2Pin.wrl
      (offset (xyz 14.98599977493286 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-247-2_Vertical (layer F.Cu) (tedit 5AC86DC3)
    (at 202 60 180)
    (descr "TO-247-2, Vertical, RM 10.9mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-2 Vertical RM 10.9mm")
    (fp_text reference D1 (at 5.45 0) (layer F.SilkS))
    (fp_text value NDSH25170A (at 5.45 3.95) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.45) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.9 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 /Transformer/out+))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 97.70444 63.5 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C8 (at 2.5 -4.29556 90) (layer F.SilkS))
    (fp_text value 1000uF (at 3.75 10.25 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 120 63.5 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C7 (at 2.5 -5 90) (layer F.SilkS))
    (fp_text value 1000uF (at 3.75 10.25 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer B.Cu) (tedit 5B301BBE)
    (at 125 67.65 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.28 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer B.Cu) (tedit 5B301BBE)
    (at 128.5 67.65 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.28 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 5 Vtrans))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 103 95.6 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 96.75 93 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C13 (at 6.75 -4) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 5.25) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 109.5 82.7125 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -2.7125 0 90) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1812_4532Metric (layer B.Cu) (tedit 5B301BBE)
    (at 212 75 270)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer B.SilkS))
    (fp_text value 2200pF (at 0 -2.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 2.1375 0 270) (size 1.125 3.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.1375 0 270) (size 1.125 3.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text IGN- (at 216.281 149.606) (layer F.SilkS))
  (gr_text IGN+ (at 216.027 106.553) (layer F.SilkS))
  (gr_text GND (at 216.535 96.012) (layer F.SilkS))
  (gr_text 1kV (at 216.662 54.229) (layer F.SilkS))
  (gr_text GND (at 71.247 90.043) (layer F.SilkS))
  (gr_text 48V (at 71.247 60.198) (layer F.SilkS))
  (gr_text GND (at 56.134 149.987) (layer F.SilkS))
  (gr_text "GND\n" (at 56.134 147.447) (layer F.SilkS))
  (gr_text GND (at 56.134 144.907) (layer F.SilkS))
  (gr_text 12V (at 56.007 142.367) (layer F.SilkS))
  (gr_text 12V (at 56.007 139.827) (layer F.SilkS))
  (gr_text 5V (at 55.499 137.287) (layer F.SilkS))
  (gr_text CGD (at 56.134 134.747) (layer F.SilkS))
  (gr_text "F IGN" (at 56.642 132.207) (layer F.SilkS))
  (gr_text Fault (at 56.515 129.667) (layer F.SilkS))
  (gr_text "C IGN" (at 56.769 127.127) (layer F.SilkS))
  (gr_text Charge (at 57.277 124.587) (layer F.SilkS))
  (gr_text Fire (at 56.007 122.047) (layer F.SilkS))
  (gr_line (start 49.5 152.5) (end 219.5 152.5) (layer Edge.Cuts) (width 0.05))
  (gr_text "Corwin Hansen\ncorwinh.com/git\nakerunakayama@gmail.com\n(206) 462 8204\n" (at 176 79) (layer B.SilkS))
  (gr_line (start 219.5 52.5) (end 49.5 52.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 219.5 152.5) (end 219.5 52.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.5 52.5) (end 49.5 152.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 6) (net_name /Transformer/out+) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 67) (xy 186 67) (xy 186 57) (xy 193 57)
      )
    )
  )
  (zone (net 6) (net_name /Transformer/out+) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160 73) (xy 154 73) (xy 154 63) (xy 160 63)
      )
    )
  )
  (zone (net 6) (net_name /Transformer/out+) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196 73) (xy 160 73) (xy 154 73) (xy 154 63) (xy 165 63)
        (xy 165 68) (xy 181 68) (xy 181 63) (xy 189 63) (xy 189 57)
        (xy 196 57)
      )
    )
  )
  (zone (net 5) (net_name Vtrans) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180 67) (xy 166 67) (xy 166 57) (xy 148 57) (xy 148 67)
        (xy 71.5 67) (xy 71.5 112.5) (xy 142.5 112.5) (xy 142.5 123) (xy 62.5 123)
        (xy 56.5 117) (xy 50 117) (xy 50 67) (xy 50 53) (xy 180 53)
      )
    )
  )
  (zone (net 5) (net_name Vtrans) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 67) (xy 71.5 67) (xy 71.5 123) (xy 62.5 123) (xy 56.5 117)
        (xy 50 117) (xy 50 53) (xy 148 53)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160 95) (xy 154 95) (xy 154 85) (xy 160 85)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 95) (xy 186 95) (xy 186 83) (xy 219 83)
      )
    )
  )
  (zone (net 8) (net_name /Transformer/in-) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 101) (xy 166 101) (xy 166 91) (xy 180 91) (xy 180 105)
        (xy 130 105) (xy 130 102) (xy 122 102) (xy 122 98) (xy 129.5 98)
        (xy 129.5 91) (xy 148 91)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 66) (xy 200 66) (xy 200 53) (xy 219 53)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 73.5) (xy 200 73.5) (xy 200 53) (xy 219 53)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.3 91.25) (xy 105.25 91.25) (xy 109 95) (xy 96 95) (xy 95.925 90.5)
        (xy 102.1 90.5) (xy 102.1 88.2) (xy 103.3 88.2)
      )
    )
  )
  (zone (net 7) (net_name "Net-(Q1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128 109) (xy 97 109) (xy 97 105.5) (xy 121 105.5) (xy 121 104)
        (xy 128 104)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118 103) (xy 98 103) (xy 98 96) (xy 118 96)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131 89) (xy 92.5 89) (xy 92.5 95.5) (xy 73 95.5) (xy 73 68.5)
        (xy 131 68.5)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.5 95) (xy 93.1 95) (xy 93.1 90.5) (xy 105 90.5)
      )
    )
  )
  (zone (net 26) (net_name "Net-(R7-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203 78.8) (xy 201 78.8) (xy 201 74.85) (xy 203 74.85)
      )
    )
  )
  (zone (net 52) (net_name "Net-(C17-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5 88.4) (xy 111.5 88.4) (xy 111.5 84.15) (xy 113.5 84.15)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.5 151) (xy 148.5 151) (xy 148.5 141) (xy 185.5 141)
      )
    )
  )
  (zone (net 5) (net_name Vtrans) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.5 123) (xy 105.5 123) (xy 105.5 112.5) (xy 142.5 112.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118 146) (xy 86.5 146) (xy 86.5 152) (xy 50 152) (xy 50 124.5)
        (xy 118 124.5)
      )
    )
  )
  (zone (net 51) (net_name "Net-(J3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.625))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 149) (xy 206 149) (xy 201.5 144.5) (xy 196 144.5) (xy 196 141.5)
        (xy 201.5 141.5) (xy 206 137) (xy 219 137)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.5 148.5) (xy 189 148.5) (xy 189 147.5) (xy 192.5 147.5)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.5 151.5) (xy 190.5 151.5) (xy 190.5 149.55) (xy 192.5 149.55)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.975 141) (xy 99.025 141) (xy 99 151.5) (xy 95 151.5) (xy 95 144.5)
        (xy 91.5 144.5) (xy 91.5 140) (xy 94.8 140) (xy 94.8 137.65) (xy 95.95 137.65)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 95) (xy 181 95) (xy 181 90) (xy 165 90) (xy 165 101)
        (xy 104 101) (xy 104 124.5) (xy 125.5 124.5) (xy 125.5 133) (xy 201 133)
        (xy 201 139) (xy 195 139) (xy 192.5 141.5) (xy 192.5 148.5) (xy 185.5 148.5)
        (xy 185.5 149) (xy 81.5 149) (xy 73 140.5) (xy 73 68.5) (xy 131 68.5)
        (xy 131 83) (xy 205.999806 82.978382) (xy 206 76.5) (xy 219 76.5)
      )
    )
  )
  (zone (net 23) (net_name "Net-(Q2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.5 151) (xy 128 151) (xy 128 143) (xy 120.5 143) (xy 120.5 140)
        (xy 142.5 140)
      )
    )
  )
  (zone (net 22) (net_name "Net-(Q2-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.5 152) (xy 106 152) (xy 106 149) (xy 120.5 149) (xy 120.5 145.5)
        (xy 125.5 145.5)
      )
    )
  )
  (zone (net 14) (net_name "Net-(D2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157 123) (xy 148.5 123) (xy 148.5 116) (xy 157 116)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 123.5) (xy 164.5 123.5) (xy 164.5 113) (xy 200 113) (xy 205 107.5)
        (xy 219 107.5)
      )
    )
  )
  (zone (net 51) (net_name "Net-(J3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 149) (xy 206 149) (xy 201.5 144.5) (xy 196 144.5) (xy 196 141.5)
        (xy 201.5 141.5) (xy 206 137) (xy 219 137)
      )
    )
  )
  (zone (net 14) (net_name "Net-(D2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157 123) (xy 148.5 123) (xy 148.5 116) (xy 157 116)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 123.5) (xy 164.5 123.5) (xy 164.5 113) (xy 200 113) (xy 205 107.5)
        (xy 219 107.5)
      )
    )
  )
)
