(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 26)
    (no_connects 0)
    (area 39.884999 28.235 59.643334 92.195001)
    (thickness 1.6)
    (drawings 59)
    (tracks 118)
    (zones 0)
    (modules 10)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.3)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 40.64 91.44)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/larraguetajunior/Desktop/PCBRPINT/))
  )
  (net 0 "")
  (net 1 "Net-(ABSP1-Pad3)")
  (net 2 "Net-(ABSP1-Pad4)")
  (net 3 "Net-(DELTAP1-Pad3)")
  (net 4 "Net-(DELTAP1-Pad4)")
  (net 5 "Net-(OAT1-Pad2)")
  (net 6 GND)
  (net 7 +3V3)
  (net 8 "Net-(BLUETOOTH1-Pad1)")
  (net 9 "Net-(BLUETOOTH1-Pad2)")
  (net 10 "Net-(GPIO1-Pad1)")
  (net 11 "Net-(GPIO1-Pad2)")
  (net 12 "Net-(TEENSYV3.6-Pad25)")
  (net 13 "Net-(TEENSYV3.6-Pad26)")
  (net 14 "Net-(TEENSYV3.6-Pad4)")
  (net 15 "Net-(TEENSYV3.6-Pad5)")
  (net 16 "Net-(TEENSYV3.6-Pad6)")
  (net 17 "Net-(TEENSYV3.6-Pad7)")
  (net 18 "Net-(TEENSYV3.6-Pad31)")
  (net 19 "Net-(TEENSYV3.6-Pad8)")
  (net 20 "Net-(TEENSYV3.6-Pad9)")
  (net 21 "Net-(TEENSYV3.6-Pad10)")
  (net 22 "Net-(TEENSYV3.6-Pad34)")
  (net 23 "Net-(TEENSYV3.6-Pad11)")
  (net 24 "Net-(TEENSYV3.6-Pad35)")
  (net 25 "Net-(TEENSYV3.6-Pad12)")
  (net 26 "Net-(TEENSYV3.6-Pad36)")
  (net 27 "Net-(TEENSYV3.6-Pad13)")
  (net 28 "Net-(TEENSYV3.6-Pad14)")
  (net 29 "Net-(TEENSYV3.6-Pad38)")
  (net 30 "Net-(TEENSYV3.6-Pad15)")
  (net 31 "Net-(TEENSYV3.6-Pad39)")
  (net 32 "Net-(TEENSYV3.6-Pad16)")
  (net 33 "Net-(TEENSYV3.6-Pad40)")
  (net 34 "Net-(TEENSYV3.6-Pad17)")
  (net 35 "Net-(TEENSYV3.6-Pad41)")
  (net 36 "Net-(TEENSYV3.6-Pad18)")
  (net 37 "Net-(TEENSYV3.6-Pad42)")
  (net 38 "Net-(TEENSYV3.6-Pad19)")
  (net 39 "Net-(TEENSYV3.6-Pad20)")
  (net 40 "Net-(TEENSYV3.6-Pad21)")
  (net 41 "Net-(TEENSYV3.6-Pad45)")
  (net 42 "Net-(TEENSYV3.6-Pad22)")
  (net 43 "Net-(TEENSYV3.6-Pad46)")
  (net 44 "Net-(TEENSYV3.6-Pad23)")
  (net 45 "Net-(TEENSYV3.6-Pad47)")
  (net 46 "Net-(TEENSYV3.6-Pad24)")
  (net 47 "Net-(TEENSYV3.6-Pad48)")
  (net 48 "Net-(GPIO1-Pad3)")
  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(ABSP1-Pad3)")
    (add_net "Net-(ABSP1-Pad4)")
    (add_net "Net-(BLUETOOTH1-Pad1)")
    (add_net "Net-(BLUETOOTH1-Pad2)")
    (add_net "Net-(DELTAP1-Pad3)")
    (add_net "Net-(DELTAP1-Pad4)")
    (add_net "Net-(GPIO1-Pad1)")
    (add_net "Net-(GPIO1-Pad2)")
    (add_net "Net-(GPIO1-Pad3)")
    (add_net "Net-(OAT1-Pad2)")
    (add_net "Net-(TEENSYV3.6-Pad10)")
    (add_net "Net-(TEENSYV3.6-Pad11)")
    (add_net "Net-(TEENSYV3.6-Pad12)")
    (add_net "Net-(TEENSYV3.6-Pad13)")
    (add_net "Net-(TEENSYV3.6-Pad14)")
    (add_net "Net-(TEENSYV3.6-Pad15)")
    (add_net "Net-(TEENSYV3.6-Pad16)")
    (add_net "Net-(TEENSYV3.6-Pad17)")
    (add_net "Net-(TEENSYV3.6-Pad18)")
    (add_net "Net-(TEENSYV3.6-Pad19)")
    (add_net "Net-(TEENSYV3.6-Pad20)")
    (add_net "Net-(TEENSYV3.6-Pad21)")
    (add_net "Net-(TEENSYV3.6-Pad22)")
    (add_net "Net-(TEENSYV3.6-Pad23)")
    (add_net "Net-(TEENSYV3.6-Pad24)")
    (add_net "Net-(TEENSYV3.6-Pad25)")
    (add_net "Net-(TEENSYV3.6-Pad26)")
    (add_net "Net-(TEENSYV3.6-Pad31)")
    (add_net "Net-(TEENSYV3.6-Pad34)")
    (add_net "Net-(TEENSYV3.6-Pad35)")
    (add_net "Net-(TEENSYV3.6-Pad36)")
    (add_net "Net-(TEENSYV3.6-Pad38)")
    (add_net "Net-(TEENSYV3.6-Pad39)")
    (add_net "Net-(TEENSYV3.6-Pad4)")
    (add_net "Net-(TEENSYV3.6-Pad40)")
    (add_net "Net-(TEENSYV3.6-Pad41)")
    (add_net "Net-(TEENSYV3.6-Pad42)")
    (add_net "Net-(TEENSYV3.6-Pad45)")
    (add_net "Net-(TEENSYV3.6-Pad46)")
    (add_net "Net-(TEENSYV3.6-Pad47)")
    (add_net "Net-(TEENSYV3.6-Pad48)")
    (add_net "Net-(TEENSYV3.6-Pad5)")
    (add_net "Net-(TEENSYV3.6-Pad6)")
    (add_net "Net-(TEENSYV3.6-Pad7)")
    (add_net "Net-(TEENSYV3.6-Pad8)")
    (add_net "Net-(TEENSYV3.6-Pad9)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 5926827F)
    (at 46.99 39.37)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference ABSP1 (at -2.03 -3.54 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 -9.95) (layer B.Fab))
    (fp_text user %R (at -1.99 -3.1 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(ABSP1-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(ABSP1-Pad4)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 5926823E)
    (at 54.61 49.53 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference BLUETOOTH1 (at 1.95 -3.82 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 -9.95 90) (layer B.Fab))
    (fp_text user %R (at 0 2.33 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(BLUETOOTH1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(BLUETOOTH1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 59268264)
    (at 54.61 39.37)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference DELTAP1 (at -2.23 -3.22 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 -9.95) (layer B.Fab))
    (fp_text user %R (at -2.23 -3.24 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(DELTAP1-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(DELTAP1-Pad4)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connect:PINHEAD1-3 (layer B.Cu) (tedit 59267F5F)
    (at 46.99 67.31)
    (fp_text reference GPIO1 (at 2.59 3.8) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 2.54 -3.81) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(GPIO1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(GPIO1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(GPIO1-Pad3)"))
  )
  (module Connect:PINHEAD1-3 (layer B.Cu) (tedit 59267F38)
    (at 46.99 59.69)
    (fp_text reference OAT1 (at 2.59 3.8) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 2.54 -3.81) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(OAT1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer B.Cu) (tedit 59267687)
    (at 45.72 54.61)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 0.63 -1.82) (layer B.SilkS))
    (fp_text value 4700 (at 0.95 -1.86) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(DELTAP1-Pad3)"))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer B.Cu) (tedit 59267754)
    (at 50.68 38.86 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 0.06 -1.71 90) (layer B.SilkS))
    (fp_text value 4700 (at 0.95 -1.86 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(DELTAP1-Pad4)"))
    (pad 2 thru_hole oval (at 1.9 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer B.Cu) (tedit 5926768B)
    (at 52.07 54.61)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 0.74 -1.88) (layer B.SilkS))
    (fp_text value 4700 (at 0.95 -1.86) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(ABSP1-Pad3)"))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer B.Cu) (tedit 59267759)
    (at 50.68 32.24 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 0.92 1.73 270) (layer B.SilkS))
    (fp_text value 4700 (at 0.95 -1.86 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(ABSP1-Pad4)"))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy:Socket_Strip_Teensy3.6_2x24_Pitch2.54mm (layer F.Cu) (tedit 59267D62)
    (at 49.53 90.17 180)
    (descr "Through hole straight socket Teensy 3.6 strip, 2x24, 2.54mm pitch, double rows")
    (tags "Through hole socket strip Teensy 3.6 THT 2x24 2.54mm double row")
    (fp_text reference TEENSYV3.6 (at 0 4.064 180) (layer F.SilkS) hide)
    (fp_text value Teensy3.6fsocket (at 2.54 60.96 180) (layer F.Fab))
    (fp_text user %R (at 0.08 0.15 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -7.62 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 25 thru_hole oval (at 7.62 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(TEENSYV3.6-Pad25)"))
    (pad 2 thru_hole oval (at -7.62 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(BLUETOOTH1-Pad2)"))
    (pad 26 thru_hole oval (at 7.62 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(TEENSYV3.6-Pad26)"))
    (pad 3 thru_hole oval (at -7.62 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(BLUETOOTH1-Pad1)"))
    (pad 27 thru_hole oval (at 7.62 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 4 thru_hole oval (at -7.62 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(TEENSYV3.6-Pad4)"))
    (pad 28 thru_hole oval (at 7.62 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(GPIO1-Pad1)"))
    (pad 5 thru_hole oval (at -7.62 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(TEENSYV3.6-Pad5)"))
    (pad 29 thru_hole oval (at 7.62 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(GPIO1-Pad2)"))
    (pad 6 thru_hole oval (at -7.62 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(TEENSYV3.6-Pad6)"))
    (pad 30 thru_hole oval (at 7.62 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(GPIO1-Pad3)"))
    (pad 7 thru_hole oval (at -7.62 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(TEENSYV3.6-Pad7)"))
    (pad 31 thru_hole oval (at 7.62 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(TEENSYV3.6-Pad31)"))
    (pad 8 thru_hole oval (at -7.62 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(TEENSYV3.6-Pad8)"))
    (pad 32 thru_hole oval (at 7.62 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(DELTAP1-Pad4)"))
    (pad 9 thru_hole oval (at -7.62 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(TEENSYV3.6-Pad9)"))
    (pad 33 thru_hole oval (at 7.62 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(DELTAP1-Pad3)"))
    (pad 10 thru_hole oval (at -7.62 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(TEENSYV3.6-Pad10)"))
    (pad 34 thru_hole oval (at 7.62 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(TEENSYV3.6-Pad34)"))
    (pad 11 thru_hole oval (at -7.62 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(TEENSYV3.6-Pad11)"))
    (pad 35 thru_hole oval (at 7.62 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(TEENSYV3.6-Pad35)"))
    (pad 12 thru_hole oval (at -7.62 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(TEENSYV3.6-Pad12)"))
    (pad 36 thru_hole oval (at 7.62 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(TEENSYV3.6-Pad36)"))
    (pad 13 thru_hole oval (at -7.62 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(TEENSYV3.6-Pad13)"))
    (pad 37 thru_hole oval (at 7.62 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(OAT1-Pad2)"))
    (pad 14 thru_hole oval (at -7.62 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(TEENSYV3.6-Pad14)"))
    (pad 38 thru_hole oval (at 7.62 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(TEENSYV3.6-Pad38)"))
    (pad 15 thru_hole oval (at -7.62 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(TEENSYV3.6-Pad15)"))
    (pad 39 thru_hole oval (at 7.62 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(TEENSYV3.6-Pad39)"))
    (pad 16 thru_hole oval (at -7.62 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(TEENSYV3.6-Pad16)"))
    (pad 40 thru_hole oval (at 7.62 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(TEENSYV3.6-Pad40)"))
    (pad 17 thru_hole oval (at -7.62 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(TEENSYV3.6-Pad17)"))
    (pad 41 thru_hole oval (at 7.62 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(TEENSYV3.6-Pad41)"))
    (pad 18 thru_hole oval (at -7.62 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(TEENSYV3.6-Pad18)"))
    (pad 42 thru_hole oval (at 7.62 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(TEENSYV3.6-Pad42)"))
    (pad 19 thru_hole oval (at -7.62 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(TEENSYV3.6-Pad19)"))
    (pad 43 thru_hole oval (at 7.62 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(ABSP1-Pad3)"))
    (pad 20 thru_hole oval (at -7.62 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(TEENSYV3.6-Pad20)"))
    (pad 44 thru_hole oval (at 7.62 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(ABSP1-Pad4)"))
    (pad 21 thru_hole oval (at -7.62 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(TEENSYV3.6-Pad21)"))
    (pad 45 thru_hole oval (at 7.62 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(TEENSYV3.6-Pad45)"))
    (pad 22 thru_hole oval (at -7.62 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(TEENSYV3.6-Pad22)"))
    (pad 46 thru_hole oval (at 7.62 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(TEENSYV3.6-Pad46)"))
    (pad 23 thru_hole oval (at -7.62 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(TEENSYV3.6-Pad23)"))
    (pad 47 thru_hole oval (at 7.62 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(TEENSYV3.6-Pad47)"))
    (pad 24 thru_hole oval (at -7.62 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(TEENSYV3.6-Pad24)"))
    (pad 48 thru_hole oval (at 7.62 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(TEENSYV3.6-Pad48)"))
    (model "../../../../../../Users/larra/Documents/GitHub/AirDataComputer/AirDataComputer/Hardware/Asgard/kicad/Asgard/KiCad libraries/teensy/3DShapes/TeensyV3.6socket.wrl"
      (at (xyz 0.3 -2.3 -0.05))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
    (model "../../../../../../Users/larraguetajunior/Documents/GitHub/AirDataComputer/Hardware/Asgard/kicad/Asgard/KiCad libraries/teensy/3DShapes/TeensyV3.6socket.wrl"
      (at (xyz 0.3 -2.3 -0.05))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (gr_text ADC (at 49.53 86.36) (layer B.SilkS))
  (gr_text BASICAIRDATA.EU (at 49.276 83.82) (layer B.SilkS))
  (gr_text DELTAP (at 52.578 35.687 90) (layer B.SilkS))
  (gr_text ABS (at 44.958 36.068 90) (layer B.SilkS))
  (gr_text BLUETOOTH (at 49.784 47.498) (layer B.SilkS))
  (gr_text A0 (at 49.53 57.15) (layer B.SilkS))
  (gr_text GND (at 54.356 59.69) (layer B.SilkS))
  (gr_text 3.3V (at 44.45 59.69) (layer B.SilkS))
  (gr_text GPIO (at 49.53 69.596) (layer B.SilkS))
  (gr_text OAT (at 49.53 61.976) (layer B.SilkS))
  (gr_text "BLUETOOTH\nOVER THERE" (at 49.403 80.391) (layer B.SilkS))
  (gr_text "SENSOR PORTS\nTHIS SIDE" (at 42.799 42.418) (layer B.SilkS))
  (gr_text "TEENSY\nUSB SIDE" (at 49.23 88.32 180) (layer F.SilkS))
  (gr_text A9 (at 54.51 67.34) (layer B.SilkS))
  (gr_text A8 (at 49.53 64.77) (layer B.SilkS))
  (gr_text A7 (at 44.4 67.28) (layer B.SilkS))
  (gr_line (start 40.64 30.48) (end 40.64 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 47.05 74.93) (end 48.3 74.93) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 52.13 74.93) (end 53.38 74.93) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 52.07 44.45) (end 52.07 46.45) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 58.42 91.44) (end 40.64 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.42 30.48) (end 58.42 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.64 30.48) (end 58.42 30.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.42 91.44) (xy 40.64 91.44) (xy 40.64 30.48) (xy 58.42 30.48)
      )
    )
  )
)
