<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="8.89" x2="41.9662" y2="8.7884" width="0" layer="20"/>
<wire x1="41.9662" y1="8.7884" x2="41.9154" y2="57.534" width="0" layer="20"/>
<wire x1="41.9154" y1="57.534" x2="-0.0508" y2="57.6356" width="0" layer="20"/>
<wire x1="-0.0508" y1="57.6356" x2="0" y2="8.89" width="0" layer="20"/>
<text>MonkeyTurk v0.3
Feather M0 Shield
mil @ DiCarlo Lab</text>
<text>USB</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>Load on</text>
<text>Status</text>
<text>330Ω</text>
<text>330Ω</text>
<text>10</text>
<text>9</text>
<text>6</text>
<text>5</text>
<text>SCL</text>
<text>SDA</text>
<text>RST</text>
<text>3V</text>
<text>Ref</text>
<text>GND</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>SCK</text>
<text>MOSI</text>
<text>MISO</text>
<text>RX</text>
<text>UTX</text>
<text>DFU</text>
<text>E</text>
<text>C</text>
<text>B</text>
<text>En</text>
<text>BAT</text>
<text>R</text>
<text>load</text>
<text>5V</text>
<text>Flyback</text>
<text>&gt;=</text>
<text>NPN</text>
<text>12 (load on)</text>
<text>11 (status)</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM-NS">
<description>&lt;h3&gt;LED 3MM PTH- No Silk&lt;/h3&gt;

3 mm, round, no silk outline of package

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12_LOCK">
<description>&lt;h3&gt;Plated Through Hole -12 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16_LOCK">
<description>&lt;h3&gt;Plated Through Hole -16 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_SLOT">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH Slot Pads&lt;/h3&gt;
Extended soldering pads. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="M9040P">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148-KIT">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D2" library="SparkFun-LED" package="LED_3MM-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X12_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X16_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="POWER_JACK_SLOT" value="POWER_JACKSLT">
<attribute name="PROD_ID" value="PRT-00119"/>
</element>
<element name="S1" library="switch" package="M9040P" value="">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="RLED" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="VALUE"/>
</element>
<element name="FLYBACK" library="SparkFun-DiscreteSemi" package="DIODE-1N4148-KIT" value="200mA/100V/1V">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="RBASE" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="TO92" value="BC337">
<attribute name="POPULARITY" value="2"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="J1" pad="10"/>
<contactref element="J3" pad="PWR"/>
<contactref element="FLYBACK" pad="C"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="RLED" pad="P$1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="RBASE" pad="P$2"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J3" pad="GND@2"/>
<contactref element="J3" pad="GND@1"/>
<contactref element="S1" pad="2"/>
<contactref element="FLYBACK" pad="A"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="7"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="D2" pad="K"/>
<contactref element="RLED" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="8"/>
<contactref element="RBASE" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
