(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.64592)
  )
  (paper "USLetter")
  (title_block
    (title "Jackrabbit RP2040 Logic Analyzer")
    (date "2022-09-14")
    (rev "A")
    (comment 2 "Ray Sun")
    (comment 3 "Brandon Gong")
    (comment 4 "Brian Cruz")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White") (material "PSR-4100WL"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.0254) (material "PSR-4000BN") (epsilon_r 3.3) (loss_tangent 0))
      (layer "F.Cu" (type "copper") (thickness 0.03556))
      (layer "dielectric 1" (type "prepreg") (thickness 1.524) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.03556))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.0254) (material "PSR-4000BN") (epsilon_r 3.3) (loss_tangent 0))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White") (material "PSR-4100WL"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 121.79 119.995)
    (grid_origin 121.79 119.995)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "+1V1")
  (net 5 "/VREF_ADC")
  (net 6 "Net-(C17-Pad2)")
  (net 7 "Net-(C18-Pad2)")
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(D2-Pad1)")
  (net 10 "Net-(D3-Pad1)")
  (net 11 "Net-(D4-Pad1)")
  (net 12 "VUSB")
  (net 13 "Net-(J1-PadA5)")
  (net 14 "/USB_D+")
  (net 15 "/USB_D-")
  (net 16 "unconnected-(J1-PadA8)")
  (net 17 "Net-(J1-PadB5)")
  (net 18 "unconnected-(J1-PadB8)")
  (net 19 "/OUT_DIG0")
  (net 20 "/OUT_DIG1")
  (net 21 "/OUT_DIG2")
  (net 22 "/OUT_DIG3")
  (net 23 "/OUT_DIG4")
  (net 24 "/OUT_DIG5")
  (net 25 "/OUT_DIG6")
  (net 26 "/OUT_DIG7")
  (net 27 "/OUT_DIG8")
  (net 28 "/OUT_DIG9")
  (net 29 "/OUT_DIG10")
  (net 30 "/OUT_DIG11")
  (net 31 "/OUT_DIG12")
  (net 32 "/OUT_DIG13")
  (net 33 "/OUT_DIG14")
  (net 34 "/OUT_DIG15")
  (net 35 "/ADC0")
  (net 36 "/ADC1")
  (net 37 "/ADC2")
  (net 38 "/ADC3")
  (net 39 "/SWCLK")
  (net 40 "/SWDIO")
  (net 41 "/D+")
  (net 42 "/D-")
  (net 43 "/QSPI_SS")
  (net 44 "/~{DIR_OUT_A}")
  (net 45 "/~{USB_BOOT}")
  (net 46 "Net-(R10-Pad2)")
  (net 47 "/~{DIR_OUT_B}")
  (net 48 "/~{RESET}")
  (net 49 "/LEDA")
  (net 50 "/LEDB")
  (net 51 "/LEDC")
  (net 52 "unconnected-(U1-Pad4)")
  (net 53 "/DIG7")
  (net 54 "/DIG6")
  (net 55 "/DIG5")
  (net 56 "/DIG4")
  (net 57 "/DIG3")
  (net 58 "/DIG2")
  (net 59 "/DIG1")
  (net 60 "/DIG0")
  (net 61 "/QSPI_SD1")
  (net 62 "/QSPI_SD2")
  (net 63 "/QSPI_SD0")
  (net 64 "/QSPI_SCLK")
  (net 65 "/QSPI_SD3")
  (net 66 "/DIG8")
  (net 67 "/DIG9")
  (net 68 "/DIG10")
  (net 69 "/DIG11")
  (net 70 "/DIG12")
  (net 71 "/DIG13")
  (net 72 "/DIG14")
  (net 73 "/DIG15")
  (net 74 "/~{OE_A}")
  (net 75 "unconnected-(U4-Pad34)")
  (net 76 "/~{OE_B}")
  (net 77 "Net-(R11-Pad1)")
  (net 78 "unconnected-(U4-Pad31)")
  (net 79 "Net-(RN1-Pad16)")
  (net 80 "Net-(RN1-Pad15)")
  (net 81 "Net-(RN1-Pad14)")
  (net 82 "Net-(RN1-Pad13)")
  (net 83 "Net-(RN1-Pad12)")
  (net 84 "Net-(RN1-Pad11)")
  (net 85 "Net-(RN1-Pad10)")
  (net 86 "Net-(RN1-Pad9)")
  (net 87 "Net-(RN2-Pad9)")
  (net 88 "Net-(RN2-Pad10)")
  (net 89 "Net-(RN2-Pad11)")
  (net 90 "Net-(RN2-Pad12)")
  (net 91 "Net-(RN2-Pad13)")
  (net 92 "Net-(RN2-Pad14)")
  (net 93 "Net-(RN2-Pad15)")
  (net 94 "Net-(RN2-Pad16)")
  (net 95 "unconnected-(J1-PadS1)")
  (footprint "jackrabbit:RP2040-QFN-56_HandSoldering" (layer "F.Cu")
    (tedit 5EF32B43)
    (at 146.936 105.39 -45)
    (descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0 -5 -45 unlocked) (layer "F.SilkS") hide)
    (fp_text value "RP2040" (at 0 5 -45 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -3.65 -2.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -3.65 -2.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/DIG0") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.65 -1.8 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/DIG1") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.65 -1.4 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/DIG2") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.65 -1 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/DIG3") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -3.65 -0.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/DIG4") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -3.65 -0.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/DIG5") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.65 0.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/DIG6") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.65 0.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/DIG7") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.65 1 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "11" smd roundrect (at -3.65 1.4 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/DIG8") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.65 1.8 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/DIG9") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -3.65 2.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "/DIG10") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -3.65 2.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/DIG11") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -2.6 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/DIG12") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -2.2 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/DIG13") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -1.8 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/DIG14") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "18" smd roundrect (at -1.4 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/DIG15") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -1 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "TESTEN") (pintype "passive"))
    (pad "20" smd roundrect (at -0.6 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R10-Pad2)") (pinfunction "XIN") (pintype "input"))
    (pad "21" smd roundrect (at -0.2 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad2)") (pinfunction "XOUT") (pintype "passive"))
    (pad "22" smd roundrect (at 0.2 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "23" smd roundrect (at 0.6 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd roundrect (at 1 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SWCLK") (pinfunction "SWCLK") (pintype "output"))
    (pad "25" smd roundrect (at 1.4 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/SWDIO") (pinfunction "SWD") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 1.8 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/~{RESET}") (pinfunction "RUN") (pintype "input"))
    (pad "27" smd roundrect (at 2.2 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/~{DIR_OUT_A}") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 2.6 3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/~{OE_A}") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.65 2.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/~{DIR_OUT_B}") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.65 2.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/~{OE_B}") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.65 1.8 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "unconnected-(U4-Pad31)") (pinfunction "GPIO20") (pintype "bidirectional+no_connect"))
    (pad "32" smd roundrect (at 3.65 1.4 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R11-Pad1)") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.65 1 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "34" smd roundrect (at 3.65 0.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "unconnected-(U4-Pad34)") (pinfunction "GPIO22") (pintype "bidirectional+no_connect"))
    (pad "35" smd roundrect (at 3.65 0.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/LEDC") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 3.65 -0.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/LEDB") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 3.65 -0.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/LEDA") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 3.65 -1 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/ADC0") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 3.65 -1.4 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/ADC1") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 3.65 -1.8 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/ADC2") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "41" smd roundrect (at 3.65 -2.2 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/ADC3") (pinfunction "GPIO29_ADC3") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 3.65 -2.6 315) (size 1.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "43" smd roundrect (at 2.6 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/VREF_ADC") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd roundrect (at 2.2 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VREG_IN") (pintype "power_in"))
    (pad "45" smd roundrect (at 1.8 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+1V1") (pinfunction "VREG_VOUT") (pintype "power_out"))
    (pad "46" smd roundrect (at 1.4 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/D-") (pinfunction "USB_DM") (pintype "bidirectional"))
    (pad "47" smd roundrect (at 1 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/D+") (pinfunction "USB_DP") (pintype "bidirectional"))
    (pad "48" smd roundrect (at 0.6 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd roundrect (at 0.2 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "50" smd roundrect (at -0.2 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "51" smd roundrect (at -0.6 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/QSPI_SD3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd roundrect (at -1 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/QSPI_SCLK") (pinfunction "QSPI_SCLK") (pintype "output"))
    (pad "53" smd roundrect (at -1.4 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/QSPI_SD0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd roundrect (at -1.8 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/QSPI_SD2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd roundrect (at -2.2 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/QSPI_SD1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd roundrect (at -2.6 -3.65 315) (size 0.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/QSPI_SS") (pinfunction "QSPI_SS") (pintype "bidirectional"))
    (pad "57" smd roundrect (at 0 0 315) (size 3.2 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.045)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 0 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 1.275 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 0 315) (size 1.651 1.651) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 -1.275 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 1.275 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 0 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 1.275 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 -1.275 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 -1.275 315) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.03 112.502 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/~{DIR_OUT_B}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "jackrabbit:PinHeader_2x04_P2.54mm_NoSilk" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 157.35 115.931 -90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (clearance 0.254)
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -2.33 -90) (layer "F.SilkS") hide)
    (fp_text value "PinHeader_2.54mm_02x04" (at 1.27 9.95 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/ADC3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/ADC2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/ADC1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/ADC0") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.348 111.5622)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 1.43 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 152.016 96.627 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.4 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MIC5319-3.3YD5" (at 0 2.4 -270 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "unconnected-(U1-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_8x0602" (layer "F.Cu")
    (tedit 58E0A8FC)
    (at 138.554 108.438 180)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RN2" (at -0.00001 -3.000005 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "220" (at 0 3 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.9 -1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/DIG15") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect (at -0.9 -1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/DIG14") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect (at -0.9 -0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/DIG13") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect (at -0.9 -0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/DIG12") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect (at -0.9 0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/DIG11") (pinfunction "R5.1") (pintype "passive"))
    (pad "6" smd rect (at -0.9 0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/DIG10") (pinfunction "R6.1") (pintype "passive"))
    (pad "7" smd rect (at -0.9 1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/DIG9") (pinfunction "R7.1") (pintype "passive"))
    (pad "8" smd rect (at -0.9 1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/DIG8") (pinfunction "R8.1") (pintype "passive"))
    (pad "9" smd rect (at 0.9 1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(RN2-Pad9)") (pinfunction "R8.2") (pintype "passive"))
    (pad "10" smd rect (at 0.9 1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(RN2-Pad10)") (pinfunction "R7.2") (pintype "passive"))
    (pad "11" smd rect (at 0.9 0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Net-(RN2-Pad11)") (pinfunction "R6.2") (pintype "passive"))
    (pad "12" smd rect (at 0.9 0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(RN2-Pad12)") (pinfunction "R5.2") (pintype "passive"))
    (pad "13" smd rect (at 0.9 -0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(RN2-Pad13)") (pinfunction "R4.2") (pintype "passive"))
    (pad "14" smd rect (at 0.9 -0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(RN2-Pad14)") (pinfunction "R3.2") (pintype "passive"))
    (pad "15" smd rect (at 0.9 -1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(RN2-Pad15)") (pinfunction "R2.2") (pintype "passive"))
    (pad "16" smd rect (at 0.9 -1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(RN2-Pad16)") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_8x0602.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "jackrabbit:SW_Push_CK_PTS815_HandSoldering" (layer "F.Cu")
    (tedit 5B0610A8)
    (at 137.665 93.706)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, https://www.ckswitches.com/media/2728/pts815.pdf")
    (tags "SPST Button Switch")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0 -2.6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 0 2.6 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.15 -1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.15 -1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 2.15 1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/~{USB_BOOT}") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at -2.15 1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/~{USB_BOOT}") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3dmodels/.local/PTS815SJK250SMTRLFS.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "jackrabbit:SW_Push_CK_PTS815_HandSoldering" (layer "F.Cu")
    (tedit 5B0610A8)
    (at 157.35 93.706)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, https://www.ckswitches.com/media/2728/pts815.pdf")
    (tags "SPST Button Switch")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at 0.000001 -2.600001 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 0 2.6 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at 2.15 -1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at -2.15 -1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.15 1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/~{RESET}") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.15 1.075) (size 1.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/~{RESET}") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3dmodels/.local/PTS815SJK250SMTRLFS.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF)
    (at 131.315 116.82)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0.000001 -3.699993 unlocked) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (thermal_gap 0.381))
    (pad "1" thru_hole circle (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.08 106.406)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "27" (at 0 1.43 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/D-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/USB_D-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 152.27 111.105 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "YEL" (at 0 1.65 -90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 11 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 51 "/LEDC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 152.016 92.944 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10u" (at 0 1.68 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "jackrabbit:Crystal_SMD_ECS-4Pin_3.2x2.5mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 141.7544 114.3308 180)
    (descr "crystal Epson Toyocom FA-238 https://support.epson.biz/td/api/doc_check.php?dl=brief_fa-238v_en.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 -2.45 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "ECS-120-18-33-JGN" (at 0 2.45 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.2 0.95 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C18-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.2 0.95 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.12 -0.95 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C17-Pad2)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.2 -0.95 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_SeikoEpson_FA238-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-20_4.4x5mm_P0.5mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 132.204 108.438 180)
    (descr "TSSOP, 20 Pin (JEDEC MO-153 Var BA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 0 -3.45 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "74LVCH245A" (at 0 3.45 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.8625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/~{DIR_OUT_B}") (pinfunction "A->B") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(RN2-Pad16)") (pinfunction "A0") (pintype "tri_state"))
    (pad "3" smd roundrect (at -2.8625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(RN2-Pad15)") (pinfunction "A1") (pintype "tri_state"))
    (pad "4" smd roundrect (at -2.8625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(RN2-Pad14)") (pinfunction "A2") (pintype "tri_state"))
    (pad "5" smd roundrect (at -2.8625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(RN2-Pad13)") (pinfunction "A3") (pintype "tri_state"))
    (pad "6" smd roundrect (at -2.8625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(RN2-Pad12)") (pinfunction "A4") (pintype "tri_state"))
    (pad "7" smd roundrect (at -2.8625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(RN2-Pad11)") (pinfunction "A5") (pintype "tri_state"))
    (pad "8" smd roundrect (at -2.8625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(RN2-Pad10)") (pinfunction "A6") (pintype "tri_state"))
    (pad "9" smd roundrect (at -2.8625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(RN2-Pad9)") (pinfunction "A7") (pintype "tri_state"))
    (pad "10" smd roundrect (at -2.8625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at 2.8625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/OUT_DIG8") (pinfunction "B7") (pintype "tri_state"))
    (pad "12" smd roundrect (at 2.8625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/OUT_DIG9") (pinfunction "B6") (pintype "tri_state"))
    (pad "13" smd roundrect (at 2.8625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/OUT_DIG10") (pinfunction "B5") (pintype "tri_state"))
    (pad "14" smd roundrect (at 2.8625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/OUT_DIG11") (pinfunction "B4") (pintype "tri_state"))
    (pad "15" smd roundrect (at 2.8625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/OUT_DIG12") (pinfunction "B3") (pintype "tri_state"))
    (pad "16" smd roundrect (at 2.8625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/OUT_DIG13") (pinfunction "B2") (pintype "tri_state"))
    (pad "17" smd roundrect (at 2.8625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/OUT_DIG14") (pinfunction "B1") (pintype "tri_state"))
    (pad "18" smd roundrect (at 2.8625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/OUT_DIG15") (pinfunction "B0") (pintype "tri_state"))
    (pad "19" smd roundrect (at 2.8625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/~{OE_B}") (pinfunction "CE") (pintype "input"))
    (pad "20" smd roundrect (at 2.8625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x5mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "jackrabbit:PinHeader_2x10_P2.54mm_Horizontal_NoSilk" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 125.727 116.82 180)
    (descr "Through hole angled pin header, 2x10, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x10 2.54mm double row")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 5.655005 -2.270001 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "PinHeader_2.54mm_02x10" (at 5.655 25.13 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 5.31 11.43 270 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/OUT_DIG14") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/OUT_DIG15") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/OUT_DIG12") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/OUT_DIG13") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/OUT_DIG10") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/OUT_DIG11") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/OUT_DIG8") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/OUT_DIG9") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/OUT_DIG6") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/OUT_DIG7") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/OUT_DIG4") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/OUT_DIG5") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/OUT_DIG2") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/OUT_DIG3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/OUT_DIG0") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/OUT_DIG1") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3dmodels/.local/HTSS-110-04-G-D-RA.stp" hide
      (offset (xyz 3.429 -11.557 4.826))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 152.905 100.31 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10u" (at 0 1.68 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.41 112.502 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.429992 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/~{OE_B}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF)
    (at 163.7 93.96)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.699991 unlocked) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (thermal_gap 0.381))
    (pad "1" thru_hole circle (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 144.777 95.484 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.4 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "W25Q16JVSNIQ" (at 0 3.4 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/QSPI_SS") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/QSPI_SD1") (pinfunction "DO(IO1)") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/QSPI_SD2") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/QSPI_SD0") (pinfunction "DI(IO0)") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/QSPI_SCLK") (pinfunction "CLK") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/QSPI_SD3") (pinfunction "IO3") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 155.318 111.105 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "GRN" (at 0 1.65 -90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 10 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 50 "/LEDB") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 133.22 112.502)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 163.446 98.532 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.65 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "RED" (at 0 1.65 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 8 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF)
    (at 131.315 93.96)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0.000001 -3.699991 unlocked) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (thermal_gap 0.381))
    (pad "1" thru_hole circle (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF)
    (at 163.7 116.82)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.699993 unlocked) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (thermal_gap 0.381))
    (pad "1" thru_hole circle (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 163.446 112.248 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.65 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "BLU" (at 0 1.65 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 9 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 49 "/LEDA") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.144 113.01 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 1.43 90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/~{USB_BOOT}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 133.22 104.374)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.41 104.374 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.429995 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/~{OE_A}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 156.588 100.056 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.82 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0ZCJ0025FF2E" (at 0 1.82 -90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 12 "VUSB") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 3 "+5V") (pintype "passive"))
    (model "${KIPRJMOD}/3dmodels/.local/OZCJ.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.03 104.374 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/~{DIR_OUT_A}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.08 104.374)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "27" (at 0 1.43 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/D+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/USB_D+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_8x0602" (layer "F.Cu")
    (tedit 58E0A8FC)
    (at 138.554 100.31 180)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RN1" (at 0.000011 -3.000005 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "220" (at 0 3 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.9 -1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/DIG7") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect (at -0.9 -1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/DIG6") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect (at -0.9 -0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/DIG5") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect (at -0.9 -0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/DIG4") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect (at -0.9 0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/DIG3") (pinfunction "R5.1") (pintype "passive"))
    (pad "6" smd rect (at -0.9 0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/DIG2") (pinfunction "R6.1") (pintype "passive"))
    (pad "7" smd rect (at -0.9 1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/DIG1") (pinfunction "R7.1") (pintype "passive"))
    (pad "8" smd rect (at -0.9 1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/DIG0") (pinfunction "R8.1") (pintype "passive"))
    (pad "9" smd rect (at 0.9 1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(RN1-Pad9)") (pinfunction "R8.2") (pintype "passive"))
    (pad "10" smd rect (at 0.9 1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(RN1-Pad10)") (pinfunction "R7.2") (pintype "passive"))
    (pad "11" smd rect (at 0.9 0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(RN1-Pad11)") (pinfunction "R6.2") (pintype "passive"))
    (pad "12" smd rect (at 0.9 0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(RN1-Pad12)") (pinfunction "R5.2") (pintype "passive"))
    (pad "13" smd rect (at 0.9 -0.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(RN1-Pad13)") (pinfunction "R4.2") (pintype "passive"))
    (pad "14" smd rect (at 0.9 -0.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(RN1-Pad14)") (pinfunction "R3.2") (pintype "passive"))
    (pad "15" smd rect (at 0.9 -1.25 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(RN1-Pad15)") (pinfunction "R2.2") (pintype "passive"))
    (pad "16" smd rect (at 0.9 -1.75 180) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(RN1-Pad16)") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_8x0602.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 137.284 114.788)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "27p" (at 0 1.43 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-20_4.4x5mm_P0.5mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 132.204 100.31 180)
    (descr "TSSOP, 20 Pin (JEDEC MO-153 Var BA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -3.45 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "74LVCH245A" (at 0 3.45 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.8625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/~{DIR_OUT_A}") (pinfunction "A->B") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(RN1-Pad16)") (pinfunction "A0") (pintype "tri_state"))
    (pad "3" smd roundrect (at -2.8625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(RN1-Pad15)") (pinfunction "A1") (pintype "tri_state"))
    (pad "4" smd roundrect (at -2.8625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(RN1-Pad14)") (pinfunction "A2") (pintype "tri_state"))
    (pad "5" smd roundrect (at -2.8625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(RN1-Pad13)") (pinfunction "A3") (pintype "tri_state"))
    (pad "6" smd roundrect (at -2.8625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(RN1-Pad12)") (pinfunction "A4") (pintype "tri_state"))
    (pad "7" smd roundrect (at -2.8625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(RN1-Pad11)") (pinfunction "A5") (pintype "tri_state"))
    (pad "8" smd roundrect (at -2.8625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(RN1-Pad10)") (pinfunction "A6") (pintype "tri_state"))
    (pad "9" smd roundrect (at -2.8625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(RN1-Pad9)") (pinfunction "A7") (pintype "tri_state"))
    (pad "10" smd roundrect (at -2.8625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at 2.8625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/OUT_DIG0") (pinfunction "B7") (pintype "tri_state"))
    (pad "12" smd roundrect (at 2.8625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/OUT_DIG1") (pinfunction "B6") (pintype "tri_state"))
    (pad "13" smd roundrect (at 2.8625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/OUT_DIG2") (pinfunction "B5") (pintype "tri_state"))
    (pad "14" smd roundrect (at 2.8625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/OUT_DIG3") (pinfunction "B4") (pintype "tri_state"))
    (pad "15" smd roundrect (at 2.8625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/OUT_DIG4") (pinfunction "B3") (pintype "tri_state"))
    (pad "16" smd roundrect (at 2.8625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/OUT_DIG5") (pinfunction "B2") (pintype "tri_state"))
    (pad "17" smd roundrect (at 2.8625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/OUT_DIG6") (pinfunction "B1") (pintype "tri_state"))
    (pad "18" smd roundrect (at 2.8625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/OUT_DIG7") (pinfunction "B0") (pintype "tri_state"))
    (pad "19" smd roundrect (at 2.8625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/~{OE_A}") (pinfunction "CE") (pintype "input"))
    (pad "20" smd roundrect (at 2.8625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x5mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 145.158 114.3308 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.43 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "27p" (at 0 1.43 90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "jackrabbit:USB_C_Receptacle_GCT_USB4105-GF-A-120" (layer "F.Cu")
    (tedit 5E1305FC)
    (at 161.075 105.39 90)
    (descr "USB Type C, right-angle, SMT")
    (tags "USB C Type-C Receptacle SMD")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (clearance 0.127)
    (attr smd)
    (fp_text reference "J1" (at 0 -2.610002 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB_C" (at 0 8 90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.105 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 2.89 0.5 90) (size 0.65 0.65) (drill 0.65) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 0.5 90) (size 0.65 0.65) (drill 0.65) (layers F&B.Cu *.Mask))
    (pad "A1" smd rect (at -3.35 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.55 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "VUSB") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/USB_D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/USB_D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(J1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "A9" smd rect (at 2.55 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "VUSB") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.35 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.05 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.25 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "VUSB") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/USB_D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/USB_D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(J1-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "B9" smd rect (at -2.25 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "VUSB") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.05 -0.8 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 0 90) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 95 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole oval (at 4.32 0 90) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 95 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole oval (at -4.32 4.18 90) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 95 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole oval (at 4.32 4.18 90) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 95 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3dmodels/.local/USB4105-GF-A.stp"
      (offset (xyz 0 -6.8 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "jackrabbit:PinHeader_1x03_P2.54mm_NoSilk" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 138.3 118.471 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (clearance 0.254)
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "PinHeader_2.54mm_01x03" (at 0 7.41 90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.54 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/SWCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/SWDIO") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 163.446 112.248 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1.43 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 142.11 97.897 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 1.43 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 270 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 149.73 99.548 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 1.43 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 -90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 158.62 103.358 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1k" (at 0 -1.43 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J1-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 156.08 103.358 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0 1.43 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1.43 -90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 142.748 102.997 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 180 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 149.222 110.851 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 1.43 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2u" (at 0 -1.43 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62E7AE0F" (layer "B.Cu")
    (tedit 62E7AE0F)
    (at 140.84 115.169 90)
    (descr "Converted using: scripting")
    (tags "svg2mod")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62E7AE0F" (at 0 0.774573 90) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -0.774573 90) (layer "B.SilkS") hide)
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 152.651 107.168)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 1.43 -180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "200" (at 0 -1.43 -180 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -180 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/VREF_ADC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 152.651 104.501 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2u" (at 0 -1.43 180 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 142.745 105.791 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 180 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 156.08 107.422 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 1.43 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1.43 -90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 163.446 98.532 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1k" (at 0 -1.43 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 152.654 100.711)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 1.43 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 180 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 158.62 107.422 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 1.43 -270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1k" (at 0 -1.43 -90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -270 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J1-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 141.729 110.851 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 1.43 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 270 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 145.793 113.01 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10k" (at 0 -1.43 180 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "/~{RESET}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 145.793 110.47 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Symbol_6.7x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 154.305 95.25 90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Symbol_6.7x6mm_SilkScreen" (at 0.75 0 90) (layer "B.Fab") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 154.302 110.851 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 1.43 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2u" (at 0 -1.43 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/VREF_ADC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62E8C5F1" (layer "B.Cu")
    (tedit 62E8C5F1)
    (at 131.3404 97.5922 180)
    (descr "Converted using: scripting")
    (tags "svg2mod")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62E8C5F1" (at 0 0.645562) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -0.645562) (layer "B.SilkS") hide)
  )
  (footprint "kibuzzard-62E7A97F" (layer "B.Cu")
    (tedit 62E7A97F)
    (at 137.665 103.104 90)
    (descr "Converted using: scripting")
    (tags "svg2mod")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62E7A97F" (at 0 2.561592 90) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -2.561592 90) (layer "B.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 144.65 97.897 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 1.43 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 147.19 97.897 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 1.43 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10k" (at 0 -1.43 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "/QSPI_SS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 144.65 94.468 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 1.43 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1k" (at 0 -1.43 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "/QSPI_SS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "/~{USB_BOOT}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 151.762 110.851 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "jackrabbit.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 1.43 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62E8C5F1" (layer "B.Cu")
    (tedit 62E8C5F1)
    (at 131.3912 113.1624 180)
    (descr "Converted using: scripting")
    (tags "svg2mod")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62E8C5F1" (at 0 0.645562) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -0.645562) (layer "B.SilkS") hide)
  )
  (gr_arc (start 121.79 92.69) (mid 122.347962 91.342962) (end 123.695 90.785) (layer "Edge.Cuts") (width 0.1016))
  (gr_arc (start 163.7 90.785) (mid 165.945064 91.714936) (end 166.875 93.96) (layer "Edge.Cuts") (width 0.1016))
  (gr_arc (start 166.875 116.82) (mid 165.945064 119.065064) (end 163.7 119.995) (layer "Edge.Cuts") (width 0.1016))
  (gr_line (start 123.695 90.785) (end 163.7 90.785) (layer "Edge.Cuts") (width 0.1016))
  (gr_line (start 121.79 92.69) (end 121.79 118.09) (layer "Edge.Cuts") (width 0.1016))
  (gr_line (start 123.695 119.995) (end 163.7 119.995) (layer "Edge.Cuts") (width 0.1016))
  (gr_line (start 166.875 93.96) (end 166.875 116.82) (layer "Edge.Cuts") (width 0.1016))
  (gr_arc (start 123.695 119.995) (mid 122.347962 119.437038) (end 121.79 118.09) (layer "Edge.Cuts") (width 0.1016))
  (gr_text "A3" (at 157.223 113.518 270) (layer "B.SilkS"))
  (gr_text "7" (at 129.918 104.5391) (layer "B.SilkS"))
  (gr_text "SWDIO" (at 143.38 114.661 270) (layer "B.SilkS"))
  (gr_text "3" (at 129.918 100.9831) (layer "B.SilkS"))
  (gr_text "A0" (at 149.73 113.518 270) (layer "B.SilkS"))
  (gr_text "SWCLK" (at 138.3 114.534 270) (layer "B.SilkS"))
  (gr_text "14" (at 132.712 111.6511) (layer "B.SilkS"))
  (gr_text "5" (at 129.918 102.7611) (layer "B.SilkS"))
  (gr_text "0" (at 132.712 99.2051) (layer "B.SilkS"))
  (gr_text "13" (at 129.918 109.8731) (layer "B.SilkS"))
  (gr_text "8" (at 132.712 106.3171) (layer "B.SilkS"))
  (gr_text "12" (at 132.712 109.8731) (layer "B.SilkS"))
  (gr_text "10" (at 132.712 108.0951) (layer "B.SilkS"))
  (gr_text "1" (at 129.918 99.2051) (layer "B.SilkS"))
  (gr_text "2" (at 132.712 100.9831) (layer "B.SilkS"))
  (gr_text "A2" (at 154.81 113.518 270) (layer "B.SilkS"))
  (gr_text "15" (at 129.918 111.6511) (layer "B.SilkS"))
  (gr_text "11" (at 129.918 108.0951) (layer "B.SilkS"))
  (gr_text "9" (at 129.918 106.3171) (layer "B.SilkS"))
  (gr_text "A1" (at 152.27 113.518 270) (layer "B.SilkS"))
  (gr_text "4" (at 132.712 102.7611) (layer "B.SilkS"))
  (gr_text "6" (at 132.712 104.5391) (layer "B.SilkS"))
  (gr_text "A" (at 165.986 112.1845 -180) (layer "F.SilkS"))
  (gr_text "A1" (at 152.27 113.899 -180) (layer "F.SilkS"))
  (gr_text "A2" (at 154.81 113.899 -180) (layer "F.SilkS"))
  (gr_text "C" (at 152.27 108.565 -180) (layer "F.SilkS"))
  (gr_text "RESET" (at 157.35 96.373 180) (layer "F.SilkS"))
  (gr_text "DIO" (at 143.38 116.5152 180) (layer "F.SilkS"))
  (gr_text "B" (at 155.318 108.565 -180) (layer "F.SilkS"))
  (gr_text "A0" (at 149.73 113.899 -180) (layer "F.SilkS"))
  (gr_text "BOOT" (at 137.665 96.373 180) (layer "F.SilkS"))
  (gr_text "A3" (at 157.35 113.899 -180) (layer "F.SilkS"))
  (gr_text "CLK" (at 138.3 116.5152 180) (layer "F.SilkS"))
  (gr_text "GND" (at 140.84 116.5152 180) (layer "F.SilkS"))
  (gr_text "PWR" (at 160.271 98.532 -180) (layer "F.SilkS"))
  (gr_text "10.00 mils" (at 113.825714 184.795) (layer "Cmts.User"))
  (gr_text "Copper Finish: " (at 20.94 189.01) (layer "Cmts.User"))
  (gr_text "No" (at 113.825714 193.225) (layer "Cmts.User"))
  (gr_text "Copper Layer Count: " (at 20.94 176.365) (layer "Cmts.User"))
  (gr_text "BOARD CHARACTERISTICS" (at 20.19 170.795) (layer "Cmts.User"))
  (gr_text "No" (at 53.497143 193.225) (layer "Cmts.User"))
  (gr_text "Impedance Control: " (at 88.982857 189.01) (layer "Cmts.User"))
  (gr_text "6.00 mils / 0.00 mils" (at 53.497143 184.795) (layer "Cmts.User"))
  (gr_text "Min track/spacing: " (at 20.94 184.795) (layer "Cmts.User"))
  (gr_text "Board Thickness: " (at 88.982857 176.365) (layer "Cmts.User"))
  (gr_text "" (at 113.825714 180.58) (layer "Cmts.User"))
  (gr_text "Min hole diameter: " (at 88.982857 184.795) (layer "Cmts.User"))
  (gr_text "64.80 mils" (at 113.825714 176.365) (layer "Cmts.User"))
  (gr_text "Edge card connectors: " (at 20.94 197.44) (layer "Cmts.User"))
  (gr_text "ENIG" (at 53.497143 189.01) (layer "Cmts.User"))
  (gr_text "Plated Board Edge: " (at 88.982857 193.225) (layer "Cmts.User"))
  (gr_text "No" (at 113.825714 189.01) (layer "Cmts.User"))
  (gr_text "Castellated pads: " (at 20.94 193.225) (layer "Cmts.User"))
  (gr_text "1775.00 mils x 1150.00 mils" (at 53.497143 180.58) (layer "Cmts.User"))
  (gr_text "No" (at 53.497143 197.44) (layer "Cmts.User"))
  (gr_text "Board overall dimensions: " (at 20.94 180.58) (layer "Cmts.User"))
  (gr_text "" (at 88.982857 180.58) (layer "Cmts.User"))
  (gr_text "2" (at 53.497143 176.365) (layer "Cmts.User"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 116.71 119.995) (xy 116.71 90.785))
    (height -12.7)
    (gr_text "1.15 in" (at 102.232 105.39 90) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 2))
    (style (thickness 0.127) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.508) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 121.79 122.535) (xy 166.875 122.535))
    (height 6.35)
    (gr_text "1.775 in" (at 144.3325 127.107) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 3))
    (style (thickness 0.127) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.508) keep_text_aligned)
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 154.302 102.215)
        (xy 151.1016 102.215)
        (xy 149.4506 103.866)
        (xy 148.841 103.2564)
        (xy 151.127 100.9704)
        (xy 153.286 100.9704)
        (xy 153.286 99.421)
        (xy 154.302 99.421)
      )
    )
  )
  (zone (net 14) (net_name "/USB_D+") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 159.255 104.49)
        (xy 159.255 104.755)
        (xy 158.493 104.755)
        (xy 158.493 103.993)
        (xy 158.747 103.993)
      )
    )
  )
  (zone (net 15) (net_name "/USB_D-") (layers F&B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 159.255 106.29)
        (xy 159.255 106.025)
        (xy 158.493 106.025)
        (xy 158.493 106.787)
        (xy 158.747 106.787)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "3V3McuFill") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1524) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 150.8984 105.39)
        (xy 146.936 109.3524)
        (xy 142.9736 105.39)
        (xy 146.936 101.4276)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.175 96.627)
        (xy 153.667 96.627)
        (xy 153.667 96.246)
        (xy 154.175 96.246)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "3V3BufFill") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.966 113.264)
        (xy 129.664 113.264)
        (xy 129.664 97.516)
        (xy 132.966 97.516)
      )
    )
  )
  (zone (net 4) (net_name "+1V1") (layer "F.Cu") (name "1V1McuFIll") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 148.6632 103.7898)
        (xy 148.5108 103.9422)
        (xy 149.984 105.4154)
        (xy 146.936 108.4634)
        (xy 146.1994 107.7268)
        (xy 146.047 107.8792)
        (xy 145.5898 107.422)
        (xy 146.1994 106.8124)
        (xy 146.936 107.549)
        (xy 149.095 105.39)
        (xy 147.7996 104.0946)
        (xy 148.2314 103.6628)
        (xy 148.5362 103.6628)
      )
    )
  )
  (zone (net 12) (net_name "VUSB") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 163.065 107.7014)
        (xy 161.668 107.7014)
        (xy 161.668 108.184)
        (xy 159.509 108.184)
        (xy 159.509 102.596)
        (xy 161.668 102.596)
        (xy 161.668 103.0786)
        (xy 163.065 103.0786)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (name "GndFill") (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 166.875 119.995)
        (xy 121.79 119.995)
        (xy 121.79 90.785)
        (xy 166.875 90.785)
      )
    )
  )
)
