(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 19)
    (no_connects 0)
    (area 130.988999 109.652999 156.539001 135.203001)
    (thickness 1.6)
    (drawings 44)
    (tracks 64)
    (zones 0)
    (modules 8)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.244)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 PB0)
  (net 4 "Net-(D1-Pad1)")
  (net 5 PB5)
  (net 6 PB3)
  (net 7 PB1)
  (net 8 PB4)
  (net 9 PB2)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net PB0)
    (add_net PB1)
    (add_net PB2)
    (add_net PB3)
    (add_net PB4)
    (add_net PB5)
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5A778999)
    (at 154.432 111.76 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Battery1 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A77EA04)
    (at 147.828 133.096)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 3.81 0) (layer F.SilkS))
    (fp_text value LED (at 3.302 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 PB0))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A778B44)
    (at 140.208 119.888)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference IC1 (at 3.937 5.334) (layer F.SilkS) hide)
    (fp_text value ATTINY85-P (at 3.937 -2.286) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 PB5))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 PB0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 PB3))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 PB1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 PB4))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 PB2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 5A778B4F)
    (at 133.096 128.524 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference Left1 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.191 -3.175 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 PB4))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 PB3))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 PB5))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 5A778B6F)
    (at 138.176 111.76 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Programmer1 (at -4.318 2.794 360) (layer F.SilkS) hide)
    (fp_text value CONN_02X03 (at -2.794 2.667 360) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 PB5))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 PB0))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 PB2))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 PB1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A77EA0C)
    (at 140.716 133.096 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 4.572 0 180) (layer F.SilkS))
    (fp_text value 200 (at 3.937 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 5A778B67)
    (at 154.432 128.524 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference Right1 (at 3.683 4.826 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 3.937 3.175 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 PB0))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 PB1))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 PB2))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 5A7798DE)
    (at 144.018 130.556 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912 180) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 180) (layer B.Fab) hide)
  )
  (gr_text ATTiny25/45/85 (at 144.0815 130.175) (layer F.SilkS))
  (gr_text "ADM '18" (at 152.908 134.112) (layer B.SilkS))
  (gr_text VCC (at 154.559 115.189 90) (layer B.SilkS))
  (gr_text GND (at 151.892 115.189 90) (layer B.SilkS))
  (gr_text PB0 (at 151.13 128.524) (layer B.SilkS))
  (gr_text PB1 (at 151.13 125.984) (layer B.SilkS))
  (gr_text PB2 (at 151.13 123.444) (layer B.SilkS))
  (gr_text VCC (at 151.13 120.904) (layer B.SilkS))
  (gr_text GND (at 136.398 128.524) (layer B.SilkS))
  (gr_text PB4 (at 136.398 125.984) (layer B.SilkS))
  (gr_text PB3 (at 136.398 123.444) (layer B.SilkS))
  (gr_text PB5 (at 136.398 120.904) (layer B.SilkS))
  (gr_text Programmer (at 145.0975 116.967) (layer B.SilkS))
  (gr_text PB5 (at 148.2725 114.554) (layer B.SilkS))
  (gr_text PB2 (at 145.034 114.4905) (layer B.SilkS))
  (gr_text PB1 (at 141.732 114.554) (layer B.SilkS))
  (gr_text GND (at 148.2725 111.5695) (layer B.SilkS))
  (gr_text PB0 (at 145.034 111.5695) (layer B.SilkS))
  (gr_text VCC (at 141.7955 111.5695) (layer B.SilkS))
  (gr_text PB0 (at 151.13 128.524) (layer F.SilkS))
  (gr_text PB1 (at 151.13 125.984) (layer F.SilkS))
  (gr_text PB2 (at 151.13 123.444) (layer F.SilkS))
  (gr_text VCC (at 151.13 120.904) (layer F.SilkS))
  (gr_text GND (at 136.398 128.524) (layer F.SilkS))
  (gr_text PB4 (at 136.398 125.984) (layer F.SilkS))
  (gr_text PB3 (at 136.398 123.444) (layer F.SilkS))
  (gr_text PB5 (at 136.398 120.904) (layer F.SilkS))
  (gr_text Battery (at 147.447 111.506) (layer F.SilkS))
  (gr_text VCC (at 154.559 115.189 90) (layer F.SilkS))
  (gr_text GND (at 151.892 115.189 90) (layer F.SilkS))
  (gr_text "Tiny Slammer!" (at 144.018 117.348) (layer F.SilkS))
  (gr_line (start 156.464 109.728) (end 156.464 135.128) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 109.728) (end 156.464 109.728) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 135.128) (end 131.064 109.728) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 135.128) (end 131.064 135.128) (angle 90) (layer Edge.Cuts) (width 0.15))
)
