(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 34)
    (no_connects 0)
    (area 147.244999 96.953185 165.162778 117.270966)
    (thickness 1.6)
    (drawings 28)
    (tracks 155)
    (zones 0)
    (modules 16)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.508)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 149.2 112.75)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +3V3)
  (net 5 "Net-(C4-Pad1)")
  (net 6 /SDA)
  (net 7 /SCL)
  (net 8 /RESET)
  (net 9 /INT)
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.762)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net /INT)
    (add_net /RESET)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5941B485)
    (at 163.805 98.145)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33) (layer Cmts.User))
    (fp_text value CONN_01X02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5651304F)
    (at 151.105 101.32 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.7526 0.0254 270) (layer F.SilkS))
    (fp_text value 10k (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 56513054)
    (at 151.105 98.78)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.775 0 90) (layer F.SilkS))
    (fp_text value 10k (at 2.54 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.175 109.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.455 -0.075 180) (layer F.SilkS))
    (fp_text value 22pF (at -3.275 0.025 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 154.9 109.475)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.525 0.1) (layer F.SilkS))
    (fp_text value 22pF (at -3 0.075) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565144FA)
    (at 160.35 105.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.185 -1.675 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.55 -1.55 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565144EF)
    (at 160.375 102.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.125 -1.475 270) (layer F.SilkS))
    (fp_text value 100nF (at -1.13 -1.525 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565144D7)
    (at 151.105 106.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.675 0 90) (layer F.SilkS))
    (fp_text value 10k (at 2.54 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565144D1)
    (at 151.105 103.86)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.7 -0.025 90) (layer F.SilkS))
    (fp_text value 10k (at 2.54 -0.05) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:ABS07-XTAL (layer F.Cu) (tedit 565217F4)
    (at 156.675 107.2)
    (tags CRYSTAL)
    (fp_text reference Y1 (at -3.03 -0.165) (layer F.SilkS))
    (fp_text value Crystal (at 0 0.47) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model "C:/Users/BSI/Google Drive/Kicad/Kicad Projects/BNO055 Breakout - Teensy/Cube.wrl"
      (at (xyz -0.063 -0.0295 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 162.535 104.38 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:LGA28 (layer F.Cu) (tedit 5650F004)
    (at 156.5 103.7125 180)
    (fp_text reference U1 (at 0 3.0275 180) (layer F.SilkS))
    (fp_text value BNO055 (at 0 2.75 180) (layer F.Fab))
    (pad 20 smd rect (at 2.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (pad 21 smd rect (at 1.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 0.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 0.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at -0.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at -0.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 27 smd rect (at -1.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 28 smd rect (at -1.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 1 smd rect (at -2.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 1.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 9 /INT))
    (pad 13 smd rect (at 1.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 0.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad 10 smd rect (at -0.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -0.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 8 smd rect (at -1.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 2.3125 -0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
    (pad 18 smd rect (at 2.3125 -0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.3125 0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad1)"))
    (pad 16 smd rect (at 2.3125 0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.3125 -0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.3125 -0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 4 smd rect (at -2.3125 0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at -2.3125 0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model "C:/Users/BSI/Google Drive/Kicad/Kicad Projects/BNO055 Breakout - Teensy/Cut.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5941B497)
    (at 163.805 113.385)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33) (layer Cmts.User))
    (fp_text value CONN_01X02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5941B4A1)
    (at 148.565 108.305)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33) (layer Cmts.User))
    (fp_text value CONN_01X02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /INT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module MyFootprints:axis_labels (layer F.Cu) (tedit 0)
    (at 157.455 114.02 180)
    (fp_text reference G*** (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer F.SilkS) hide)
  )
  (module MyFootprints:BSI_LOGO (layer F.Cu) (tedit 0)
    (at 150.47 114.02)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text SCL (at 161.392 113.258) (layer F.SilkS))
  (gr_text SDA (at 161.392 116.052) (layer F.SilkS))
  (gr_text GND (at 161.1634 98.0942) (layer F.SilkS))
  (gr_text 3V3 (at 161.265 100.7104) (layer F.SilkS))
  (gr_text RST (at 150.724 108.432) (layer F.SilkS))
  (gr_text INT (at 150.724 110.972) (layer F.SilkS))
  (gr_line (start 147.37255 116.647348) (end 147.295 116.2806) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.584292 116.946165) (end 147.37255 116.647348) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.898856 117.147276) (end 147.584292 116.946165) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.284877 117.220965) (end 147.898856 117.147276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.1229 117.220965) (end 148.284877 117.220965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.508921 117.147276) (end 164.1229 117.220965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.823486 116.946165) (end 164.508921 117.147276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.035227 116.647348) (end 164.823486 116.946165) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.112777 116.2806) (end 165.035227 116.647348) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.112777 97.94355) (end 165.112777 116.2806) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.035227 97.57683) (end 165.112777 97.94355) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.823486 97.278014) (end 165.035227 97.57683) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.508921 97.076874) (end 164.823486 97.278014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.1229 97.003186) (end 164.508921 97.076874) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.284877 97.003186) (end 164.1229 97.003186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.284877 97.003186) (end 148.284877 97.003186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.898856 97.076874) (end 148.284877 97.003186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.584292 97.278014) (end 147.898856 97.076874) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.37255 97.57683) (end 147.584292 97.278014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.295 97.94355) (end 147.37255 97.57683) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.295 116.2806) (end 147.295 97.94355) (layer Edge.Cuts) (width 0.1))
  (gr_text "EME IMU v1.1\nCopyright 2017" (at 156.185 104.495) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.9046 97.4846) (xy 164.6432 97.4846) (xy 164.6432 116.6362) (xy 147.93 116.6362) (xy 147.93 97.4846)
        (xy 147.93 97.4846)
      )
    )
  )
)
