<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.159" y2="0" width="0" layer="20"/>
<wire x1="35.159" y1="0" x2="35.159" y2="19.99" width="0" layer="20"/>
<wire x1="35.159" y1="19.99" x2="0" y2="19.99" width="0" layer="20"/>
<wire x1="0" y1="19.99" x2="0" y2="0" width="0" layer="20"/>
<text>0.1uF</text>
<text>680</text>
<text>10K</text>
<text>Incubator Control
Board V2.0
</text>
<text>by
Ecolotronics
</text>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_FEMALE_LOCK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Locking Female Headers&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/SP-140520-XX-001.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Locking Footprint&lt;/h3&gt;
Pins are staggered 0.005" off center to lock pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NO_NO-SILK">
</package>
</packages>
</library>
<library name="Seeed-Capacitor">
<packages>
<package name="PC-D5.3MM">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="capacitor-wima" package="C2.5-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VOUT__GND_TMP_CNT_LGT_INA_INB" library="SparkFun-Connectors" package="1X08_FEMALE_LOCK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09233"/>
<attribute name="SF_ID" value="PRT-09279"/>
<attribute name="VALUE"/>
</element>
<element name="CNT_INA_INB" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LIGHTS" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="12V_GND" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TEMPERATURE" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN_EXT" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN_ENT" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN_8.5V" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SYSTEM_5V" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LIGHT_SWITCH" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_NO-SILK" value="JUMPER-SMT_2_NO_NO-SILK"/>
<element name="C1" library="Seeed-Capacitor" package="PC-D5.3MM" value="22uF">
<attribute name="MPN" value="KS 100uF/16V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Seeed-Capacitor" package="PC-D5.3MM" value="22uF">
<attribute name="MPN" value="KS 100uF/16V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="12V_INPUT_" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="TEMP" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="LIGHT_CNTL" library="SparkFun-Resistors" package="AXIAL-0.3" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="12V_GND" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="3"/>
<contactref element="FAN_EXT" pad="2"/>
<contactref element="FAN_ENT" pad="2"/>
<contactref element="LIGHT_SWITCH" pad="3"/>
<contactref element="12V_INPUT_" pad="2"/>
<contactref element="SYSTEM_5V" pad="3"/>
<contactref element="C2" pad="+"/>
<contactref element="FAN_8.5V" pad="3"/>
<contactref element="C1" pad="+"/>
<contactref element="TEMPERATURE" pad="1"/>
</signal>
<signal name="TEMP_READING">
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="4"/>
<contactref element="TEMPERATURE" pad="2"/>
<contactref element="TEMP" pad="P$2"/>
</signal>
<signal name="VIN">
<contactref element="12V_GND" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="FAN_8.5V" pad="1"/>
<contactref element="SYSTEM_5V" pad="1"/>
<contactref element="12V_INPUT_" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="2"/>
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="SYSTEM_5V" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="R2" pad="P$1"/>
<contactref element="TEMP" pad="P$1"/>
</signal>
<signal name="CONTROL">
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="5"/>
<contactref element="CNT_INA_INB" pad="1"/>
</signal>
<signal name="LIGHT">
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="6"/>
<contactref element="LIGHT_CNTL" pad="P$1"/>
</signal>
<signal name="IN_A">
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="7"/>
<contactref element="CNT_INA_INB" pad="2"/>
</signal>
<signal name="IN_B">
<contactref element="VOUT__GND_TMP_CNT_LGT_INA_INB" pad="8"/>
<contactref element="CNT_INA_INB" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="LIGHT_SWITCH" pad="1"/>
<contactref element="LIGHT_CNTL" pad="P$2"/>
</signal>
<signal name="FAN">
<contactref element="FAN_EXT" pad="1"/>
<contactref element="FAN_ENT" pad="1"/>
<contactref element="FAN_8.5V" pad="2"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="N$2">
<contactref element="LIGHTS" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="LIGHT_SWITCH" pad="2"/>
<contactref element="LIGHTS" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
