<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3" y1="0" x2="43" y2="0" width="0" layer="20"/>
<wire x1="47" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="65" y2="3" width="0" layer="20" curve="90"/>
<wire x1="65" y1="3" x2="65" y2="53" width="0" layer="20"/>
<wire x1="65" y1="53" x2="62" y2="56" width="0" layer="20" curve="90"/>
<wire x1="62" y1="56" x2="3" y2="56" width="0" layer="20"/>
<wire x1="3" y1="56" x2="0" y2="53" width="0" layer="20" curve="90"/>
<wire x1="0" y1="53" x2="0" y2="37.5" width="0" layer="20"/>
<wire x1="0" y1="37.5" x2="1" y2="36.5" width="0" layer="20" curve="90"/>
<wire x1="1" y1="36.5" x2="4" y2="36.5" width="0" layer="20"/>
<wire x1="4" y1="36.5" x2="5" y2="35.5" width="0" layer="20" curve="-90"/>
<wire x1="5" y1="35.5" x2="5" y2="20.5" width="0" layer="20"/>
<wire x1="5" y1="20.5" x2="4" y2="19.5" width="0" layer="20" curve="-90"/>
<wire x1="4" y1="19.5" x2="1" y2="19.5" width="0" layer="20"/>
<wire x1="1" y1="19.5" x2="0" y2="18.5" width="0" layer="20" curve="90"/>
<wire x1="0" y1="18.5" x2="0" y2="3" width="0" layer="20"/>
<hole x="3.5" y="3.5" drill="2.8"/>
<hole x="3.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="3.5" drill="2.8"/>
<text>TOP</text>
<text>BOTTOM</text>
<wire x1="44" y1="19" x2="44" y2="1" width="0" layer="20"/>
<wire x1="46" y1="19" x2="46" y2="1" width="0" layer="20"/>
<wire x1="45" y1="20" x2="46" y2="19" width="0" layer="20" curve="-90"/>
<wire x1="45" y1="20" x2="44" y2="19" width="0" layer="20" curve="90"/>
<wire x1="44" y1="1" x2="43" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="46" y1="1" x2="47" y2="0" width="0" layer="20" curve="90"/>
<text>E7Systems</text>
</plain>
<libraries>
<library name="FLYFISH">
<packages>
<package name="PIN_20X2">
</package>
</packages>
</library>
<library name="tango">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MAGJACK">
<description>&lt;h3&gt;RJ45 Ethernet MagJack-Compatible&lt;/h3&gt;
tDocu shows where the cable plugs in
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/MagJack.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MAGJACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_PTH_BREAD">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector Breadboard Compatible&lt;/h3&gt;
Breadboard-friendly pins. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/18742.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220AH">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K1" library="FLYFISH" package="PIN_20X2" value="PIN20X2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="tango" package="DO41-10" value="1N4001">
<attribute name="MF" value="NTE ELECTRONICS"/>
<attribute name="MPN" value="1N4001"/>
<attribute name="OC_NEWARK" value="10M8464"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="1k">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="MCF 0.25W 1K"/>
<attribute name="OC_NEWARK" value="38K0327"/>
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-09556"/>
<attribute name="SF_ID" value="PRT-08534"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="POWER_JACK_PTH_BREAD" value="POWER_JACKPTH_BREAD">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="PRT-10811"/>
</element>
<element name="Q1" library="transistor-power" package="TO220AH" value="TIP120">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="TIP120"/>
<attribute name="OC_NEWARK" value="58K9558"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2k">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="MCF 0.25W 1K"/>
<attribute name="OC_NEWARK" value="38K0327"/>
<attribute name="PROD_ID" value="RES-12182"/>
</element>
</elements>
<signals>
<signal name="S$28">
</signal>
<signal name="S$33">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$60">
</signal>
<signal name="S$61">
</signal>
<signal name="S$213">
</signal>
<signal name="S$234">
</signal>
<signal name="N$7">
</signal>
<signal name="GND">
</signal>
<signal name="+5V">
<contactref element="K1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="PWR"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="8"/>
<contactref element="Q1" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="B"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="P$1"/>
<contactref element="K1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="K1" pad="11"/>
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="J2" pad="GND"/>
<contactref element="Q1" pad="E"/>
<contactref element="K1" pad="9"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="1"/>
<contactref element="K1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
