<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<circle x="11.2" y="11.2" radius="11.2" width="0.0762" layer="46"/>
<text>gChart</text>
<text>BLF</text>
<text>5A</text>
</plain>
<libraries>
<library name="gch-CN5710">
<description>Consonance CN5710 1A High Brightness LED Driver IC http://www.consonance-elec.com/</description>
<packages>
<package name="SOT89-5">
<description>SOT89-5 CN5710</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8S1">
<description>&lt;b&gt;8S1&lt;/b&gt; 8-lead (0.150" Wide Body)&lt;p&gt;
Plastic Gull Wing Small Outline (JEDEC SOIC)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="gch_UPDI_Pads">
<packages>
<package name="UPDI_PADS">
<description>UPDI Programming Key pads</description>
</package>
</packages>
</library>
<library name="gch_0603">
<packages>
<package name="0603_STANDARD">
<description>0603 Standard footprint (not undersized, according to Vishay specs)</description>
</package>
</packages>
</library>
<library name="gch_SOD323">
<packages>
<package name="SOD323">
<description>SOD323 Diode</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CR1" library="gch-CN5710" package="SOT89-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CR2" library="gch-CN5710" package="SOT89-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CR3" library="gch-CN5710" package="SOT89-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CR4" library="gch-CN5710" package="SOT89-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CR5" library="gch-CN5710" package="SOT89-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T412" library="atmel" package="8S1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$7" library="gch_UPDI_Pads" package="UPDI_PADS" value=""/>
<element name="R1" library="gch_0603" package="0603_STANDARD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="gch_0603" package="0603_STANDARD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="gch_0603" package="0603_STANDARD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="gch_0603" package="0603_STANDARD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="gch_0603" package="0603_STANDARD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C" library="gch_0603" package="0603_STANDARD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D" library="gch_SOD323" package="SOD323" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW+" library="testpad" package="TP20R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED+" library="testpad" package="TP20R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW-" library="testpad" package="TP20R" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED-" library="testpad" package="TP20R" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="D" pad="2"/>
<contactref element="T412" pad="1"/>
<contactref element="E$7" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="T412" pad="6"/>
<contactref element="E$7" pad="2"/>
</signal>
<signal name="S$3">
<contactref element="R1" pad="2"/>
<contactref element="CR1" pad="3"/>
</signal>
<signal name="S$5">
<contactref element="R2" pad="2"/>
<contactref element="CR2" pad="3"/>
</signal>
<signal name="S$8">
<contactref element="R3" pad="2"/>
<contactref element="CR3" pad="3"/>
</signal>
<signal name="S$10">
<contactref element="R4" pad="2"/>
<contactref element="CR4" pad="3"/>
</signal>
<signal name="S$12">
<contactref element="R5" pad="2"/>
<contactref element="CR5" pad="3"/>
</signal>
<signal name="S$14">
<contactref element="CR2" pad="1"/>
<contactref element="T412" pad="4"/>
<contactref element="CR3" pad="1"/>
<contactref element="CR4" pad="1"/>
<contactref element="CR5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="CR2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="CR1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="CR3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="CR4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="CR5" pad="2"/>
<contactref element="C" pad="2"/>
<contactref element="E$7" pad="3"/>
<contactref element="T412" pad="8"/>
<contactref element="LED-" pad="TP"/>
<contactref element="SW-" pad="TP"/>
</signal>
<signal name="VDD">
<contactref element="D" pad="1"/>
<contactref element="C" pad="1"/>
<contactref element="CR1" pad="4"/>
<contactref element="CR2" pad="4"/>
<contactref element="CR3" pad="4"/>
<contactref element="CR4" pad="4"/>
<contactref element="CR5" pad="4"/>
</signal>
<signal name="S$4">
<contactref element="T412" pad="5"/>
<contactref element="CR1" pad="1"/>
</signal>
<signal name="LED">
<contactref element="CR2" pad="5"/>
<contactref element="CR1" pad="5"/>
<contactref element="CR3" pad="5"/>
<contactref element="CR4" pad="5"/>
<contactref element="CR5" pad="5"/>
<contactref element="LED+" pad="TP"/>
</signal>
<signal name="S$6">
<contactref element="SW+" pad="TP"/>
<contactref element="T412" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
