(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 64)
    (zones 0)
    (modules 22)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.2)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J3-Pad1)")
  (net 2 GND)
  (net 3 /Enc1PosV)
  (net 4 Enc1A)
  (net 5 Enc0A)
  (net 6 Enc1B)
  (net 7 Enc0B)
  (net 8 Enc1Z)
  (net 9 Enc0Z)
  (net 10 3v3)
  (net 11 5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1.2)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Enc1PosV)
    (add_net 3v3)
    (add_net 5V)
    (add_net Enc0A)
    (add_net Enc0B)
    (add_net Enc0Z)
    (add_net Enc1A)
    (add_net Enc1B)
    (add_net Enc1Z)
    (add_net GND)
    (add_net "Net-(J3-Pad1)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41D)
    (at 139.7 106.68)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77) (layer F.SilkS))
    (fp_text value Conn_01x12_Female (at 0 30.71) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 3v3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 Enc1A))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 Enc1B))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 Enc1Z))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 3v3))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 5V))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 Enc0A))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 Enc0B))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 Enc0Z))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 144.78 107.95 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -0.254 -2.032 270) (layer F.SilkS))
    (fp_text value SolderJumper_3_Bridged12 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 10 3v3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 11 5V) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 3 /Enc1PosV))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 144.78 123.19 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -2.032 270) (layer F.SilkS))
    (fp_text value SolderJumper_3_Bridged12 (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 1 "Net-(J3-Pad1)"))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 11 5V) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 10 3v3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264CE)
    (at 149.86 99.06)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264DA)
    (at 149.86 142.24)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264D2)
    (at 160.02 99.06)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264DD)
    (at 160.02 142.24)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 111.76 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Enc1A))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 127 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 Enc0A))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 114.3 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Enc1B))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 129.54 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 Enc0B))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 117.225001 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.286 -0.122999 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 Enc1Z))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 132.08 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 Enc0Z))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B05B-XH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 158.496 107.95 270)
    (descr "JST XH series connector, B05B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J2 (at -2.794 5.08 270) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 5 4.6 270) (layer F.Fab))
    (fp_text user %R (at 5 2.7 270) (layer F.Fab))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 Enc1Z))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 Enc1B))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 Enc1A))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 /Enc1PosV))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B05B-XH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B05B-XH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 158.496 124.46 270)
    (descr "JST XH series connector, B05B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J3 (at 14.224 2.54 270) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 5 4.6 270) (layer F.Fab))
    (fp_text user %R (at 5 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 Enc0A))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 Enc0B))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 Enc0Z))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B05B-XH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268ED)
    (at 140.208 139.7)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP1 (at -5.588 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268B9)
    (at 150.876 110.236)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP2 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 Enc1A))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268BD)
    (at 151.892 113.284)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP3 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 Enc1B))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268C1)
    (at 150.876 117.348)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP4 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 Enc1Z))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268CA)
    (at 150.368 127)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP5 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 Enc0A))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268CD)
    (at 144.78 129.54)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP6 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 Enc0B))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268DB)
    (at 150.876 132.08)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP7 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 9 Enc0Z))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 134.62 96.52) (end 134.62 93.98) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.56 96.52) (end 165.1 96.52) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.62 144.78) (end 132.08 144.78) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.56 144.78) (end 162.56 147.32) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "M0 Encoder" (at 162.56 129.54 90) (layer F.SilkS))
  (gr_text "M1 Encoder" (at 162.56 112.776 90) (layer F.SilkS))
  (gr_text 5V (at 144.78 111.252) (layer F.SilkS))
  (gr_text 5V (at 144.78 126.492) (layer F.SilkS))
  (gr_text 3v3 (at 144.78 119.888) (layer F.SilkS))
  (gr_text 3v3 (at 145.288 104.648) (layer F.SilkS))
  (gr_line (start 165.1 144.78) (end 165.1 96.52) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 147.32) (end 162.56 147.32) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 96.52) (end 132.08 144.78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 93.98) (end 134.62 93.98) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 137.16) (xy 138.43 137.16) (xy 138.43 105.41) (xy 161.29 105.41)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.2524 99.935667) (xy 135.354 99.935667) (xy 135.354 99.961067) (xy 135.4302 99.961067) (xy 135.4302 99.986467)
        (xy 135.481 99.986467) (xy 135.481 100.011867) (xy 135.5572 100.011867) (xy 135.5572 100.037267) (xy 135.608 100.037267)
        (xy 135.608 100.062667) (xy 135.6334 100.062667) (xy 135.6334 100.088067) (xy 135.6842 100.088067) (xy 135.6842 100.113467)
        (xy 135.735 100.113467) (xy 135.735 100.138867) (xy 135.7604 100.138867) (xy 135.7604 100.164267) (xy 135.8112 100.164267)
        (xy 135.8112 100.189667) (xy 135.8366 100.189667) (xy 135.8366 100.215067) (xy 135.862 100.215067) (xy 135.862 100.240467)
        (xy 135.9128 100.240467) (xy 135.9128 100.265867) (xy 135.9382 100.265867) (xy 135.9382 100.291267) (xy 135.9636 100.291267)
        (xy 135.9636 100.316667) (xy 136.0144 100.316667) (xy 136.0144 100.342067) (xy 136.0398 100.342067) (xy 136.0398 100.367467)
        (xy 136.0652 100.367467) (xy 136.0652 100.392867) (xy 136.0906 100.392867) (xy 136.0906 100.418267) (xy 136.116 100.418267)
        (xy 136.116 100.443667) (xy 136.1414 100.443667) (xy 136.1414 100.469067) (xy 136.1668 100.469067) (xy 136.1668 100.494467)
        (xy 136.2176 100.494467) (xy 136.2176 100.469067) (xy 136.243 100.469067) (xy 136.243 100.443667) (xy 136.2684 100.443667)
        (xy 136.2684 100.418267) (xy 136.2938 100.418267) (xy 136.2938 100.392867) (xy 136.3192 100.392867) (xy 136.3192 100.367467)
        (xy 136.3446 100.367467) (xy 136.3446 100.342067) (xy 136.37 100.342067) (xy 136.37 100.316667) (xy 136.4208 100.316667)
        (xy 136.4208 100.291267) (xy 136.4462 100.291267) (xy 136.4462 100.265867) (xy 136.4716 100.265867) (xy 136.4716 100.240467)
        (xy 136.497 100.240467) (xy 136.497 100.215067) (xy 136.5478 100.215067) (xy 136.5478 100.189667) (xy 136.5732 100.189667)
        (xy 136.5732 100.164267) (xy 136.624 100.164267) (xy 136.624 100.138867) (xy 136.6494 100.138867) (xy 136.6494 100.113467)
        (xy 136.7002 100.113467) (xy 136.7002 100.088067) (xy 136.7256 100.088067) (xy 136.7256 100.062667) (xy 136.7764 100.062667)
        (xy 136.7764 100.037267) (xy 136.8272 100.037267) (xy 136.8272 100.011867) (xy 136.9034 100.011867) (xy 136.9034 99.986467)
        (xy 136.9542 99.986467) (xy 136.9542 99.961067) (xy 137.0304 99.961067) (xy 137.0304 99.935667) (xy 137.132 99.935667)
        (xy 137.132 99.910267) (xy 137.64 99.910267) (xy 137.64 99.935667) (xy 137.767 99.935667) (xy 137.767 99.961067)
        (xy 137.8432 99.961067) (xy 137.8432 99.986467) (xy 137.9194 99.986467) (xy 137.9194 100.011867) (xy 137.9702 100.011867)
        (xy 137.9702 100.037267) (xy 138.021 100.037267) (xy 138.021 100.062667) (xy 138.0718 100.062667) (xy 138.0718 100.088067)
        (xy 138.1226 100.088067) (xy 138.1226 100.113467) (xy 138.1734 100.113467) (xy 138.1734 100.138867) (xy 138.1988 100.138867)
        (xy 138.1988 100.164267) (xy 138.2242 100.164267) (xy 138.2242 100.189667) (xy 138.2496 100.189667) (xy 138.2496 100.215067)
        (xy 138.275 100.215067) (xy 138.275 100.240467) (xy 138.3258 100.240467) (xy 138.3258 100.291267) (xy 138.3512 100.291267)
        (xy 138.3512 100.316667) (xy 138.3766 100.316667) (xy 138.3766 100.342067) (xy 138.402 100.342067) (xy 138.402 100.367467)
        (xy 138.4274 100.367467) (xy 138.4274 100.418267) (xy 138.4528 100.418267) (xy 138.4528 100.443667) (xy 138.4782 100.443667)
        (xy 138.4782 100.494467) (xy 138.5036 100.494467) (xy 138.5036 100.545267) (xy 138.529 100.545267) (xy 138.529 100.596067)
        (xy 138.5544 100.596067) (xy 138.5544 100.646867) (xy 138.5798 100.646867) (xy 138.5798 100.723067) (xy 138.6052 100.723067)
        (xy 138.6052 100.850067) (xy 138.6306 100.850067) (xy 138.6306 101.027867) (xy 138.656 101.027867) (xy 138.656 101.307267)
        (xy 138.6306 101.307267) (xy 138.6306 101.459667) (xy 138.6052 101.459667) (xy 138.6052 101.561267) (xy 138.5798 101.561267)
        (xy 138.5798 101.637467) (xy 138.5544 101.637467) (xy 138.5544 101.713667) (xy 138.529 101.713667) (xy 138.529 101.764467)
        (xy 138.5036 101.764467) (xy 138.5036 101.815267) (xy 138.4782 101.815267) (xy 138.4782 101.840667) (xy 138.4528 101.840667)
        (xy 138.4528 101.891467) (xy 138.4274 101.891467) (xy 138.4274 101.942267) (xy 138.402 101.942267) (xy 138.402 101.993067)
        (xy 138.3766 101.993067) (xy 138.3766 102.018467) (xy 138.3512 102.018467) (xy 138.3512 102.043867) (xy 138.3258 102.043867)
        (xy 138.3258 102.094667) (xy 138.3004 102.094667) (xy 138.3004 102.120067) (xy 138.275 102.120067) (xy 138.275 102.145467)
        (xy 138.2496 102.145467) (xy 138.2496 102.196267) (xy 138.2242 102.196267) (xy 138.2242 102.221667) (xy 138.1988 102.221667)
        (xy 138.1988 102.247067) (xy 138.1734 102.247067) (xy 138.1734 102.272467) (xy 138.148 102.272467) (xy 138.148 102.297867)
        (xy 138.1226 102.297867) (xy 138.1226 102.323267) (xy 138.0972 102.323267) (xy 138.0972 102.348667) (xy 138.0718 102.348667)
        (xy 138.0718 102.399467) (xy 138.0464 102.399467) (xy 138.0464 102.424867) (xy 138.021 102.424867) (xy 138.021 102.450267)
        (xy 137.9702 102.450267) (xy 137.9702 102.475667) (xy 137.9448 102.475667) (xy 137.9448 102.501067) (xy 137.9194 102.501067)
        (xy 137.9194 102.526467) (xy 137.894 102.526467) (xy 137.894 102.551867) (xy 137.8686 102.551867) (xy 137.8686 102.577267)
        (xy 137.8432 102.577267) (xy 137.8432 102.602667) (xy 137.8178 102.602667) (xy 137.8178 102.628067) (xy 137.7924 102.628067)
        (xy 137.7924 102.653467) (xy 137.767 102.653467) (xy 137.767 102.678867) (xy 137.7416 102.678867) (xy 137.7416 102.704267)
        (xy 137.7162 102.704267) (xy 137.7162 102.729667) (xy 137.6908 102.729667) (xy 137.6908 102.755067) (xy 137.6654 102.755067)
        (xy 137.6654 102.780467) (xy 137.64 102.780467) (xy 137.64 102.805867) (xy 137.6146 102.805867) (xy 137.6146 102.831267)
        (xy 137.5892 102.831267) (xy 137.5892 102.856667) (xy 137.5638 102.856667) (xy 137.5638 102.882067) (xy 137.5384 102.882067)
        (xy 137.5384 102.907467) (xy 137.513 102.907467) (xy 137.513 102.932867) (xy 137.4876 102.932867) (xy 137.4876 102.958267)
        (xy 137.4622 102.958267) (xy 137.4622 102.983667) (xy 137.4368 102.983667) (xy 137.4368 103.009067) (xy 137.4114 103.009067)
        (xy 137.4114 103.034467) (xy 137.386 103.034467) (xy 137.386 103.059867) (xy 137.3606 103.059867) (xy 137.3606 103.085267)
        (xy 137.3098 103.085267) (xy 137.3098 103.110667) (xy 137.2844 103.110667) (xy 137.2844 103.136067) (xy 137.259 103.136067)
        (xy 137.259 103.161467) (xy 137.2336 103.161467) (xy 137.2336 103.186867) (xy 137.2082 103.186867) (xy 137.2082 103.212267)
        (xy 137.1828 103.212267) (xy 137.1828 103.237667) (xy 137.1574 103.237667) (xy 137.1574 103.263067) (xy 137.132 103.263067)
        (xy 137.132 103.288467) (xy 137.1066 103.288467) (xy 137.1066 103.313867) (xy 137.0812 103.313867) (xy 137.0812 103.339267)
        (xy 137.0558 103.339267) (xy 137.0558 103.364667) (xy 137.0304 103.364667) (xy 137.0304 103.390067) (xy 137.005 103.390067)
        (xy 137.005 103.415467) (xy 136.9796 103.415467) (xy 136.9796 103.440867) (xy 136.9542 103.440867) (xy 136.9542 103.466267)
        (xy 136.9288 103.466267) (xy 136.9288 103.491667) (xy 136.9034 103.491667) (xy 136.9034 103.517067) (xy 136.878 103.517067)
        (xy 136.878 103.542467) (xy 136.8526 103.542467) (xy 136.8526 103.567867) (xy 136.8272 103.567867) (xy 136.8272 103.593267)
        (xy 136.8018 103.593267) (xy 136.8018 103.618667) (xy 136.7764 103.618667) (xy 136.7764 103.644067) (xy 136.751 103.644067)
        (xy 136.751 103.669467) (xy 136.7256 103.669467) (xy 136.7256 103.694867) (xy 136.7002 103.694867) (xy 136.7002 103.720267)
        (xy 136.6748 103.720267) (xy 136.6748 103.745667) (xy 136.624 103.745667) (xy 136.624 103.771067) (xy 136.5986 103.771067)
        (xy 136.5986 103.796467) (xy 136.5732 103.796467) (xy 136.5732 103.821867) (xy 136.5478 103.821867) (xy 136.5478 103.847267)
        (xy 136.5224 103.847267) (xy 136.5224 103.872667) (xy 136.497 103.872667) (xy 136.497 103.898067) (xy 136.4716 103.898067)
        (xy 136.4716 103.923467) (xy 136.4462 103.923467) (xy 136.4462 103.948867) (xy 136.4208 103.948867) (xy 136.4208 103.974267)
        (xy 136.3954 103.974267) (xy 136.3954 103.999667) (xy 136.37 103.999667) (xy 136.37 104.025067) (xy 136.3446 104.025067)
        (xy 136.3446 104.050467) (xy 136.3192 104.050467) (xy 136.3192 104.075867) (xy 136.2938 104.075867) (xy 136.2938 104.101267)
        (xy 136.243 104.101267) (xy 136.243 104.126667) (xy 136.1414 104.126667) (xy 136.1414 104.101267) (xy 136.0906 104.101267)
        (xy 136.0906 104.075867) (xy 136.0652 104.075867) (xy 136.0652 104.050467) (xy 136.0398 104.050467) (xy 136.0398 104.025067)
        (xy 136.0144 104.025067) (xy 136.0144 103.999667) (xy 135.989 103.999667) (xy 135.989 103.974267) (xy 135.9636 103.974267)
        (xy 135.9636 103.948867) (xy 135.9382 103.948867) (xy 135.9382 103.923467) (xy 135.9128 103.923467) (xy 135.9128 103.898067)
        (xy 135.8874 103.898067) (xy 135.8874 103.872667) (xy 135.862 103.872667) (xy 135.862 103.847267) (xy 135.8366 103.847267)
        (xy 135.8366 103.821867) (xy 135.8112 103.821867) (xy 135.8112 103.796467) (xy 135.7858 103.796467) (xy 135.7858 103.771067)
        (xy 135.7604 103.771067) (xy 135.7604 103.745667) (xy 135.735 103.745667) (xy 135.735 103.720267) (xy 135.6842 103.720267)
        (xy 135.6842 103.694867) (xy 135.6588 103.694867) (xy 135.6588 103.669467) (xy 135.6334 103.669467) (xy 135.6334 103.644067)
        (xy 135.608 103.644067) (xy 135.608 103.618667) (xy 135.5826 103.618667) (xy 135.5826 103.593267) (xy 135.5572 103.593267)
        (xy 135.5572 103.567867) (xy 135.5318 103.567867) (xy 135.5318 103.542467) (xy 135.5064 103.542467) (xy 135.5064 103.517067)
        (xy 135.481 103.517067) (xy 135.481 103.491667) (xy 135.4556 103.491667) (xy 135.4556 103.466267) (xy 135.4302 103.466267)
        (xy 135.4302 103.440867) (xy 135.4048 103.440867) (xy 135.4048 103.415467) (xy 135.3794 103.415467) (xy 135.3794 103.390067)
        (xy 135.354 103.390067) (xy 135.354 103.364667) (xy 135.3286 103.364667) (xy 135.3286 103.339267) (xy 135.3032 103.339267)
        (xy 135.3032 103.313867) (xy 135.2778 103.313867) (xy 135.2778 103.288467) (xy 135.2524 103.288467) (xy 135.2524 103.263067)
        (xy 135.227 103.263067) (xy 135.227 103.237667) (xy 135.2016 103.237667) (xy 135.2016 103.212267) (xy 135.1762 103.212267)
        (xy 135.1762 103.186867) (xy 135.1508 103.186867) (xy 135.1508 103.161467) (xy 135.1254 103.161467) (xy 135.1254 103.136067)
        (xy 135.1 103.136067) (xy 135.1 103.110667) (xy 135.0746 103.110667) (xy 135.0746 103.085267) (xy 135.0238 103.085267)
        (xy 135.0238 103.059867) (xy 134.9984 103.059867) (xy 134.9984 103.034467) (xy 134.973 103.034467) (xy 134.973 103.009067)
        (xy 134.9476 103.009067) (xy 134.9476 102.983667) (xy 134.9222 102.983667) (xy 134.9222 102.958267) (xy 134.8968 102.958267)
        (xy 134.8968 102.932867) (xy 134.8714 102.932867) (xy 134.8714 102.907467) (xy 134.846 102.907467) (xy 134.846 102.882067)
        (xy 134.8206 102.882067) (xy 134.8206 102.856667) (xy 134.7952 102.856667) (xy 134.7952 102.831267) (xy 134.7698 102.831267)
        (xy 134.7698 102.805867) (xy 134.7444 102.805867) (xy 134.7444 102.780467) (xy 134.719 102.780467) (xy 134.719 102.755067)
        (xy 134.6936 102.755067) (xy 134.6936 102.729667) (xy 134.6682 102.729667) (xy 134.6682 102.704267) (xy 134.6428 102.704267)
        (xy 134.6428 102.678867) (xy 134.6174 102.678867) (xy 134.6174 102.653467) (xy 134.592 102.653467) (xy 134.592 102.628067)
        (xy 134.5666 102.628067) (xy 134.5666 102.602667) (xy 134.5412 102.602667) (xy 134.5412 102.577267) (xy 134.5158 102.577267)
        (xy 134.5158 102.551867) (xy 134.4904 102.551867) (xy 134.4904 102.526467) (xy 134.465 102.526467) (xy 134.465 102.501067)
        (xy 134.4396 102.501067) (xy 134.4396 102.475667) (xy 134.4142 102.475667) (xy 134.4142 102.450267) (xy 134.3634 102.450267)
        (xy 134.3634 102.399467) (xy 134.3126 102.399467) (xy 134.3126 102.374067) (xy 134.2872 102.374067) (xy 134.2872 102.348667)
        (xy 134.2618 102.348667) (xy 134.2618 102.297867) (xy 134.2364 102.297867) (xy 134.2364 102.272467) (xy 134.211 102.272467)
        (xy 134.211 102.247067) (xy 134.1856 102.247067) (xy 134.1856 102.221667) (xy 134.1602 102.221667) (xy 134.1602 102.196267)
        (xy 134.1348 102.196267) (xy 134.1348 102.145467) (xy 134.1094 102.145467) (xy 134.1094 102.120067) (xy 134.084 102.120067)
        (xy 134.084 102.094667) (xy 134.0586 102.094667) (xy 134.0586 102.043867) (xy 134.0332 102.043867) (xy 134.0332 102.018467)
        (xy 134.0078 102.018467) (xy 134.0078 101.993067) (xy 133.9824 101.993067) (xy 133.9824 101.942267) (xy 133.957 101.942267)
        (xy 133.957 101.891467) (xy 133.9316 101.891467) (xy 133.9316 101.840667) (xy 133.9062 101.840667) (xy 133.9062 101.815267)
        (xy 133.8808 101.815267) (xy 133.8808 101.764467) (xy 133.8554 101.764467) (xy 133.8554 101.688267) (xy 133.83 101.688267)
        (xy 133.83 101.637467) (xy 133.8046 101.637467) (xy 133.8046 101.561267) (xy 133.7792 101.561267) (xy 133.7792 101.485067)
        (xy 133.7538 101.485067) (xy 133.7538 101.358067) (xy 133.7284 101.358067) (xy 133.7284 100.977067) (xy 133.7538 100.977067)
        (xy 133.7538 100.824667) (xy 133.7792 100.824667) (xy 133.7792 100.723067) (xy 133.8046 100.723067) (xy 133.8046 100.646867)
        (xy 133.83 100.646867) (xy 133.83 100.596067) (xy 133.8554 100.596067) (xy 133.8554 100.545267) (xy 133.8808 100.545267)
        (xy 133.8808 100.494467) (xy 133.9062 100.494467) (xy 133.9062 100.443667) (xy 133.9316 100.443667) (xy 133.9316 100.418267)
        (xy 133.957 100.418267) (xy 133.957 100.367467) (xy 133.9824 100.367467) (xy 133.9824 100.342067) (xy 134.0078 100.342067)
        (xy 134.0078 100.316667) (xy 134.0332 100.316667) (xy 134.0332 100.291267) (xy 134.0586 100.291267) (xy 134.0586 100.240467)
        (xy 134.084 100.240467) (xy 134.084 100.215067) (xy 134.1348 100.215067) (xy 134.1348 100.189667) (xy 134.1602 100.189667)
        (xy 134.1602 100.164267) (xy 134.1856 100.164267) (xy 134.1856 100.138867) (xy 134.211 100.138867) (xy 134.211 100.113467)
        (xy 134.2618 100.113467) (xy 134.2618 100.088067) (xy 134.3126 100.088067) (xy 134.3126 100.062667) (xy 134.3634 100.062667)
        (xy 134.3634 100.037267) (xy 134.4142 100.037267) (xy 134.4142 100.011867) (xy 134.465 100.011867) (xy 134.465 99.986467)
        (xy 134.5412 99.986467) (xy 134.5412 99.961067) (xy 134.6174 99.961067) (xy 134.6174 99.935667) (xy 134.7444 99.935667)
        (xy 134.7444 99.910267) (xy 135.2524 99.910267)
      )
    )
  )
)
