(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 103)
    (zones 0)
    (modules 14)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VCC)
  (net 3 /SCL)
  (net 4 /SDA)
  (net 5 "Net-(SW1-Pad1)")
  (net 6 "Net-(SW2-Pad1)")
  (net 7 "Net-(SW3-Pad1)")
  (net 8 "Net-(SW4-Pad1)")
  (net 9 "Net-(SW5-Pad1)")
  (net 10 "Net-(SW6-Pad1)")
  (net 11 "Net-(U1-Pad5)")
  (net 12 "Net-(TP2-Pad1)")
  (net 13 "Net-(TP3-Pad1)")
  (net 14 "Net-(TP4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(SW3-Pad1)")
    (add_net "Net-(SW4-Pad1)")
    (add_net "Net-(SW5-Pad1)")
    (add_net "Net-(SW6-Pad1)")
    (add_net "Net-(TP2-Pad1)")
    (add_net "Net-(TP3-Pad1)")
    (add_net "Net-(TP4-Pad1)")
    (add_net "Net-(U1-Pad5)")
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 161.544 82.296 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 /VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 5CE5BFB4)
    (at 144.526 83.82)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 -1.648) (layer F.Fab) hide)
    (fp_text value TxD (at 0 -2.286) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Mask F.Cu)
      (net 13 "Net-(TP3-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 5CEDCEE2)
    (at 137.922 83.82)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.648) (layer F.Fab) hide)
    (fp_text value RxD (at 0 -2.032) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Mask F.Cu F.SilkS)
      (net 14 "Net-(TP4-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 5CE5BFC5)
    (at 155.956 90.17)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP2 (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value UPDI (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Mask F.Cu)
      (net 12 "Net-(TP2-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 5A0F774F)
    (at 147.828 90.17)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value GND (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 153.416 83.82 270)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 -5.28 90) (layer F.SilkS))
    (fp_text value ATtiny1614-SS (at -0.254 0.254 180) (layer F.Fab))
    (pad 14 smd roundrect (at 2.475 -3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at 2.475 -2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(SW3-Pad1)"))
    (pad 12 smd roundrect (at 2.475 -1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(SW2-Pad1)"))
    (pad 11 smd roundrect (at 2.475 0 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(SW1-Pad1)"))
    (pad 10 smd roundrect (at 2.475 1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(TP2-Pad1)"))
    (pad 9 smd roundrect (at 2.475 2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /SCL))
    (pad 8 smd roundrect (at 2.475 3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /SDA))
    (pad 7 smd roundrect (at -2.475 3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(TP3-Pad1)"))
    (pad 6 smd roundrect (at -2.475 2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(TP4-Pad1)"))
    (pad 5 smd roundrect (at -2.475 1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U1-Pad5)"))
    (pad 4 smd roundrect (at -2.475 0 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(SW6-Pad1)"))
    (pad 3 smd roundrect (at -2.475 -1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(SW5-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(SW4-Pad1)"))
    (pad 1 smd roundrect (at -2.475 -3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer B.Cu) (tedit 5A02FE24)
    (at 107.95 94.234)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW6 (at -2.54 2.794) (layer B.SilkS))
    (fp_text value SW_Push (at -2.54 -12.954) (layer B.Fab))
    (fp_text user %R (at -2.54 2.794) (layer B.Fab))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 -2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 "Net-(SW6-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer B.Cu) (tedit 5A02FE24)
    (at 127 94.234)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW5 (at -2.54 2.794) (layer B.SilkS))
    (fp_text value SW_Push (at -2.54 -12.954) (layer B.Fab))
    (fp_text user %R (at -2.54 2.794) (layer B.Fab))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 -2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 "Net-(SW5-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer B.Cu) (tedit 5A02FE24)
    (at 146.05 94.234)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW4 (at -2.54 2.794) (layer B.SilkS))
    (fp_text value SW_Push (at -2.54 -12.954) (layer B.Fab))
    (fp_text user %R (at -2.54 2.794) (layer B.Fab))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 -2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(SW4-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer B.Cu) (tedit 5A02FE24)
    (at 165.1 94.234)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW3 (at -2.54 2.794) (layer B.SilkS))
    (fp_text value SW_Push (at -2.54 -12.954) (layer B.Fab))
    (fp_text user %R (at -2.54 2.794) (layer B.Fab))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 -2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(SW3-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer B.Cu) (tedit 5A02FE24)
    (at 184.15 94.234)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW2 (at -2.54 2.794) (layer B.SilkS))
    (fp_text value SW_Push (at -2.54 -12.954) (layer B.Fab))
    (fp_text user %R (at -2.54 2.794) (layer B.Fab))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 -2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(SW2-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer B.Cu) (tedit 5A02FE24)
    (at 203.2 94.234)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW1 (at -2.54 2.794) (layer B.SilkS))
    (fp_text value SW_Push (at -2.54 -12.954) (layer B.Fab))
    (fp_text user %R (at -2.54 2.794) (layer B.Fab))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 -2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(SW1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 97.028 88.9 270)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J2 (at 5.08 2.032 90) (layer F.SilkS))
    (fp_text value Qwiic (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad MP smd roundrect (at 2.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -2.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 4 smd roundrect (at 1.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /SCL))
    (pad 3 smd roundrect (at 0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /SDA))
    (pad 2 smd roundrect (at -0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VCC))
    (pad 1 smd roundrect (at -1.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 209.296 88.9 90)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J1 (at 5.08 1.778 90) (layer F.SilkS))
    (fp_text value Qwiic (at -7.62 1.524 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad MP smd roundrect (at 2.8 1.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -2.8 1.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 4 smd roundrect (at 1.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /SCL))
    (pad 3 smd roundrect (at 0.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /SDA))
    (pad 2 smd roundrect (at -0.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VCC))
    (pad 1 smd roundrect (at -1.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RxD (at 137.922 81.534) (layer F.SilkS))
  (gr_text TxD (at 144.78 81.534) (layer F.SilkS))
  (gr_text UPDI (at 154.432 92.202) (layer F.SilkS))
  (gr_line (start 93.472 78.74) (end 93.472 99.568) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.472 99.568) (end 212.852 99.568) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.852 78.74) (end 212.852 99.568) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.472 78.74) (end 212.852 78.74) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.344 79.248) (xy 212.344 99.06) (xy 93.98 99.06) (xy 93.98 79.248)
      )
    )
  )
  (zone (net 2) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.344 79.248) (xy 212.344 99.06) (xy 93.98 99.06) (xy 93.98 79.248)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.344 84.963) (xy 212.344 92.837) (xy 209.55 92.837) (xy 209.55 84.963)
      )
    )
  )
)
