(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 44)
    (zones 0)
    (modules 8)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 Pwr_5v)
  (net 2 Ground)
  (net 3 S_OutA)
  (net 4 S_OutR)
  (net 5 S_OutL)
  (net 6 "Net-(R1-Pad1)")
  (net 7 "Net-(R2-Pad1)")
  (net 8 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Ground)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net Pwr_5v)
    (add_net S_OutA)
    (add_net S_OutL)
    (add_net S_OutR)
  )
  (module Button_Schwartz:Button (layer F.Cu) (tedit 5C364B22)
    (at 135.25 100.75 180)
    (fp_text reference BttnL (at 0 -2.85 180) (layer F.SilkS))
    (fp_text value BttnL (at 0 1.35 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.25 -2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 6.25 -2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 S_OutL))
    (pad 4 thru_hole circle (at 6.25 2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -6.25 2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 Pwr_5v))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 142 108.75 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R1 (at 6.45 -0.25 180) (layer F.SilkS))
    (fp_text value R (at 6.35 2.86 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Ground))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 144 87.5)
    (fp_text reference "" (at 152.25 100.75) (layer F.SilkS))
    (fp_text value "" (at 152.25 100.75) (layer F.SilkS))
    (fp_text user BttnA (at 154.5 99.65) (layer F.Fab))
    (fp_text user BttnR (at 163 114.35) (layer F.Fab))
    (fp_text user BttnL (at 146 111.65) (layer F.Fab))
  )
  (module Button_Schwartz:Button (layer F.Cu) (tedit 5C364B2A)
    (at 152.25 100.75)
    (fp_text reference BttnR (at 0 2.75) (layer F.SilkS))
    (fp_text value BttnR (at 0.25 -1.75) (layer F.Fab))
    (pad 3 thru_hole circle (at -6.25 2.5) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 Pwr_5v))
    (pad 4 thru_hole circle (at 6.25 2.5) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.25 -2.5) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 S_OutR))
    (pad 1 thru_hole circle (at -6.25 -2.5) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(R2-Pad1)"))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 137.25 112)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R2 (at 6.25 0) (layer F.SilkS))
    (fp_text value R (at 6.35 2.86) (layer F.Fab))
    (pad 2 thru_hole oval (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Ground))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 148.83 115.25 270)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (fp_text reference J1 (at 4.385 -2.27 270) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 4.385 12.43 270) (layer F.Fab))
    (fp_text user %R (at 2.77 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 S_OutL))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 S_OutA))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 S_OutR))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Ground))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Pwr_5v))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 145.5 108.75)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R3 (at 6.5 0.25) (layer F.SilkS))
    (fp_text value R (at 6.35 2.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Ground))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Schwartz:Button (layer F.Cu) (tedit 5C364B33)
    (at 143.75 88.75 180)
    (fp_text reference BttnA (at 0 -2.85 180) (layer F.SilkS))
    (fp_text value BttnA (at 0 1.35 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.25 -2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 6.25 -2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 S_OutA))
    (pad 4 thru_hole circle (at 6.25 2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -6.25 2.5 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 Pwr_5v))
  )
  (gr_text R (at 143.75 117.25) (layer F.SilkS))
  (gr_text A (at 141.25 117.25) (layer F.SilkS))
  (gr_text L (at 138.75 117.25) (layer F.SilkS))
  (gr_circle (center 130.5 85.5) (end 130.5 83.5) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 157 85.5) (end 157 83.5) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 157 114) (end 157 112) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 130.5 114) (end 130.5 112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.5 117) (end 126.5 82.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160 118) (end 127.5 118) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161 82.5) (end 161 117) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.5 81.5) (end 160 81.5) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 127.5 82.5) (end 127.5 81.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 127.5 117) (end 126.5 117) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 160 117) (end 160 118) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 160 82.5) (end 161 82.5) (angle -90) (layer Edge.Cuts) (width 0.1))
)
