<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="25.4" y1="0" x2="25.4" y2="19.05" width="0.254" layer="20"/>
<wire x1="0" y1="19.05" x2="0" y2="0" width="0.254" layer="20"/>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0.254" layer="20"/>
<text>VFD Breakout v2 KD0GLS 2017</text>
<text>+5V</text>
<text>+HV</text>
<text>GND</text>
<text>DI</text>
<text>CK</text>
<text>LD</text>
<text>BL</text>
<wire x1="0" y1="19.05" x2="25.4" y2="19.05" width="0.254" layer="20" curve="-180"/>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="IV-18">
<description>IV-18 VFD tube</description>
</package>
<package name="TSSOP28">
<description>TSSOP28</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="1X07">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="VFD1" library="kd0gls" package="IV-18" value="IV-18"/>
<element name="U1" library="kd0gls" package="TSSOP28" value="MAX6921AU">
<attribute name="VALUE"/>
</element>
<element name="C2" library="kd0gls" package="0805" value="CAPACITOR.0805"/>
<element name="C1" library="kd0gls" package="0805" value="CAPACITOR.0805"/>
<element name="J1" library="SparkFun" package="1X07" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="21"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="VFD1" pad="1"/>
</signal>
<signal name="OUT1">
<contactref element="U1" pad="4"/>
<contactref element="VFD1" pad="12"/>
</signal>
<signal name="OUT2">
<contactref element="U1" pad="3"/>
<contactref element="VFD1" pad="11"/>
</signal>
<signal name="OUT3">
<contactref element="U1" pad="2"/>
<contactref element="VFD1" pad="10"/>
</signal>
<signal name="OUT4">
<contactref element="U1" pad="1"/>
<contactref element="VFD1" pad="9"/>
</signal>
<signal name="OUT5">
<contactref element="U1" pad="28"/>
<contactref element="VFD1" pad="5"/>
</signal>
<signal name="OUT6">
<contactref element="U1" pad="27"/>
<contactref element="VFD1" pad="4"/>
</signal>
<signal name="OUT7">
<contactref element="U1" pad="26"/>
<contactref element="VFD1" pad="3"/>
</signal>
<signal name="OUT8">
<contactref element="U1" pad="25"/>
<contactref element="VFD1" pad="2"/>
</signal>
<signal name="OUT10">
<contactref element="U1" pad="19"/>
<contactref element="VFD1" pad="18"/>
</signal>
<signal name="OUT11">
<contactref element="U1" pad="18"/>
<contactref element="VFD1" pad="19"/>
</signal>
<signal name="OUT12">
<contactref element="U1" pad="17"/>
<contactref element="VFD1" pad="22"/>
</signal>
<signal name="OUT13">
<contactref element="U1" pad="16"/>
<contactref element="VFD1" pad="21"/>
</signal>
<signal name="OUT14">
<contactref element="U1" pad="15"/>
<contactref element="VFD1" pad="20"/>
</signal>
<signal name="OUT15">
<contactref element="U1" pad="14"/>
<contactref element="VFD1" pad="16"/>
</signal>
<signal name="OUT16">
<contactref element="U1" pad="13"/>
<contactref element="VFD1" pad="15"/>
</signal>
<signal name="OUT18">
<contactref element="U1" pad="11"/>
<contactref element="VFD1" pad="17"/>
</signal>
<signal name="OUT17">
<contactref element="U1" pad="12"/>
<contactref element="VFD1" pad="14"/>
</signal>
<signal name="BLANK">
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="U1" pad="22"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="DIN">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="LOAD">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="+HV">
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="VFD1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
