(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 1192)
    (zones 0)
    (modules 34)
    (nets 90)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad14)")
  (net 2 "Net-(U1-Pad17)")
  (net 3 "Net-(U1-Pad18)")
  (net 4 "Net-(U1-Pad19)")
  (net 5 "Net-(U1-Pad20)")
  (net 6 "Net-(U1-Pad23)")
  (net 7 "Net-(U3-Pad16)")
  (net 8 "Net-(U3-Pad17)")
  (net 9 "Net-(U3-Pad18)")
  (net 10 "Net-(U4-Pad8)")
  (net 11 "Net-(U4-Pad9)")
  (net 12 "Net-(U5-Pad16)")
  (net 13 "Net-(U5-Pad15)")
  (net 14 "Net-(U5-Pad13)")
  (net 15 "Net-(U5-Pad12)")
  (net 16 "Net-(U5-Pad10)")
  (net 17 "Net-(U5-Pad2)")
  (net 18 "Net-(C3-Pad1)")
  (net 19 GND)
  (net 20 "Net-(C4-Pad1)")
  (net 21 /A10)
  (net 22 /D4)
  (net 23 /D5)
  (net 24 /D6)
  (net 25 /D7)
  (net 26 /D3)
  (net 27 /D2)
  (net 28 /D1)
  (net 29 /D0)
  (net 30 -5V)
  (net 31 /A0)
  (net 32 /A1)
  (net 33 /A2)
  (net 34 +12V)
  (net 35 /A3)
  (net 36 /A4)
  (net 37 /A5)
  (net 38 /A6)
  (net 39 /A7)
  (net 40 /A8)
  (net 41 /A9)
  (net 42 /A15)
  (net 43 /A12)
  (net 44 /A13)
  (net 45 /A14)
  (net 46 /A11)
  (net 47 RESb)
  (net 48 MCU39)
  (net 49 RESCDIV)
  (net 50 8080HOLD)
  (net 51 DISINT)
  (net 52 CLKMON)
  (net 53 SP1)
  (net 54 +5V)
  (net 55 "Net-(J1-Pad2)")
  (net 56 "Net-(J1-Pad3)")
  (net 57 "Net-(J1-Pad4)")
  (net 58 "Net-(J1-Pad5)")
  (net 59 "Net-(U2-Pad1)")
  (net 60 "Net-(U2-Pad44)")
  (net 61 "Net-(C2-Pad1)")
  (net 62 "Net-(C5-Pad1)")
  (net 63 "Net-(C5-Pad2)")
  (net 64 "Net-(C6-Pad2)")
  (net 65 "Net-(C6-Pad1)")
  (net 66 "Net-(C7-Pad1)")
  (net 67 /CTS)
  (net 68 "Net-(J2-Pad3)")
  (net 69 /RX)
  (net 70 /TX)
  (net 71 "Net-(J2-Pad6)")
  (net 72 "Net-(J3-Pad12)")
  (net 73 "Net-(J3-Pad13)")
  (net 74 "Net-(J3-Pad14)")
  (net 75 "Net-(J3-Pad15)")
  (net 76 "Net-(J3-Pad16)")
  (net 77 "Net-(J3-Pad17)")
  (net 78 "Net-(J3-Pad18)")
  (net 79 "Net-(J3-Pad19)")
  (net 80 "Net-(J3-Pad21)")
  (net 81 "Net-(J3-Pad22)")
  (net 82 "Net-(J3-Pad23)")
  (net 83 "Net-(J3-Pad24)")
  (net 84 MCU20)
  (net 85 MCU19)
  (net 86 MCU18)
  (net 87 MCU17)
  (net 88 DISHOLD)
  (net 89 RES)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net -5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CTS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /RX)
    (add_net /TX)
    (add_net 8080HOLD)
    (add_net CLKMON)
    (add_net DISHOLD)
    (add_net DISINT)
    (add_net GND)
    (add_net MCU17)
    (add_net MCU18)
    (add_net MCU19)
    (add_net MCU20)
    (add_net MCU39)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad14)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad18)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad21)")
    (add_net "Net-(J3-Pad22)")
    (add_net "Net-(J3-Pad23)")
    (add_net "Net-(J3-Pad24)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad44)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad16)")
    (add_net "Net-(U5-Pad2)")
    (add_net RES)
    (add_net RESCDIV)
    (add_net RESb)
    (add_net SP1)
  )
  (net_class HiPower ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 28.9357 98.7501 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C12 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 28.9052 91.2216 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C14 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 -5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 54.5795 86.7816)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C15 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 +12V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:IDC_Header_Straight_40pins (layer F.Cu) (tedit 0)
    (at 21.1785 113.939 90)
    (descr "40 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J3 (at 24.13 -7.62 90) (layer F.SilkS))
    (fp_text value "8080 BUS" (at -1.59004 4.60248 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /A10))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /D4))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /D5))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /D6))
    (pad 6 thru_hole oval (at 5.08 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /D7))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /D3))
    (pad 8 thru_hole oval (at 7.62 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /D2))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /D1))
    (pad 10 thru_hole oval (at 10.16 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /D0))
    (pad 11 thru_hole oval (at 12.7 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 -5V))
    (pad 12 thru_hole oval (at 12.7 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "Net-(J3-Pad12)"))
    (pad 13 thru_hole oval (at 15.24 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "Net-(J3-Pad13)"))
    (pad 14 thru_hole oval (at 15.24 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "Net-(J3-Pad14)"))
    (pad 15 thru_hole oval (at 17.78 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "Net-(J3-Pad15)"))
    (pad 16 thru_hole oval (at 17.78 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "Net-(J3-Pad16)"))
    (pad 17 thru_hole oval (at 20.32 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "Net-(J3-Pad17)"))
    (pad 18 thru_hole oval (at 20.32 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "Net-(J3-Pad18)"))
    (pad 19 thru_hole oval (at 22.86 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 "Net-(J3-Pad19)"))
    (pad 20 thru_hole oval (at 22.86 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 21 thru_hole oval (at 25.4 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(J3-Pad21)"))
    (pad 22 thru_hole oval (at 25.4 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "Net-(J3-Pad22)"))
    (pad 23 thru_hole oval (at 27.94 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 "Net-(J3-Pad23)"))
    (pad 24 thru_hole oval (at 27.94 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "Net-(J3-Pad24)"))
    (pad 25 thru_hole oval (at 30.48 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /A0))
    (pad 26 thru_hole oval (at 30.48 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /A1))
    (pad 27 thru_hole oval (at 33.02 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /A2))
    (pad 28 thru_hole oval (at 33.02 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 +12V))
    (pad 29 thru_hole oval (at 35.56 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /A3))
    (pad 30 thru_hole oval (at 35.56 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /A4))
    (pad 31 thru_hole oval (at 38.1 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /A5))
    (pad 32 thru_hole oval (at 38.1 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 /A6))
    (pad 33 thru_hole oval (at 40.64 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 /A7))
    (pad 34 thru_hole oval (at 40.64 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 /A8))
    (pad 35 thru_hole oval (at 43.18 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /A9))
    (pad 36 thru_hole oval (at 43.18 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /A15))
    (pad 37 thru_hole oval (at 45.72 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /A12))
    (pad 38 thru_hole oval (at 45.72 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 /A13))
    (pad 39 thru_hole oval (at 48.26 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 /A14))
    (pad 40 thru_hole oval (at 48.26 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 /A11))
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 64.0512 93.2282)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 4.05892 -3.50012) (layer F.SilkS))
    (fp_text value 47k (at 3.92684 -0.04318) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 86 MCU18))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 54 +5V))
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 69.7128 105.885 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at 4.08178 -2.6416 90) (layer F.SilkS))
    (fp_text value 47k (at 3.9624 0.04318 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 87 MCU17))
  )
  (module Housings_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 54130A77)
    (at 33.8226 68.7883)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U1 (at -0.23368 -3.2385 180) (layer F.SilkS))
    (fp_text value 8080A (at 7.52348 3.29946) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /A10))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /D6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D3))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D2))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /D1))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /D0))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 -5V))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 RES))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 8080HOLD))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(J3-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(J3-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad19)"))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad20)"))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(J3-Pad21)"))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(J3-Pad22)"))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad23)"))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(J3-Pad24)"))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /A0))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /A1))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /A2))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 +12V))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /A3))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /A4))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /A5))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A6))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /A7))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A8))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A9))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A15))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /A12))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /A13))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A14))
    (pad 40 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /A11))
    (model Housings_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 54130A77)
    (at 77.6376 63.0098)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at -0.37592 -3.37566) (layer F.SilkS))
    (fp_text value PIC18LF2420-E_SP (at 3.76682 15.81912 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 RESb))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 MCU39))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 RESCDIV))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 8080HOLD))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 DISINT))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 CLKMON))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 SP1))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C3-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 MCU20))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 MCU19))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 MCU18))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 MCU17))
    (pad 15 thru_hole oval (at 7.62 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 DISHOLD))
    (pad 16 thru_hole oval (at 7.62 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U3-Pad16)"))
    (pad 17 thru_hole oval (at 7.62 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U3-Pad17)"))
    (pad 18 thru_hole oval (at 7.62 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U3-Pad18)"))
    (pad 19 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 20 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 21 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /D0))
    (pad 22 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /D1))
    (pad 23 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D2))
    (pad 24 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D3))
    (pad 25 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D4))
    (pad 26 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D5))
    (pad 27 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /D6))
    (pad 28 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D7))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 54130A77)
    (at 55.6133 99.2784)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U5 (at 0 -5.22) (layer F.SilkS))
    (fp_text value 74HC4049N,652 (at 3.84556 10.12444 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(U5-Pad16)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U5-Pad15)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U5-Pad13)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U5-Pad12)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U5-Pad10)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(J3-Pad15)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(U2-Pad44)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(J3-Pad22)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U5-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 76.8807 117.274 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 94.6455 73.8937)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at -0.30988 -2.27838) (layer F.SilkS))
    (fp_text value .1uF (at 2.2352 -2.29108) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(C2-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 83.2002 101.656 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 1.4478 2.2733 270) (layer F.SilkS))
    (fp_text value 22pF (at 1.26492 -2.44348 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 83.2002 109.741 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 22pF (at 1.25 2.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 91.6584 77.8408 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 2.63144 2.20726 180) (layer F.SilkS))
    (fp_text value .1uF (at 0.1651 2.2479 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 63 "Net-(C5-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 94.3839 108.204)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 64 "Net-(C6-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 88.4199 108.301)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(C7-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 94.4905 77.8231)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -0.59436 2.38252) (layer F.SilkS))
    (fp_text value .1uF (at 1.87198 2.37236) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 64.6582 86.8477 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 1.25 -2.5 180) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 72.6364 66.8757 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 72.6313 74.4728 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 29.0347 111.62 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C13 (at 5.33146 -0.02794 270) (layer F.SilkS))
    (fp_text value "4.7uF Tant" (at 2.9972 -2.48158 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 60.2234 93.2282 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C16 (at 1.25 -2.5 180) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 47.9349 62.3341 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C17 (at 4.57708 -0.01524 270) (layer F.SilkS))
    (fp_text value "1uF Tant" (at 1.2319 -2.6924 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 89 RES))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 552FFC30)
    (at 28.9509 73.7768 90)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D1 (at 5.1435 1.59766 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 4.89458 -1.77546 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 270) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 270) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 89 RES))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors:PINHEAD1-6 (layer F.Cu) (tedit 0)
    (at 59.1287 62.9514 180)
    (attr virtual)
    (fp_text reference J1 (at 0 -3.75 180) (layer F.SilkS))
    (fp_text value JTAG (at -0.1016 2.42062 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -6.35 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 54 +5V))
    (pad 2 thru_hole oval (at -3.81 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 55 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at -1.27 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 56 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 1.27 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 57 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 3.81 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 58 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 6.35 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 19 GND))
  )
  (module Connectors:PINHEAD1-6 (layer F.Cu) (tedit 0)
    (at 90.3402 115.89)
    (attr virtual)
    (fp_text reference J2 (at 0 -3.75) (layer F.SilkS))
    (fp_text value RS232 (at -0.03302 2.43586) (layer F.Fab))
    (pad 6 thru_hole oval (at 6.35 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 71 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 3.81 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 70 /TX))
    (pad 4 thru_hole oval (at 1.27 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 69 /RX))
    (pad 3 thru_hole oval (at -1.27 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 68 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at -3.81 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 67 /CTS))
    (pad 1 thru_hole oval (at -6.35 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 19 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 70.2589 62.3291 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "+5v PWR" (at -2.6797 1.08458 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 36.8249 62.1106 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at -0.11176 -3.02768 90) (layer F.SilkS))
    (fp_text value RES_ENA (at -3.0099 1.31572 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "Net-(J3-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 RES))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 28.9103 85.3897 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.08432 2.27838 90) (layer F.SilkS))
    (fp_text value 100k (at 3.8354 -0.02794 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 89 RES))
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 69.7154 118.191 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 3.86588 -2.59334 90) (layer F.SilkS))
    (fp_text value 47k (at 3.94716 -0.00762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 54 +5V))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 84 MCU20))
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 72.7075 81.0235 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 4.05892 -3.50012 270) (layer F.SilkS))
    (fp_text value 47k (at 3.81 3.81 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 85 MCU19))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 54 +5V))
  )
  (module Housings_QFP:LQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 60.5765 74.6938)
    (descr "LQFP44 (see Appnote_PCB_Guidelines_TRINAMIC_packages.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at -6.1976 -7.65302 180) (layer F.SilkS))
    (fp_text value XC9536VQFP44 (at 0 7.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.85 -4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -5.85 -3.2) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 23 /D5))
    (pad 3 smd rect (at -5.85 -2.4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 22 /D4))
    (pad 4 smd rect (at -5.85 -1.6) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 5 smd rect (at -5.85 -0.8) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 26 /D3))
    (pad 6 smd rect (at -5.85 0) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 89 RES))
    (pad 7 smd rect (at -5.85 0.8) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 50 8080HOLD))
    (pad 8 smd rect (at -5.85 1.6) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad14)"))
    (pad 9 smd rect (at -5.85 2.4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J1-Pad4)"))
    (pad 10 smd rect (at -5.85 3.2) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J1-Pad5)"))
    (pad 11 smd rect (at -5.85 4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J1-Pad2)"))
    (pad 12 smd rect (at -4 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J3-Pad13)"))
    (pad 13 smd rect (at -3.2 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(J3-Pad19)"))
    (pad 14 smd rect (at -2.4 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad17)"))
    (pad 15 smd rect (at -1.6 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 54 +5V))
    (pad 16 smd rect (at -0.8 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad23)"))
    (pad 17 smd rect (at 0 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 18 smd rect (at 0.8 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 1.6 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J3-Pad14)"))
    (pad 20 smd rect (at 2.4 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(J3-Pad17)"))
    (pad 21 smd rect (at 3.2 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(J3-Pad23)"))
    (pad 22 smd rect (at 4 5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(J3-Pad18)"))
    (pad 23 smd rect (at 5.85 4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad19)"))
    (pad 24 smd rect (at 5.85 3.2) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J1-Pad3)"))
    (pad 25 smd rect (at 5.85 2.4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 26 smd rect (at 5.85 1.6) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 54 +5V))
    (pad 27 smd rect (at 5.85 0.8) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 29 /D0))
    (pad 28 smd rect (at 5.85 0) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 28 /D1))
    (pad 29 smd rect (at 5.85 -0.8) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 52 CLKMON))
    (pad 30 smd rect (at 5.85 -1.6) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 51 DISINT))
    (pad 31 smd rect (at 5.85 -2.4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 49 RESCDIV))
    (pad 32 smd rect (at 5.85 -3.2) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 27 /D2))
    (pad 33 smd rect (at 5.85 -4) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 48 MCU39))
    (pad 34 smd rect (at 4 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 47 RESb))
    (pad 35 smd rect (at 3.2 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 54 +5V))
    (pad 36 smd rect (at 2.4 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 53 SP1))
    (pad 37 smd rect (at 1.6 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 84 MCU20))
    (pad 38 smd rect (at 0.8 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 85 MCU19))
    (pad 39 smd rect (at 0 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 86 MCU18))
    (pad 40 smd rect (at -0.8 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 87 MCU17))
    (pad 41 smd rect (at -1.6 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 88 DISHOLD))
    (pad 42 smd rect (at -2.4 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 24 /D6))
    (pad 43 smd rect (at -3.2 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 25 /D7))
    (pad 44 smd rect (at -4 -5.85 90) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U2-Pad44)"))
    (model Housings_QFP.3dshapes/LQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 54130A77)
    (at 89.2658 83.6397)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at -0.37084 -3.34518) (layer F.SilkS))
    (fp_text value HIN232ECBNZ (at 4.03606 8.91794 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(C5-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(C6-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(C6-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(C7-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /CTS))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U4-Pad8)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U4-Pad9)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U3-Pad16)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U3-Pad17)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U3-Pad18)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 /RX))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 /TX))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +5V))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 0)
    (at 77.0484 105.74 90)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference X1 (at 0.08128 -3.38074 90) (layer F.SilkS))
    (fp_text value 10Mhz (at 3.63474 -3.44932 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 "Net-(C3-Pad1)"))
  )
  (gr_text "Design © B.Grieb / Tauntek" (at 52.29098 108.31322 90) (layer F.SilkS))
  (gr_text "8080\nICE" (at 88.011 72.3265) (layer F.SilkS))
  (gr_text TaunTek (at 92.45092 69.41058) (layer F.SilkS))
  (gr_line (start 14.8971 119.70004) (end 14.8971 59.1947) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 98.70694 119.70004) (end 14.86154 119.70004) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 98.6917 59.1947) (end 98.6917 119.70004) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 14.8971 59.1947) (end 98.6917 59.1947) (layer Edge.Cuts) (width 0.2))
  (gr_text "JonB Retro" (at 92.62564 66.78414) (layer F.SilkS))
)
