(kicad_pcb (version 20171130) (host pcbnew 5.0.0)
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 337)
    (zones 0)
    (modules 15)
    (nets 65)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1778)
    (trace_clearance 0.1778)
    (zone_clearance 0.208)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.3556)
    (via_drill 0.1016)
    (via_min_size 0.3556)
    (via_min_drill 0.1016)
    (uvia_size 0.1778)
    (uvia_drill 0.0762)
    (uvias_allowed no)
    (uvia_min_size 0.1778)
    (uvia_min_drill 0.0762)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF33F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/breakout/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(P7-Pad21)")
  (net 4 "Net-(P7-Pad22)")
  (net 5 PWR_ENABLE)
  (net 6 FPGA_VBATT)
  (net 7 JX_VCCO_12)
  (net 8 JX_VCCO_33_34)
  (net 9 JX_VCCO_13)
  (net 10 3V3_I2C)
  (net 11 JX_MGTAVCC)
  (net 12 JX_MGTAVTT)
  (net 13 MIO15)
  (net 14 MIO10)
  (net 15 MIO13)
  (net 16 MIO14)
  (net 17 MIO0)
  (net 18 MIO48)
  (net 19 MIO51)
  (net 20 MIO49)
  (net 21 MIO47)
  (net 22 MIO46)
  (net 23 MIO11)
  (net 24 MIO12)
  (net 25 USB_ID)
  (net 26 USB_OTG_P)
  (net 27 USB_OTG_N)
  (net 28 USB_OTG_CPEN)
  (net 29 USB_VBUS_OTG)
  (net 30 GPO_0)
  (net 31 GPO_1)
  (net 32 GPO_2)
  (net 33 GPO_3)
  (net 34 "Net-(P2-Pad82)")
  (net 35 JTAG_TCK)
  (net 36 JTAG_TMS)
  (net 37 JTAG_TDO)
  (net 38 JTAG_TDI)
  (net 39 Carrier_Reset)
  (net 40 IO_00_33_JX1)
  (net 41 IO_L16_33_JX1_P)
  (net 42 IO_L16_33_JX1_N)
  (net 43 IO_L18_33_JX1_P)
  (net 44 IO_L18_33_JX1_N)
  (net 45 IO_L20_33_JX1_P)
  (net 46 IO_L20_33_JX1_N)
  (net 47 IO_L22_33_JX1_P)
  (net 48 IO_L22_33_JX1_N)
  (net 49 IO_L01_33_JX1_P)
  (net 50 IO_L01_33_JX1_N)
  (net 51 "Net-(P7-Pad41)")
  (net 52 "Net-(P7-Pad45)")
  (net 53 "Net-(P7-Pad49)")
  (net 54 "Net-(P7-Pad42)")
  (net 55 "Net-(P7-Pad46)")
  (net 56 "Net-(P7-Pad50)")
  (net 57 "Net-(P7-Pad54)")
  (net 58 PG_MODULE)
  (net 59 AUXADC)
  (net 60 AUXDAC1)
  (net 61 VDDA_GPO_PWR)
  (net 62 AUXDAC2)
  (net 63 FPGA_DONE)
  (net 64 PG_1P8V)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.3556)
    (via_drill 0.1016)
    (uvia_dia 0.1778)
    (uvia_drill 0.0762)
    (add_net +5V)
    (add_net 3V3_I2C)
    (add_net AUXADC)
    (add_net AUXDAC1)
    (add_net AUXDAC2)
    (add_net Carrier_Reset)
    (add_net FPGA_DONE)
    (add_net FPGA_VBATT)
    (add_net GND)
    (add_net GPO_0)
    (add_net GPO_1)
    (add_net GPO_2)
    (add_net GPO_3)
    (add_net IO_00_33_JX1)
    (add_net IO_L01_33_JX1_N)
    (add_net IO_L01_33_JX1_P)
    (add_net IO_L16_33_JX1_N)
    (add_net IO_L16_33_JX1_P)
    (add_net IO_L18_33_JX1_N)
    (add_net IO_L18_33_JX1_P)
    (add_net IO_L20_33_JX1_N)
    (add_net IO_L20_33_JX1_P)
    (add_net IO_L22_33_JX1_N)
    (add_net IO_L22_33_JX1_P)
    (add_net JTAG_TCK)
    (add_net JTAG_TDI)
    (add_net JTAG_TDO)
    (add_net JTAG_TMS)
    (add_net JX_MGTAVCC)
    (add_net JX_MGTAVTT)
    (add_net JX_VCCO_12)
    (add_net JX_VCCO_13)
    (add_net JX_VCCO_33_34)
    (add_net MIO0)
    (add_net MIO10)
    (add_net MIO11)
    (add_net MIO12)
    (add_net MIO13)
    (add_net MIO14)
    (add_net MIO15)
    (add_net MIO46)
    (add_net MIO47)
    (add_net MIO48)
    (add_net MIO49)
    (add_net MIO51)
    (add_net "Net-(P2-Pad82)")
    (add_net "Net-(P7-Pad21)")
    (add_net "Net-(P7-Pad22)")
    (add_net "Net-(P7-Pad41)")
    (add_net "Net-(P7-Pad42)")
    (add_net "Net-(P7-Pad45)")
    (add_net "Net-(P7-Pad46)")
    (add_net "Net-(P7-Pad49)")
    (add_net "Net-(P7-Pad50)")
    (add_net "Net-(P7-Pad54)")
    (add_net PG_1P8V)
    (add_net PG_MODULE)
    (add_net PWR_ENABLE)
    (add_net USB_ID)
    (add_net USB_OTG_CPEN)
    (add_net USB_OTG_N)
    (add_net USB_OTG_P)
    (add_net USB_VBUS_OTG)
    (add_net VDDA_GPO_PWR)
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 5B5A36E3)
    (at 84.963 101.092 180)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Power_Breakout (at -2.3749 5.3848 270) (layer F.SilkS))
    (fp_text user %R (at 0 11.43 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 PWR_ENABLE))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 FPGA_VBATT))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 JX_VCCO_12))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 JX_VCCO_33_34))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 JX_VCCO_13))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 3V3_I2C))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 JX_MGTAVTT))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 JX_MGTAVCC))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module breakoutBoard:Cysized (layer B.Cu) (tedit 0)
    (at 123.6472 112.8776 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Project:BERGSTAK_100_PIN1_RIGHT (layer F.Cu) (tedit 59E998F9)
    (at 142.8242 114.046 270)
    (fp_text reference P4 (at -21.55 0) (layer F.SilkS))
    (fp_text value CONN_02X50 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -19.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -19.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -18.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -18.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -18 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -18 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -17.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -17.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -16.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -16.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 64 PG_1P8V))
    (pad 11 smd rect (at -15.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 58 PG_MODULE))
    (pad 12 smd rect (at -15.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 13 smd rect (at -14.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -14.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -14 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -14 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -13.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at -13.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -12.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -12.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -11.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at -11.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at -10.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -10.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -10 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at -10 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at -9.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -9.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -8.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at -8.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 31 smd rect (at -7.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -7.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at -6.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd rect (at -6.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at -6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at -6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at -5.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 38 smd rect (at -5.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at -4.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -4.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 41 smd rect (at -3.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 42 smd rect (at -3.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 43 smd rect (at -2.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -2.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 45 smd rect (at -2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at -2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 47 smd rect (at -1.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -1.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 49 smd rect (at -0.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 50 smd rect (at -0.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 51 smd rect (at 0.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 0.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 53 smd rect (at 1.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 54 smd rect (at 1.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 55 smd rect (at 2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 56 smd rect (at 2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 57 smd rect (at 2.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 58 smd rect (at 2.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 59 smd rect (at 3.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 60 smd rect (at 3.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 61 smd rect (at 4.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 62 smd rect (at 4.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 63 smd rect (at 5.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 64 smd rect (at 5.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 65 smd rect (at 6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 66 smd rect (at 6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 67 smd rect (at 6.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 68 smd rect (at 6.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 69 smd rect (at 7.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 70 smd rect (at 7.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 71 smd rect (at 8.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 72 smd rect (at 8.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 73 smd rect (at 9.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 74 smd rect (at 9.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 75 smd rect (at 10 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 76 smd rect (at 10 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 77 smd rect (at 10.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 78 smd rect (at 10.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 JX_VCCO_33_34))
    (pad 79 smd rect (at 11.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 JX_VCCO_33_34))
    (pad 80 smd rect (at 11.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 JX_VCCO_33_34))
    (pad 81 smd rect (at 12.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 82 smd rect (at 12.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 83 smd rect (at 13.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 84 smd rect (at 13.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 85 smd rect (at 14 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 86 smd rect (at 14 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 87 smd rect (at 14.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 88 smd rect (at 14.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 89 smd rect (at 15.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 90 smd rect (at 15.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 91 smd rect (at 16.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 92 smd rect (at 16.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 93 smd rect (at 17.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 94 smd rect (at 17.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 95 smd rect (at 18 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 96 smd rect (at 18 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 97 smd rect (at 18.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 98 smd rect (at 18.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 9 JX_VCCO_13))
    (pad 99 smd rect (at 19.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 100 smd rect (at 19.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 22.1742 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -22.1742 0 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Project:BERGSTAK_100_PIN1_RIGHT (layer F.Cu) (tedit 5AEF6D68)
    (at 98.4758 114.1222 270)
    (fp_text reference P3 (at -21.55 0) (layer F.SilkS))
    (fp_text value CONN_02X50 (at 0.878 -0.29 270) (layer F.Fab))
    (pad 1 smd rect (at -19.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 35 JTAG_TCK))
    (pad 2 smd rect (at -19.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 36 JTAG_TMS))
    (pad 3 smd rect (at -18.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 37 JTAG_TDO))
    (pad 4 smd rect (at -18.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 38 JTAG_TDI))
    (pad 5 smd rect (at -18 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 PWR_ENABLE))
    (pad 6 smd rect (at -18 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 39 Carrier_Reset))
    (pad 7 smd rect (at -17.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 6 FPGA_VBATT))
    (pad 8 smd rect (at -17.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 63 FPGA_DONE))
    (pad 9 smd rect (at -16.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 40 IO_00_33_JX1))
    (pad 10 smd rect (at -16.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -15.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 41 IO_L16_33_JX1_P))
    (pad 12 smd rect (at -15.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -14.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 42 IO_L16_33_JX1_N))
    (pad 14 smd rect (at -14.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -14 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -14 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -13.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 43 IO_L18_33_JX1_P))
    (pad 18 smd rect (at -13.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -12.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 44 IO_L18_33_JX1_N))
    (pad 20 smd rect (at -12.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -11.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at -11.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at -10.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 45 IO_L20_33_JX1_P))
    (pad 24 smd rect (at -10.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -10 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 46 IO_L20_33_JX1_N))
    (pad 26 smd rect (at -10 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at -9.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -9.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -8.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 47 IO_L22_33_JX1_P))
    (pad 30 smd rect (at -8.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 31 smd rect (at -7.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 48 IO_L22_33_JX1_N))
    (pad 32 smd rect (at -7.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at -6.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd rect (at -6.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at -6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 49 IO_L01_33_JX1_P))
    (pad 36 smd rect (at -6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at -5.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 50 IO_L01_33_JX1_N))
    (pad 38 smd rect (at -5.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at -4.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -4.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 41 smd rect (at -3.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 42 smd rect (at -3.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 43 smd rect (at -2.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -2.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 45 smd rect (at -2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at -2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 47 smd rect (at -1.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -1.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 49 smd rect (at -0.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 50 smd rect (at -0.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 51 smd rect (at 0.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 0.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 53 smd rect (at 1.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 54 smd rect (at 1.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 55 smd rect (at 2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 56 smd rect (at 2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 57 smd rect (at 2.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 58 smd rect (at 2.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 59 smd rect (at 3.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 60 smd rect (at 3.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 61 smd rect (at 4.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 62 smd rect (at 4.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 63 smd rect (at 5.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 64 smd rect (at 5.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 65 smd rect (at 6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 66 smd rect (at 6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 67 smd rect (at 6.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 68 smd rect (at 6.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 69 smd rect (at 7.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 70 smd rect (at 7.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 71 smd rect (at 8.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 72 smd rect (at 8.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 73 smd rect (at 9.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 74 smd rect (at 9.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 75 smd rect (at 10 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 76 smd rect (at 10 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 77 smd rect (at 10.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 78 smd rect (at 10.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 7 JX_VCCO_12))
    (pad 79 smd rect (at 11.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 7 JX_VCCO_12))
    (pad 80 smd rect (at 11.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 7 JX_VCCO_12))
    (pad 81 smd rect (at 12.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 82 smd rect (at 12.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 83 smd rect (at 13.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 84 smd rect (at 13.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 85 smd rect (at 14 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 86 smd rect (at 14 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 87 smd rect (at 14.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 88 smd rect (at 14.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 89 smd rect (at 15.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 90 smd rect (at 15.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 91 smd rect (at 16.4 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 92 smd rect (at 16.4 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 93 smd rect (at 17.2 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 94 smd rect (at 17.2 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 95 smd rect (at 18 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 96 smd rect (at 18 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 97 smd rect (at 18.8 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 98 smd rect (at 18.8 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 99 smd rect (at 19.6 -2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 100 smd rect (at 19.6 2.2 270) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 22.1742 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 JTAG_TMS))
    (pad "" thru_hole circle (at -22.1742 0 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Project:BERGSTAK_100_PIN1_RIGHT (layer F.Cu) (tedit 5AEF6E14)
    (at 120.65 147.066 180)
    (fp_text reference P2 (at -21.55 0 270) (layer F.SilkS))
    (fp_text value CONN_02X50 (at -0.898 0 180) (layer F.Fab))
    (pad 1 smd rect (at -19.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 30 GPO_0))
    (pad 2 smd rect (at -19.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 31 GPO_1))
    (pad 3 smd rect (at -18.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 32 GPO_2))
    (pad 4 smd rect (at -18.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 33 GPO_3))
    (pad 5 smd rect (at -18 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -18 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -17.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 59 AUXADC))
    (pad 8 smd rect (at -17.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 60 AUXDAC1))
    (pad 9 smd rect (at -16.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 61 VDDA_GPO_PWR))
    (pad 10 smd rect (at -16.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 62 AUXDAC2))
    (pad 11 smd rect (at -15.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -15.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -14.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -14.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -14 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -14 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -13.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at -13.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -12.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -12.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -11.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at -11.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at -10.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -10.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -10 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at -10 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at -9.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -9.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -8.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at -8.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 31 smd rect (at -7.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -7.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at -6.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd rect (at -6.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at -6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at -6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at -5.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 38 smd rect (at -5.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at -4.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -4.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 41 smd rect (at -3.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 42 smd rect (at -3.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 43 smd rect (at -2.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -2.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 45 smd rect (at -2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at -2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 47 smd rect (at -1.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -1.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 49 smd rect (at -0.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 50 smd rect (at -0.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 51 smd rect (at 0.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 0.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 53 smd rect (at 1.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 54 smd rect (at 1.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 55 smd rect (at 2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 56 smd rect (at 2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 57 smd rect (at 2.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 58 smd rect (at 2.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 59 smd rect (at 3.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 60 smd rect (at 3.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 61 smd rect (at 4.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 62 smd rect (at 4.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 63 smd rect (at 5.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 64 smd rect (at 5.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 65 smd rect (at 6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 66 smd rect (at 6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 67 smd rect (at 6.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 68 smd rect (at 6.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 69 smd rect (at 7.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 70 smd rect (at 7.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 71 smd rect (at 8.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 72 smd rect (at 8.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 73 smd rect (at 9.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 74 smd rect (at 9.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 75 smd rect (at 10 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 76 smd rect (at 10 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 77 smd rect (at 10.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 78 smd rect (at 10.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 79 smd rect (at 11.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 80 smd rect (at 11.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 81 smd rect (at 12.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 10 3V3_I2C))
    (pad 82 smd rect (at 12.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P2-Pad82)"))
    (pad 83 smd rect (at 13.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 84 smd rect (at 13.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 85 smd rect (at 14 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 13 MIO15))
    (pad 86 smd rect (at 14 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 24 MIO12))
    (pad 87 smd rect (at 14.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 14 MIO10))
    (pad 88 smd rect (at 14.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 MIO11))
    (pad 89 smd rect (at 15.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 90 smd rect (at 15.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 91 smd rect (at 16.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 15 MIO13))
    (pad 92 smd rect (at 16.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 22 MIO46))
    (pad 93 smd rect (at 17.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 16 MIO14))
    (pad 94 smd rect (at 17.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 21 MIO47))
    (pad 95 smd rect (at 18 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 96 smd rect (at 18 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 97 smd rect (at 18.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 17 MIO0))
    (pad 98 smd rect (at 18.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 20 MIO49))
    (pad 99 smd rect (at 19.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 MIO48))
    (pad 100 smd rect (at 19.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 19 MIO51))
    (pad 2 thru_hole circle (at 22.1742 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 GPO_1))
    (pad "" thru_hole circle (at -22.1742 0 180) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Project:BERGSTAK_100_PIN1_RIGHT (layer F.Cu) (tedit 5B47C21C)
    (at 120.65 73.66)
    (fp_text reference P1 (at -21.55 0 90) (layer F.SilkS))
    (fp_text value CONN_02X50 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -19.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -19.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -18.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -18.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -18 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 11 JX_MGTAVCC))
    (pad 6 smd rect (at -18 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -17.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 11 JX_MGTAVCC))
    (pad 8 smd rect (at -17.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -16.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 11 JX_MGTAVCC))
    (pad 10 smd rect (at -16.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -15.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 11 JX_MGTAVCC))
    (pad 12 smd rect (at -15.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -14.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -14.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -14 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -14 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -13.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at -13.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -12.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -12.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -11.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at -11.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at -10.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -10.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -10 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at -10 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at -9.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -9.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -8.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at -8.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 12 JX_MGTAVTT))
    (pad 31 smd rect (at -7.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -7.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 12 JX_MGTAVTT))
    (pad 33 smd rect (at -6.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd rect (at -6.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at -6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at -6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at -5.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 38 smd rect (at -5.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at -4.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -4.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 41 smd rect (at -3.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 42 smd rect (at -3.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 43 smd rect (at -2.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -2.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 45 smd rect (at -2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 9 JX_VCCO_13))
    (pad 46 smd rect (at -2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 9 JX_VCCO_13))
    (pad 47 smd rect (at -1.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -1.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 49 smd rect (at -0.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 50 smd rect (at -0.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 51 smd rect (at 0.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 0.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 53 smd rect (at 1.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 54 smd rect (at 1.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 55 smd rect (at 2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 56 smd rect (at 2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 57 smd rect (at 2.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 58 smd rect (at 2.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 59 smd rect (at 3.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 60 smd rect (at 3.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 61 smd rect (at 4.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 62 smd rect (at 4.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 63 smd rect (at 5.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 25 USB_ID))
    (pad 64 smd rect (at 5.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 65 smd rect (at 6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 66 smd rect (at 6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 67 smd rect (at 6.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 26 USB_OTG_P))
    (pad 68 smd rect (at 6.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 29 USB_VBUS_OTG))
    (pad 69 smd rect (at 7.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 27 USB_OTG_N))
    (pad 70 smd rect (at 7.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 28 USB_OTG_CPEN))
    (pad 71 smd rect (at 8.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 72 smd rect (at 8.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 73 smd rect (at 9.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 74 smd rect (at 9.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 75 smd rect (at 10 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 76 smd rect (at 10 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 77 smd rect (at 10.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 78 smd rect (at 10.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 79 smd rect (at 11.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 80 smd rect (at 11.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 81 smd rect (at 12.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 82 smd rect (at 12.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 83 smd rect (at 13.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 84 smd rect (at 13.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 85 smd rect (at 14 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 86 smd rect (at 14 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 87 smd rect (at 14.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 88 smd rect (at 14.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 89 smd rect (at 15.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 90 smd rect (at 15.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 91 smd rect (at 16.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 92 smd rect (at 16.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 93 smd rect (at 17.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 94 smd rect (at 17.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 95 smd rect (at 18 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 96 smd rect (at 18 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 97 smd rect (at 18.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 98 smd rect (at 18.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 99 smd rect (at 19.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 100 smd rect (at 19.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 22.1742 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -22.1742 0) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Connectors_Samtec:MECF-30-0_-NP-L-DV_Edge (layer F.Cu) (tedit 5B240730)
    (at 120.5738 165.1)
    (descr "Highspeed card edge connector for PCB's with 30 contacts (not polarized)")
    (tags "conn samtec card-edge high-speed")
    (attr virtual)
    (fp_text reference P7 (at 0 -6.35) (layer F.SilkS))
    (fp_text value CONN_02X30 (at 0 -3.81) (layer F.Fab))
    (fp_line (start -19.925 5) (end -19.925 -5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19.925 5) (end 19.925 -5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -20.25 -5) (end -19.925 -5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 20.25 -5) (end 19.925 -5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -19.925 5) (end 19.925 5) (layer Edge.Cuts) (width 0.12))
    (fp_text user %R (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at -18.405 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -18.405 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -17.135 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -17.135 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -15.865 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 18 MIO48))
    (pad 6 smd rect (at -15.865 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 19 MIO51))
    (pad 7 smd rect (at -14.595 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -14.595 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -13.325 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 17 MIO0))
    (pad 10 smd rect (at -13.325 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 20 MIO49))
    (pad 11 smd rect (at -12.055 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -12.055 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -10.785 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 16 MIO14))
    (pad 14 smd rect (at -10.785 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 21 MIO47))
    (pad 15 smd rect (at -9.515 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -9.515 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -8.245 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 15 MIO13))
    (pad 18 smd rect (at -8.245 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 22 MIO46))
    (pad 19 smd rect (at -6.975 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -6.975 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -5.705 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P7-Pad21)"))
    (pad 22 smd rect (at -5.705 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(P7-Pad22)"))
    (pad 23 smd rect (at -4.435 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -4.435 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -3.165 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 14 MIO10))
    (pad 26 smd rect (at -3.165 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 23 MIO11))
    (pad 27 smd rect (at -1.895 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -1.895 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -0.625 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 13 MIO15))
    (pad 30 smd rect (at -0.625 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 24 MIO12))
    (pad 31 smd rect (at 0.645 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at 0.645 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 1.915 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 34 smd rect (at 1.915 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 35 smd rect (at 3.185 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 3.185 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 4.455 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 38 smd rect (at 4.455 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 39 smd rect (at 5.725 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 5.725 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 41 smd rect (at 6.995 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(P7-Pad41)"))
    (pad 42 smd rect (at 6.995 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(P7-Pad42)"))
    (pad 43 smd rect (at 8.265 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at 8.265 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 45 smd rect (at 9.535 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(P7-Pad45)"))
    (pad 46 smd rect (at 9.535 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(P7-Pad46)"))
    (pad 47 smd rect (at 10.805 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at 10.805 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 49 smd rect (at 12.075 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(P7-Pad49)"))
    (pad 50 smd rect (at 12.075 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(P7-Pad50)"))
    (pad 51 smd rect (at 13.345 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 13.345 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 53 smd rect (at 14.615 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 58 PG_MODULE))
    (pad 54 smd rect (at 14.615 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(P7-Pad54)"))
    (pad 55 smd rect (at 15.885 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 56 smd rect (at 15.885 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 57 smd rect (at 17.155 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 5 PWR_ENABLE))
    (pad 58 smd rect (at 17.155 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 63 FPGA_DONE))
    (pad 59 smd rect (at 18.425 2.5) (size 0.56 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 60 smd rect (at 18.425 2.5) (size 0.56 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 93.5736 67.31)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at -0.1016 4.318) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 147.574 67.31)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0.127 4.318) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5B5FB110)
    (at 93.5736 159.3344)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at -4.8006 6.6546) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 147.574 159.3344)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at -0.2921 4.6353) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5B5A3703)
    (at 84.9376 131.2672)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value MIO_Breakout (at 2.1717 23.5331 90) (layer F.SilkS))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 MIO12))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 MIO11))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 MIO46))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 MIO47))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 MIO49))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 MIO51))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 MIO15))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 MIO10))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 MIO13))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 MIO14))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 MIO0))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 MIO48))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5B5A36F3)
    (at 124.079 65.659 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value USB_OTG_Breakout (at -2.5146 5.9182 180) (layer F.SilkS))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 USB_ID))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 USB_OTG_P))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 USB_OTG_N))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 USB_VBUS_OTG))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 USB_OTG_CPEN))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 5B5A3C3B)
    (at 84.963 104.013)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "IO_L Breakout" (at 2.1844 18.6817 90) (layer F.SilkS))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 IO_L16_33_JX1_P))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 IO_L16_33_JX1_N))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 IO_L18_33_JX1_P))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 IO_L18_33_JX1_N))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 IO_L20_33_JX1_P))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 IO_L20_33_JX1_N))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 IO_L22_33_JX1_P))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 IO_L22_33_JX1_N))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 IO_L01_33_JX1_P))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 IO_L01_33_JX1_N))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module breakoutBoard:Cysized (layer F.Cu) (tedit 0)
    (at 119.888 113.0046)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_line (start 151.4983 62.865) (end 151.511 63.4111) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.058 62.865) (end 151.4983 62.865) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.1469 163.322) (end 83.058 62.865) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.6475 163.322) (end 83.1469 163.322) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.3427 163.322) (end 100.6094 163.322) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.9827 163.322) (end 140.5128 163.322) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.511 163.322) (end 151.511 63.373) (layer Edge.Cuts) (width 0.15))
  (gr_text "CySat 1 - SDR Breakout Board" (at 149.098 112.395 90) (layer F.SilkS))
  (gr_text JX3 (at 104.14 68.453) (layer F.SilkS))
  (gr_text JX4 (at 103.886 152.908) (layer F.SilkS))
  (gr_text JX2 (at 145.542 137.16 90) (layer F.SilkS))
  (gr_text JX1 (at 93.218 130.81 90) (layer F.SilkS))
  (gr_line (start 151.5618 163.3222) (end 140.97 163.3222) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.408))
    (min_thickness 0.08)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.716 146.05) (xy 140.716 148.082) (xy 100.584 148.082) (xy 100.584 145.923) (xy 140.716 145.923)
        (xy 140.716 146.177)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.408))
    (min_thickness 0.08)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.441 134.239) (xy 97.409 134.239) (xy 97.409 93.98) (xy 99.441 93.98)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.408))
    (min_thickness 0.08)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.716 74.676) (xy 100.584 74.676) (xy 100.584 72.644) (xy 140.716 72.644)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.408))
    (min_thickness 0.08)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.891 134.112) (xy 141.732 134.112) (xy 141.732 93.98) (xy 143.891 93.98)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.208))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.3713 163.1696) (xy 151.3713 62.992) (xy 83.2104 62.992) (xy 83.2104 163.1696) (xy 100.4443 163.1696)
        (xy 100.4443 160.2232) (xy 100.2157 160.2232) (xy 100.2157 159.9819) (xy 100.8126 159.9819) (xy 100.8126 169.9133)
        (xy 140.335 169.9133) (xy 140.335 159.9692) (xy 140.9446 159.9692) (xy 140.9446 160.2613) (xy 140.716 160.2613)
        (xy 140.716 163.1823) (xy 151.3713 163.1823)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.208))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.3713 163.1696) (xy 151.3713 62.992) (xy 83.2104 62.992) (xy 83.2104 163.1696) (xy 100.4443 163.1696)
        (xy 100.4443 160.2232) (xy 100.2157 160.2232) (xy 100.2157 159.9819) (xy 100.8126 159.9819) (xy 100.8126 169.9133)
        (xy 140.335 169.9133) (xy 140.335 159.9692) (xy 140.9446 159.9692) (xy 140.9446 160.2613) (xy 140.716 160.2613)
        (xy 140.716 163.1823) (xy 151.3713 163.1823)
      )
    )
  )
)
