(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 105)
    (zones 0)
    (modules 32)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.1)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.4 6.4)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VREF)
  (net 3 /VDD)
  (net 4 /IN+)
  (net 5 /OUT+)
  (net 6 /IN-)
  (net 7 /OUT-)
  (net 8 /OUT_SS)
  (net 9 /OUT_HPF)
  (net 10 /VBAT)
  (net 11 "Net-(C4-Pad1)")
  (net 12 "Net-(C6-Pad1)")
  (net 13 "Net-(R5-Pad1)")
  (net 14 "Net-(R10-Pad2)")
  (net 15 "Net-(R13-Pad2)")
  (net 16 "Net-(R8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /IN+)
    (add_net /IN-)
    (add_net /OUT+)
    (add_net /OUT-)
    (add_net /OUT_HPF)
    (add_net /OUT_SS)
    (add_net /VBAT)
    (add_net /VDD)
    (add_net /VREF)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R8-Pad1)")
  )
  (module Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal (layer F.Cu) (tedit 5B7745C6)
    (at 42 19.5 180)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J3 (at 1 -2.55) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1 7.45) (layer F.Fab))
    (fp_text user %R (at 1 2.5) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /VBAT))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 22.35 37 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -3 -0.8) (layer F.SilkS))
    (fp_text value 10G (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 6 /IN-))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 /OUT-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 23.6 23 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -3.25 -0.1) (layer F.SilkS))
    (fp_text value 10G (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 /IN+))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 5 /OUT+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 42 31.5 270)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J4 (at 0 -5.2 90) (layer F.SilkS))
    (fp_text value BNC (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 /OUT_HPF))
    (pad 2 thru_hole oval (at 5.08 -5.08 270) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08 270) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 52.5 42)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 14.5 15.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 52.5 15.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 14.5 42)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Button_Switch_THT:SW_DIP_SPSTx01_Slide_6.7x4.1mm_W7.62mm_P2.54mm_LowProfile (layer F.Cu) (tedit 5A4E1404)
    (at 34.74 15.5 180)
    (descr "1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile")
    (tags "DIP Switch SPST Slide 7.62mm 300mil LowProfile")
    (fp_text reference SW1 (at 10.44 0.8) (layer F.SilkS))
    (fp_text value SW_SPST (at 3.81 3.11) (layer F.Fab))
    (fp_text user on (at 4.485 -1.3425) (layer F.Fab))
    (fp_text user %R (at 6.39 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /VBAT))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx01_Slide_6.7x4.1mm_W7.62mm_P2.54mm_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 18.27 20.36 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.01 -0.01) (layer F.SilkS))
    (fp_text value 100n (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 14.69 22.42)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.19 0.08) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 2 /VREF))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 14.66 20.37 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.16 -0.06) (layer F.SilkS))
    (fp_text value 100n (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VREF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 18.29 22.42)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.23 0.17) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 3 /VDD))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 2 /VREF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 18.28 18.3 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.68 -0.02) (layer F.SilkS))
    (fp_text value 1u (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 31.92 32.78 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at -0.03 -1.88 90) (layer F.SilkS))
    (fp_text value LTC6241 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /OUT_SS))
    (pad 6 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R13-Pad2)"))
    (pad 5 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R8-Pad1)"))
    (pad 4 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDD))
    (pad 3 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R10-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R5-Pad1)"))
    (pad 1 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_DIP_SPSTx01_Slide_6.7x4.1mm_W7.62mm_P2.54mm_LowProfile (layer F.Cu) (tedit 5A4E1404)
    (at 30.21 41.27)
    (descr "1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile")
    (tags "DIP Switch SPST Slide 7.62mm 300mil LowProfile")
    (fp_text reference SW2 (at 5.21 -3.15) (layer F.SilkS))
    (fp_text value SW_SPST (at 3.81 3.11) (layer F.Fab))
    (fp_text user on (at 4.485 -1.3425) (layer F.Fab))
    (fp_text user %R (at 6.39 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /OUT_SS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx01_Slide_6.7x4.1mm_W7.62mm_P2.54mm_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 27.1025 41.27 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.7625 -0.1) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 12 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 15 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 22.335 29.955 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -0.075 -2.085 90) (layer F.SilkS))
    (fp_text value LTC6241 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /OUT-))
    (pad 6 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /IN-))
    (pad 5 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VREF))
    (pad 4 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDD))
    (pad 3 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VREF))
    (pad 2 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /IN+))
    (pad 1 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /OUT+))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 31.91 37.56 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 2.68 -0.11) (layer F.SilkS))
    (fp_text value 90k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 15 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 8 /OUT_SS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.87 32.43)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.9 0.15) (layer F.SilkS))
    (fp_text value 200k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 14 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 27.12 43.35)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.89 0.03) (layer F.SilkS))
    (fp_text value 100n (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical (layer F.Cu) (tedit 5A1DBFC3)
    (at 17.22 33.43 180)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference J2 (at 3.025 0.025 270) (layer F.SilkS))
    (fp_text value U.FL (at 0.475 3.2) (layer F.Fab))
    (fp_text user %R (at 0.475 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.475 -1.475 180) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 /VREF))
    (pad 1 smd rect (at -1.05 0 180) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /IN-))
    (pad 2 smd rect (at 0.475 1.475 180) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 /VREF))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (offset (xyz 0.4749999928262157 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical (layer F.Cu) (tedit 5A1DBFC3)
    (at 17.22 26.48 180)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference J1 (at 2.975 0.075 270) (layer F.SilkS))
    (fp_text value U.FL (at 0.475 3.2) (layer F.Fab))
    (fp_text user %R (at 0.475 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.475 -1.475 180) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 /VREF))
    (pad 1 smd rect (at -1.05 0 180) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /IN+))
    (pad 2 smd rect (at 0.475 1.475 180) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 /VREF))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (offset (xyz 0.4749999928262157 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 22.32 34.78 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -2.68 -1.22) (layer F.SilkS))
    (fp_text value 2p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 6 /IN-))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 /OUT-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 23.58 25.13 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -3.03 0.28) (layer F.SilkS))
    (fp_text value 2p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 4 /IN+))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 /OUT+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 38.13 33.17 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -3.31 0.12 90) (layer F.SilkS))
    (fp_text value 200 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 11 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 9 /OUT_HPF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 38.23 29.57 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -3.75 -0.04 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 11 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.87 30.38)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0.05 -1.35) (layer F.SilkS))
    (fp_text value 200k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 14 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 3 /VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 30.5325 27.48 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.8875 0.05) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 13 "Net-(R5-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 16 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.87 34.43 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1.4 -1.4) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 7 /OUT-))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 14 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.87 27.48 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -0.15 1.35) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 5 /OUT+))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 13 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 36.16 33.2 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.86 -0.21 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /OUT_SS))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Differential charge amplifier v1.0\nayeiser@mit.edu" (at 29 34 180) (layer B.SilkS))
  (gr_arc (start 52.5 15.5) (end 55 15.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 52.5 42) (end 52.5 44.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 14.5 42) (end 12 42) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 14.5 15.5) (end 14.5 13) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 52.5 44.5) (end 14.5 44.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55 15.5) (end 55 42) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 14.5 13) (end 52.5 13) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 12 42) (end 12 15.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 21.57 28.98) (xy 21.57 27.23) (xy 21.82 27.23) (xy 21.82 28.73) (xy 23.47 28.73)
        (xy 23.45 21.4025) (xy 20.75 21.3975) (xy 20.75 24.725) (xy 15.67 24.73) (xy 15.67 24.48)
        (xy 20.5 24.475) (xy 20.5 21.1475) (xy 23.72 21.1525) (xy 23.72 28.98)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 15.67 28.48) (xy 15.67 24.53) (xy 15.92 24.53) (xy 15.92 28.48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 21.57 27.38) (xy 21.57 26.28) (xy 21.17 25.83) (xy 20.12 25.83) (xy 19.55 26.325)
        (xy 19.55 27.575) (xy 18.77 28.48) (xy 15.67 28.48) (xy 15.67 28.23) (xy 18.67 28.23)
        (xy 19.3 27.5) (xy 19.3 26.2) (xy 19.97 25.58) (xy 21.27 25.58) (xy 21.82 26.18)
        (xy 21.82 27.38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 15.67 35.434976) (xy 15.67 31.484976) (xy 15.92 31.484976) (xy 15.92 35.434976)
      )
    )
  )
  (zone (net 2) (net_name /VREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 19.045 38.9) (xy 19.0525 35.46) (xy 15.5475 35.44) (xy 15.57 24.43) (xy 20.5 24.43)
        (xy 20.5 21.15) (xy 23.72 21.15) (xy 23.72 29.48) (xy 22.47 30.73) (xy 22.45 38.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 20.32 30.93) (xy 20.32 32.68) (xy 20.57 32.68) (xy 20.57 31.18) (xy 22.22 31.18)
        (xy 22.2 38.65) (xy 19.3 38.65) (xy 19.3 35.15) (xy 15.65 35.15) (xy 15.65 35.45)
        (xy 19.05 35.45) (xy 19.05 38.9) (xy 22.45 38.9) (xy 22.47 30.93)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 20.3 32.55) (xy 20.3 33.6) (xy 20.15 33.75) (xy 19.75 33.75) (xy 19.55 33.55)
        (xy 19.55 32.25) (xy 18.75 31.45) (xy 15.65 31.45) (xy 15.65 31.7) (xy 18.65 31.7)
        (xy 19.3 32.35) (xy 19.3 33.65) (xy 19.65 34) (xy 20.25 34) (xy 20.55 33.7)
        (xy 20.55 32.55)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 55 44.5) (xy 12 44.5) (xy 12 13) (xy 55 13)
      )
    )
  )
)
