<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.32" y2="0" width="0" layer="20"/>
<wire x1="20.32" y1="0" x2="20.32" y2="27.94" width="0" layer="20"/>
<wire x1="20.32" y1="27.94" x2="0" y2="27.94" width="0" layer="20"/>
<wire x1="0" y1="27.94" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="NS73M FM Transmitter Breakout">
<description>Generated from &lt;b&gt;NS73M FM Transmitter Breakout.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="EAGLE-LIBRARY-ENGR-245-S22_NS73M">
</package>
</packages>
</library>
<library name="AB26T-32.768KHZ-E">
<packages>
<package name="XTAL_AB26T-32.768KHZ-E">
</package>
</packages>
</library>
<library name="EEEFK1A560SR">
<packages>
<package name="CAP_EEEFK1A560SR">
</package>
</packages>
</library>
<library name="ESR10EZPF1001">
<packages>
<package name="RESC2012X65N">
</package>
</packages>
</library>
<library name="HTSW-108-08-T-S-RA">
<packages>
<package name="SAMTEC_HTSW-108-08-T-S-RA">
</package>
<package name="ANTENNA">
</package>
</packages>
</library>
<library name="GCM2195C1K103FA16D">
<packages>
<package name="CAPC2012X95N">
</package>
</packages>
</library>
<library name="CMA-4544PF-W">
<packages>
<package name="MIC_CMA-4544PF-W">
</package>
</packages>
</library>
<library name="ERJP06J103V">
<packages>
<package name="RES_ERJP06J103V">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="NS73M FM Transmitter Breakout" package="EAGLE-LIBRARY-ENGR-245-S22_NS73M" value="EAGLE-LIBRARY-ENGR-245-S22_NS73M">
<attribute name="NAME"/>
</element>
<element name="Y1" library="AB26T-32.768KHZ-E" package="XTAL_AB26T-32.768KHZ-E" value="AB26T-32.768KHZ-E">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 32.768kHz WATCH CRYSTAL, 6.2 x 02.1MM CYLINDER PACKAGE "/>
<attribute name="MF" value="Abracon LLC"/>
<attribute name="MP" value="AB26T-32.768KHZ-E"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="Radial Abracon LLC"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/AB26T-32.768KHZ-E/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="EEEFK1A560SR" package="CAP_EEEFK1A560SR" value="EEEFK1A560SR">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" CAP ALUM 56UF 20% 10V SMD "/>
<attribute name="MF" value="Panasonic Electronic Components"/>
<attribute name="MP" value="EEE-FK1A560SR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="RADIAL-2 Panasonic"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/EEE-FK1A560SR/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="HTSW-108-08-T-S-RA" package="SAMTEC_HTSW-108-08-T-S-RA" value="HTSW-108-08-T-S-RA">
<attribute name="MANUFACTURER" value="Samtec"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="R"/>
<attribute name="STANDARD" value="Manufacturer Recommendations"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="HTSW-108-08-T-S-RA" package="ANTENNA" value="ANTENNA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="GCM2195C1K103FA16D" package="CAPC2012X95N" value="GCM2195C1K103FA16D">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" SMD capacitor C0G(EIA) with capacitance 10000pF Tol.1%. Rated voltage 80Vdc 125C "/>
<attribute name="MF" value="Murata"/>
<attribute name="MP" value="GCM2195C1K103FA16D"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 Murata"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/GCM2195C1K103FA16D/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="MK1" library="CMA-4544PF-W" package="MIC_CMA-4544PF-W" value="CMA-4544PF-W">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="CUI_PURCHASE_URL" value="https://www.cuidevices.com/product/audio/microphones/electret-condenser-microphones/cma-4544pf-w?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value=" 9.7 mm, Omnidirectional, PCB Mount, 3.0 Vdc, Electret Condenser Microphone "/>
<attribute name="MF" value="CUI Devices"/>
<attribute name="MP" value="CMA-4544PF-W"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/CMA-4544PF-W/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ESR10EZPF1001" package="RESC2012X65N" value="ESR10EZPF1001">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 1 kOhms ±1% 0.4W, 2/5W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film "/>
<attribute name="MF" value="Rohm"/>
<attribute name="MP" value="ESR10EZPF1001"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 Rohm Semiconductor"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/ESR10EZPF1001/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ESR10EZPF1001" package="RESC2012X65N" value="ESR10EZPF1001">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 1 kOhms ±1% 0.4W, 2/5W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film "/>
<attribute name="MF" value="Rohm"/>
<attribute name="MP" value="ESR10EZPF1001"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 Rohm Semiconductor"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/ESR10EZPF1001/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="ERJP06J103V" package="RES_ERJP06J103V" value="ERJP06J103V">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 10 kOhms ±5% 0.5W, 1/2W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film  "/>
<attribute name="MF" value="Panasonic Electronic"/>
<attribute name="MP" value="ERJ-P06J103V"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012-2 Panasonic"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/ERJ-P06J103V/?ref=eda"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="11"/>
<contactref element="Y1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="01"/>
<contactref element="MK1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="07"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RFO">
<contactref element="U1" pad="15"/>
<contactref element="J2" pad="01"/>
</signal>
<signal name="TEB">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="03"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="04"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="05"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="10"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="MK1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="AUDIO">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
