<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<text>I CAN
REFLOW!</text>
<circle x="25.4" y="25.4" radius="25.4" width="0.254" layer="20"/>
<hole x="25.4" y="47.625" drill="4.7625"/>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="CR1220">
<packages>
<package name="CR1220-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="Q2" library="transistor" package="SOT23-BEC" value="MMBT3904">
<attribute name="NAME"/>
</element>
<element name="Q1" library="transistor" package="SOT23-BEC" value="MMBT3904">
<attribute name="NAME"/>
</element>
<element name="U$1" library="CR1220" package="CR1220-SMD" value="CR1220-SMD"/>
</elements>
<signals>
<signal name="GND">
<contactref element="Q2" pad="E"/>
<contactref element="Q1" pad="E"/>
<contactref element="U$1" pad="CENTER"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="LEFT"/>
<contactref element="U$1" pad="RIGHT"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="Q2" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="B"/>
</signal>
<signal name="N$6">
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="Q2" pad="B"/>
</signal>
<signal name="N$7">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="1"/>
<contactref element="Q1" pad="C"/>
<contactref element="C2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
